> Safety, Electrical, and Environmental Certifications
> This chapter lists FCC warnings, as well as safety, electrical and environmental certifications for the ASR 5000 system.
> Federal Communications Commission Warning
> The ASR 5000 complies with the limits for a Class A digital device, pursuant to Part 15 of the FCC Rules and Regulations. Operation is subject to the following two conditions:

> • | This device must not cause harmful interference.

> • | This device must withstand any interference received, including interference that may cause undesired operation.

> These limits provide reasonable protection against harmful interference when this equipment is operated in a commercial environment. This equipment generates, uses, and can radiate radio-frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio and television communications. Operation of this equipment in a residential area is likely to cause interference, in which case your organization is responsible for the expenses incurred to correct the interference.
> ICS Notice
> This Class A digital apparatus complies with Canadian ICES-003.
> Cet appareil numérique de la classe A est conforme à la norme NMB-003 du Canada.
> Laser Notice
> The lasers in this equipment are Class 1 devices. Class 1 laser devices are not considered to be hazardous.
> Safety Certifications
> The ASR 5000 complies with all safety certifications listed below.

> • | UL60950 - Standard for Safety for Information Technology Equipment, 3rd Edition

> • | European Union EN 60950 (CE Mark)

> Electrical Certifications
> The ASR 5000 complies with all electrical certifications listed below.

> • | Telcordia GR-1089-Core, Network Equipment-Building System (NEBS) Requirements: Electromagnetic Compatibility and Electrical Safety Criteria for Network Telecommunication Equipment

> • | FCC, Part 15 B, Class A Requirements for Non-residential Equipment

> • | ETSI EN 300 019

> • | ETSI 300 386

> • | ETSI/EN 300 386-2 Electrical Fast Transients

> • | SBC TP76200MP

> • | Taiwan - BMSI

> Environmental Certifications
> The ASR 5000 complies with all environmental certifications listed below.

> • | Telcordia GR-63-Core, Network Equipment-Building System (NEBS) Requirements: Physical Protection

> • | The chassis equipped with the 165A PFU is compliant to the European Union’s RoHS Directive (Directive 2002/95/EC)

> • | Waste Electrical and Electronic Equipment (WEEE) Directive 2002/96/EC

> Acoustic Noise
> The maximum acoustic noise level for the ASR 5000 chassis is 76 dBA.
> Caution: The maximum acoustic noise level of the ASR 5000 exceeds 70 dBA.
> Caution: Maschinenlärminformations-Verordnung - 3. GPSGV, der höchste Schalldruckpegel beträgt 76 dB(A) gemäss EN ISO 7779.
> Electromagnetic Compatibility (EMC) Compliance
> Electromagnetic compatibility is the ability of electronic devices to operate as intended in proximity to other electronic devices or in the presence of electromagnetic fields. Unintentional radio frequency emissions from an electronic device and immunity of the device to radio frequency interference from other electromagnetic sources are included within electromagnetic compatibility.
> Japan VCCI-A
> The ASR 5000 has been registered for compliance with the Voluntary Council for Control of Interference, VCCI.
> Korean EMC
> Class A device (Broadcasting Communication Device for Office Use): This device obtained EMC registration for office use (Class A), and may be used in places other than home. Sellers and/or users need to take note of this.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883