> ACS IMSI Pool Configuration Mode Commands
> The ACS IMSI Pool Configuration Mode is used to define pool of subscriber’s International Mobile Station Identifier numbers within the ACS Configuration Mode. IMSI pool configuration facilitates creation of rules to handle the packets coming from or going to a group of subscriber of IMSI numbers within an access policy.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> This command exits the current configuration mode and returns to the Executive mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to change to the Executive mode.
> exit
> This command exits the current configuration mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> imsi
> This command specifies an individual or a range of subscriber IMSI numbers to add to the IMSI pool.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imsi { imsi_num | range start_imsi to end_imsi }
> no
> Removes the specified subscriber IMSI number(s) that were configured previously from this IMSI pool.
> imsi_num
> Specifies an individual subscriber IMSI number to add to this IMSI pool.
> imsi_num is the IMSI number, and must be a sequence of hexadecimal digits between 1 and 15.
> range start_imsi to end_imsi
> Specifies a range of subscriber IMSI numbers to add to this IMSI pool.
> start_imsi must be a sequence of hexadecimal numbers between 1 and 15 digits. This is the start IMSI number of subscriber IMSI range and must be less than end_imsi.
> end_imsi must be a sequence of hexadecimal numbers between 1 and 15 digits. This is the end IMSI number of subscriber IMSI range and must be greater than start_imsi.
> Usage
> Use this command to specify the individual or range of subscriber IMSI numbers in an IMSI pool. Up to 10 sets of IMSI numbers can be configured in each IMSI pool.
> Example
> The following command adds the specified range of IMSI numbers to the IMSI pool:
> imsi range <start_imsi> to <end_imsi>

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883