> show multicast-sessions
> This chapter includes the show multicast-sessions command output tables.
> show multicast-sessions all
> show multicast-sessions all Command Output Descriptions

> Field | Description
> vvvvv | Displays service and session state information. This column provides a code consisting of three characters. From left-to-right, the first character represents the Session Type that the subscriber is using. The possible sessopm types are:
> • | B: BCMCS
> • | M: MBMS Multicast
> • | R: MBMS Broadcast
> From left-to-right, the second character represents the Framing Type. The possible framing types are:
> • | H: HDLC Like
> • | S: Segment Based
> • | x: Not Applicable
> From left-to-right, the third character represents the Flow Type. The possible flow types are:
> • | F: Flow
> • | P: Program
> • | u: Unknown
> From left-to-right, the fourth character represents the Call State of the session. The possible call states are:
> • | C: Connected
> • | c: Connecting
> • | D: Disconnecting
> • | u: Unknown
> From left-to-right, the fifth character represents the Link Status of the session. The possible idle states are:
> • | A: Online/Active
> • | D: Dormant/Idle
> CALLID | Displays the subscriber’s call identification (callid) number.
> FLOW ID | Displays the flow identification for multicast service session.
> MCAST ADDR | Displays the IP address of Broadcast Multicast service center.
> APN/PORT | Displays the APN name or port number through which the multicast services is provided.
> PEER ADDR | Displays the IP address of Access Gateway to which the subscriber is attached.
> TIME-IDLE | Displays the amount of time that the subscriber session has been idle either in an active or dormant state.

> ‌
> show multicast-sessions full all
> show multicast-sessions full all Command Output Descriptions

> Field | Description
> Flow Id | Hex value indicating the Flow ID.
> state | Indicates the status of session. The possible status are:
> • | Connected
> • | Connecting
> • | Disconnecting
> • | Unknown
> Access Type | Indicates the access type of broadcast-multicast service. Possible values are:
> • | mbms-bearer: access through MBMS bearer context
> • | mbms-ue: access through MBMS UE context
> Flow ID Type | Indicates the Flow ID type.
> callid | Displays the call identification number (callid).
> connect time | Displays the time of connection starts.
> call duration | Specifies total duration of call session in hh:mm:ss format
> idle time | Displays the amount of time that the multicast session has been idle either in an active or dormant state.
> idle time left | Shows the amount of idle time left before timeout.
> session time left | How much session time is left for the specified multicast session.
> Multicast ip address | The IP address of the interface in the session.
> peer address | The IP address of the peer in the session.
> source context | Specifies the name of a configured source context from which the session was initiated.
> destination context | Specifies the name of a configured destination context through which the subscribers are provided access to the packet data network.
> output pkts | Indicates the number of packets transmitted.
> output bytes | Indicates the number of bytes transmitted.
> outputs pkts dropped | Indicates the number of packets that were dropped while receiving data for this multicast session.
> pk rate to peer (bps) | The peak data rate, in bits per second, obtained for data sent from the subscriber to the network during the last sampling period.
> pk rate to peer (pps) | The peak data rate, in packets per second, obtained for data received from the network by the subscriber during the last sampling period.
> ave rate to peer (bps) | The average data rate, in bits per second, obtained for data received from the network by the subscriber during the last sampling period.
> ave rate to peer (pps) | The average data rate, in packets per second, obtained for data received from the network by the subscriber during the last sampling period.
> sust rate to peer (bps) | The mean data rate, in bits per second, obtained for data received from the network by the subscriber during the last three sampling periods.
> sust rate to peer (pps) | The mean data rate, in packets per second, obtained for data received from the network by the subscriber during the last three sampling periods.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883