> Installation Procedure Overview
> This chapter briefly describes the steps and tools that are required for the physical installation of the chassis.
> Chassis Components
> The following graphic and table illustrate the chassis and describe its subcomponents:
> The Chassis and Its Sub-components
> Chassis and Sub-component Identification Key

> Item | Description
> 1 | Chassis: Supports 16 front-loading slots for application cards and 32 rear-loading slots for line cards. The chassis ships with blanking panels over every slot except the following: 1, 8, 17, and 24. These are intentionally left uncovered for the initial installation of system components.
> 2 | Mounting brackets: Supports installation in a standard 19-inch rack or telecommunications cabinet. Standard and mid-mount options are supported. In addition, each bracket contains an electro-static discharge jack for use when handling equipment.
> 3 | Upper fan tray: Draws air up through the chassis for cooling and ventilation and exhausts the air through the vents at the upper-rear of the chassis.
> 4 | Upper bezel: Covers the upper fan tray bay.
> 5 | Lower fan tray cover: Secures the lower fan tray assembly. The cover also provides an air baffle allowing air to enter into the chassis.
> 6 | Lower bezel: Covers the lower fan tray bay.
> 7 | Lower fan tray assembly: Draws air into the chassis through the chassis' front and sides for cooling and ventilation. It is equipped with a particulate air filter to prevent dust and debris from entering the system.
> 8 | Power Filter Units (PFUs): Each of the system’s two 165 amp PFUs provides -48 VDC power to the chassis and its associated cards. Each load-sharing PFU operates independently from the other to ensure maximum power feed redundancy.

> ‌
> Installation at a Glance
> The list below summarizes the installation process for the chassis.

> • | Unpack the chassis and cards

> • | Determine which chassis mounting option to use: standard or mid-mount.

> • | Install the chassis into a standard 19-inch equipment rack or telecommunications cabinet.

> • | Connect the chassis to earth ground.

> • | Install application cards into the front of the chassis.

> • | Install line cards into the rear of the chassi.s

> • | Connect data cables to the line cards.

> • | Connect power cables to the chassis.

> • | Apply power to the chassis.

> • | Verify that the installation was successful.

> Once the installation has been validated, you will be directed to the Administration and Configuration Reference that provides instructions on how to configure the system for operation.
> Required Tools and Equipment
> This section lists the tools and equipment needed for installation.
> Hand Tools
> The following hand tools are required for installation of the chassis, application and line cards, fan tray assemblies, and power filter units:

> • | Phillips #1 and #2 screwdrivers. Used to tighten thumb-screws on cards, fan tray assemblies, PFUs, and mounting brackets.

> • | 9/16-inch nut driver or ratchet and socket set. Used to connect power and return cables.

> • | 3/8-inch nut driver or ratchet and socket set. Used to connect grounding cables.

> • | Grounding wrist and/or heel straps. Used to prevent Electro-Static Discharge (ESD) as discussed in the Protecting Against Electro-static Discharge section that follows.

> Equipment
> The following equipment is necessary to install the chassis and verify that it is ready for configuration:

> • | Standard 19-inch (48.26 cm) equipment rack or telecommunications cabinet with mounting hardware (Additional hardware, such as extension brackets (not supplied), may be used to install the chassis in a standard 23-inch (58.42 cm) cabinet or rack.)

> • | DC power supply capable of providing Between -40 and -60 VDC @ 145 amps for the ASR 5000 chassis.

> • | Console cable supplied with the Switch Processor I/O (SPIO) line card.

> • | A computer or terminal server with a 9-pin RS-232C serial port, or 25-to-9-pin male RS-232C adapter. It will be connected to the SPIO's Console port for accessing the command line interface (CLI) for initial system configuration.

> Protecting Against Electro-static Discharge
> Electro-Static Discharge (ESD) can cause serious damage to the chassis, its sub-components, and/or the cards installed in the chassis. To prevent damage from ESD, you must take proper grounding precautions before handling the chassis or any of its components.
> To aid in the prevention of ESD damage, the chassis and its mounting brackets are equipped with ESD jacks. Use the jacks in conjunction with grounding wrist straps when handling the chassis and/or its components. The following figure shows the location of the jacks.
> Important: Before the ESD you use the jacks on the chassis and its mounting brackets to provide ESD protection, you must first connect the chassis to earth ground as described in the Chassis Installation chapter of this document.
> Chassis ESD Plug Locations
> Federal Communications Commission Warning
> This device complies with the limits for a Class A digital device, pursuant to Part 15 of the FCC Rules and Regulations. Operation is subject to the following two conditions:

> • | This device may not cause harmful interference.

> • | This device must withstand any interference received, including interference that may cause undesired operation.

> The system platform has been tested and found to comply with the limits for a Class A digital device pursuant to Part 15 of the FCC Rules and Regulations. These limits are designed to provide reasonable protection against harmful interference when this equipment is operated in a commercial environment. This equipment generates, uses, and can radiate radio-frequency energy and, if not installed and used in accordance with the instruction manual, may cause harmful interference to radio and television communications. Operation of this equipment in a residential area is likely to cause interference in which case the user will be required to correct the interference at his or her own expense.
> Shielded cables must be used with this unit to ensure compliance with the FCC Class A limits.
> ICS Notice
> This Class A digital apparatus complies with Canadian ICES-003.
> Cet appareil numérique de la classe A est conforme à la norme NMB-003 du Canada.
> Laser Notice
> The lasers in this equipment are Class 1 devices. Class 1 laser devices are not considered to be hazardous.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883