> CSCF URN List Configuration Mode Commands
> The CSCF URN List Configuration Mode is used to map URNs to URIs for emergency and local call services.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> cscf-urn-service-mapping
> Adds an entry to the service URN mapping table that maps uniform resource names (URNs) to URIs in order to direct specific service-oriented identifiers to the proper location in a network. The table is used after CSCF translation if the result is a local service.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> [ no ] cscf-urn-service-mapping urn urn uri uri
> no
> Removes an entry from the service URN mapping table.
> urn urn
> Specifies the URN to be routed via a URL to the appropriate destination. urn must be from 1 to 79 alpha and/or numeric characters.
> uri uri
> Specifies the URI used to route the URN to the appropriate location. uri must be from 1 to 79 alpha and/or numeric characters.
> Usage
> Use this command to add an entry to the service URN mapping table that routes a translated URN to a URI for local services.
> Important: Service URN mapping tables are limited to 30 URN to URI mapping entries.
> Example
> The following command map URN business to URI corp@123.45.678.9:5020 and adds it to the service URN mapping table:
> cscf-urn-service-mapping urn business uri corp@123.45.678.9:5020
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883