> GPRS Service Configuration Mode Commands
> The GPRS Service Configuration Mode is used within the context configuration mode to define the criteria the SGSN needs to operate within a GPRS network. The GPRS Service works with other services, such as SGSN GPRS Tunneling Protocol (see SGTP Service Configuration Mode Commands) and Mobile Application Part (see MAP Service Configuration Mode Commands), to handle communication parameters required to work with other network entities such as the base station subsystem (BSS).
> The prompt for this mode appears as:
> [context_name]hostname(config-gprs-service)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> accounting
> Defines the accounting context name and enables/disables specific types of CDR generation for the accounting in the GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> accounting { cdr-types { mcdr | scdr | sms { mo-cdr | mt-cdr } + | context cntx_name }
> default accounting cdr-types
> no accounting ( cdr-types | context }
> default
> Returns the system to default CDR generation which includes M-CDR, S-CDR, and SMS CDRs.
> no
> Disables all CDR types.
> cdr-types { mcdr | scdr | sms { mo-cdr | mt-cdr }
> Default: all types enabled.
> Defines the types of CDRs to be generated within the specified GPRS service for accounting:

> • | mcdr: Enables generation of M-CDRs.

> • | scdr: Enables generation of S-CDRs.

> • | sms: Enables generation of SMS-type CDRs based on one of the following:

> • | mo-cdr: SMS CDRs originates from the mobile.

> • | mt-cdr: SMS CDRs terminates at the mobile.

> +
> This symbol indicates that more than one keyword can be used and repeated. This enables you to include more than one type of CDR selection in a single command.
> context cntx_name
> Specifies an accounting context to be associated with the GPRS service.
> cntx_name: Define a string of 1 to 79 alphanumeric characters.
> Usage
> Use this command to define the type of CDRs to generate for GPRS service. By default all types of CDRs are generated. Note that change of this configuration will be applied to new calls and/or to new PDP contexts only.
> By default, generation of the S-CDR, M-CDR, SMS-MT-CDR, and SMS MO-CDR types is enabled.
> Example
> The following command configures the system to generate only M-CDRs for accounting in the current GPRS service:
> accounting cdr-types mcdr
> admin-disconnect-behavior
> This command defines some of the actions the SGSN will take during an Admin-Disconnect procedure.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> admin-disconnect-behavior { clear-subscription | detach-type { reattach-not-required | reattach-required } }
> default admin-disconnect-behavior { clear-subscription | detach-type }
> clear-subscription
> Including this keyword in the configuration instructs the SGSN to clear subscriber contexts and the subscription data database whenever the clear subscribers all command is issued (from the Exec mode) for attached subscribers. As well, the SGSN will issue an appropriate Map-Purge-MS-Req to the HLR if needed.
> Default: disabled
> detach-type
> Including this keyword defines which type of detach instruction to include in the Detach-Request message during an Admin-Disconnect procedure. One of the following options must be included when this command is entered:

> • | reattach-not-required

> • | reattach-required

> Default: reattach-required
> default
> Including the default keyword in the command, instructs the SGSN to use the default value for the specified parameter.
> no
> Returns the SGSN to the default where this clear function is disabled
> Usage
> Using he clear subscribers all command (in the Exec Mode) will clear subscriber contexts and the subscription data database, and if needed, issue an appropriate Map-Purge-MS-Req to the HLR.
> Include the clear-subscription keyword with this command configuration to ensure that more than attached MM-context and active PDP-contexts are cleared when the clear subscribers all command is issued for attached subscribers.
> To clear subscription data for detached subscribers, refer to the sgsn clear-detached-subscriptions command described in the Exec mode chapter.
> Including the detach-type keyword with this command instructs the SGSN to include either a ‘reattach-required’ or a ‘reattach-no-required’ instruction in the Detach-Request message.
> Example
> Enable the clearing function so that subscription data is cleared from the HLR database:
> admin-disconnect-behavior clear-subscription
> associate-dscp-template
> Identifies a DSCP template to be associated with the GPRS service.
> Important: This command can be used before the associated DSCP template instance is created and configured but care should be used to match the template names.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> associate-dscp-template downlink template_name
> no associate-dscp-template downlink
> no
> Removes the template association definition from the configuration.
> template_name
> Specifies a unique DSCP template to associate with this GPRS service.
> template_name must be a string of 1 to 64 alphanumeric characters with dots (.), dashes (-), and forward slashes (/) but with no spaces.
> Usage
> Use this command to associate DSCP templates with this GPRS service. A single template can be associated with multiple GPRS services.
> Related commands:

> • | The dscp-template command in the SGSN Global configuration mode creates / deletes an instance of a template. This command also provides access to the mode containing all the configuration commands used to define DSCP settings for the control packets and data packets for a particular GPRS service (see the DSCP Template Configuration Mode Commands section).

> • | To check the list of DSCP templates configured, use the show sgsn-mode command documented in the Exec Mode Commands section.

> Example
> The following command associates the template with DSCP settings for traffic going through one of the SGSNs located in Paris mobile network:
> associate-dscp-template dscp-template-paris3
> associate-service
> Identifies services to be associated with the GPRS Service.
> Important: This command can be used before the associated service instance is created and configured but care should be used to match the service names.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] associate-service { gs name | map name | sgtp name } [ context ctxt_name ]
> no
> Removes the service association definition from the configuration.
> gs name
> Specifies the Gs service configuration to associate with this GPRS service.
> name must be a string of 1 to 63 alphanumeric characters with no spaces.
> map name
> Specifies the MAP service configuration to associate with this GPRS service.
> name must be a string of 1 to 63 alphanumeric characters with no spaces.
> sgtp name
> Specifies the SGTP service configuration to associate with this GPRS service.
> name must be a string of 1 to 63 alpha numeric characters with no spaces.
> context ctxt_name
> Defines the context in which the service was created.
> ctxt_name must be a string of 1 to 63 alphanumeric characters with no spaces.
> Usage
> Use this command to associate other services, that have been or will be configured, to this GPRS service.
> Example
> The following command associates Gs service gs1 with this GPRS service.
> associate-service gs gs1 context sgsn2
> cc profile
> Configures the charging characteristic (CC) profile index properties.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] cc profile index { buckets number | interval time | tariff time1 mins hours [ time2 mins hours [ time3 mins hours [ time4 mins hours ] ] ] | volume { downlink octets uplink octets | total octets } }
> default cc profile index
> no
> Removes the a specific charging characteristics configuration definition.
> default
> Resets the charging characteristics to system defaults.
> index
> Configures a profile index for the parameter to be specified. index can be configured to any integer value from 0 to 15.
> Important: 3GPP standards suggest that profile index values of 1, 2, 4, and 8 be used for hot billing, flat rate billing, prepaid billing and normal billing, respectively. A single charging characteristics profile can contain multiple behavior settings.
> buckets number
> Default: 4
> Specifies the number of statistics container changes due to QoS changes or tariff time that can occur before an accounting record should be closed.
> number can be configured to any integer value from 1 through 4.
> interval time
> time is measured in seconds and can be configured to any integer value from 60 to 40,000,000.
> tariff time1 mins hours time2 mins hours time3 mins hours time4 mins hours
> Specifies time-of-day time values to close the current statistics container (but not necessarily the accounting record). Six different tariff times may be specified. If less than six times are required, the same time can be specified multiple times.
> Important: The system assumes that the billing system uses the day/date to determine if the statistics container represents an actual tariff period.
> For each of the different tariff times, the following parameters must be configured:

> • | mins: The minutes of the hour, an integer value from 0 to 59.

> • | hours: The hour of the day, an integer value from 0 to 23.

> volume { downlink vol_down_octets uplink vol_up_octets | total total_octets }
> Specifies the downlink, uplink, and total volumes that must be met before closing a CDR.
> vol_down_octets : Measured in octets; can be configured to any integer value from 100,000 to 4,000,000,000.
> vol_up_octets : Measured in octets; can be configured to any integer value from 100,000 to 4,000,000,000.
> total_octets : The total traffic volume (up and downlink) measured in octets; can be configured to any integer value from 100,000 to 4,000,000,000.
> Usage
> Charging characteristics consist of a profile index and behavior settings. This command configures profile indexes for the SGSN’s charging characteristics. The SGSN supports up to 16 profile indexes.
> This command works in conjunction with the cc-sgsn command located in the APN configuration mode that dictates which CCs should be used for subscriber PDP contexts.
> Example
> The following command configures a profile index of 10 for tariff times of 7:00 AM and 7:30 PM:
> cc profile 10 tariff time1 0 7 time2 30 19
> check-imei-timeout-action
> This command configures the action to be taken on the Gf interface if a Check-IMEI fails due to a timeout.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> check-imei-timeout-action [ continue | reject ]
> default check-imei-timeout-action
> default
> Rejects the Attach or ISRAU procedure if a Check-IMEI timeout occurs.
> continue
> Instructs the SGSN to continue the Attach or ISRAU procedure if a Check-IMEI timeout occurs because the EIR is not reachable. This functionality matches standard call flow.
> reject
> Instructs the SGSN to reject the Attach or ISRAU procedure if a Check-IMEI timeout occurs.
> Usage
> Use this command to control the SGSN reaction if a Check-IMEI fails due to a timeout.
> The continue option allows the SGSN to go forward with the MS Attach if the first Check-IMEI fails to reach the EIR due to a timeout. Any subsequent activity (such as a RAU or Service Request would force another Check-IMEI towards the EIR. If this subsequent MAP Check-IMEI should fail, then the same policy of continuing the procedure would apply.
> Example
> Use the following command to reject Attach Requests if the Check-IMEI timer runs out:
> check-imei-timeout-action reject
> ciphering-algorithm
> This command configures the priority, ordering, for the use of the GPRS encryption ciphering algorithms.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ciphering-algorithm { negotiation-failure-action { reject [ failure-code cause_code ] | use-geo0 } priority priority [ algorithm ] }
> default ciphering-algorithm priority priority
> default
> Returns the system ciphering-algorithm priority to the default of GEA0 - which means that no ciphering will be done.
> negotiation-failure-action { reject [ failure-code cause_code ] | use-geo0 }
> This set of keywords configure the SGSN's action if there is not a match between the MS and SGSN ciphering algorithm configurations.

> • | reject: Instructs the SGSN to reject a call when the ciphering algorithms do not match.

> • | failure-code cause_code: Instructs the SGSN to include a GMM cause code in the Reject message. Enter an integer from 2 to 111; default code is 14 (GPRS services not allowed in this PLMN). Refer to the GMM failure cause codes listed below (information has been taken from section 10.5.5.14 of the 3GPP TS 124.008 v7.2.0 R7):

> • | 2 - IMSI unknown in HLR

> • | 3 - Illegal MS

> • | 6 - Illegal ME

> • | 7 - GPRS services not allowed

> • | 8 - GPRS services and non-GPRS services not allowed

> • | 9 - MSID cannot be derived by the network

> • | 10 - Implicitly detached

> • | 11 - PLMN not allowed

> • | 12 - Location Area not allowed

> • | 13 - Roaming not allowed in this location area

> • | 14 - GPRS services not allowed in this PLMN

> • | 15 - No Suitable Cells In Location Area

> • | 16 -MSC temporarily not reachable

> • | 17 - Network failure

> • | 20 - MAC failure

> • | 21 - Synch failure

> • | 22 - Congestion

> • | 23 - GSM authentication unacceptable

> • | 40 - No PDP context activated

> • | 48 to 63 - retry upon entry into a new cell

> • | 95 - Semantically incorrect message

> • | 96 - Invalid mandatory information

> • | 97 - Message type non-existent or not implemented

> • | 98 - Message type not compatible with state

> • | 99 - Information element non-existent or not implemented

> • | 100 - Conditional IE error

> • | 101 - Message not compatible with the protocol state

> • | 111 - Protocol error, unspecified

> • | use-geo0: Instructs the SGSN to honor the Attach/RAU Request without ciphering (geo0). This is the default action for negotiation failure.

> priority priority algorithm
> Defines the priority, order of use, for the ciphering algorithm.
> priority: Must be an integer from 1 to 4.
> algorithm
> Identifies the algorithm to be matched to the priority. Options include:

> • | gea0 - No ciphering

> • | gea1 - GPRS Encryption Algorithm - GEA1

> • | gea2 - GPRS Encryption Algorithm - GEA2

> • | gea3 - GPRS Encryption Algorithm - GEA3

> Usage
> Use this command to specify the order (priority) of usage for the GPRS encryption algorithms. All of the GPRS encapsulation algorithms use a 64-bit key derived from a common mechanism: the mobile receives a random challenge, then the SIM calculates an authentication signature and an encryption key.
> Also use this command to define the action to be taken if there is not a match between the MS and the SGSN ciphering algorithm configurations.
> Example
> The following command sets no ciphering to be used after two encryption algorithms have been used:
> ciphering-algorithm priority 3 gea0
> The following command configures the SGSN to reject calls if the ciphering algorithm configurations don’t match:
> ciphering-algorithm negotiation-failure-action reject
> dns israu-mcc-mnc-encoding
> Configures either decimal or hexadecimal format for the MCC and MNC values in the DNS query.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> dns israu-mcc-mnc-encoding { decimal | hexidecimal }
> default dns israu-mcc-mnc-encoding
> default
> Resets the SGSN to send the MCC and MNC values in decimal format for DNS queries.
> decimal
> Default.
> Instructs the SGSN to send the MCC and MNC in decimal format in the DNS query.
> hexadecimal
> Instructs the SGSN to send the MCC and MNC in hexadecimal format in the DNS query.
> Usage
> Use this command to determine the type of encoding for the MCC and MNC to be included in the DNS query. For example:
> In decimal, the MNC/MCC in a DNS query would appear like:
> rac0017.lac42e3.mnc310.mcc722.gprs
> In hexadecimal, the MNC/MCC in a DNS query would appear like:
> rac0017.lac42e3.mnc0136.mcc02d2.gprs
> Example
> Use hexadecimal values for the MCC/MNC in the DNS query.
> dns israu-mcc-mnc-encoding hexadecimal
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the previous configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> gmm
> This command defines the GPRS mobility management parameters for the SGSN service.
> Important: The gmm command can be repeated to set each timer as needed.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gmm { accept-procedure [ new-tlli | old-tlli ] | ciph-gmm-msg-from-unknown-ms { detach | ignore } | mobile-reachable-timeout mins | negotiate-t3314-timeout secs | purge-timeout mins | T3302-timeout mins | T3312-timeout mins | T3313-timeout secs | T3350-timeout secs | T3360-timeout secs | T3370-timeout secs | trau-timeout secs }
> default gmm { ciph-gmm-msg-from-unknown-ms | mobile-reachable-timeout | negotiate-t3314-timeout | purge-timeout | T3302-timeout | T3312-timeout | T3313-timeout | T3350-timeout | T3360-timeout | T3370-timeout | trau-timeout }
> no gmm negotiate-t3314-timeout
> default
> Resets the specified timer timeout to the system default.
> no
> Removes the specified GMM definition from the configuration.
> accept-procedure [ new-tlli | old-tlli ]
> Default: new-tlli
> This keyword enables the use of either a new TLLI (temporary logical link identifier) or an old TLLI for attach-accept or RAU-accept messages sent by the SGSN to the MS during related procedures.
> ciph-gmm-msg-from-unknown-ms { detach | ignore }
> Configures how the SGSN will behave when it receives a ciphered GMM message from an unknown MS.
> detach - Instructs the SGSN to send a Detach message to the MS.
> ignore - Instructs the SGSN to send an Ignore (drop) message to the MS.
> Default: ignore
> mobile-reachable-timeout mins
> Default: 58 minutes
> Timer value for the mobile reachability timer.
> mins must be an integer from 4 to 1440.
> negotiate-T3314-timeout secs
> Set the number of seconds for the T3314-timeout ready timer value. Value sent out from SGSN so MS can negotiate ready timer.
> secs must be an integer from 0 to 11160. Default is 44 seconds.

> • | If the MS does not send the ready timer in the Attach/RAU request, then the SGSN sends this T3314-timeout (ready timer) value.

> • | If the MS sends the requested value of the ready timer in the Attach/RAU Request, and if the requested value is less than or equal to the value of the negotiate-T3314-timeout timer, then the SGSN sends Att/RAU Accept with the requested T3314 value.

> • | If the MS sends the requested value of the ready timer in the Attach/RAU Request, and if the requested value is greater than the value of the negotiate-T3314-timeout timer, then the SGSN sends Att/RAU Accept with the negotiate-T3314-timeout value.

> Important: This is the only GMM timer that can be disabled by entering no at the beginning of the command syntax. no gmm negotiate-t3314-timeout By disabling negotiation of the T3314-timeout value, if the MS sends the requested value of the ready timer in the Att/RAU Request, then the SGSN sends the T3314-timeout value in the Att/RAU Accept.
> purge-timeout mins
> Default: 10080 minutes
> Value defines the mm-context lifetime in minutes.
> mins must be an integer from 1 to 20160.
> T3302-timeout mins
> Default: 12 minutes
> Defines the number of minutes for timer to send to MS.
> mins is an integer from 1 to 186.
> T3312-timeout min
> Default: 54 minutes
> Periodic RAU update timer to send to MS.
> mins is an integer from 0 to 186.
> T3313-timeout secs
> Default: 5 seconds
> Initial page timeout timer for retransmission for Paging Requests.
> secs is an integer from 1 to 60.
> T3314-timeout secs
> Default: 44 seconds
> Ready Timer for controlling Cell Update Procedure.
> secs must be an integer from 0 to 11519.
> T3350-timeout secs
> Default :6 seconds
> Retransmission timer for Attach Accept/RAU Accept/P-TMSI Realloc Command.
> secs must be an integer from 1 to 20.
> T3360-timeout secs
> Default :6 seconds
> Retransmission timer for Authentication Request.
> secs must be an integer from 1 to 20.
> T3370-timeout secs
> Default :6 seconds
> Retransmission timer for Identity Request.
> secs must be an integer from 1 to 20.
> trau-timeout secs
> This timer is available in releases 9.0 and higher.
> Default: 30
> Specifies the number of seconds the “old” 3G SGSN waits to purge the MS’s data. This timer is started by the “old” SGSN after completion of the inter-SGSN RAU.
> secs : Must be an integer from 5 to 60.
> Usage
> Use this command to set GMM timers.
> Example
> Set the t3370 timer expiration for 15 seconds:
> gmm t3370-timeout 15
> llc
> Configures the timers that control the data flow for the logical link control (LLC) sub-layer.
> Important: This command may be repeated as often as necessary to define the needed timers.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> llc { iov-ui-in-xid-reset | n201u-max { sapi11 pkt-size | sapi3 pkt-size | sapi5 pkt-size | sapi9 pkt-size } | nu-overflow-detection high-watermark high_num low-watermark low_num increment-oc| pdu-lifetime secs | reset-vur | t200 sapi1 time | t200 [ sapi11 time | sapi3 time | sapi5 time | sapi7 time | sapi9 time ] | uplink-pdu-len-validation }
> default llc { iov-ui-in-xid-reset | n201u-max { sapi11 | sapi3 | sapi5 | sapi9 } | nu-overflow-detection | pdu-lifetime | reset-vur | T200 [ sapi1 | sapi11 | sapi3 | sapi5 | sapi7 | sapi9 ] | uplink-pdu-len-validation }
> no llc { iov-ui-in-xid-reset | nu-overflow-detection | reset-vur | uplink-pdu-len-validation }
> default
> Resets the configuration to the default values.
> no
> Disables the uplink-pdu-len-validation .
> iov-ui-in-xid-reset
> This keyword makes it possible for the operator to configure whether or not to send IOV-UI in an XID-RESET. This is useful when the MS is not setup to accept IOV-UI (for example, MS sends Attach/RAU Requests with cksn=7) and including IOV-UI in the XID-Reset would result in Attach/RAU failure.
> Default: Enabled
> n201u-max sapi n pkt_size
> This keyword sets the maximum number of octets, per service access point identifier (SAPI), for the downlink data packets. This is the upper limit that the SGSN will negotiate with the subscriber for packets sent from the SGSN to the BSC.
> sapi n : Command must identify one of the following SAPI: sapi11, sapi3, sapi5, or sapi9.
> pkt_size : Must be an integer from 140 to 1520. Default size is 1520 octets.
> nu-overflow-detection high-watermark high_num low-watermark low_num increment-oc
> Enables/disables overflow detection for the N(u) counter and setting overflow high/low thresholds facilitates ciphering synchronization between the MS and SGSN.
> high_num: Enter an integer between 1 and 511.
> low_num: Enter an integer between 0 and 510.
> If the expected value of nu(Vur) is greater than or equal to the configured high-watermark, and the received nu(LFN) is less than or equal to the configured low-watermark, the SGSN increments the overflow counter (VurOC).
> The recommended overflow settings are as follows:llc nu-overflow-detection high-watermark 496 low-watermark 15 increment-oc While expecting a packet with 496 < nu < 511 and a packet with 0 < nu < 15 is received, overflow is detected and VurOC is incremented.
> pdu-lifetime secs
> Defines LLC layer PDU lifetime at the BSC. .
> secs must be an integer from 0 to 90.
> Default: 6
> reset-vur
> Enables/disables the mechanism to reset the Vur value maintained at LLC if the intra RAU request is received with N(U) = 0
> Default: Disabled
> T200 sapi1 time
> Sets the retransmission timer (in seconds) for sapi1.
> time must be an integer of 1 to 10.
> Default: 5
> T200 sapi11 time
> Sets the retransmission timer (in seconds) for sapi11.
> time must be an integer of 1 to 50.
> Default: 40
> T200 sapi3 time
> Sets the retransmission timer (in seconds) for sapi3.
> time must be an integer of 1 to 10.
> Default: 5
> T200 sapi5 time
> Sets the retransmission timer (in seconds) for sapi5.
> time must be an integer of 1 to 20.
> Default: 10
> T200 sapi7 time
> Sets the retransmission timer (in seconds) for sapi7.
> time must be an integer of 1 to 40.
> Default: 20
> T200 sapi9 time
> Sets the retransmission timer (in seconds) for sapi9.
> time must be an integer of 1 to 40.
> Default: 20
> uplink-pdu-len-validation
> Available in releases 8.1 and higher.
> This feature enables validation of the size of the uplink LLC packets. With validation enabled, the SGSN will drop any uplinked packets that are larger than the negotiated limit.
> If the no form of the command is used, then this feature is disabled. The SGSN will be more flexible with uplink packet sizes. So if the SGSN and MS have a mismatch and the MS sends packets that are larger than expected, then the SGSN will not drop the packets.
> Default: Enabled.
> Usage
> Use the command repeatedly to configure additional timers and features for the LLC sub-layer.
> Example
> Set the T200 retransmission timer to timeout at 12 seconds for SAPI5:
> llc t200 sapi5 12
> Use the following command to instruct the SGSN to ignore the N201_U packet size limits for uplink packets from an MS:
> no uplink-pdu-len-validation
> nri
> This command configures the network resource identifier (NRI) to identify a specific SGSN. The NRI is stored in the P-TMSI. The SGSN uses a portion of this NRI to set the parameters for Gb flex (SGSN pooling) functionality.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> nri length nri_length { nri-value nri_value | null-nri-value null_nri_value non-broadcast-lac lac_id rac rac_id [ nri-value value }
> no nri
> no
> Removes the configured NRI value and location in P-TMSI for retrieval by this SGSN operator policy.
> nri length nri_length
> Specifies the number of bits to be used in the P-TMSI, bits 23 to 18. to define the network resource identifier (NRI). The NRI length configuration also sets the maximum size of the pool. If not configured, the NRI length will be of zero length.
> nri_length : Must be an integer from 1 to 6 to identify the number of bits.
> null-nri-value null_nri_value
> Configures the null NRI value which must be unique across the pool areas. This keyword is used for the offloading procedure for SGSN pooling (enabled with the sgsn offloading command, see the Exec Mode chapter).
> null_nri_value : 0 (zero) indicates the keyword is not to be used and 1 to 63 are used to identify the SGSN to be used for the offloading procedure for SGSN pooling. There is no default value for this parameter.
> non-broadcast lac lac_id rac rac_id
> Defines the non-broadcast LAC/RAC to be used in combination with the null-NRI for the offloading procedure.
> lac_id defines a location area code associated with a BSS. Must be an integer between 1 and 65535.
> rac_id defines the remote area code to be associated with a BSS. Must be an integer between 1 and 255.
> nri-value nri_value
> Specifies the MS-assigned value of the NRI to retrieve from the P-TMSI. This value must not exceed the maximum possible value specified by the NRI length. The NRI value must be unique across the pool or across all overlapping pools.
> nri_value must be an integer from 1 to 63 to identify a specific SGSN in a pool. Use of 0 (zero) value is not recommended.
> Multiple NRI values can be identified by providing multiple nri-values separated by a blank space for example: nri length 6 nri-value 29 43 61
> Usage
> Use this command to add or remove the Gb flex pool configuration for this GPRS service. The command can be repeated to specify different values for any of the keyword parameters. If more than one NRI is configured, the GPRS service will round-robin between the available NRIs when new subscribers (re)connect.
> Use this command to retrieve the NRI (identity of an SGSN) stored in in bits 23 to 18 of the packet-temporary mobile subscriber identity (P-TMSI). If more than one NRI value is configured, the GPRS service will round-robin between the available NRIs when new subscribers (re)connect.
> Example
> The following command specifies the the NRI length as 5 bits, identifies SGSN 23 with LAC 222 and RAC 12 for offloading procedure with NRIs 6 and 41:
> nri length 5 null-nri-value 34 non-broadcast lac 222 rac 12 nri-value 6 41
> paging-policy
> Configures the paging parameters for the GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> paging-policy { last-known-area { all | bsc | cell | location-area | routing-area } + | max-retransmissions retran_num }
> no paging-policy last-known-area { bsc | cell | location-area | routing-area }
> default paging-policy { last-known-area | max-retransmissions }
> no
> Disables the paging-policy definition for this GPRS service configuration.
> default
> Resets the defaults for parameters managed by this paging policy.
> last-known-area
> Select one or more paging areas and enter them in preferred paging order:

> • | all : Pages in the last known BSC.

> • | bsc : Pages in last known BSC.

> • | cell : Pages in last known cell.

> • | location-area : Pages in last known location area.

> • | routing-area : Pages in last known routing area.

> By default, paging occurs in the following order:
> cell, BSC, routing area, location area.
> max-retransmission retran_num
> Configures the maximum number of retries for a page request per paging area.
> retran_num: Enter an integer from 0 to 5.

> • | 2 : default.

> • | 0 : disables retransmission for paging request so that the SGSN only sends a single 2G PS-paging request to the BSC with no retransmissions.

> +
> Keywords can be repeated or combined as needed to complete the paging policy configuration.
> Usage
> Use this command to configure the order of preference for retransmitting into specified paging-areas.
> Example
> Use the following command to instruct the SGSN to page the cell and BSC as the last-known areas :
> paging-policy last-known-area cell bsc
> peer-nsei
> This command associates a peer (remote) network service entity (NSEI) for a BSS with this GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> peer-nsei nse_id { lac lac_id rac rac_id | pooled }
> [ no ] peer-nsei nse_id { lac lac_id rac rac_id | pooled }
> no
> Removes the NSEI LAC/RAC or pooling configuration from this BSS peer configuration.
> nse_id
> Defines the NSEI for this GPRS service.
> nse_id must be an integer from 0 to 65535.
> lac lac_id
> Defines a location area code associated with the NSE BSS.
> lac_id must be an integer between 1 and 65535.
> rac rac_id
> Defines the remote area code to be associated with the NSE BSS
> rac_id must be an integer between 1 and 255.
> pooled
> Enables pooling with non-pooled BSCs within the pool area.
> Usage
> Use this command repeatedly to associate one or more LAC/RAC combinations and/or pooling with this peer-GPRS service configuration.
> The Network Service Entity (NSE) at the BSS and the SGSN provides the network management functionality required for the operation of the Gb interface. Each NSE is identified by means of NSE identifier (NSEI).
> Example
> The following command configures the NSE with identifier as 4114 having location area code 234 and routing area code as 22:
> peer-nsei 4114 lac 234 rac 22
> The following command enables Gb flex (pooling) functionality for this GPRS service:
> peer-nsei 4114 pooled
> plmn
> This command identifies the Public Land Mobile Network (PLMN) for the GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> plmn id mcc mcc_num mnc mnc_num
> no plmn id
> no
> Removes the PLMN information from the configuration for the current SGSN service.
> mcc mcc_num
> Define the mobile country code (MCC) portion of the PLMN Id.
> mnc_num must be a 3 digit integer from 100 to 999.
> mnc mnc_num
> Define the mobile network code (MNC) portion of the PLMN Id.
> mnc_num must be a 2 or 3 digit integer from 00 to 999.
> Usage
> Use this command to set PLMN parameters for the current SGSN service.
> Example
> The following command identifies the PLMN MCC as 200 and the MNC as 10:
> plmn id mcc 200 mnc 10
> setup-timout
> This command configures the maximum number of seconds allowed for session setup.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> setup-timout seconds
> default setup-timout
> default
> Returns the configuration to the default, 60 seconds.
> seconds
> An integer from 1 to 1000000.
> Usage
> Use this command to set the time allowed for session setup.
> Example
> The following command sets the maximum session setup time to 300 seconds:
> setup-timout 300
> sgsn-context-request
> This command specifies whether or not the PTMSI signature check should be skipped if the PTMSI signature is not included in the SGSN context request.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn-context-request ptmsi-signature-absence allowed
> default sgsn-context-request ptmsi-signature-absence
> no sgsn-context-request ptmsi-signature-absence allowed
> default
> Returns the configuration to the default action to perform the PTMSI signature check.
> no
> Removes this definition from the system configuration.
> Usage
> Use this command to skip the PTMSI signature check.
> Example
> The following command instructs the system to perform the PTMSI signature check.
> default sgsn-context-request ptmsi-signature-absence
> sgsn-number
> Define the SGSN E.164 number to be used when interacting via MAP protocol for this GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn-number sgsn_number
> no sgsn-number
> no
> Disables the use of this definition in the system configuration.
> sgsn-number
> Enter a string of 1 to 16 digits to identify the SGSN’s E.164 identification.
> Usage
> Use this command to identify the ISDN number for the SGSN associated with this GPRS service.
> The SGSN supports multiple SGSN numbers – different numbers in the 2G GPRS service configuration and the the 3G SGSN service configuration. If an HLR-initiated dialog is received, the SGSN will perform a lookup based on the IMSI and find the correct SGSN number with which the MS is associated. Subsequent messaging will use this address.
> Example
> Disable the E.164 number for this GPRS service.
> no sgsn-number
> sm
> This command configures the session management (SM) parameters associated with this particular GPRS service context.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sm { activate-max-retransmissions num_retries | deactivate- max-retransmissions num_retries | ignore-pco-decode-error | modify-max-retransmissions num_retries | partial-apn-match | requested-apn-from-first-subrec | t3385-timeout secs | t3386-timeout secs | t3395-timeout secs | trim-trailing-spaces-in-apn }
> default sm { activate-max-retransmissions | deactivate-max-retransmissions | ignore-pco-decode-error | modify-max-retransmissions | t3385-timeout | t3386-timeout | t3395-timeout | trim-trailing-spaces-in-apn }
> default
> Resets the SM parameters to the defaults.
> activate-max-retransmissions num_retries
> Defines the maximum number of retries to transmit ‘activate PDP context request’.
> num_retries : Must be an integer from 1 to 10.
> Default: 4
> deactivate-max-retransmissions num_retries
> Defines the maximum number of retries to transmit ‘deactivate PDP context request’.
> num_retries : Must be an integer from 1 to 10.
> Default: 4
> ignore-pco-decode-error
> Enables the SGSN to ignore received decode errors that are due to incorrectly encoded PCO IE length in SM Requests.
> Default: disabled
> modify-max-retransmissions num_retries
> Defines the maximum number of retries to transmit ‘modify PDP context request’.
> num_retries: integer from 1 to 10.
> Default: 4
> partial-apn-match
> Enables partial matching of requested APN during APN selection.
> Partial APN or APN with trailing spaces may be present in an Activate Request because incorrect information was keyed in by the user. Though it is valid to reject such Activation Requests, it increases the signaling between the MS and the SGSN. This has an impact on the radio resources.
> requested-apn-from-first-subrec
> Enables use of a ‘requested APN’ from the first subscription record. When this feature is enabled, the PDP Activation is not rejected during APN Selection; instead, the APN from the first subscription record is used as the requested APN and the SGSN continues with the rest of the APN Selection process.
> A requested APN is an optional IE in an Activate PDP Request. To get the requested PDP type, if multiple PDP subscription records exist for the subscriber, then the MS has to include the APN information to choose the PDP subscription record during APN selection. Otherwise, such activations will be rejected during APN selection (per TS 23.060 Appendix A). Though it is valid to reject such activation requests, it increases the signaling between the MS and the SGSN, which impacts the radio resources.
> t3385-timeout secs
> Defines the maximum amount of time for retransmission of ‘activate request’ messages.
> secs : Must be an integer from 1 to 60.
> Default: 8
> t3386-timeout secs
> Defines the maximum amount of time for retransmission of ‘modify request’ messages.
> secs : Must be an integer from 1 to 60.
> Default: 8 seconds.
> t3395-timeout secs
> Defines the maximum amount of time for retransmission of ‘deactivate request’ messages.
> secs : Must be an integer from 1 to 60.
> Default: 8
> trim-trailing-spaces-in-apn
> Enables SGSN to strip off any trailing space(s) in requested APN.
> If a requested APN in an Activate PDP Context Request has any trailing spaces, then those trailing spaces will be removed and the length field will be updated.
> Usage
> Repeat this command with different keywords (parameters) to configure the SM (session management) as needed for this GPRS service. Keywords can be used to optimize signaling between the MS and the SGSN to reduce the impact on the radio resources.
> Example
> Reset the number of retransmission messages for deactivate PDP context request to 5.
> sm deactivate-max-retransmissions 5
> sndcp
> Define the sub-network dependent convergence protocol (SNDCP) network packet data unit (N-PDU) reassembly timeout interval associated with this GPRS service.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sndcp reassembly-timeout seconds
> default sndcp reassembly-timeout
> default
> Resets the timer configuration to the default value of 30 seconds.
> seconds
> Defines the the number of seconds the SGSN waits for all the SNDCP segments to arrive before dropping all the disassembled segments.
> seconds: Must be an integer from 1 to 300.
> Usage
> Use this command to modify the SNDCP reassembly timer. This timer starts as soon as the first N-PDU segment is received (either in-order or out-of-order). If all the segments belong to the N-PDU arrive before the timer expires then the segments are reassembled. If all the segments do not arrive before the timer expires, then the stored segments are discarded.
> Example
> Reset the default for the timer.
> default sndcp reassembly-timeout

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883