> DSCP Template Configuration Mode Commands
> The DSCP Template Configuration Mode provides the commands to configure DSCP marking for control packets and data packets for Gb over IP. Any number of DSCP templates can be generated in the SGSN Global configuration mode and then a template can be associated with one or more GPRS Services via the commands in the GPRS Service configuration mode.
> The prompt for this mode appears as:
> [local]<hostname>(config-dscp-template-<template_name>)#
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> control-packet
> Configures the diffserv code point marking (DSCP) value for 3GPP quality of service (QoS) class downlink control packets.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> control-packet qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | cs1 | cs2 | cs3 | cs4 | cs5 | cs6 | cs7 | ef }
> default control-packet
> default
> Resets the quality of service (QoS) DSCP setting to the ‘BE’ (best effort) default value.
> DSCP marking option
> Select one of the following downlink DSCP options for the control packets:

> • | af11: Assured Forwarding 11 per-hop-behavior (PHB)
> • | be: Best Effort for Forwarding
> • | af12: Assured Forwarding 12 PHB
> • | cs1: Class Selector 1 PHB
> • | af13: Assured Forwarding 13 PHB
> • | cs2: Class Selector 2 PHB
> • | af21: Assured Forwarding 21 PHB
> • | cs3: Class Selector 3 PHB
> • | af22: Assured Forwarding 22 PHB
> • | cs4: Class Selector 4 PHB
> • | af23: Assured Forwarding 23 PHB
> • | cs5: Class Selector 5 PHB
> • | af31: Assured Forwarding 31 PHB
> • | cs6: Class Selector 6 PHB
> • | af32: Assured Forwarding 32 PHB
> • | cs7: Class Selector 7 PHB
> • | af33: Assured Forwarding 33 PHB
> • | ef: Expedited forwarding PHB
> • | af41: Assured Forwarding 41 PHB
> • | af42: Assured Forwarding 42 PHB
> • | af43: Assured Forwarding 43 PHB

> ‌
> Usage
> This command configures the QoS DSCP marking type for downlink control packets.
> Related commands:

> • | To create/delete a DSCP template, use the dscp-template in the SGSN Global configuration mode (see the SGSN Global Configuration Mode Commands section).

> • | To associated a specpific DSCP template with a specific GPRS service configuration, use the associate-dscp-template downlink documented in the GPRS Service Configuration Mode Commands section.

> • | To check values configured for DSCP templates, use the show sgsn-mode command documented in the Exec Mode Commands section.

> Example
> Use a command similar to the following to set expedited forward per-hop behavior for the downlink control packets:
> control-packet qos-dscp ef
> Use the following command to reset the default best effort per-hop behavior:
> default control-packet
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Return to the Exec mode.
> exit
> Exits the current configuration mode and returns to the previous configuration mode.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Return to the context configuration mode.
> data-packet
> Configures the diffserv code point marking (DSCP) value for 3GPP quality of service (QoS) class downlink data packets.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> control-packet { background | conversationa | interactive { priority1 | priority2 | priority3 } | streaming } qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | cs1 | cs2 | cs3 | cs4 | cs5 | cs6 | cs7 | ef }
> default data-packet { background | conversationa | interactive { priority1 | priority2 | priority3 } | streaming }
> default
> Resets the quality of service (QoS) DSCP setting to the be (best effort) default value.
> background | conversationa | interactive | streaming
> Select the QoS traffic class of service for the downlink data packets.
> priority1 | priority2 | priority3
> Select the traffic handling priority to be applied to the specified traffic class.
> DSCP option
> Select one of the following DSCP settings for the selected traffic class. Default is best effort (be) for all traffic classes settings.

> • | af11: Assured Forwarding 11 per-hop-behavior (PHB)
> • | be: Best Effort for Forwarding
> • | af12: Assured Forwarding 12 PHB
> • | cs1: Class Selector 1 PHB
> • | af13: Assured Forwarding 13 PHB
> • | cs2: Class Selector 2 PHB
> • | af21: Assured Forwarding 21 PHB
> • | cs3: Class Selector 3 PHB
> • | af22: Assured Forwarding 22 PHB
> • | cs4: Class Selector 4 PHB
> • | af23: Assured Forwarding 23 PHB
> • | cs5: Class Selector 5 PHB
> • | af31: Assured Forwarding 31 PHB
> • | cs6: Class Selector 6 PHB
> • | af32: Assured Forwarding 32 PHB
> • | cs7: Class Selector 7 PHB
> • | af33: Assured Forwarding 33 PHB
> • | ef: Expedited forwarding PHB
> • | af41: Assured Forwarding 41 PHB
> • | af42: Assured Forwarding 42 PHB
> • | af43: Assured Forwarding 43 PHB

> ‌
> Usage
> This command configures the QoS DSCP marking type for downlink data packets. DSCP levels indicate how packets are to be handled
> Related commands:

> • | To create/delete a DSCP template, use the dscp-template in the SGSN Global configuration mode (see the SGSN Global Configuration Mode Commands section).

> • | To associated a specpific DSCP template with a specific GPRS service configuration, use the associate-dscp-template downlink documented in the GPRS Service Configuration Mode Commands section.

> • | To check values configured for DSCP templates, use the show sgsn-mode command documented in the Exec Mode Commands section.

> Example
> Use a command similar to the following to set expedited forward per-hop behavior for the downlink control packets:
> control-packet qos-dscp ef
> Use the following command to reset the default best effort per-hop behavior:
> default control-packet

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883