> LTE Forbidden Tracking Area Configuration Mode Commands
> The LTE Forbidden Tracking Area Configuration Mode is used to create and manage forbidden tracking area code configurations.
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> tac
> Configures a tracking area code or area codes where a UE, associated with this LTE policy, is restricted from participating in a handover scenario.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] tac area_code
> no
> Removes a configured forbidden handover area code or area codes from this policy. If no tracking area code is specified, then all tracking area codes are removed.
> area_code
> Specifies a tracking area code or area codes from which UEs are restricted from participating in a handover. area_code must be an integer value from 0 to 65535. Multiple area codes can be entered (up to 128 in a single line).
> Usage
> Use this command to configure tracking area codes that will be forbidden to UEs associated with this LTE policy.
> Example
> The following command configures two tracking area codes (1, 2, 3, 4, 5, 6, 7, 8) where a UE, associated with this LTE policy, is restricted from participating in a handover scenario:
> tac 1 2 3 4 5 6 7 8

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883