> CSCF Schema Statistics
> The CSCF schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SCM
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the CSCF Schema

> Variables | Description | Data Type
> vpnname | VPN Name This is a key variable. | String
> vpnid | VPN ID This is a key variable. | Int32
> svcname | Service Name This is a key variable. | String
> svcid | Service ID This is a key variable. | Int32
> curregusers | Current Registered Users Type: Gauge | Int32
> failedauth | Total number of Failed Authentications. | Int64
> regexp | Total number of Registration Expires. | Int64
> total-roaming-ue-regs | Total number of Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-regs | Total number of 200 OK Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-regs | Total number of Failed Registrations from Roaming UE. | Int64
> total-roaming-ue-regs-403 | Total number of 403 responses to Registration from Roaming UE. | Int64
> total-roaming-ue-re-regs | Total number of Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-re- regs | Total number of 200 OK Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-re-regs | Total number of Failed Re-Registrations from Roaming UE. | Int64
> total-roaming-ue-re-regs-403 | Total number of 403 responses to Re-Registration from Roaming UE. | Int64
> total-roaming-ue-de-regs | Total number of De-Registrations from Roaming UE. | Int64
> total-roaming-ue-succ-de-regs | Total number of 200 OK De-Registrations from Roaming UE. | Int64
> total-roaming-ue-fail-de-regs | Total number of Failed De-Registrations from Roaming UE. | Int64
> total-roaming-ue-de-regs- 403 | Total number of 403 responses to De-Registration from Roaming UE. | Int64
> de-regs-fromue | Total number of De-registrations from UE. | Int64
> de-regs-fromnw | Total number of De-registrations from Network. | Int64
> sec-regs | Total number of Secure Registrations. | Int64
> fail-sec-regs | Total number of Failed Secure Registrations | Int64
> emerg-regs | Total number of Emergency Registrations. | Int64
> mo-call-succ-rate | Mobile Originating calls success rate. | Float
> mt-call-succ-rate | Mobile Terminating calls success rate. | Float
> mo-voice-call-succ-rate | Mobile Originating VOICE calls success rate. | Float
> mt-voice-call-succ-rate | Mobile Terminating VOICE calls success rate. | Float
> mo-video-call-succ-rate | Mobile Originating VIDEO calls success rate. | Float
> mt-video-call-succ-rate | Mobile Terminating VIDEO calls success rate. | Float
> callattrx | Total number of Call Attempts received. | Int64
> callatttx | Total number of Call Attempts transmitted. | Int64
> callsuccrx | Total number of Call Success received. | Int64
> callsucctx | Total number of Call Success transmitted. | Int64
> callfailrx | Total number of Call Failures received. | Int64
> callfailtx | Total number of Call Failures transmitted. | Int64
> curcscfsess | Total number of current CSCF Sessions. Type: Gauge | Int32
> totalcscfsess | Total number of CSCF Sessions. | Int64
> call-resp-3xxrx | Total number of Call 3xx Responses received. | Int64
> call-resp-3xxtx | Total number of Call 3xx Responses transmitted. | Int64
> call-resp-402rx | Total number of Call 402 Responses received. | Int64
> call-resp-402tx | Total number of Call 402 Responses transmitted. | Int64
> call-resp-403rx | Total number of Call 403 Responses received. | Int64
> call-resp-403tx | Total number of Call 403 Responses transmitted. | Int64
> call-resp-404rx | Total number of Call 404 Responses received. | Int64
> call-resp-404tx | Total number of Call 404 Responses transmitted. | Int64
> call-resp-407rx | Total number of Call 407 Responses received. | Int64
> call-resp-407tx | Total number of Call 407 Responses transmitted. | Int64
> call-resp-408rx | Total number of Call 408 Responses received. | Int64
> call-resp-408tx | Total number of Call 408 Responses transmitted. | Int64
> call-resp-420rx | Total number of Call 420 Responses received. | Int64
> call-resp-420tx | Total number of Call 420 Responses transmitted. | Int64
> call-resp-421rx | Total number of Call 421 Responses received. | Int64
> call-resp-421tx | Total number of Call 421 Responses transmitted. | Int64
> call-resp-480rx | Total number of Call 480 Responses received. | Int64
> call-resp-480tx | Total number of Call 480 Responses transmitted. | Int64
> call-resp-486rx | Total number of Call 486 Responses received. | Int64
> call-resp-486tx | Total number of Call 486 Responses transmitted. | Int64
> call-resp-487rx | Total number of Call 487 Responses received. | Int64
> call-resp-487tx | Total number of Call 487 Responses transmitted. | Int64
> call-resp-488rx | Total number of Call 488 Responses received. | Int64
> call-resp-488tx | Total number of Call 488 Responses transmitted. | Int64
> call-resp-4xxrx | Total number of Call 4xx Responses received. | Int64
> call-resp-4xxtx | Total number of Call 4xx Responses transmitted. | Int64
> call-resp-500rx | Total number of Call 500 Responses received. | Int64
> call-resp-500tx | Total number of Call 500 Responses transmitted. | Int64
> call-resp-503rx | Total number of Call 503 Responses received. | Int64
> call-resp-503tx | Total number of Call 503 Responses transmitted. | Int64
> call-resp-5xxrx | Total number of Call 5xx Responses received. | Int64
> call-resp-5xxtx | Total number of Call 5xx Responses transmitted. | Int64
> call-resp-6xxrx | Total number of Call 6xx Responses received. | Int64
> call-resp-6xxtx | Total number of Call 6xx Responses transmitted. | Int64
> call-rel-attrx | Total number of Call Release Attempts received. | Int64
> call-rel-atttx | Total number of Call Release Attempts transmitted. | Int64
> call-rel-succrx | Total number of Call Release Success received. | Int64
> call-rel-succtx | Total number of Call Release Success transmitted. | Int64
> call-rel-failrx | Total number of Call Release Failures received. | Int64
> call-rel-failtx | Total number of Call Release Failures transmitted. | Int64
> reg-attrx | Total number of Registration Attempts received. | Int64
> reg-atttx | Total number of Registration Attempts transmitted. | Int64
> reg-succrx | Total number of Registration Successes received. | Int64
> reg-succtx | Total number of Registration Successes transmitted. | Int64
> reg-failrx | Total number of Registration Failures received. | Int64
> reg-failtx | Total number of Registration Failures transmitted. | Int64
> reg-resp-401rx | Total number of Registration 401 Responses received. | Int64
> reg-resp-401tx | Total number of Registration 401 Responses transmitted. | Int64
> reg-resp-403rx | Total number of Registration 403 Responses received. | Int64
> reg-resp-403tx | Total number of Registration 403 Responses transmitted. | Int64
> reg-resp-404rx | Total number of Registration 404 Responses received. | Int64
> reg-resp-404tx | Total number of Registration 404 Responses transmitted. | Int64
> reg-resp-420rx | Total number of Registration 420 Responses received. | Int64
> reg-resp-420tx | Total number of Registration 420 Responses transmitted. | Int64
> reg-resp-439rx | Total number of Registration 439 Responses received. | Int64
> reg-resp-439tx | Total number of Registration 439 Responses transmitted. | Int64
> reg-resp-4xxrx | Total number of Registration 4xx Responses received. | Int64
> reg-resp-4xxtx | Total number of Registration 4xx Responses transmitted. | Int64
> reg-resp-500rx | Total number of Registration 500 Responses received. | Int64
> reg-resp-500tx | Total number of Registration 500 Responses transmitted. | Int64
> reg-resp-5xxrx | Total number of Registration 5xx Responses received. | Int64
> reg-resp-5xxtx | Total number of Registration 5xx Responses transmitted. | Int64
> reg-resp-6xxrx | Total number of Registration 6xx Responses received. | Int64
> reg-resp-6xxtx | Total number of Registration 6xx Responses transmitted. | Int64
> rereg-attrx | Total number of Refresh Registration Attempts received. | Int64
> rereg-atttx | Total number of Refresh Registration Attempts transmitted. | Int64
> rereg-succrx | Total Refresh Registration Successes received. | Int64
> rereg-succtx | Total number of Refresh Registration Successes transmitted. | Int64
> rereg-failrx | Total number of Refresh Registration Failures received. | Int64
> rereg-failtx | Total number of Refresh Registration Failures transmitted. | Int64
> rereg-resp-401rx | Total number of Refresh Registration 401 Responses received. | Int64
> rereg-resp-401tx | Total number of Refresh Registration 401 Responses transmitted. | Int64
> rereg-resp-403rx | Total number of Refresh Registration 403 Responses received. | Int64
> rereg-resp-403tx | Total number of Refresh Registration 403 Responses transmitted. | Int64
> rereg-resp-404rx | Total number of Refresh Registration 404 Responses received. | Int64
> rereg-resp-404tx | Total number of Refresh Registration 404 Responses transmitted. | Int64
> rereg-resp-420rx | Total number of Refresh Registration 420 Responses received. | Int64
> rereg-resp-420tx | Total number of Refresh Registration 420 Responses transmitted. | Int64
> rereg-resp-439rx | Total number of Refresh Registration 439 Responses received. | Int64
> rereg-resp-439tx | Total number of Refresh Registration 439 Responses transmitted. | Int64
> rereg-resp-4xxrx | Total number of Refresh Registration 4xx Responses received. | Int64
> rereg-resp-4xxtx | Total number of Refresh Registration 4xx Responses transmitted. | Int64
> rereg-resp-500rx | Total number of Refresh Registration 500 Responses received. | Int64
> rereg-resp-500tx | Total number of Refresh Registration 500 Responses transmitted. | Int64
> rereg-resp-5xxrx | Total number of Refresh Registration 5xx Responses received. | Int64
> rereg-resp-5xxtx | Total number of Refresh Registration 5xx Responses transmitted. | Int64
> rereg-resp-6xxrx | Total number of Refresh Registration 6xx Responses received. | Int64
> rereg-resp-6xxtx | Total number of Refresh Registration 6xx Responses transmitted. | Int64
> dereg-attrx | Total number of Deregistration Attempts received. | Int64
> dereg-atttx | Total number of Deregistration Attempts transmitted. | Int64
> dereg-succrx | Total number of Deregistration Successes received. | Int64
> dereg-succtx | Total number of Deregistration Successes transmitted. | Int64
> dereg-failrx | Total number of Deregistration Failures received. | Int64
> dereg-failtx | Total number of Deregistration Failures transmitted. | Int64
> dereg-resp-401rx | Total number of Deregister 401 Responses received. | Int64
> dereg-resp-401tx | Total number of Deregister 401 Responses transmitted. | Int64
> dereg-resp-403rx | Total number of Deregister 403 Responses received. | Int64
> dereg-resp-403tx | Total number of Deregister 403 Responses transmitted. | Int64
> dereg-resp-404rx | Total number of Deregister 404 Responses received. | Int64
> dereg-resp-404tx | Total number of Deregister 404 Responses transmitted. | Int64
> dereg-resp-420rx | Total number of Deregister 420 Responses received. | Int64
> dereg-resp-420tx | Total number of Deregister 420 Responses transmitted. | Int64
> dereg-resp-4xxrx | Total number of Deregister 4xx Responses received. | Int64
> dereg-resp-4xxtx | Total number of Deregister 4xx Responses transmitted. | Int64
> dereg-resp-500rx | Total number of Deregister 500 Responses received. | Int64
> dereg-resp-500tx | Total number of Deregister 500 Responses transmitted. | Int64
> dereg-resp-5xxrx | Total number of Deregister 5xx Responses received. | Int64
> dereg-resp-5xxtx | Total number of Deregister 5xx Responses transmitted. | Int64
> dereg-resp-6xxrx | Total number of Deregister 6xx Responses received. | Int64
> dereg-resp-6xxtx | Total number of Deregister 6xx Responses transmitted. | Int64
> subscribe-attempt-rx | Total number of Subscribe Attempts Received | Int64
> subscribe-attempt-tx | Total number of Subscribe Attempts Transmitted | Int64
> subscribe-success-rx | Total number of Subscribe Success Received | Int64
> subscribe-success-tx | Total number of Subscribe Success Transmitted | Int64
> subscribe-failure-rx | Total number of Subscribe Failure Received | Int64
> subscribe-failure-tx | Total number of Subscribe Failure Transmitted | Int64
> notify-attempt-rx | Total number of Notify Attempts Received | Int64
> notify-attempt-tx | Total number of Notify Attempts Transmitted | Int64
> notify-success-rx | Total number of Notify Success Received | Int64
> notify-success-tx | Total number of Notify Success Transmitted | Int64
> notify-failure-rx | Total number of Notify Failure Received | Int64
> notify-failure-tx | Total number of Notify Failure Transmitted | Int64
> publish-attempt-rx | Total number of Publish Attempts Received | Int64
> publish-attempt-tx | Total number of Publish Attempts Transmitted | Int64
> publish-success-rx | Total number of Publish Success Received | Int64
> publish-success-tx | Total number of Publish Success Transmitted | Int64
> publish-failure-rx | Total number of Publish Failure Received | Int64
> publish-failure-tx | Total number of Publish Failure Transmitted | Int64
> msgsum-subs-attrx | Total number of “msg-summary” Subscription Attempts received. | Int64
> msgsum-subs-atttx | Total number of “msg-summary” Subscription Attempts transmitted. | Int64
> msgsum-subs-succrx | Total number of “msg-summary” Subscription Successes received. | Int64
> msgsum-subs-succtx | Total number of “msg-summary” Subscription Successes transmitted. | Int64
> msgsum-subs-failrx | Total number of “msg-summary” Subscription Failures received. | Int64
> msgsum-subs-failtx | Total number of “msg-summary” Subscription Failures transmitted. | Int64
> msgsum-subs-resp-200rx | Total number of “msg-summary” Subscription 200 Responses received. | Int64
> msgsum-subs-resp-200tx | Total number of “msg-summary” Subscription 200 Responses transmitted. | Int64
> msgsum-subs-resp-202rx | Total number of “msg-summary” Subscription 202 Responses received. | Int64
> msgsum-subs-resp-202tx | Total number of “msg-summary” Subscription 202 Responses transmitted. | Int64
> msgsum-subs-resp-400rx | Total number of “msg-summary” Subscription 400 Responses received. | Int64
> msgsum-subs-resp-400tx | Total number of “msg-summary” Subscription 400 Responses transmitted. | Int64
> msgsum-subs-resp-403rx | Total number of “msg-summary” Subscription 403 Responses received. | Int64
> msgsum-subs-resp-403tx | Total number of “msg-summary” Subscription 403 Responses transmitted. | Int64
> msgsum-subs-resp-481rx | Total number of “msg-summary” Subscription 481 Responses received. | Int64
> msgsum-subs-resp-481tx | Total number of “msg-summary” Subscription 481 Responses transmitted. | Int64
> msgsum-subs-resp-489rx | Total number of “msg-summary” Subscription 489 Responses received. | Int64
> msgsum-subs-resp-489tx | Total number of “msg-summary” Subscription 489 Responses transmitted. | Int64
> msgsum-subs-resp-500rx | Total number of “msg-summary” Subscription 500 Responses received. | Int64
> msgsum-subs-resp-500tx | Total number of “msg-summary” Subscription 500 Responses transmitted. | Int64
> msgsum-subs-resp-3xxrx | Total number of “msg-summary” Subscription 3XX Responses received. | Int64
> msgsum-subs-resp-3xxtx | Total number of “msg-summary” Subscription 3XX Responses transmitted. | Int64
> msgsum-subs-resp-4xxrx | Total number of “msg-summary” Subscription 4XX Responses received. | Int64
> msgsum-subs-resp-4xxtx | Total number of “msg-summary” Subscription 4XX Responses transmitted. | Int64
> msgsum-subs-resp-5xxrx | Total number of “msg-summary” Subscription 5XX Responses received. | Int64
> msgsum-subs-resp-5xxtx | Total number of “msg-summary” Subscription 5XX Responses transmitted. | Int64
> msgsum-subs-resp-6xxrx | Total number of “msg-summary” Subscription 6XX Responses received. | Int64
> msgsum-subs-resp-6xxtx | Total number of “msg-summary” Subscription 6XX Responses transmitted. | Int64
> msgsum-resubs-attrx | Total number of “msg-summary” Refresh Subscription Attempts received. | Int64
> msgsum-resubs-atttx | Total number of “msg-summary” Refresh Subscription Attempts transmitted. | Int64
> msgsum-resubs-succrx | Total number of “msg-summary” Refresh Subscription Successes received. | Int64
> msgsum-resubs-succtx | Total number of “msg-summary” Refresh Subscription Successes transmitted. | Int64
> msgsum-resubs-failrx | Total number of “msg-summary” Refresh Subscription Failures received. | Int64
> msgsum-resubs-failtx | Total number of “msg-summary” Refresh Subscription Failures transmitted. | Int64
> msgsum-resubs-resp-200rx | Total number of “msg-summary” Refresh Subscription 200 Responses received. | Int64
> msgsum-resubs-resp-200tx | Total number of “msg-summary” Refresh Subscription 200 Responses transmitted. | Int64
> msgsum-resubs-resp-202rx | Total number of “msg-summary” Refresh Subscription 202 Responses received. | Int64
> msgsum-resubs-resp-202tx | Total number of “msg-summary” Refresh Subscription 202 Responses transmitted. | Int64
> msgsum-resubs-resp-400rx | Total number of “msg-summary” Refresh Subscription 400 Responses received. | Int64
> msgsum-resubs-resp-400tx | Total number of “msg-summary” Refresh Subscription 400 Responses transmitted. | Int64
> msgsum-resubs-resp-403rx | Total number of “msg-summary” Refresh Subscription 403 Responses received. | Int64
> msgsum-resubs-resp-403tx | Total number of “msg-summary” Refresh Subscription 403 Responses transmitted. | Int64
> msgsum-resubs-resp-481rx | Total number of “msg-summary” Refresh Subscription 481 Responses received. | Int64
> msgsum-resubs-resp-481tx | Total number of “msg-summary” Refresh Subscription 481 Responses transmitted. | Int64
> msgsum-resubs-resp-489rx | Total number of “msg-summary” Refresh Subscription 489 Responses received. | Int64
> msgsum-resubs-resp-489tx | Total number of “msg-summary” Refresh Subscription 489 Responses transmitted. | Int64
> msgsum-resubs-resp-500rx | Total number of “msg-summary” Refresh Subscription 500 Responses received. | Int64
> msgsum-resubs-resp-500tx | Total number of “msg-summary” Refresh Subscription 500 Responses transmitted. | Int64
> msgsum-resubs-resp-3xxrx | Total number of “msg-summary” Refresh Subscription 3XX Responses received. | Int64
> msgsum-resubs-resp-3xxtx | Total number of “msg-summary” Refresh Subscription 3XX Responses transmitted. | Int64
> msgsum-resubs-resp-4xxrx | Total number of “msg-summary” Refresh Subscription 4XX Responses received. | Int64
> msgsum-resubs-resp-4xxtx | Total number of “msg-summary” Refresh Subscription 4XX Responses transmitted. | Int64
> msgsum-resubs-resp-5xxrx | Total number of “msg-summary” Refresh Subscription 5XX Responses received. | Int64
> msgsum-resubs-resp-5xxtx | Total number of “msg-summary” Refresh Subscription 5XX Responses transmitted. | Int64
> msgsum-resubs-resp-6xxrx | Total number of “msg-summary” Refresh Subscription 6XX Responses received. | Int64
> msgsum-resubs-resp-6xxtx | Total number of “msg-summary” Refresh Subscription 6XX Responses transmitted. | Int64
> msgsum-unsubs-attrx | Total number of “msg-summary” Un-Subscription Attempts received. | Int64
> msgsum-unsubs-atttx | Total number of “msg-summary” Un-Subscription Attempts transmitted. | Int64
> msgsum-unsubs-succrx | Total number of “msg-summary” Un-Subscription Successes received. | Int64
> msgsum-unsubs-succtx | Total number of “msg-summary” Un-Subscription Successes transmitted. | Int64
> msgsum-unsubs-failrx | Total number of “msg-summary” Un-Subscription Failures received. | Int64
> msgsum-unsubs-failtx | Total number of “msg-summary” Un-Subscription Failures transmitted. | Int64
> msgsum-unsubs-resp-200rx | Total number of “msg-summary” Un-Subscription 200 Responses received. | Int64
> msgsum-unsubs-resp-200tx | Total number of “msg-summary” Un-Subscription 200 Responses transmitted. | Int64
> msgsum-unsubs-resp-202rx | Total number of “msg-summary” Un-Subscription 202 Responses received. | Int64
> msgsum-unsubs-resp-202tx | Total number of “msg-summary” Un-Subscription 202 Responses transmitted. | Int64
> msgsum-unsubs-resp-400rx | Total number of “msg-summary” Un-Subscription 400 Responses received. | Int64
> msgsum-unsubs-resp-400tx | Total number of “msg-summary” Un-Subscription 400 Responses transmitted. | Int64
> msgsum-unsubs-resp-403rx | Total number of “msg-summary” Un-Subscription 403 Responses received. | Int64
> msgsum-unsubs-resp-403tx | Total number of “msg-summary” Un-Subscription 403 Responses transmitted. | Int64
> msgsum-unsubs-resp-481rx | Total number of “msg-summary” Un-Subscription 481 Responses received. | Int64
> msgsum-unsubs-resp-481tx | Total number of “msg-summary” Un-Subscription 481 Responses transmitted. | Int64
> msgsum-unsubs-resp-489rx | Total number of “msg-summary” Un-Subscription 489 Responses received. | Int64
> msgsum-unsubs-resp-489tx | Total number of “msg-summary” Un-Subscription 489 Responses transmitted. | Int64
> msgsum-unsubs-resp-500rx | Total number of “msg-summary” Un-Subscription 500 Responses received. | Int64
> msgsum-unsubs-resp-500tx | Total number of “msg-summary” Un-Subscription 500 Responses transmitted. | Int64
> msgsum-unsubs-resp-3xxrx | Total number of “msg-summary” Un-Subscription 3XX Responses received. | Int64
> msgsum-unsubs-resp-3xxtx | Total number of “msg-summary” Un-Subscription 3XX Responses transmitted. | Int64
> msgsum-unsubs-resp-4xxrx | Total number of “msg-summary” Un-Subscription 4XX Responses received. | Int64
> msgsum-unsubs-resp-4xxtx | Total number of “msg-summary” Un-Subscription 4XX Responses transmitted. | Int64
> msgsum-unsubs-resp-5xxrx | Total number of “msg-summary” Un-Subscription 5XX Responses received. | Int64
> msgsum-unsubs-resp-5xxtx | Total number of “msg-summary” Un-Subscription 5XX Responses transmitted. | Int64
> msgsum-unsubs-resp-6xxrx | Total number of “msg-summary” Un-Subscription 6XX Responses received. | Int64
> msgsum-unsubs-resp-6xxtx | Total number of “msg-summary” Un-Subscription 6XX Responses transmitted. | Int64
> msgsum-notify-attrx | Total number of “msg-summary” Notify Attempts received. | Int64
> msgsum-notify-atttx | Total number of “msg-summary” Notify Attempts transmitted. | Int64
> msgsum-notify-succrx | Total number of “msg-summary” Notify Successes received. | Int64
> msgsum-notify-succtx | Total number of “msg-summary” Notify Successes transmitted. | Int64
> msgsum-notify-failrx | Total number of “msg-summary” Notify Failures received. | Int64
> msgsum-notify-failtx | Total number of “msg-summary” Notify Failures transmitted. | Int64
> msgsum-notify-resp-3xxrx | Total number of “msg-summary” Notify 3XX Responses received. | Int64
> msgsum-notify-resp-3xxtx | Total number of “msg-summary” Notify 3XX Responses transmitted. | Int64
> msgsum-notify-resp-400rx | Total number of “msg-summary” Notify 400 Responses received. | Int64
> msgsum-notify-resp-400tx | Total number of “msg-summary” Notify 400 Responses transmitted. | Int64
> msgsum-notify-resp-481rx | Total number of “msg-summary” Notify 481 Responses received. | Int64
> msgsum-notify-resp-481tx | Total number of “msg-summary” Notify 481 Responses transmitted. | Int64
> msgsum-notify-resp-489rx | Total number of “msg-summary” Notify 489 Responses received. | Int64
> msgsum-notify-resp-489tx | Total number of “msg-summary” Notify 489 Responses transmitted. | Int64
> msgsum-notify-resp-4xxrx | Total number of “msg-summary” Notify 4XX Responses received. | Int64
> msgsum-notify-resp-4xxtx | Total number of “msg-summary” Notify 4XX Responses transmitted. | Int64
> msgsum-notify-resp-500rx | Total number of “msg-summary” Notify 500 Responses received. | Int64
> msgsum-notify-resp-500tx | Total number of “msg-summary” Notify 500 Responses transmitted. | Int64
> msgsum-notify-resp-5xxrx | Total number of “msg-summary” Notify 5XX Responses received. | Int64
> msgsum-notify-resp-5xxtx | Total number of “msg-summary” Notify 5XX Responses transmitted. | Int64
> msgsum-notify-resp-6xxrx | Total number of “msg-summary” Notify 6XX Responses received. | Int64
> msgsum-notify-resp-6xxtx | Total number of “msg-summary” Notify 6XX Responses transmitted. | Int64
> msgsum-pub-attrx | Total number of “msg-summary” Publish Attempts received. | Int64
> msgsum-pub-atttx | Total number of “msg-summary” Publish Attempts transmitted. | Int64
> msgsum-pub-succrx | Total number of “msg-summary” Publish Successes received. | Int64
> msgsum-pub-succtx | Total number of “msg-summary” Publish Successes transmitted. | Int64
> msgsum-pub-failrx | Total number of “msg-summary” Publish Failures received. | Int64
> msgsum-pub-failtx | Total number of “msg-summary” Publish Failures transmitted. | Int64
> msgsum-pub-resp-3xxrx | Total number of “msg-summary” Publish 3XX Responses received. | Int64
> msgsum-pub-resp-3xxtx | Total number of “msg-summary” Publish 3XX Responses transmitted. | Int64
> msgsum-pub-resp-400rx | Total number of “msg-summary” Publish 400 Responses received. | Int64
> msgsum-pub-resp-400tx | Total number of “msg-summary” Publish 400 Responses transmitted. | Int64
> msgsum-pub-resp-404rx | Total number of “msg-summary” Publish 404 Responses received. | Int64
> msgsum-pub-resp-404tx | Total number of “msg-summary” Publish 404 Responses transmitted. | Int64
> msgsum-pub-resp-412rx | Total number of “msg-summary” Publish 412 Responses received. | Int64
> msgsum-pub-resp-412tx | Total number of “msg-summary” Publish 412 Responses transmitted. | Int64
> msgsum-pub-resp-423rx | Total number of “msg-summary” Publish 423 Responses received. | Int64
> msgsum-pub-resp-423tx | Total number of “msg-summary” Publish 423 Responses transmitted. | Int64
> msgsum-pub-resp-489rx | Total number of “msg-summary” Publish 489 Responses received. | Int64
> msgsum-pub-resp-489tx | Total number of “msg-summary” Publish 489 Responses transmitted. | Int64
> msgsum-pub-resp-4xxrx | Total number of “msg-summary” Publish 4XX Responses received. | Int64
> msgsum-pub-resp-4xxtx | Total number of “msg-summary” Publish 4XX Responses transmitted. | Int64
> msgsum-pub-resp-500rx | Total number of “msg-summary” Publish 500 Responses received. | Int64
> msgsum-pub-resp-500tx | Total number of “msg-summary” Publish 500 Responses transmitted. | Int64
> msgsum-pub-resp-503rx | Total number of “msg-summary” Publish 503 Responses received. | Int64
> msgsum-pub-resp-503tx | Total number of “msg-summary” Publish 503 Responses transmitted. | Int64
> msgsum-pub-resp-5xxrx | Total number of “msg-summary” Publish 5XX Responses received. | Int64
> msgsum-pub-resp-5xxtx | Total number of “msg-summary” Publish 5XX Responses transmitted. | Int64
> msgsum-pub-resp-6xxrx | Total number of “msg-summary” Publish 6XX Responses received. | Int64
> msgsum-pub-resp-6xxtx | Total number of “msg-summary” Publish 6XX Responses transmitted. | Int64
> msgsum-unpub-attrx | Total number of “msg-summary” Un-Publish Attempts received. | Int64
> msgsum-unpub-atttx | Total number of “msg-summary” Un-Publish Attempts transmitted. | Int64
> msgsum-unpub-succrx | Total number of “msg-summary” Un-Publish Successes received. | Int64
> msgsum-unpub-succtx | Total number of “msg-summary” Un-Publish Successes transmitted. | Int64
> msgsum-unpub-failrx | Total number of “msg-summary” Un-Publish Failures received. | Int64
> msgsum-unpub-failtx | Total number of “msg-summary” Un-Publish Failures transmitted. | Int64
> msgsum-unpub-resp-3xxrx | Total number of “msg-summary” Un-Publish 3XX Responses received. | Int64
> msgsum-unpub-resp-3xxtx | Total number of “msg-summary” Un-Publish 3XX Responses transmitted. | Int64
> msgsum-unpub-resp-400rx | Total number of “msg-summary” Un-Publish 400 Responses received. | Int64
> msgsum-unpub-resp-400tx | Total number of “msg-summary” Un-Publish 400 Responses transmitted. | Int64
> msgsum-unpub-resp-404rx | Total number of “msg-summary” Un-Publish 404 Responses received. | Int64
> msgsum-unpub-resp-404tx | Total number of “msg-summary” Un-Publish 404 Responses transmitted. | Int64
> msgsum-unpub-resp-412rx | Total number of “msg-summary” Un-Publish 412 Responses received. | Int64
> msgsum-unpub-resp-412tx | Total number of “msg-summary” Un-Publish 412 Responses transmitted. | Int64
> msgsum-unpub-resp-423rx | Total number of “msg-summary” Un-Publish 423 Responses received. | Int64
> msgsum-unpub-resp-423tx | Total number of “msg-summary” Un-Publish 423 Responses transmitted. | Int64
> msgsum-unpub-resp-489rx | Total number of “msg-summary” Un-Publish 489 Responses received. | Int64
> msgsum-unpub-resp-489tx | Total number of “msg-summary” Un-Publish 489 Responses transmitted. | Int64
> msgsum-unpub-resp-4xxrx | Total number of “msg-summary” Un-Publish 4XX Responses received. | Int64
> msgsum-unpub-resp-4xxtx | Total number of “msg-summary” Un-Publish 4XX Responses transmitted. | Int64
> msgsum-unpub-resp-500rx | Total number of “msg-summary” Un-Publish 500 Responses received. | Int64
> msgsum-unpub-resp-500tx | Total number of “msg-summary” Un-Publish 500 Responses transmitted. | Int64
> msgsum-unpub-resp-503rx | Total number of “msg-summary” Un-Publish 503 Responses received. | Int64
> msgsum-unpub-resp-503tx | Total number of “msg-summary” Un-Publish 503 Responses transmitted. | Int64
> msgsum-unpub-resp-5xxrx | Total number of “msg-summary” Un-Publish 5XX Responses received. | Int64
> msgsum-unpub-resp-5xxtx | Total number of “msg-summary” Un-Publish 5XX Responses transmitted. | Int64
> msgsum-unpub-resp-6xxrx | Total number of “msg-summary” Un-Publish 6XX Responses received. | Int64
> msgsum-unpub-resp-6xxtx | Total number of “msg-summary” Un-Publish 6XX Responses transmitted. | Int64
> pres-subs-attrx | Total number of “presence” Subscription Attempts received. | Int64
> pres-subs-atttx | Total number of “presence” Subscription Attempts transmitted. | Int64
> pres-subs-succrx | Total number of “presence” Subscription Successes received. | Int64
> pres-subs-succtx | Total number of “presence” Subscription Successes transmitted. | Int64
> pres-subs-failrx | Total number of “presence” Subscription Failures received. | Int64
> pres-subs-failtx | Total number of “presence” Subscription Failures transmitted. | Int64
> pres-subs-resp-200rx | Total number of “presence” Subscription 200 Responses received. | Int64
> pres-subs-resp-200tx | Total number of “presence” Subscription 200 Responses transmitted. | Int64
> pres-subs-resp-202rx | Total number of “presence” Subscription 202 Responses received. | Int64
> pres-subs-resp-202tx | Total number of “presence” Subscription 202 Responses transmitted. | Int64
> pres-subs-resp-400rx | Total number of “presence” Subscription 400 Responses received. | Int64
> pres-subs-resp-400tx | Total number of “presence” Subscription 400 Responses transmitted. | Int64
> pres-subs-resp-403rx | Total number of “presence” Subscription 403 Responses received. | Int64
> pres-subs-resp-403tx | Total number of “presence” Subscription 403 Responses transmitted. | Int64
> pres-subs-resp-481rx | Total number of “presence” Subscription 481 Responses received. | Int64
> pres-subs-resp-481tx | Total number of “presence” Subscription 481 Responses transmitted. | Int64
> pres-subs-resp-489rx | Total number of “presence” Subscription 489 Responses received. | Int64
> pres-subs-resp-489tx | Total number of “presence” Subscription 489 Responses transmitted. | Int64
> pres-subs-resp-500rx | Total number of “presence” Subscription 500 Responses received. | Int64
> pres-subs-resp-500tx | Total number of “presence” Subscription 500 Responses transmitted. | Int64
> pres-subs-resp-3xxrx | Total number of “presence” Subscription 3XX Responses received. | Int64
> pres-subs-resp-3xxtx | Total number of “presence” Subscription 3XX Responses transmitted. | Int64
> pres-subs-resp-4xxrx | Total number of “presence” Subscription 4XX Responses received. | Int64
> pres-subs-resp-4xxtx | Total number of “presence” Subscription 4XX Responses transmitted. | Int64
> pres-subs-resp-5xxrx | Total number of “presence” Subscription 5XX Responses received. | Int64
> pres-subs-resp-5xxtx | Total number of “presence” Subscription 5XX Responses transmitted. | Int64
> pres-subs-resp-6xxrx | Total number of “presence” Subscription 6XX Responses received. | Int64
> pres-subs-resp-6xxtx | Total number of “presence” Subscription 6XX Responses transmitted. | Int64
> pres-resubs-attrx | Total number of “presence” Refresh Subscription Attempts received. | Int64
> pres-resubs-atttx | Total number of “presence” Refresh Subscription Attempts transmitted. | Int64
> pres-resubs-succrx | Total number of “presence” Refresh Subscription Successes received. | Int64
> pres-resubs-succtx | Total number of “presence” Refresh Subscription Successes transmitted. | Int64
> pres-resubs-failrx | Total number of “presence” Refresh Subscription Failures received. | Int64
> pres-resubs-failtx | Total number of “presence” Refresh Subscription Failures transmitted. | Int64
> pres-resubs-resp-200rx | Total number of “presence” Refresh Subscription 200 Responses received. | Int64
> pres-resubs-resp-200tx | Total number of “presence” Refresh Subscription 200 Responses transmitted. | Int64
> pres-resubs-resp-202rx | Total number of “presence” Refresh Subscription 202 Responses received. | Int64
> pres-resubs-resp-202tx | Total number of “presence” Refresh Subscription 202 Responses transmitted. | Int64
> pres-resubs-resp-400rx | Total number of “presence” Refresh Subscription 400 Responses received. | Int64
> pres-resubs-resp-400tx | Total number of “presence” Refresh Subscription 400 Responses transmitted. | Int64
> pres-resubs-resp-403rx | Total number of “presence” Refresh Subscription 403 Responses received. | Int64
> pres-resubs-resp-403tx | Total number of “presence” Refresh Subscription 403 Responses transmitted. | Int64
> pres-resubs-resp-481rx | Total number of “presence” Refresh Subscription 481 Responses received. | Int64
> pres-resubs-resp-481tx | Total number of “presence” Refresh Subscription 481 Responses transmitted. | Int64
> pres-resubs-resp-489rx | Total number of “presence” Refresh Subscription 489 Responses received. | Int64
> pres-resubs-resp-489tx | Total number of “presence” Refresh Subscription 489 Responses transmitted. | Int64
> pres-resubs-resp-500rx | Total number of “presence” Refresh Subscription 500 Responses received. | Int64
> pres-resubs-resp-500tx | Total number of “presence” Refresh Subscription 500 Responses transmitted. | Int64
> pres-resubs-resp-3xxrx | Total number of “presence” Refresh Subscription 3XX Responses received. | Int64
> pres-resubs-resp-3xxtx | Total number of “presence” Refresh Subscription 3XX Responses transmitted. | Int64
> pres-resubs-resp-4xxrx | Total number of “presence” Refresh Subscription 4XX Responses received. | Int64
> pres-resubs-resp-4xxtx | Total number of “presence” Refresh Subscription 4XX Responses transmitted. | Int64
> pres-resubs-resp-5xxrx | Total number of “presence” Refresh Subscription 5XX Responses received. | Int64
> pres-resubs-resp-5xxtx | Total number of “presence” Refresh Subscription 5XX Responses transmitted. | Int64
> pres-resubs-resp-6xxrx | Total number of “presence” Refresh Subscription 6XX Responses received. | Int64
> pres-resubs-resp-6xxtx | Total number of “presence” Refresh Subscription 6XX Responses transmitted. | Int64
> pres-unsubs-attrx | Total number of “presence” Un-Subscription Attempts received. | Int64
> pres-unsubs-atttx | Total number of “presence” Un-Subscription Attempts transmitted. | Int64
> pres-unsubs-succrx | Total number of “presence” Un-Subscription Successes received. | Int64
> pres-unsubs-succtx | Total number of “presence” Un-Subscription Successes transmitted. | Int64
> pres-unsubs-failrx | Total number of “presence” Un-Subscription Failures received. | Int64
> pres-unsubs-failtx | Total number of “presence” Un-Subscription Failures transmitted. | Int64
> pres-unsubs-resp-200rx | Total number of “presence” Un-Subscription 200 Responses received. | Int64
> pres-unsubs-resp-200tx | Total number of “presence” Un-Subscription 200 Responses transmitted. | Int64
> pres-unsubs-resp-202rx | Total number of “presence” Un-Subscription 202 Responses received. | Int64
> pres-unsubs-resp-202tx | Total number of “presence” Un-Subscription 202 Responses transmitted. | Int64
> pres-unsubs-resp-400rx | Total number of “presence” Un-Subscription 400 Responses received. | Int64
> pres-unsubs-resp-400tx | Total number of “presence” Un-Subscription 400 Responses transmitted. | Int64
> pres-unsubs-resp-403rx | Total number of “presence” Un-Subscription 403 Responses received. | Int64
> pres-unsubs-resp-403tx | Total number of “presence” Un-Subscription 403 Responses transmitted. | Int64
> pres-unsubs-resp-481rx | Total number of “presence” Un-Subscription 481 Responses received. | Int64
> pres-unsubs-resp-481tx | Total number of “presence” Un-Subscription 481 Responses transmitted. | Int64
> pres-unsubs-resp-489rx | Total number of “presence” Un-Subscription 489 Responses received. | Int64
> pres-unsubs-resp-489tx | Total number of “presence” Un-Subscription 489 Responses transmitted. | Int64
> pres-unsubs-resp-500rx | Total number of “presence” Un-Subscription 500 Responses received. | Int64
> pres-unsubs-resp-500tx | Total number of “presence” Un-Subscription 500 Responses transmitted. | Int64
> pres-unsubs-resp-3xxrx | Total number of “presence” Un-Subscription 3XX Responses received. | Int64
> pres-unsubs-resp-3xxtx | Total number of “presence” Un-Subscription 3XX Responses transmitted. | Int64
> pres-unsubs-resp-4xxrx | Total number of “presence” Un-Subscription 4XX Responses received. | Int64
> pres-unsubs-resp-4xxtx | Total number of “presence” Un-Subscription 4XX Responses transmitted. | Int64
> pres-unsubs-resp-5xxrx | Total number of “presence” Un-Subscription 5XX Responses received. | Int64
> pres-unsubs-resp-5xxtx | Total number of “presence” Un-Subscription 5XX Responses transmitted. | Int64
> pres-unsubs-resp-6xxrx | Total number of “presence” Un-Subscription 6XX Responses received. | Int64
> pres-unsubs-resp-6xxtx | Total number of “presence” Un-Subscription 6XX Responses transmitted. | Int64
> pres-notify-attrx | Total number of “presence” Notify Attempts received. | Int64
> pres-notify-atttx | Total number of “presence” Notify Attempts transmitted. | Int64
> pres-notify-succrx | Total number of “presence” Notify Successes received. | Int64
> pres-notify-succtx | Total number of “presence” Notify Successes transmitted. | Int64
> pres-notify-failrx | Total number of “presence” Notify Failures received. | Int64
> pres-notify-failtx | Total number of “presence” Notify Failures transmitted. | Int64
> pres-notify-resp-3xxrx | Total number of “presence” Notify 3XX Responses received. | Int64
> pres-notify-resp-3xxtx | Total number of “presence” Notify 3XX Responses transmitted. | Int64
> pres-notify-resp-400rx | Total number of “presence” Notify 400 Responses received. | Int64
> pres-notify-resp-400tx | Total number of “presence” Notify 400 Responses transmitted. | Int64
> pres-notify-resp-481rx | Total number of “presence” Notify 481 Responses received. | Int64
> pres-notify-resp-481tx | Total number of “presence” Notify 481 Responses transmitted. | Int64
> pres-notify-resp-489rx | Total number of “presence” Notify 489 Responses received. | Int64
> pres-notify-resp-489tx | Total number of “presence” Notify 489 Responses transmitted. | Int64
> pres-notify-resp-4xxrx | Total number of “presence” Notify 4XX Responses received. | Int64
> pres-notify-resp-4xxtx | Total number of “presence” Notify 4XX Responses transmitted. | Int64
> pres-notify-resp-500rx | Total number of “presence” Notify 500 Responses received. | Int64
> pres-notify-resp-500tx | Total number of “presence” Notify 500 Responses transmitted. | Int64
> pres-notify-resp-5xxrx | Total number of “presence” Notify 5XX Responses received. | Int64
> pres-notify-resp-5xxtx | Total number of “presence” Notify 5XX Responses transmitted. | Int64
> pres-notify-resp-6xxrx | Total number of “presence” Notify 6XX Responses received. | Int64
> pres-notify-resp-6xxtx | Total number of “presence” Notify 6XX Responses transmitted. | Int64
> pres-pub-attrx | Total number of “presence” Publish Attempts received. | Int64
> pres-pub-atttx | Total number of “presence” Publish Attempts transmitted. | Int64
> pres-pub-succrx | Total number of “presence” Publish Successes received. | Int64
> pres-pub-succtx | Total number of “presence” Publish Successes transmitted. | Int64
> pres-pub-failrx | Total number of “presence” Publish Failures received. | Int64
> pres-pub-failtx | Total number of “presence” Publish Failures transmitted. | Int64
> pres-pub-resp-3xxrx | Total number of “presence” Publish 3XX Responses received. | Int64
> pres-pub-resp-3xxtx | Total number of “presence” Publish 3XX Responses transmitted. | Int64
> pres-pub-resp-400rx | Total number of “presence” Publish 400 Responses received. | Int64
> pres-pub-resp-400tx | Total number of “presence” Publish 400 Responses transmitted. | Int64
> pres-pub-resp-404rx | Total number of “presence” Publish 404 Responses received. | Int64
> pres-pub-resp-404tx | Total number of “presence” Publish 404 Responses transmitted. | Int64
> pres-pub-resp-412rx | Total number of “presence” Publish 412 Responses received. | Int64
> pres-pub-resp-412tx | Total number of “presence” Publish 412 Responses transmitted. | Int64
> pres-pub-resp-423rx | Total number of “presence” Publish 423 Responses received. | Int64
> pres-pub-resp-423tx | Total number of “presence” Publish 423 Responses transmitted. | Int64
> pres-pub-resp-489rx | Total number of “presence” Publish 489 Responses received. | Int64
> pres-pub-resp-489tx | Total number of “presence” Publish 489 Responses transmitted. | Int64
> pres-pub-resp-4xxrx | Total number of “presence” Publish 4XX Responses received. | Int64
> pres-pub-resp-4xxtx | Total number of “presence” Publish 4XX Responses transmitted. | Int64
> pres-pub-resp-500rx | Total number of “presence” Publish 500 Responses received. | Int64
> pres-pub-resp-500tx | Total number of “presence” Publish 500 Responses transmitted. | Int64
> pres-pub-resp-503rx | Total number of “presence” Publish 503 Responses received. | Int64
> pres-pub-resp-503tx | Total number of “presence” Publish 503 Responses transmitted. | Int64
> pres-pub-resp-5xxrx | Total number of “presence” Publish 5XX Responses received. | Int64
> pres-pub-resp-5xxtx | Total number of “presence” Publish 5XX Responses transmitted. | Int64
> pres-pub-resp-6xxrx | Total number of “presence” Publish 6XX Responses received. | Int64
> pres-pub-resp-6xxtx | Total number of “presence” Publish 6XX Responses transmitted. | Int64
> pres-unpub-attrx | Total number of “presence” Un-Publish Attempts received. | Int64
> pres-unpub-atttx | Total number of “presence” Un-Publish Attempts transmitted. | Int64
> pres-unpub-succrx | Total number of “presence” Un-Publish Successes received. | Int64
> pres-unpub-succtx | Total number of “presence” Un-Publish Successes transmitted. | Int64
> pres-unpub-failrx | Total number of “presence” Un-Publish Failures received. | Int64
> pres-unpub-failtx | Total number of “presence” Un-Publish Failures transmitted. | Int64
> pres-unpub-resp-3xxrx | Total number of “presence” Un-Publish 3XX Responses received. | Int64
> pres-unpub-resp-3xxtx | Total number of “presence” Un-Publish 3XX Responses transmitted. | Int64
> pres-unpub-resp-400rx | Total number of “presence” Un-Publish 400 Responses received. | Int64
> pres-unpub-resp-400tx | Total number of “presence” Un-Publish 400 Responses transmitted. | Int64
> pres-unpub-resp-404rx | Total number of “presence” Un-Publish 404 Responses received. | Int64
> pres-unpub-resp-404tx | Total number of “presence” Un-Publish 404 Responses transmitted. | Int64
> pres-unpub-resp-412rx | Total number of “presence” Un-Publish 412 Responses received. | Int64
> pres-unpub-resp-412tx | Total number of “presence” Un-Publish 412 Responses transmitted. | Int64
> pres-unpub-resp-423rx | Total number of “presence” Un-Publish 423 Responses received. | Int64
> pres-unpub-resp-423tx | Total number of “presence” Un-Publish 423 Responses transmitted. | Int64
> pres-unpub-resp-489rx | Total number of “presence” Un-Publish 489 Responses received. | Int64
> pres-unpub-resp-489tx | Total number of “presence” Un-Publish 489 Responses transmitted. | Int64
> pres-unpub-resp-4xxrx | Total number of “presence” Un-Publish 4XX Responses received. | Int64
> pres-unpub-resp-4xxtx | Total number of “presence” Un-Publish 4XX Responses transmitted. | Int64
> pres-unpub-resp-500rx | Total number of “presence” Un-Publish 500 Responses received. | Int64
> pres-unpub-resp-500tx | Total number of “presence” Un-Publish 500 Responses transmitted. | Int64
> pres-unpub-resp-503rx | Total number of “presence” Un-Publish 503 Responses received. | Int64
> pres-unpub-resp-503tx | Total number of “presence” Un-Publish 503 Responses transmitted. | Int64
> pres-unpub-resp-5xxrx | Total number of “presence” Un-Publish 5XX Responses received. | Int64
> pres-unpub-resp-5xxtx | Total number of “presence” Un-Publish 5XX Responses transmitted. | Int64
> pres-unpub-resp-6xxrx | Total number of “presence” Un-Publish 6XX Responses received. | Int64
> pres-unpub-resp-6xxtx | Total number of “presence” Un-Publish 6XX Responses transmitted. | Int64
> reg-subs-attrx | Total number of “reg” Subscription Attempts received. | Int64
> reg-subs-atttx | Total number of “reg” Subscription Attempts transmitted. | Int64
> reg-subs-succrx | Total number of “reg” Subscription Successes received. | Int64
> reg-subs-succtx | Total number of “reg” Subscription Successes transmitted. | Int64
> reg-subs-failrx | Total number of “reg” Subscription Failures received. | Int64
> reg-subs-failtx | Total number of “reg” Subscription Failures transmitted. | Int64
> reg-subs-resp-200rx | Total number of “reg” Subscription 200 Responses received. | Int64
> reg-subs-resp-200tx | Total number of “reg” Subscription 200 Responses transmitted. | Int64
> reg-subs-resp-202rx | Total number of “reg” Subscription 202 Responses received. | Int64
> reg-subs-resp-202tx | Total number of “reg” Subscription 202 Responses transmitted. | Int64
> reg-subs-resp-400rx | Total number of “reg” Subscription 400 Responses received. | Int64
> reg-subs-resp-400tx | Total number of “reg” Subscription 400 Responses transmitted. | Int64
> reg-subs-resp-403rx | Total number of “reg” Subscription 403 Responses received. | Int64
> reg-subs-resp-403tx | Total number of “reg” Subscription 403 Responses transmitted. | Int64
> reg-subs-resp-481rx | Total number of “reg” Subscription 481 Responses received. | Int64
> reg-subs-resp-481tx | Total number of “reg” Subscription 481 Responses transmitted. | Int64
> reg-subs-resp-489rx | Total number of “reg” Subscription 489 Responses received. | Int64
> reg-subs-resp-489tx | Total number of “reg” Subscription 489 Responses transmitted. | Int64
> reg-subs-resp-500rx | Total number of “reg” Subscription 500 Responses received. | Int64
> reg-subs-resp-500tx | Total number of “reg” Subscription 500 Responses transmitted. | Int64
> reg-subs-resp-3xxrx | Total number of “reg” Subscription 3XX Responses received. | Int64
> reg-subs-resp-3xxtx | Total number of “reg” Subscription 3XX Responses transmitted. | Int64
> reg-subs-resp-4xxrx | Total number of “reg” Subscription 4XX Responses received. | Int64
> reg-subs-resp-4xxtx | Total number of “reg” Subscription 4XX Responses transmitted. | Int64
> reg-subs-resp-5xxrx | Total number of “reg” Subscription 5XX Responses received. | Int64
> reg-subs-resp-5xxtx | Total number of “reg” Subscription 5XX Responses transmitted. | Int64
> reg-subs-resp-6xxrx | Total number of “reg” Subscription 6XX Responses received. | Int64
> reg-subs-resp-6xxtx | Total number of “reg” Subscription 6XX Responses transmitted. | Int64
> reg-resubs-attrx | Total number of “reg” Refresh Subscription Attempts received. | Int64
> reg-resubs-atttx | Total number of “reg” Refresh Subscription Attempts transmitted. | Int64
> reg-resubs-succrx | Total number of “reg” Refresh Subscription Successes received. | Int64
> reg-resubs-succtx | Total number of “reg” Refresh Subscription Successes transmitted. | Int64
> reg-resubs-failrx | Total number of “reg” Refresh Subscription Failures received. | Int64
> reg-resubs-failtx | Total number of “reg” Refresh Subscription Failures transmitted. | Int64
> reg-resubs-resp-200rx | Total number of “reg” Refresh Subscription 200 Responses received. | Int64
> reg-resubs-resp-200tx | Total number of “reg” Refresh Subscription 200 Responses transmitted. | Int64
> reg-resubs-resp-202rx | Total number of “reg” Refresh Subscription 202 Responses received. | Int64
> reg-resubs-resp-202tx | Total number of “reg” Refresh Subscription 202 Responses transmitted. | Int64
> reg-resubs-resp-400rx | Total number of “reg” Refresh Subscription 400 Responses received. | Int64
> reg-resubs-resp-400tx | Total number of “reg” Refresh Subscription 400 Responses transmitted. | Int64
> reg-resubs-resp-403rx | Total number of “reg” Refresh Subscription 403 Responses received. | Int64
> reg-resubs-resp-403tx | Total number of “reg” Refresh Subscription 403 Responses transmitted. | Int64
> reg-resubs-resp-481rx | Total number of “reg” Refresh Subscription 481 Responses received. | Int64
> reg-resubs-resp-481tx | Total number of “reg” Refresh Subscription 481 Responses transmitted. | Int64
> reg-resubs-resp-489rx | Total number of “reg” Refresh Subscription 489 Responses received. | Int64
> reg-resubs-resp-489tx | Total number of “reg” Refresh Subscription 489 Responses transmitted. | Int64
> reg-resubs-resp-500rx | Total number of “reg” Refresh Subscription 500 Responses received. | Int64
> reg-resubs-resp-500tx | Total number of “reg” Refresh Subscription 500 Responses transmitted. | Int64
> reg-resubs-resp-3xxrx | Total number of “reg” Refresh Subscription 3XX Responses received. | Int64
> reg-resubs-resp-3xxtx | Total number of “reg” Refresh Subscription 3XX Responses transmitted. | Int64
> reg-resubs-resp-4xxrx | Total number of “reg” Refresh Subscription 4XX Responses received. | Int64
> reg-resubs-resp-4xxtx | Total number of “reg” Refresh Subscription 4XX Responses transmitted. | Int64
> reg-resubs-resp-5xxrx | Total number of “reg” Refresh Subscription 5XX Responses received. | Int64
> reg-resubs-resp-5xxtx | Total number of “reg” Refresh Subscription 5XX Responses transmitted. | Int64
> reg-resubs-resp-6xxrx | Total number of “reg” Refresh Subscription 6XX Responses received. | Int64
> reg-resubs-resp-6xxtx | Total number of “reg” Refresh Subscription 6XX Responses transmitted. | Int64
> reg-unsubs-attrx | Total number of “reg” Un-Subscription Attempts received. | Int64
> reg-unsubs-atttx | Total number of “reg” Un-Subscription Attempts transmitted. | Int64
> reg-unsubs-succrx | Total number of “reg” Un-Subscription Successes received. | Int64
> reg-unsubs-succtx | Total number of “reg” Un-Subscription Successes transmitted. | Int64
> reg-unsubs-failrx | Total number of “reg” Un-Subscription Failures received. | Int64
> reg-unsubs-failtx | Total number of “reg” Un-Subscription Failures transmitted. | Int64
> reg-unsubs-resp-200rx | Total number of “reg” Un-Subscription 200 Responses received. | Int64
> reg-unsubs-resp-200tx | Total number of “reg” Un-Subscription 200 Responses transmitted. | Int64
> reg-unsubs-resp-202rx | Total number of “reg” Un-Subscription 202 Responses received. | Int64
> reg-unsubs-resp-202tx | Total number of “reg” Un-Subscription 202 Responses transmitted. | Int64
> reg-unsubs-resp-400rx | Total number of “reg” Un-Subscription 400 Responses received. | Int64
> reg-unsubs-resp-400tx | Total number of “reg” Un-Subscription 400 Responses transmitted. | Int64
> reg-unsubs-resp-403rx | Total number of “reg” Un-Subscription 403 Responses received. | Int64
> reg-unsubs-resp-403tx | Total number of “reg” Un-Subscription 403 Responses transmitted. | Int64
> reg-unsubs-resp-481rx | Total number of “reg” Un-Subscription 481 Responses received. | Int64
> reg-unsubs-resp-481tx | Total number of “reg” Un-Subscription 481 Responses transmitted. | Int64
> reg-unsubs-resp-489rx | Total number of “reg” Un-Subscription 489 Responses received. | Int64
> reg-unsubs-resp-489tx | Total number of “reg” Un-Subscription 489 Responses transmitted. | Int64
> reg-unsubs-resp-500rx | Total number of “reg” Un-Subscription 500 Responses received. | Int64
> reg-unsubs-resp-500tx | Total number of “reg” Un-Subscription 500 Responses transmitted. | Int64
> reg-unsubs-resp-3xxrx | Total number of “reg” Un-Subscription 3XX Responses received. | Int64
> reg-unsubs-resp-3xxtx | Total number of “reg” Un-Subscription 3XX Responses transmitted. | Int64
> reg-unsubs-resp-4xxrx | Total number of “reg” Un-Subscription 4XX Responses received. | Int64
> reg-unsubs-resp-4xxtx | Total number of “reg” Un-Subscription 4XX Responses transmitted. | Int64
> reg-unsubs-resp-5xxrx | Total number of “reg” Un-Subscription 5XX Responses received. | Int64
> reg-unsubs-resp-5xxtx | Total number of “reg” Un-Subscription 5XX Responses transmitted. | Int64
> reg-unsubs-resp-6xxrx | Total number of “reg” Un-Subscription 6XX Responses received. | Int64
> reg-unsubs-resp-6xxtx | Total number of “reg” Un-Subscription 6XX Responses transmitted. | Int64
> reg-notify-attrx | Total number of “reg” Notify Attempts received. | Int64
> reg-notify-atttx | Total number of “reg” Notify Attempts transmitted. | Int64
> reg-notify-succrx | Total number of “reg” Notify Successes received. | Int64
> reg-notify-succtx | Total number of “reg” Notify Successes transmitted. | Int64
> reg-notify-failrx | Total number of “reg” Notify Failures received. | Int64
> reg-notify-failtx | Total number of “reg” Notify Failures transmitted. | Int64
> reg-notify-resp-3xxrx | Total number of “reg” Notify 3XX Responses received. | Int64
> reg-notify-resp-3xxtx | Total number of “reg” Notify 3XX Responses transmitted. | Int64
> reg-notify-resp-400rx | Total number of “reg” Notify 400 Responses received. | Int64
> reg-notify-resp-400tx | Total number of “reg” Notify 400 Responses transmitted. | Int64
> reg-notify-resp-481rx | Total number of “reg” Notify 481 Responses received. | Int64
> reg-notify-resp-481tx | Total number of “reg” Notify 481 Responses transmitted. | Int64
> reg-notify-resp-489rx | Total number of “reg” Notify 489 Responses received. | Int64
> reg-notify-resp-489tx | Total number of “reg” Notify 489 Responses transmitted. | Int64
> reg-notify-resp-4xxrx | Total number of “reg” Notify 4XX Responses received. | Int64
> reg-notify-resp-4xxtx | Total number of “reg” Notify 4XX Responses transmitted. | Int64
> reg-notify-resp-500rx | Total number of “reg” Notify 500 Responses received. | Int64
> reg-notify-resp-500tx | Total number of “reg” Notify 500 Responses transmitted. | Int64
> reg-notify-resp-5xxrx | Total number of “reg” Notify 5XX Responses received. | Int64
> reg-notify-resp-5xxtx | Total number of “reg” Notify 5XX Responses transmitted. | Int64
> reg-notify-resp-6xxrx | Total number of “reg” Notify 6XX Responses received. | Int64
> reg-notify-resp-6xxtx | Total number of “reg” Notify 6XX Responses transmitted. | Int64
> reg-pub-attrx | Total number of “reg” Publish Attempts received. | Int64
> reg-pub-atttx | Total number of “reg” Publish Attempts transmitted. | Int64
> reg-pub-succrx | Total number of “reg” Publish Successes received. | Int64
> reg-pub-succtx | Total number of “reg” Publish Successes transmitted. | Int64
> reg-pub-failrx | Total number of “reg” Publish Failures received. | Int64
> reg-pub-failtx | Total number of “reg” Publish Failures transmitted. | Int64
> reg-pub-resp-3xxrx | Total number of “reg” Publish 3XX Responses received. | Int64
> reg-pub-resp-3xxtx | Total number of “reg” Publish 3XX Responses transmitted. | Int64
> reg-pub-resp-400rx | Total number of “reg” Publish 400 Responses received. | Int64
> reg-pub-resp-400tx | Total number of “reg” Publish 400 Responses transmitted. | Int64
> reg-pub-resp-404rx | Total number of “reg” Publish 404 Responses received. | Int64
> reg-pub-resp-404tx | Total number of “reg” Publish 404 Responses transmitted. | Int64
> reg-pub-resp-412rx | Total number of “reg” Publish 412 Responses received. | Int64
> reg-pub-resp-412tx | Total number of “reg” Publish 412 Responses transmitted. | Int64
> reg-pub-resp-423rx | Total number of “reg” Publish 423 Responses received. | Int64
> reg-pub-resp-423tx | Total number of “reg” Publish 423 Responses transmitted. | Int64
> reg-pub-resp-489rx | Total number of “reg” Publish 489 Responses received. | Int64
> reg-pub-resp-489tx | Total number of “reg” Publish 489 Responses transmitted. | Int64
> reg-pub-resp-4xxrx | Total number of “reg” Publish 4XX Responses received. | Int64
> reg-pub-resp-4xxtx | Total number of “reg” Publish 4XX Responses transmitted. | Int64
> reg-pub-resp-500rx | Total number of “reg” Publish 500 Responses received. | Int64
> reg-pub-resp-500tx | Total number of “reg” Publish 500 Responses transmitted. | Int64
> reg-pub-resp-503rx | Total number of “reg” Publish 503 Responses received. | Int64
> reg-pub-resp-503tx | Total number of “reg” Publish 503 Responses transmitted. | Int64
> reg-pub-resp-5xxrx | Total number of “reg” Publish 5XX Responses received. | Int64
> reg-pub-resp-5xxtx | Total number of “reg” Publish 5XX Responses transmitted. | Int64
> reg-pub-resp-6xxrx | Total number of “reg” Publish 6XX Responses received. | Int64
> reg-pub-resp-6xxtx | Total number of “reg” Publish 6XX Responses transmitted. | Int64
> reg-unpub-attrx | Total number of “reg” Un-Publish Attempts received. | Int64
> reg-unpub-atttx | Total number of “reg” Un-Publish Attempts transmitted. | Int64
> reg-unpub-succrx | Total number of “reg” Un-Publish Successes received. | Int64
> reg-unpub-succtx | Total number of “reg” Un-Publish Successes transmitted. | Int64
> reg-unpub-failrx | Total number of “reg” Un-Publish Failures received. | Int64
> reg-unpub-failtx | Total number of “reg” Un-Publish Failures transmitted. | Int64
> reg-unpub-resp-3xxrx | Total number of “reg” Un-Publish 3XX Responses received. | Int64
> reg-unpub-resp-3xxtx | Total number of “reg” Un-Publish 3XX Responses transmitted. | Int64
> reg-unpub-resp-400rx | Total number of “reg” Un-Publish 400 Responses received. | Int64
> reg-unpub-resp-400tx | Total number of “reg” Un-Publish 400 Responses transmitted. | Int64
> reg-unpub-resp-404rx | Total number of “reg” Un-Publish 404 Responses received. | Int64
> reg-unpub-resp-404tx | Total number of “reg” Un-Publish 404 Responses transmitted. | Int64
> reg-unpub-resp-412rx | Total number of “reg” Un-Publish 412 Responses received. | Int64
> reg-unpub-resp-412tx | Total number of “reg” Un-Publish 412 Responses transmitted. | Int64
> reg-unpub-resp-423rx | Total number of “reg” Un-Publish 423 Responses received. | Int64
> reg-unpub-resp-423tx | Total number of “reg” Un-Publish 423 Responses transmitted. | Int64
> reg-unpub-resp-489rx | Total number of “reg” Un-Publish 489 Responses received. | Int64
> reg-unpub-resp-489tx | Total number of “reg” Un-Publish 489 Responses transmitted. | Int64
> reg-unpub-resp-4xxrx | Total number of “reg” Un-Publish 4XX Responses received. | Int64
> reg-unpub-resp-4xxtx | Total number of “reg” Un-Publish 4XX Responses transmitted. | Int64
> reg-unpub-resp-500rx | Total number of “reg” Un-Publish 500 Responses received. | Int64
> reg-unpub-resp-500tx | Total number of “reg” Un-Publish 500 Responses transmitted. | Int64
> reg-unpub-resp-503rx | Total number of “reg” Un-Publish 503 Responses received. | Int64
> reg-unpub-resp-503tx | Total number of “reg” Un-Publish 503 Responses transmitted. | Int64
> reg-unpub-resp-5xxrx | Total number of “reg” Un-Publish 5XX Responses received. | Int64
> reg-unpub-resp-5xxtx | Total number of “reg” Un-Publish 5XX Responses transmitted. | Int64
> reg-unpub-resp-6xxrx | Total number of “reg” Un-Publish 6XX Responses received. | Int64
> reg-unpub-resp-6xxtx | Total number of “reg” Un-Publish 6XX Responses transmitted. | Int64
> winfo-subs-attrx | Total number of “winfo” Subscription Attempts received. | Int64
> winfo-subs-atttx | Total number of “winfo” Subscription Attempts transmitted. | Int64
> winfo-subs-succrx | Total number of “winfo” Subscription Successes received. | Int64
> winfo-subs-succtx | Total number of “winfo” Subscription Successes transmitted. | Int64
> winfo-subs-failrx | Total number of “winfo” Subscription Failures received. | Int64
> winfo-subs-failtx | Total number of “winfo” Subscription Failures transmitted. | Int64
> winfo-subs-resp-200rx | Total number of “winfo” Subscription 200 Responses received. | Int64
> winfo-subs-resp-200tx | Total number of “winfo” Subscription 200 Responses transmitted. | Int64
> winfo-subs-resp-202rx | Total number of “winfo” Subscription 202 Responses received. | Int64
> winfo-subs-resp-202tx | Total number of “winfo” Subscription 202 Responses transmitted. | Int64
> winfo-subs-resp-400rx | Total number of “winfo” Subscription 400 Responses received. | Int64
> winfo-subs-resp-400tx | Total number of “winfo” Subscription 400 Responses transmitted. | Int64
> winfo-subs-resp-403rx | Total number of “winfo” Subscription 403 Responses received. | Int64
> winfo-subs-resp-403tx | Total number of “winfo” Subscription 403 Responses transmitted. | Int64
> winfo-subs-resp-481rx | Total number of “winfo” Subscription 481 Responses received. | Int64
> winfo-subs-resp-481tx | Total number of “winfo” Subscription 481 Responses transmitted. | Int64
> winfo-subs-resp-489rx | Total number of “winfo” Subscription 489 Responses received. | Int64
> winfo-subs-resp-489tx | Total number of “winfo” Subscription 489 Responses transmitted. | Int64
> winfo-subs-resp-500rx | Total number of “winfo” Subscription 500 Responses received. | Int64
> winfo-subs-resp-500tx | Total number of “winfo” Subscription 500 Responses transmitted. | Int64
> winfo-subs-resp-3xxrx | Total number of “winfo” Subscription 3XX Responses received. | Int64
> winfo-subs-resp-3xxtx | Total number of “winfo” Subscription 3XX Responses transmitted. | Int64
> winfo-subs-resp-4xxrx | Total number of “winfo” Subscription 4XX Responses received. | Int64
> winfo-subs-resp-4xxtx | Total number of “winfo” Subscription 4XX Responses transmitted. | Int64
> winfo-subs-resp-5xxrx | Total number of “winfo” Subscription 5XX Responses received. | Int64
> winfo-subs-resp-5xxtx | Total number of “winfo” Subscription 5XX Responses transmitted. | Int64
> winfo-subs-resp-6xxrx | Total number of “winfo” Subscription 6XX Responses received. | Int64
> winfo-subs-resp-6xxtx | Total number of “winfo” Subscription 6XX Responses transmitted. | Int64
> winfo-resubs-attrx | Total number of “winfo” Refresh Subscription Attempts received. | Int64
> winfo-resubs-atttx | Total number of “winfo” Refresh Subscription Attempts transmitted. | Int64
> winfo-resubs-succrx | Total number of “winfo” Refresh Subscription Successes received. | Int64
> winfo-resubs-succtx | Total number of “winfo” Refresh Subscription Successes transmitted. | Int64
> winfo-resubs-failrx | Total number of “winfo” Refresh Subscription Failures received. | Int64
> winfo-resubs-failtx | Total number of “winfo” Refresh Subscription Failures transmitted. | Int64
> winfo-resubs-resp-200rx | Total number of “winfo” Refresh Subscription 200 Responses received. | Int64
> winfo-resubs-resp-200tx | Total number of “winfo” Refresh Subscription 200 Responses transmitted. | Int64
> winfo-resubs-resp-202rx | Total number of “winfo” Refresh Subscription 202 Responses received. | Int64
> winfo-resubs-resp-202tx | Total number of “winfo” Refresh Subscription 202 Responses transmitted. | Int64
> winfo-resubs-resp-400rx | Total number of “winfo” Refresh Subscription 400 Responses received. | Int64
> winfo-resubs-resp-400tx | Total number of “winfo” Refresh Subscription 400 Responses transmitted. | Int64
> winfo-resubs-resp-403rx | Total number of “winfo” Refresh Subscription 403 Responses received. | Int64
> winfo-resubs-resp-403tx | Total number of “winfo” Refresh Subscription 403 Responses transmitted. | Int64
> winfo-resubs-resp-481rx | Total number of “winfo” Refresh Subscription 481 Responses received. | Int64
> winfo-resubs-resp-481tx | Total number of “winfo” Refresh Subscription 481 Responses transmitted. | Int64
> winfo-resubs-resp-489rx | Total number of “winfo” Refresh Subscription 489 Responses received. | Int64
> winfo-resubs-resp-489tx | Total number of “winfo” Refresh Subscription 489 Responses transmitted. | Int64
> winfo-resubs-resp-500rx | Total number of “winfo” Refresh Subscription 500 Responses received. | Int64
> winfo-resubs-resp-500tx | Total number of “winfo” Refresh Subscription 500 Responses transmitted. | Int64
> winfo-resubs-resp-3xxrx | Total number of “winfo” Refresh Subscription 3XX Responses received. | Int64
> winfo-resubs-resp-3xxtx | Total number of “winfo” Refresh Subscription 3XX Responses transmitted. | Int64
> winfo-resubs-resp-4xxrx | Total number of “winfo” Refresh Subscription 4XX Responses received. | Int64
> winfo-resubs-resp-4xxtx | Total number of “winfo” Refresh Subscription 4XX Responses transmitted. | Int64
> winfo-resubs-resp-5xxrx | Total number of “winfo” Refresh Subscription 5XX Responses received. | Int64
> winfo-resubs-resp-5xxtx | Total number of “winfo” Refresh Subscription 5XX Responses transmitted. | Int64
> winfo-resubs-resp-6xxrx | Total number of “winfo” Refresh Subscription 6XX Responses received. | Int64
> winfo-resubs-resp-6xxtx | Total number of “winfo” Refresh Subscription 6XX Responses transmitted. | Int64
> winfo-unsubs-attrx | Total number of “winfo” Un-Subscription Attempts received. | Int64
> winfo-unsubs-atttx | Total number of “winfo” Un-Subscription Attempts transmitted. | Int64
> winfo-unsubs-succrx | Total number of “winfo” Un-Subscription Successes received. | Int64
> winfo-unsubs-succtx | Total number of “winfo” Un-Subscription Successes transmitted. | Int64
> winfo-unsubs-failrx | Total number of “winfo” Un-Subscription Failures received. | Int64
> winfo-unsubs-failtx | Total number of “winfo” Un-Subscription Failures transmitted. | Int64
> winfo-unsubs-resp-200rx | Total number of “winfo” Un-Subscription 200 Responses received. | Int64
> winfo-unsubs-resp-200tx | Total number of “winfo” Un-Subscription 200 Responses transmitted. | Int64
> winfo-unsubs-resp-202rx | Total number of “winfo” Un-Subscription 202 Responses received. | Int64
> winfo-unsubs-resp-202tx | Total number of “winfo” Un-Subscription 202 Responses transmitted. | Int64
> winfo-unsubs-resp-400rx | Total number of “winfo” Un-Subscription 400 Responses received. | Int64
> winfo-unsubs-resp-400tx | Total number of “winfo” Un-Subscription 400 Responses transmitted. | Int64
> winfo-unsubs-resp-403rx | Total number of “winfo” Un-Subscription 403 Responses received. | Int64
> winfo-unsubs-resp-403tx | Total number of “winfo” Un-Subscription 403 Responses transmitted. | Int64
> winfo-unsubs-resp-481rx | Total number of “winfo” Un-Subscription 481 Responses received. | Int64
> winfo-unsubs-resp-481tx | Total number of “winfo” Un-Subscription 481 Responses transmitted. | Int64
> winfo-unsubs-resp-489rx | Total number of “winfo” Un-Subscription 489 Responses received. | Int64
> winfo-unsubs-resp-489tx | Total number of “winfo” Un-Subscription 489 Responses transmitted. | Int64
> winfo-unsubs-resp-500rx | Total number of “winfo” Un-Subscription 500 Responses received. | Int64
> winfo-unsubs-resp-500tx | Total number of “winfo” Un-Subscription 500 Responses transmitted. | Int64
> winfo-unsubs-resp-3xxrx | Total number of “winfo” Un-Subscription 3XX Responses received. | Int64
> winfo-unsubs-resp-3xxtx | Total number of “winfo” Un-Subscription 3XX Responses transmitted. | Int64
> winfo-unsubs-resp-4xxrx | Total number of “winfo” Un-Subscription 4XX Responses received. | Int64
> winfo-unsubs-resp-4xxtx | Total number of “winfo” Un-Subscription 4XX Responses transmitted. | Int64
> winfo-unsubs-resp-5xxrx | Total number of “winfo” Un-Subscription 5XX Responses received. | Int64
> winfo-unsubs-resp-5xxtx | Total number of “winfo” Un-Subscription 5XX Responses transmitted. | Int64
> winfo-unsubs-resp-6xxrx | Total number of “winfo” Un-Subscription 6XX Responses received. | Int64
> winfo-unsubs-resp-6xxtx | Total number of “winfo” Un-Subscription 6XX Responses transmitted. | Int64
> winfo-notify-attrx | Total number of “winfo” Notify Attempts received. | Int64
> winfo-notify-atttx | Total number of “winfo” Notify Attempts transmitted. | Int64
> winfo-notify-succrx | Total number of “winfo” Notify Successes received. | Int64
> winfo-notify-succtx | Total number of “winfo” Notify Successes transmitted. | Int64
> winfo-notify-failrx | Total number of “winfo” Notify Failures received. | Int64
> winfo-notify-failtx | Total number of “winfo” Notify Failures transmitted. | Int64
> winfo-notify-resp-3xxrx | Total number of “winfo” Notify 3XX Responses received. | Int64
> winfo-notify-resp-3xxtx | Total number of “winfo” Notify 3XX Responses transmitted. | Int64
> winfo-notify-resp-400rx | Total number of “winfo” Notify 400 Responses received. | Int64
> winfo-notify-resp-400tx | Total number of “winfo” Notify 400 Responses transmitted. | Int64
> winfo-notify-resp-481rx | Total number of “winfo” Notify 481 Responses received. | Int64
> winfo-notify-resp-481tx | Total number of “winfo” Notify 481 Responses transmitted. | Int64
> winfo-notify-resp-489rx | Total number of “winfo” Notify 489 Responses received. | Int64
> winfo-notify-resp-489tx | Total number of “winfo” Notify 489 Responses transmitted. | Int64
> winfo-notify-resp-4xxrx | Total number of “winfo” Notify 4XX Responses received. | Int64
> winfo-notify-resp-4xxtx | Total number of “winfo” Notify 4XX Responses transmitted. | Int64
> winfo-notify-resp-500rx | Total number of “winfo” Notify 500 Responses received. | Int64
> winfo-notify-resp-500tx | Total number of “winfo” Notify 500 Responses transmitted. | Int64
> winfo-notify-resp-5xxrx | Total number of “winfo” Notify 5XX Responses received. | Int64
> winfo-notify-resp-5xxtx | Total number of “winfo” Notify 5XX Responses transmitted. | Int64
> winfo-notify-resp-6xxrx | Total number of “winfo” Notify 6XX Responses received. | Int64
> winfo-notify-resp-6xxtx | Total number of “winfo” Notify 6XX Responses transmitted. | Int64
> winfo-pub-attrx | Total number of “winfo” Publish Attempts received. | Int64
> winfo-pub-atttx | Total number of “winfo” Publish Attempts transmitted. | Int64
> winfo-pub-succrx | Total number of “winfo” Publish Successes received. | Int64
> winfo-pub-succtx | Total number of “winfo” Publish Successes transmitted. | Int64
> winfo-pub-failrx | Total number of “winfo” Publish Failures received. | Int64
> winfo-pub-failtx | Total number of “winfo” Publish Failures transmitted. | Int64
> winfo-pub-resp-3xxrx | Total number of “winfo” Publish 3XX Responses received. | Int64
> winfo-pub-resp-3xxtx | Total number of “winfo” Publish 3XX Responses transmitted. | Int64
> winfo-pub-resp-400rx | Total number of “winfo” Publish 400 Responses received. | Int64
> winfo-pub-resp-400tx | Total number of “winfo” Publish 400 Responses transmitted. | Int64
> winfo-pub-resp-404rx | Total number of “winfo” Publish 404 Responses received. | Int64
> winfo-pub-resp-404tx | Total number of “winfo” Publish 404 Responses transmitted. | Int64
> winfo-pub-resp-412rx | Total number of “winfo” Publish 412 Responses received. | Int64
> winfo-pub-resp-412tx | Total number of “winfo” Publish 412 Responses transmitted. | Int64
> winfo-pub-resp-423rx | Total number of “winfo” Publish 423 Responses received. | Int64
> winfo-pub-resp-423tx | Total number of “winfo” Publish 423 Responses transmitted. | Int64
> winfo-pub-resp-489rx | Total number of “winfo” Publish 489 Responses received. | Int64
> winfo-pub-resp-489tx | Total number of “winfo” Publish 489 Responses transmitted. | Int64
> winfo-pub-resp-4xxrx | Total number of “winfo” Publish 4XX Responses received. | Int64
> winfo-pub-resp-4xxtx | Total number of “winfo” Publish 4XX Responses transmitted. | Int64
> winfo-pub-resp-500rx | Total number of “winfo” Publish 500 Responses received. | Int64
> winfo-pub-resp-500tx | Total number of “winfo” Publish 500 Responses transmitted. | Int64
> winfo-pub-resp-503rx | Total number of “winfo” Publish 503 Responses received. | Int64
> winfo-pub-resp-503tx | Total number of “winfo” Publish 503 Responses transmitted. | Int64
> winfo-pub-resp-5xxrx | Total number of “winfo” Publish 5XX Responses received. | Int64
> winfo-pub-resp-5xxtx | Total number of “winfo” Publish 5XX Responses transmitted. | Int64
> winfo-pub-resp-6xxrx | Total number of “winfo” Publish 6XX Responses received. | Int64
> winfo-pub-resp-6xxtx | Total number of “winfo” Publish 6XX Responses transmitted. | Int64
> winfo-unpub-attrx | Total number of “winfo” Un-Publish Attempts received. | Int64
> winfo-unpub-atttx | Total number of “winfo” Un-Publish Attempts transmitted. | Int64
> winfo-unpub-succrx | Total number of “winfo” Un-Publish Successes received. | Int64
> winfo-unpub-succtx | Total number of “winfo” Un-Publish Successes transmitted. | Int64
> winfo-unpub-failrx | Total number of “winfo” Un-Publish Failures received. | Int64
> winfo-unpub-failtx | Total number of “winfo” Un-Publish Failures transmitted. | Int64
> winfo-unpub-resp-3xxrx | Total number of “winfo” Un-Publish 3XX Responses received. | Int64
> winfo-unpub-resp-3xxtx | Total number of “winfo” Un-Publish 3XX Responses transmitted. | Int64
> winfo-unpub-resp-400rx | Total number of “winfo” Un-Publish 400 Responses received. | Int64
> winfo-unpub-resp-400tx | Total number of “winfo” Un-Publish 400 Responses transmitted. | Int64
> winfo-unpub-resp-404rx | Total number of “winfo” Un-Publish 404 Responses received. | Int64
> winfo-unpub-resp-404tx | Total number of “winfo” Un-Publish 404 Responses transmitted. | Int64
> winfo-unpub-resp-412rx | Total number of “winfo” Un-Publish 412 Responses received. | Int64
> winfo-unpub-resp-412tx | Total number of “winfo” Un-Publish 412 Responses transmitted. | Int64
> winfo-unpub-resp-423rx | Total number of “winfo” Un-Publish 423 Responses received. | Int64
> winfo-unpub-resp-423tx | Total number of “winfo” Un-Publish 423 Responses transmitted. | Int64
> winfo-unpub-resp-489rx | Total number of “winfo” Un-Publish 489 Responses received. | Int64
> winfo-unpub-resp-489tx | Total number of “winfo” Un-Publish 489 Responses transmitted. | Int64
> winfo-unpub-resp-4xxrx | Total number of “winfo” Un-Publish 4XX Responses received. | Int64
> winfo-unpub-resp-4xxtx | Total number of “winfo” Un-Publish 4XX Responses transmitted. | Int64
> winfo-unpub-resp-500rx | Total number of “winfo” Un-Publish 500 Responses received. | Int64
> winfo-unpub-resp-500tx | Total number of “winfo” Un-Publish 500 Responses transmitted. | Int64
> winfo-unpub-resp-503rx | Total number of “winfo” Un-Publish 503 Responses received. | Int64
> winfo-unpub-resp-503tx | Total number of “winfo” Un-Publish 503 Responses transmitted. | Int64
> winfo-unpub-resp-5xxrx | Total number of “winfo” Un-Publish 5XX Responses received. | Int64
> winfo-unpub-resp-5xxtx | Total number of “winfo” Un-Publish 5XX Responses transmitted. | Int64
> winfo-unpub-resp-6xxrx | Total number of “winfo” Un-Publish 6XX Responses received. | Int64
> winfo-unpub-resp-6xxtx | Total number of “winfo” Un-Publish 6XX Responses transmitted. | Int64
> message-attrx | Total number of Message attempts received. | Int32
> message-atttx | Total number of Message attempts transmitted. | Int32
> message-succrx | Total number of Message success received. | Int32
> message-succtx | Total number of Message success transmitted. | Int32
> message-failrx | Total number of Message failures received. | Int32
> message-failtx | Total number of Message failures transmitted. | Int32
> message-3xx-rx | Total number of Message 3xx Responses received. | Int32
> message-3xx-tx | Total number of Message 3xx Responses transmitted. | Int32
> message-400-rx | Total number of Message 400 Responses received. | Int32
> message-400-tx | Total number of Message 400 Responses transmitted. | Int32
> message-403-rx | Total number of Message 403 Responses received. | Int32
> message-403-tx | Total number of Message 403 Responses transmitted. | Int32
> message-404-rx | Total number of Message 404 Responses received. | Int32
> message-404-tx | Total number of Message 404 Responses transmitted. | Int32
> message-413-rx | Total number of Message 413 Responses received. | Int32
> message-413-tx | Total number of Message 413 Responses transmitted. | Int32
> message-415-rx | Total number of Message 415 Responses received. | Int32
> message-415-tx | Total number of Message 415 Responses transmitted. | Int32
> message-416-rx | Total number of Message 416 Responses received. | Int32
> message-416-tx | Total number of Message 416 Responses transmitted. | Int32
> message-420-rx | Total number of Message 420 Responses received. | Int32
> message-420-tx | Total number of Message 420 Responses transmitted. | Int32
> message-421-rx | Total number of Message 421 Response received. | Int32
> message-421-tx | Total number of Message 421 Responses transmitted. | Int32
> message-480-rx | Total number of Message 480 Responses received. | Int32
> message-480-tx | Total number of Message 480 Responses transmitted. | Int32
> message-488-rx | Total number of Message 488 Responses received. | Int32
> message-488-tx | Total number of Message 488 Responses transmitted. | Int32
> message-4xx-rx | Total number of Message 4xx Responses received. | Int32
> message-4xx-tx | Total number of Message 4xx Responses transmitted. | Int32
> message-500-rx | Total number of Message 500 Responses received. | Int32
> message-500-tx | Total number of Message 500 Responses transmitted. | Int32
> message-513-rx | Total number of Message 513 Responses received. | Int32
> message-513-tx | Total number of Message 513 Responses transmitted. | Int32
> message-5xx-rx | Total number of Message 5xx Responses received. | Int32
> message-5xx-tx | Total number of Message 5xx Responses transmitted. | Int32
> message-6xx-rx | Total number of Message 6xx Responses received. | Int32
> message-6xx-tx | Total number of Total Message 6xx Responses transmitted. | Int32
> callrejpdf | Total number of Call Rejects from PDF. | Int64
> callrejloc | Total number of Call Rejects from Proxy (local). | Int64
> sesstimeexp | Total number of Session Timer Expires. | Int64
> hssacc | Total number of HSS Accesses. | Int64
> emergcalls | Total number of Emergency Calls. | Int64
> emerg-priv-calls | Total number of User-requested Privacy Calls. Applicable only for E-CSCF. | Int64
> tollfreecalls | Total number of Toll Free Calls. | Int64
> premservcalls | Total number of Premium Service Calls. | Int64
> internationalcalls | Total number of International Calls. | Int64
> longDistancecalls | Total number of Long Distance Calls. | Int64
> opassistcalls | Total number of Operator Assisted Calls. | Int64
> dirassistcalls | Total number of Directory Assisted Calls. | Int64
> largerthansipmaxsize | Total number of Too Large SIP Messages. | Int64
> rtp-sent | Total number of RTP packets sent. | Int64
> rtcp-sent | Total number of RTCP packets sent. | Int64
> rtp-recv | Total number of RTP packets received. | Int64
> msrp-sent | Total number of MSRP TCP packets sent. | Int64
> msrp-recv | Total number of MSRP TCP packets received. | Int64
> callrel-from-ue | Total number of Call Releases initiated by UE. | Int64
> callrel-from-nw | Total number of Call Releases initiated by Network. | Int64
> callrel-from-radioloss | Total number of Call Releases initiated by Radio Loss. | Int64
> callrel-from-local | Total number of Call Releases initiated by CSCF (Local). | Int64
> sigcomp-req-comp | Total number of Requests Compressed. | Int64
> sigcomp-req-decomp | Total number of Requests Decompressed. | Int64
> sigcomp-resp-comp | Total number of Responses Compressed. | Int64
> sigcomp-resp-decomp | Total number of Responses Decompressed. | Int64
> sigcomp-nack-rx | Total number of NACK Packets received. | Int64
> sigcomp-nack-tx | Total number of NACK Packets transmitted. | Int64
> sigcomp-comp-fail | Total number of Compression Failures. | Int64
> sigcomp-decomp-fail | Total number of Decompression Failures. | Int64
> sigcomp-bestout-compratio | Best Outgoing Message Compression Ratio | Float
> sigcomp-worstout-compratio | Worst Outgoing Message Compression Ratio | Float
> sigcomp-bestin-compratio | Best Incoming Message Compression Ratio | Float
> sigcomp-worstin-compratio | Worst Incoming Message Compression Ratio | Float
> sigcomp-averagein- compratio | Average Incoming Message Compression Ratio | Float
> sigcomp-averageout- compratio | Average Outgoing Message Compression Ratio | Float
> min-invite-proc-time | Minimum Invite Process Time | Int32
> max-invite-proc-time | Maximum Invite Process Timer | Int32
> min-first-resp-time | Minimum First Response Time | Int32
> max-first-resp-time | Maximum First Response Time | Int32
> min-post-dial-delay | Minimum Post-Dial Delay | Int32
> max-post-dial-delay | Maximum Post-Dial Delay | Int32
> min-session-setup-delay | Minimum Session Setup Delay | Int32
> max-session-setup-delay | Maximum Session Setup Delay | Int32
> min-post-answer-delay | Minimum Post Answer Delay | Int32
> max-post-answer-delay | Maximum Post Answer Delay | Int32
> min-session-rel-delay | Minimum Session Release Delay | Int32
> max-session-rel-delay | Maximum Session Release Delay | Int32
> active-tcp-conn | Total number of Active TCP connections. Type: Gauge | Int64
> closed-tcp-conn | Total number of Closed TCP connections. | Int64
> succ-tcp-conn-out | Total number of Successful Outgoing connections. | Int64
> fail-tcp-conn-out | Total number of Failed Outgoing connections. | Int64
> succ-tcp-conn-in | Total number of Successful Incoming connections. | Int64
> fail-tcp-conn-in | Total number of Failed Incoming connections. | Int64
> migrated-tcp-conn | Total number of TCP connections migrated from Cscfmgr to Sessmgr for load balancing. | Int64
> packet-tcp-rx | Total number of TCP/IP packets received by CSCF service. | Int64
> packet-tcp-tx | Total number of TCP/IP packets transmitted by CSCF service. | Int64
> bytes-tcp-rx | Total number of TCP/IP bytes received by CSCF service. | Int64
> bytes-tcp-tx | Total number of TCP/IP bytes transmitted by CSCF service. | Int64
> message-tcp-request-rx | Total number of TCP requests received over TCP. | Int64
> message-tcp-request-tx | Total number of TCP requests transmitted over TCP. | Int64
> message-tcp-response-rx | Total number of TCP responses received over TCP. | Int64
> message-tcp-response-tx | Total number of TCP responses transmitted over TCP. | Int64
> message-tcp-mtu-switch | Total number of times CSCF switched from UDP to TCP because of message size larger than MTU. | Int64
> sip-tcp-subs | Total number of subscribers using TCP for SIP. Type: Gauge | Int64
> msrp-active-tcp-conn | Total number of active MSRP TCP connections. | Int64
> msrp-closed-tcp-conn | Total number of closed MSRP TCP connections. | Int64
> msrp-succ-tcp-conn-out | Total number of outgoing MSRP TCP connections established successfully. | Int64
> msrp-fail-tcp-conn-out | Total number of failed outgoing MSRP TCP connections. | Int64
> msrp-succ-tcp-conn-in | Total number of incoming MSRP TCP connections established successfully. | Int64
> msrp-fail-tcp-conn-in | Total number of failed incoming MSRP TCP connections. | Int64
> msrp-packet-rx | Total number of MSRP packets received. | Int64
> msrp-packet-tx | Total number of MSRP packets transmitted. | Int64
> msrp-bytes-rx | Total number of MSRP bytes received. | Int64
> msrp-bytes-tx | Total number of MSRP bytes transmitted. | Int64
> msrp-tcp-subs | Total number of subscribers with TCP connection for MSRP. Type: Gauge | Int64
> reg-rejdueto-secagree | Total number of Registration Rejects due to Security Agreement | Int64
> reg-rejdueto-algomismatch | Total number of Registration Rejects due to Algorithm Mismatch | Int64
> msg-drops-duetoerror | Total number of Message drops due to error. | Int64
> sec-rereg | Total number of Secure re-registrations | Int64
> sec-dereg | Total number of Secure de-registrations | Int64
> msgs-withincorr-sec-verify | Total number of Messages with Incorrect security Verify | Int64
> sec-assoc-rejects | Total number of Security Associations rejected. | Int64
> sub-with-sec-conn | Total number of Subscribers with secure connections. Type: Gauge | Int32
> sub-with-unsec-conn | Total number of Subscribers with unsecure connections. Type: Gauge | Int32
> ipsec-pktrx | Total number of IP-Sec Packets received. | Int64
> ipsec-pkttx | Total number of IP-Sec Packets transmitted. | Int64
> ipsec-octrx | Total number of IP-Sec Octets received. | Int64
> ipsec-octtx | Total number of IP-Sec Octets transmitted. | Int64
> active-ipsec-tcp-conn | Total number of Active IPSec TCP connections Type: Gauge | Int64
> closed-ipsec-tcp-conn | Total number of Closed IPSec TCP connections | Int64
> succ-ipsec-tcp-conn-out | Total number of Successful IPSec Outgoing connections | Int64
> fail-ipsec-tcp-conn-out | Total number of Failed IPSec Outgoing connections | Int64
> succ-ipsec-tcp-conn-in | Total number of Successful IPSec Incoming connections | Int64
> fail-ipsec-tcp-conn-in | Total number of Failed IPSec Incoming connections | Int64
> regreqrx | Total number of Register requests received. | Int64
> regreqtx | Total number of Register requests transmitted. | Int64
> invreqrx | Total number of Invite requests received. | Int64
> invreqtx | Total number of Invite requests transmitted. | Int64
> ackreqrx | Total number of ACK requests received. | Int64
> ackreqtx | Total number of ACK requests transmitted. | Int64
> byereqrx | Total number of Bye requests received. | Int64
> byereqtx | Total number of Bye requests transmitted. | Int64
> cancreqrx | Total number of Cancel requests received. | Int64
> cancreqtx | Total number of Cancel requests transmitted. | Int64
> optreqrx | Total number of Options requests received. | Int64
> optreqtx | Total number of Options requests transmitted. | Int64
> prackreqrx | Total number of PRACK requests received. | Int64
> prackreqtx | Total number of PRACK requests transmitted. | Int64
> subreqrx | Total number of Subscribe requests received. | Int64
> subreqtx | Total number of Subscribe requests transmitted. | Int64
> notreqrx | Total number of Notify requests received. | Int64
> notreqtx | Total number of Notify requests transmitted. | Int64
> refreqrx | Total number of Refer requests received. | Int64
> refreqtx | Total number of Refer requests transmitted. | Int64
> inforeqrx | Total number of Info requests received. | Int64
> inforeqtx | Total number of Info requests transmitted. | Int64
> updreqrx | Total number of Update requests received. | Int64
> updreqtx | Total number of Update requests transmitted. | Int64
> msgreqrx | Total number of Message requests received. | Int64
> msgreqtx | Total number of Message requests transmitted. | Int64
> pubreqrx | Total number of Publish requests received. | Int64
> pubreqtx | Total number of Publish requests transmitted. | Int64
> tryrsprx | Total number of Trying responses received. | Int64
> tryrsptx | Total number of Trying responses transmitted. | Int64
> rngrsprx | Total number of Ringing responses received. | Int64
> rngrsptx | Total number of Ringing responses transmitted. | Int64
> fwdrsprx | Total number of Forwarded responses received. | Int64
> fwdrsptx | Total number of Forwarded responses transmitted. | Int64
> quersprx | Total number of Queued responses received. | Int64
> quersptx | Total number of Queued responses transmitted. | Int64
> prgrsprx | Total number of Progress responses received. | Int64
> prgrsptx | Total number of Progress responses transmitted. | Int64
> 200-regrsprx | Total number of 200OK Register responses received. | Int64
> 200-regrsptx | Total number of 200OK Register responses transmitted. | Int64
> 200-invrsprx | Total number of 200OK Invite responses received. | Int64
> 200-invrsptx | Total number of 200OK Invite responses transmitted. | Int64
> 200-byersprx | Total number of 200OK Bye responses received. | Int64
> 200-byersptx | Total number of 200OK Bye responses transmitted. | Int64
> 200-cnlrsprx | Total number of 200OK Cancel responses received. | Int64
> 200-cnlrsptx | Total number of 200OK Cancel responses transmitted. | Int64
> 200-optrsprx | Total number of 200OK Options responses received. | Int64
> 200-optrsptx | Total number of 200OK Options responses transmitted. | Int64
> 200-prackrsprx | Total number of 200OK PRACK responses received. | Int64
> 200-prackrsptx | Total number of 200OK PRACK responses transmitted. | Int64
> 200-subrsprx | Total number of 200OK Subscribe responses received. | Int64
> 200-subrsptx | Total number of 200OK Subscribe responses transmitted. | Int64
> 200-notrsprx | Total number of 200OK Notify responses received. | Int64
> 200-notrsptx | Total number of 200OK Notify responses transmitted. | Int64
> 200-infrsprx | Total number of 200OK Info responses received. | Int64
> 200-infrsptx | Total number of 200OK Info responses transmitted. | Int64
> 200-updrsprx | Total number of 200OK Update responses received. | Int64
> 200-updrsptx | Total number of 200OK Update responses transmitted. | Int64
> 200-pubrsprx | Total number of 200OK Publish responses received. | Int64
> 200-pubrsptx | Total number of 200OK Publish responses transmitted. | Int64
> 200-refrsprx | Total number of 200OK Refer responses received. | Int64
> 200-refrsptx | Total number of 200OK Refer responses transmitted. | Int64
> 200-msgrsprx | Total number of 200OK Message responses received. | Int64
> 200-msgrsptx | Total number of 200OK Message responses transmitted. | Int64
> 202-refrsprx | Total number of 202Accepted Refer responses received. | Int64
> 202-refrsptx | Total number of 202Accepted Refer responses transmitted. | Int64
> 202-subrsprx | Total number of 202Accepted Subscribe responses received. | Int64
> 202-subrsptx | Total number of 202Accepted Subscribe responses transmitted. | Int64
> mchrsprx | Total number of Multiple Choices responses received. | Int64
> mchrsptx | Total number of Multiple Choices responses transmitted. | Int64
> mpersprx | Total number of Moved Permanently responses received. | Int64
> mpersptx | Total number of Moved Permanently responses transmitted. | Int64
> mtersprx | Total number of Moved Temporarily responses received. | Int64
> mtersptx | Total number of Moved Temporarily responses transmitted. | Int64
> upxrsprx | Total number of Use Proxy responses received. | Int64
> upxrsptx | Total number of Use Proxy responses transmitted. | Int64
> altrsprx | Total number of Alternative Service responses received. | Int64
> altrsptx | Total number of Alternative Service responses transmitted. | Int64
> brqerrrx | Total number of BadRequest errors received. | Int64
> brqerrtx | Total number of BadRequest errors transmitted. | Int64
> uauerrrx | Total number of UnAuthorized errors received. | Int64
> uauerrtx | Total number of UnAuthorized errors transmitted. | Int64
> prerrrx | Total number of Payment Required Errors received. | Int64
> prerrtx | Total number of Payment Required Errors transmitted. | Int64
> forerrrx | Total number of Forbidden errors received. | Int64
> forerrtx | Total number of Forbidden errors transmitted. | Int64
> nfderrrx | Total number of NotFound errors received. | Int64
> nfderrtx | Total number of NotFound errors transmitted. | Int64
> mnaerrrx | Total number of MethodNotAllowed errors received. | Int64
> mnaerrtx | Total number of MethodNotAllowed errors transmitted. | Int64
> nac406errrx | Total number of NotAcceptable(406) errors received. | Int64
> nac406errtx | Total number of NotAcceptable(406) errors transmitted. | Int64
> parerrrx | Total number of ProxyAuthRequired errors received. | Int64
> parerrtx | Total number of ProxyAuthRequired errors transmitted. | Int64
> rtoerrrx | Total number of RequestTimeout errors received. | Int64
> rtoerrtx | Total number of RequestTimeout errors transmitted. | Int64
> conferrrx | Total number of Conflict Errors received. | Int64
> conferrtx | Total number of Conflict Errors transmitted. | Int64
> lrerrrx | Total number of Length Required Errors received. | Int64
> lrerrtx | Total number of Length Required Errors transmitted. | Int64
> gonerrrx | Total number of Gone errors received. | Int64
> gonerrtx | Total number of Gone errors transmitted. | Int64
> crferrrx | Total number of ConditionalRequestFail errors received. | Int64
> crferrtx | Total number of ConditionalRequestFail errors transmitted. | Int64
> relerrrx | Total number of RequestEntityTooLarge errors received. | Int64
> relerrtx | Total number of RequestEntityTooLarge errors transmitted. | Int64
> rulerrrx | Total number of RequestURITooLong errors received. | Int64
> rulerrtx | Total number of RequestURITooLong errors transmitted. | Int64
> umterrrx | Total number of UnsupportedMediaType errors received. | Int64
> umterrtx | Total number of UnsupportedMediaType errors transmitted. | Int64
> uuserrrx | Total number of Unsupported URI Scheme errors received. | Int64
> uuserrtx | Total number of Unsupported URI Scheme errors transmitted. | Int64
> bexerrrx | Total number of BadExtension errors received. | Int64
> bexerrtx | Total number of BadExtension errors transmitted. | Int64
> exrerrrx | Total number of Extension Required errors received. | Int64
> exrerrtx | Total number of Extension Required errors transmitted. | Int64
> sitserrrx | Total number of Session Interval Too Small errors received | Int64
> sitserrtx | Total number of Session Interval Too Small errors transmitted | Int64
> fhloerrrx | Total number of First Hop Lacks Outbound Support (439) errors received. | Int64
> fhloerrtx | Total number of First Hop Lacks Outbound Support (439) errors transmitted. | Int64
> itberrrx | Total number of Interval Too Brief errors received. | Int64
> itberrtx | Total number of Interval Too Brief errors transmitted. | Int64
> blierrrx | Total number of Bad Location Information errors received. | Int64
> blierrtx | Total number of Bad Location Information errors transmitted. | Int64
> tnaerrrx | Total number of TempNotAvailable errors received. | Int64
> tnaerrtx | Total number of TempNotAvailable errors transmitted. | Int64
> tdnerrrx | Total number of Transaction Does Not Exist errors received. | Int64
> tdnerrtx | Total number of Transaction Does Not Exist errors transmitted. | Int64
> ldterrrx | Total number of LoopDetected errors received. | Int64
> ldterrtx | Total number of LoopDetected errors transmitted. | Int64
> tmherrrx | Total number of TooManyHops errors received. | Int64
> tmherrtx | Total number of TooManyHops errors transmitted. | Int64
> adierrrx | Total number of AddrIncomplete errors received. | Int64
> adierrtx | Total number of AddrIncomplete errors transmitted. | Int64
> amberrrx | Total number of Ambiguous errors received. | Int64
> amberrtx | Total number of Ambiguous errors transmitted. | Int64
> bhrerrrx | Total number of BusyHere errors received. | Int64
> bhrerrtx | Total number of BusyHere errors transmitted. | Int64
> rqcerrrx | Total number of RequestCancel errors received. | Int64
> rqcerrtx | Total number of RequestCancel errors transmitted. | Int64
> namerrrx | Total number of NotAcceptableMedia errors received. | Int64
> namerrtx | Total number of NotAcceptableMedia errors transmitted. | Int64
> beerrrx | Total number of Bad Event errors received. | Int64
> beerrtx | Total number of Bad Event errors transmitted. | Int64
> trperrrx | Total number of Request Pending errors received. | Int64
> trperrtx | Total number of Request Pending errors transmitted. | Int64
> udperrrx | Total number of Undecipherable errors received. | Int64
> udperrtx | Total number of Undecipherable errors transmitted. | Int64
> sarerrrx | Total number of sec-agree Required Errors received. | Int64
> sarerrtx | Total number of Sec-agree Required Errors transmitted. | Int64
> ineerrrx | Total number of InternalError errors received. | Int64
> ineerrtx | Total number of InternalError errors transmitted. | Int64
> nimerrrx | Total number of NotImplemented errors received. | Int64
> nimerrtx | Total number of NotImplemented errors transmitted. | Int64
> bgterrrx | Total number of BadGateway errors received. | Int64
> bgterrtx | Total number of BadGateway errors transmitted. | Int64
> suaerrrx | Total number of ServiceUnavailable errors received. | Int64
> suaerrtx | Total number of ServiceUnavailable errors transmitted. | Int64
> gtterrrx | Total number of GatewayTimeout errors received. | Int64
> gtterrtx | Total number of GatewayTimeout errors transmitted. | Int64
> bsverrrx | Total number of BadSipVersion errors received. | Int64
> bsverrtx | Total number of BadSipVersion errors transmitted. | Int64
> mtlerrrx | Total number of Message Too Large errors received. | Int64
> mtlerrtx | Total number of Message Too Large errors transmitted. | Int64
> pcferrrx | Total number of Precondition Failure errors received. | Int64
> pcferrtx | Total number of Precondition Failure errors transmitted. | Int64
> bewerrrx | Total BusyEverywhere errors received. Total number of | Int64
> bewerrtx | Total number of BusyEverywhere errors transmitted. | Int64
> decerrrx | Total number of Decline errors received. | Int64
> decerrtx | Total number of Decline errors transmitted. | Int64
> neaerrrx | Total number of NotExistAnywhere errors received. | Int64
> neaerrtx | Total number of NotExistAnywhere errors transmitted. | Int64
> nac606errrx | Total number of NotAcceptable(606) errors received. | Int64
> nac606errtx | Total number of NotAcceptable(606) errors transmitted. | Int64
> callsetuptime | Sum of setup times – For calculating average call setup time. | Int64
> callscounted | Total number of calls, for which setup time is added in setup times. | Int64
> tot-sip-invalid-msgs-rx | Total number of SIP Invalid Messages received. | Int64
> tot-sip-msgs-rx | Total number of SIP Messages received. | Int64
> tot-sip-msgs-tx | Total number of SIP Messages transmitted. | Int64
> tot-sip-msgs-proc | Total number of SIP Messages Processed. | Int64
> regreqretx | Total number of REGISTER Requests Re-transmitted. | Int64
> invreqretx | Total number of INVITE Requests Re-transmitted. | Int64
> byereqretx | Total number of BYE Requests Re-transmitted. | Int64
> cancreqretx | Total number of CANCEL Requests Re-transmitted. | Int64
> ackreqretx | Total number of ACK Requests Re-Transmitted | Int64
> notifyreqretx | Total number of NOTIFY Requests Re-Transmitted | Int64
> publishreqretx | Total number of PUBLISH Requests Re-Transmitted | Int64
> referreqretx | Total number of REFER Requests Re-Transmitted | Int64
> subscribereqretx | Total number of SUBSCRIBE Requests Re-Transmitted | Int64
> req-retx | Total number of SIP Requests Re-transmitted. | Int64
> resp-retx | Total number of SIP Responses Re-Transmiited. | Int64
> reqresp-retx | Total number of SIP messages Re-transmitted. | Int64
> calldur-lt-01sec | Total calls with duration less than 01 sec. | Int32
> calldur-01to10sec | Total calls with duration between 01 and 10 seconds. | Int32
> calldur-10to30sec | Total calls with duration between 10 and 30 seconds. | Int32
> calldur-30to60sec | Total calls with duration between 30 and 60 seconds. | Int32
> calldur-60to90sec | Total calls with duration between 60 and 90 seconds. | Int32
> calldur-90to120sec | Total calls with duration between 90 and 120 seconds. | Int32
> calldur-120to150sec | Total calls with duration between 120 and 150 seconds. | Int32
> calldur-150to180sec | Total calls with duration between 150 and 180 seconds. | Int32
> calldur-03to04min | Total calls with duration between 03 and 04 minutes. | Int32
> calldur-04to05min | Total calls with duration between 04 and 05 minutes. | Int32
> calldur-05to06min | Total calls with duration between 05 and 06 minutes. | Int32
> calldur-06to07min | Total calls with duration between 06 and 07 minutes. | Int32
> calldur-07to08min | Total calls with duration between 07 and 08 minutes. | Int32
> calldur-08to09min | Total calls with duration between 08 and 09 minutes. | Int32
> calldur-09to11min | Total calls with duration between 09 and 11 minutes. | Int32
> calldur-11to13min | Total calls with duration between 11 and 13 minutes. | Int32
> calldur-13to15min | Total calls with duration between 13 and 15 minutes. | Int32
> calldur-15to17min | Total calls with duration between 15 and 17 minutes. | Int32
> calldur-17to19min | Total calls with duration between 17 and 19 minutes. | Int32
> calldur-19to21min | Total calls with duration between 19 and 21 minutes. | Int32
> calldur-21to23min | Total calls with duration between 21 and 23 minutes. | Int32
> calldur-23to25min | Total calls with duration between 23 and 25 minutes. | Int32
> calldur-25to27min | Total calls with duration between 25 and 27 minutes. | Int32
> calldur-27to29min | Total calls with duration between 27 and 29 minutes. | Int32
> calldur-29to60min | Total calls with duration between 29 and 60 minutes. | Int32
> calldur-gt-60min | Total calls with duration more than 60 minutes. | Int32
> subsetup<200ms | Total number of subscriptions setup in less than 200 milliseconds. | Int32
> subsetup200-400ms | Total number of subscriptions setup in 200 to 400 milliseconds. | Int32
> subsetup400-600ms | Total number of subscriptions setup in 400 to 600 milliseconds. | Int32
> subsetup600-800ms | Total number of subscriptions setup in 600 to 800 milliseconds. | Int32
> subsetup800-1000ms | Total number of subscriptions setup in 800 to 1000 milliseconds. | Int32
> subsetup1000-1200ms | Total number of subscriptions setup in 1000 to 1200 milliseconds. | Int32
> subsetup1200-1400ms | Total number of subscriptions setup in 1200 to 1400 milliseconds. | Int32
> subsetup1400-1600ms | Total number of subscriptions setup in 1400 to 1600 milliseconds. | Int32
> subsetup1600-1800ms | Total number of subscriptions setup in 1600 to 1800 milliseconds. | Int32
> subsetup1800-2000ms | Total number of subscriptions setup in 1800 to 2000 milliseconds. | Int32
> subsetup2000-2200ms | Total number of subscriptions setup in 2000 to 2200 milliseconds. | Int32
> subsetup2200-2400ms | Total number of subscriptions setup in 2200 to 2400 milliseconds. | Int32
> subsetup2400-2600ms | Total number of subscriptions setup in 2400 to 2600 milliseconds. | Int32
> subsetup2600-2800ms | Total number of subscriptions setup in 2600 to 2800 milliseconds. | Int32
> subsetup2800-3000ms | Total number of subscriptions setup in 2800 to 3000 milliseconds. | Int32
> subsetup3-5sec | Total number of subscriptions setup in 3 to 5 seconds. | Int32
> subsetup5-7sec | Total number of subscriptions setup in 5 to 7 seconds. | Int32
> subsetup7-9sec | Total number of subscriptions setup in 7 to 9 seconds. | Int32
> subsetup9-11sec | Total number of subscriptions setup in 9 to 11 seconds. | Int32
> subsetup11-13sec | Total number of subscriptions setup in 11 to 13 seconds. | Int32
> subsetup13-15sec | Total number of subscriptions setup in 13 to 15 seconds. | Int32
> subsetup15-17sec | Total number of subscriptions setup in 15 to 17 seconds. | Int32
> subsetup17-19sec | Total number of subscriptions setup in 17 to 19 seconds. | Int32
> subsetup19-21sec | Total number of subscriptions setup in 19 to 21 seconds. | Int32
> subsetup>21sec | Total number of subscriptions setup in more than 21 seconds. | Int32
> subdur<1hr | Total number of subscription duration less than 1 hour. | Int32
> subdur1-2hr | Total number of subscription duration 1 to 2 hours. | Int32
> subdur2-3hr | Total number of subscription duration 2 to 3 hours. | Int32
> subdur3-4hr | Total number of subscription duration 3 to 4 hours. | Int32
> subdur4-5hr | Total number of subscription duration 4 to 5 hours. | Int32
> subdur5-6hr | Total number of subscription duration 5 to 6 hours. | Int32
> subdur6-7hr | Total number of subscription duration 6 to 7 hours. | Int32
> subdur7-8hr | Total number of subscription duration 7 to 8 hours. | Int32
> subdur8-9hr | Total number of subscription duration 8 to 9 hours. | Int32
> subdur9-10hr | Total number of subscription duration 9 to 10 hours. | Int32
> subdur>10hr | Total number of subscription duration more than 10 hours. | Int32
> curr-reg-subs | Total number of currently registered users. Type: Gauge | Int64
> active-reg-subs | Total number of active registered users. Type: Gauge | Int64
> curr-sigcomp-subs | Total number of currently registered SIGCOMP users. Type: Gauge | Int64
> active-sigcomp-subs | Total number of active registered SIGCOMP users. Type: Gauge | Int64
> curr-ipsec-subs | Total number of currently registered IPSEC users. Type: Gauge | Int64
> active-ipsec-subs | Total number of active registered IPSEC users. Type: Gauge | Int64
> active-voip-subs | Active registered VOIP users. Type: Gauge | Int64
> curr-presence-subs | Total number of currently registered PRESENCE users. Type: Gauge | Int64
> active-presence-subs | Total number of active registered PRESENCE users. Type: Gauge | Int64
> active-im-subs | Total number of active registered IM users. Type: Gauge | Int64
> dpeca-curr-sessions | The total number of DPECA sessions currently active. Type: Gauge | Int32
> dpeca-tot-sess-init | Total number of DPECA sessions initiated by sending AAR Initial Request message. | Int32
> dpeca-tot-sess-terminated | Total number of terminated DPECA sessions. | Int32
> dpeca-tot-sess-failovers | Total number of peer-switches attempted. | Int32
> dpeca-tot-sess-failover-err | Total number of peer-switches failed. | Int32
> dpeca-tot-msg-received | Total number of messages received. | Int32
> dpeca-tot-msg-sent | Total number of messages sent. | Int32
> dpeca-tot-aar-sent | Total number of AAR request messages sent from DPECA module. | Int32
> dpeca-tot-aaa-received | Total number of AAA answer messages received. | Int32
> dpeca-tot-uncorr-aaa | Total number of Uncorrelated AAA messages. | Int32
> dpeca-tot-uncorr-sta | Total number of Uncorrelated STA messages. | Int32
> dpeca-tot-aari-sent | Total number of AAR Initial requests sent. | Int32
> dpeca-tot-aaai-received | Total number of AAA answer messages received in response to the AAR-Initial requests. | Int32
> dpeca-tot-aaai-accepted | Total number of AAA messages accepted as successful without any errors. | Int32
> dpeca-tot-aaai-rejected | Total number of AAA messages rejected as erroneous. | Int32
> dpeca-tot-aaai-timeout | Total number of AAA answers to Initial request timed out. | Int32
> dpeca-tot-aaru-sent | Total number of AAR Update messages sent | Int32
> dpeca-tot-aaau-received | Total number of AAA answer messages received in response to the AAR-Update requests. | Int32
> dpeca-tot-aaau-timeout | Total number of AAA answers to Update request timed out. | Int32
> dpeca-tot-str-sent | Total number of STR messages sent. | Int32
> dpeca-tot-sta-received | Total number of STA messages received. | Int32
> dpeca-tot-sta-timeout | Total number of STA answers timed out. | Int32
> dpeca-tot-asr-received | Total number of ASR messages received. | Int32
> dpeca-tot-asa-sent | Total number of ASA messages sent. | Int32
> dpeca-tot-rar-received | Total number of RAR messages received. | Int32
> dpeca-tot-raa-sent | Total number of RAA messages sent. | Int32
> dpeca-tot-protocol-err | Total number of diameter protocol errors that were received from PCRF. | Int32
> dpeca-tot-aaa-parse-err | Total number of AAA parse-errors. | Int32
> dpeca-tot-unk-sess-req | Total number of unknown session requests. | Int32
> dpeca-tot-unk-cmd-codes | Total number of unknown command codes (unsupported command codes). | Int32
> dpeca-tc-logout | Total number of sessions terminated as the user logged out. | Int32
> dpeca-tc-service-not-prov | Total number of sessions terminated as the requested service is not provided. | Int32
> dpeca-tc-bad-ans | Total number of sessions terminated with a bad answer. | Int32
> dpeca-tc-administrative | Total number of sessions terminated administratively. | Int32
> dpeca-tc-link-broken | Total number of sessions terminated due to link broken. | Int32
> dpeca-tc-auth-expired | Total number of sessions terminated due to auth-expiry. | Int32
> dpeca-tc-user-moved | Total number of sessions terminated as the user-moved. | Int32
> dpeca-tc-session-timeout | Total number of sessions terminated due to session timeout. | Int32
> dpeca-auth-rejected | Total number of authorization rejected errors. | Int32
> dpeca-other-errors | Total number of other miscellaneous DPECA errors. | Int32
> dpeca-exp-res-invalid- service-info | Total number of answer messages received with Experimental-Result-Code as 5061 - INVALID_SERVICE_INFORMATION. | Int32
> dpeca-exp-res-filter- restrictions | Total number of answer messages received with Experimental-Result-Code as 5062 - FILTER_RESTRICTIONS. | Int32
> dpeca-exp-res-req-service- not-authorized | Total number of answer messages received with Experimental-Result-Code as 5063 - REQUESTED_SERVICE_NOT_AUTHORIZED. | Int32
> dpeca-exp-res-duplicated-af-session | Total number of answer messages received with Experimental-Result-Code as 5064 - DUPLICATED_AF_SESSION. | Int32
> dpeca-exp-res-ipcan-session-not-avail | Total number of answer messages received with Experimental-Result-Code as 5065 - IP_CAN_SESSION_NOT_AVAILABLE | Int32
> perf-att-init-reg | Total number of initial registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-init-reg-3gpp-geran | Total number of initial registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-3gpp-utran- fdd | Total number of initial registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-3gpp2-1x | Total number of initial registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-ieee-80211a | Total number of initial registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-ieee-80211b | Total number of initial registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-init-reg-other-at | Total number of initial registrations received at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg | Total number of success responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-init-reg-3gpp- geran | Total number of success responses sent for initial registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-3gpp-utran-fdd | Total number of success responses sent for initial registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-3gpp2-1x | Total number of success responses sent for initial registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-ieee- 80211a | Total number of success responses sent for initial registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-ieee- 80211b | Total number of success responses sent for initial registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-init-reg-other | Total number of success responses sent for initial registration for any other access technologies. Applicable only for P-CSCF. | Int64
> perf-fail-init-reg | Total number of failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-401 | Total number of (401 Unauthorized) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-403 | Total number of (403 Forbidden) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-404 | Total number of (404 Not Found) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-420 | Total number of (420 Bad Extension) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-500 | Total number of (500 Internal Error) failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-init-reg-other | Total number of other failure responses sent for initial registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-mean-init-reg-setup | Average time (in milliseconds) between the instance REGISTER is received by P-CSCF and 200 response is sent for the REGISTER. The average is reset every 10 minutes. Applicable only for P-CSCF. Type: Gauge | Int32
> perf-att-rereg | Total number of refresh registrations received at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-rereg-3gpp-geran | Total number of refresh registrations received at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-rereg-3gpp-utran-fdd | Total number of refresh registrations received at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-rereg-3gpp2-1x | Total number of refresh registrations received at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-rereg-ieee-80211a | Total number of refresh registrations received at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-rereg-ieee-80211b | Total number of refresh registrations received at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-rereg-other-at | Total number of refresh registrations received at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-rereg | Total number of success responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-rereg-3gpp-geran | Total number of success responses sent for refresh registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-3gpp-utran- fdd | Total number of success responses sent for refresh registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-3gpp2-1x | Total number of success responses sent for refresh registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-ieee-80211a | Total number of success responses sent for refresh registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-ieee-80211b | Total number of success responses sent for refresh registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-rereg-other | Total number of success responses sent for refresh registration for any other access technology. Applicable only for P-CSCF. | Int64
> perf-fail-rereg | Total number of failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF | Int64
> perf-fail-rereg-401 | Total number of (401 Unauthorized) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-403 | Total number of (403 Forbidden) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-404 | Total number of (404 Not Found) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-420 | Total number of (420 Bad Extension) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-500 | Total number of (500 Internal Error) failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-rereg-other | Total number of other failure responses sent for refresh registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-ue | Total number of de-registrations received from UE at CSCF. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-ue-3gpp- geran | Total number of de-registrations received from UE at CSCF with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-3gpp-utran-fdd | Total number of de-registrations received from UE at CSCF with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-3gpp2-1x | Total number of de-registrations received from UE at CSCF with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-ieee- 80211a | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-ieee- 80211b | Total number of de-registrations received from UE at CSCF with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-att-dereg-ue-other-at | Total number of de-registrations received from UE at CSCF for any other access technology. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue | Total number of success responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-succ-dereg-ue-3gpp- geran | Total number of success responses sent for de-registration with access technology 3GPP-GERAN. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-3gpp- utran-fdd | Total number of success responses sent for de-registration with access technology 3GPP-UTRAN-FDD. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue- 3gpp2-1x | Total number of success responses sent for de-registration with access technology 3GPP2-1X. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-ieee- 80211a | Total number of success responses sent for de-registration with access technology IEEE-802.11a. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-ieee- 80211b | Total number of success responses sent for de-registration with access technology IEEE-802.11b. Applicable only for P-CSCF. | Int64
> perf-succ-dereg-ue-other | Total number of success responses sent for de-registration for any other access technology. Applicable only for P-CSCF. | Int64
> perf-fail-dereg-ue | Total number of failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF | Int64
> perf-fail-dereg-ue-401 | Total number of (401 Unauthorized) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-403 | Total number of (403 Forbidden) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-404 | Total number of (404 Not Found) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-420 | Total number of (420 Bad Extension) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-500 | Total number of (500 Internal Error) failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-fail-dereg-ue-other | Total number of other failure responses sent for de-registration. Applicable only for P-CSCF & S-CSCF. | Int64
> perf-att-dereg-hss | Total number of de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-dereg-hss | Total number of success responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss | Total number of failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-hss-other | Total number of other failure responses for de-registrations initiated by HSS at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-dereg-serv | Total number of de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-dereg-serv | Total number of success responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv | Total number of failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-401 | Total number of (401 Unauthorized) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-403 | Total number of (403 Forbidden) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-404 | Total number of (404 Not Found) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-420 | Total number of (420 Bad Extension) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-500 | Total number of (500 Internal Error) failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-dereg-serv-other | Total number of other failure responses for de-registrations initiated by Service Platform at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-3rdparty-reg | Total number of 3rd Party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-3rdparty-reg | Total number of success responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg | Total number of failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-401 | Total number of (401 Unauthorized) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-403 | Total number of (403 Forbidden) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-404 | Total number of (404 Not Found) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-420 | Total number of (420 Bad Extension) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-500 | Total number of (500 Internal Error) failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-fail-3rdparty-reg-other | Total number of other failure responses for 3rd party registrations initiated by S-CSCF. Applicable only for S-CSCF. | Int64
> perf-att-uar | Total number of user registration status query procedures attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-succ-uaa | Total number of success response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-fail-uaa | Total number of failure response for user registration status queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-att-sar | Total number of S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-succ-saa | Total number of success responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-fail-saa | Total number of failure responses for S-CSCF registration/de-registration notification procedures. Applicable only for S-CSCF. | Int64
> perf-att-session | Total number of attempted session establishments at CSCF. | Int64
> perf-succ-session-180 | Total number of 180 responses for successful session establishments at CSCF. | Int64
> perf-succ-session-200 | Total number of 200 responses (without 180 response) for successful session establishments at CSCF. | Int64
> perf-ans-session | Total number of 200 responses for session establishments at CSCF. | Int64
> perf-fail-session | Total number of failure responses for session establishments at CSCF. | Int64
> perf-att-lir | Total number of user location query procedures attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-succ-lia | Total number of success responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-fail-lia | Total number of failure responses for user location queries attempted at I-CSCF. Applicable only for I-CSCF. | Int64
> perf-att-session-frm-oth- domain | Total number of session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-frbdn-session-frm-oth- domain | Total number of forbidden sessions for session establishments from users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-att-session-to-oth-domain | Total number of session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-frbdn-session-to-oth-domain | Total number of forbidden sessions for session establishments to users of other domains. Applicable only for I-CSCF & S-CSCF. | Int64
> perf-att-init-reg-visited | Total number of initial registrations of visiting users from other IMS network domains. Applicable only for P-CSCF. | Int64
> perf-frbdn-init-reg-visited | Total number of forbidden messages sent for the visiting users. Applicable only for P-CSCF. | Int64
> perf-rmg-users-out | Total number of roaming users to other network domains. Applicable only for S-CSCF. | Int64
> perf-att-mar | Total number of Multimedia-Authentication-Requests attempted. Applicable only for S-CSCF. | Int64
> perf-succ-maa | Total number of successful Multimedia-Authentication-Answers received. Applicable only for S-CSCF. | Int64
> perf-fail-maa | Total number of failure Multimedia-Authentication-Answers received. Applicable only for S-CSCF. | Int64
> perf-att-ppr | Total number of HSS-initiated user profile updates attempted. Applicable only for S-CSCF. | Int64
> perf-succ-ppa | Total number of success responses for HSS-initiated user profile update. Applicable only for S-CSCF. | Int64
> perf-fail-ppa | Total number of failure responses for HSS-initiated user profile update. Applicable only for S-CSCF. | Int64
> perf-att-subscribe | Total number of subscription procedures attempted at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-subscribe | Total number of success responses for subscriptions. Applicable only for S-CSCF. | Int64
> perf-fail-subscribe | Total number of failure responses for subscriptions. Applicable only for S-CSCF. | Int64
> perf-att-notify | Total number of notify procedures attempted at S-CSCF. Applicable only for S-CSCF. | Int64
> perf-succ-notify | Total number of success responses for notify. Applicable only for S-CSCF. | Int64
> perf-fail-notify | Total number of failure responses for notify. Applicable only for S-CSCF. | Int64
> de2a-session-init | Total number of DE2A sessions initiated by sending UDR message. | Int32
> de2a-session-active | Total number of DE2A sessions currently active. | Int32
> de2a-udr-sent | Total number UDR messages sent. | Int32
> de2a-uda-received | Total number of UDA messages received | Int32
> de2a-uda-err-3xxx | Total number of messages with protocol errors. | Int32
> de2a-uda-parse-err | Total number of bad UDA messages received. | Int32
> de2a-udr-err | Total number of UDR send errors. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883