> Exec Mode Commands (D-S)
> This chapter contains the commands in the Exec Mode from debug to system.
> debug
> The following commands send information to the logging facility for review:
> debug ip
> Enables/disables the debug options for IP debugging. If logging is enabled, results are sent to the logging system.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip { arp | interface | route }
> no
> Indicates the IP debugging is to be disabled for the IP interfaces/function specified.
> arp | interface name | route
> Specifies which IP interfaces/function to debug.
> arp: indicates debug is to be enabled for the address resolution protocol.
> interface: indicates debug is to be enabled for the IP interfaces.
> route: indicates debug is to be enabled for the route selection and updates.
> Usage
> The debug IP command is valuable when troubleshooting network problems between nodes. The debugging is stopped by using the no keyword.
> Caution: Issuing this command could negatively impact system performance depending on system configuration and/or loading.
> Example
> The following commands enable/disable debugging for ARP.
> debug ip arpno debug ip arp
> The following enables/disables debugging for IP interfaces.
> debug ip interface
> no debug ip interface
> The following enables/disables debugging for routing.
> debug ip routeno debug ip route
> debug ip bgp
> This command enables BGP (Border Gateway Protocol) debug flags. If logging is enabled, results are sent to the logging system.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip bgp { all | event | filters | fsm | keepalives | updates { inbound | outbound } }
> no
> Disable the specified BGP debug flags.
> all
> Enable all BGP debug flags.
> event
> Enable debugging of all BGP protocol events.
> filters
> Enable debugging of all BGP filters.
> fsm
> Enable debugging of BGP Finite State Machine
> keepalives
> Enable debugging of all BGP keepalives.
> updates {inbound | outbound}
> Enable debugging of BGP updates.
> inbound: Debug all BGP inbound updates.
> outbound: Debug all BGP outbound updates.
> Usage
> Use this command to enable or disable BGP debug flags.
> Example
> The following command disables all BGP debug flags enabled by any of the debug ip bgp commands:
> no debug ip bgp all
> The following command enables all BGP debug flags:
> debug ip bgp all
> debug ip ospf all
> This command enables all OSPF (Open Shortest Path First) debug flags. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf all
> no
> Disable all OSPF debug flags.
> Usage
> Use this command to enable or disable all OSPF debug flags.
> Example
> The following command disables all OPSF debug flags enabled by any of the debug ip ospf commands:
> no debug ip ospf all
> The following command enables all OSPF debug flags:
> debug ip ospf all
> debug ip ospf event
> This command enables debugging of OSPF protocol events. If logging is enabled, results are sent to the logging system. If no keywords are specified, all events are enabled for debugging.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf event [ abr | asbr | vl | lsa | os | router ]
> no
> Disable debugging the specified OSPF event. If no keywords are specified, all events are disabled.
> abr
> Specifies debugging of ABR events.
> asbr
> Specifies debugging of ASBR events.
> vl
> Specifies debugging of VL events.
> lsa
> Specifies debugging of link state advertisement (LSA) events.
> os
> Specifies debugging of OS events.
> router
> Specifies debugging of router events.
> Usage
> Use this command to output debug information for OSPF events.
> Example
> To enable all event debug information, enter the following command;
> debug ip ospf event
> To disable all event debug information, enter the following command;
> no debug ip ospf event
> debug ip ospf ism
> This command enables OSPF Interface State Machine (ISM) troubleshooting, based on ISM information type. If no keywords are specified all ISM information types are enabled. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf ism [ events | status | timers ]
> no
> Disable debugging the specified ISM information. If no keywords are specified, all information is disabled.
> events
> Enable debugging ISM event information.
> status
> Enable debugging ISM status information.
> timers
> Enable debugging ISM timer information.
> Usage
> Use this command to output ISM debug information.
> Example
> To enable all ISM debug information, enter the following command;
> debug ip ospf ism
> To disable all ISM debug information, enter the following command;
> no debug ip ospf ism
> debug ip ospf lsa
> This command enables troubleshooting on OSPF Link State Advertisements (LSAs), based on the specific LSA option. If no keywords are specified, all options are enabled. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf lsa [ flooding | generate | install | refresh | maxage | refresh ]
> no
> Disables the specified LSA debug information. If no keyword is specified, all LSA debug information is disabled.
> flooding
> Enable LSA flooding information.
> generate
> Enable LSA generation information.
> install
> Enable LSA install information.
> maxage
> Enable LSA maximum age information in seconds. The maximum age is 3600 seconds.
> refresh
> Enable LSA refresh information.
> Usage
> Use this command to output debug information for LSAs.
> Example
> To enable all LSA debug information, enter the following command;
> debug ip ospf lsa
> To disable all LSA debug information, enter the following command;
> no debug ip ospf lsa
> debug ip ospf nsm
> This command enables troubleshooting OSPF Neighbor State Machines (NSMs), based on the specific NSM information type. If no keyword is specified, all NSM information types are enabled. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf nsm [ status | events | timers ]
> no
> Disables the debugging the specified NSM information type. If no keyword is specified, all information types are disabled.
> events
> Enables debugging NSM event information.
> status
> Enables debugging NSM status information.
> timers
> Enables debugging NSM timer information.
> Usage
> Use this command to output debug information for OSPF NSMs
> Example
> To enable all NSM debug information, enter the following command;
> debug ip ospf nsm
> To disable all NSM debug information, enter the following command;
> no debug ip ospf nsm
> debug ip ospf packet
> This command enables troubleshooting of specific OSPF packet information. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf packet { all | dd | hello | ls-ack | ls-request | ls-update } [ send | recv ] [ detail ]
> no
> Disable debugging of the specified packet information.
> all
> Enable debugging all OSPF packet information.
> dd
> Enable debugging database descriptions.
> hello
> Enable debugging hello packets.
> ls-ack
> Enable debugging link state acknowledgements.
> ls-request
> Enable debugging link state requests.
> ls-update
> Enable debugging link state updates.
> send
> Enable debugging only on sent packets.
> recv
> Enable debugging only on received packets.
> detail
> Enable detailed information in the debug output.
> Usage
> Use this command to output specific OSPF packet information.
> Example
> To enable all packet debug information, enter the following command;
> debug ip ospf packet all
> To disable all route debug information, enter the following command;
> no debug ip ospf packet all
> debug ip ospf route
> This command sets the route calculation method to use in debugging OSPF routes. If no route calculation method is specified, all methods are enabled. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf route [ ase | ia | install | spf ]
> no
> Disables debugging of route information. If no keyword is specified all information types are disabled.
> ase
> Enables debugging information on external route calculations.
> ia
> Enables debugging information on Inter-Area route calculations.
> install
> Enables debugging information on route installation.
> spf
> Enables debugging information on SPF route calculations.
> Usage
> Use this command to output debug information for OSPF routes.
> Example
> To enable all route debug information, enter the following command;
> debug ip ospf route
> To disable all route debug information, enter the following command;
> no debug ip ospf route
> debug ip ospf router
> This command sets the debug option for OSPF router information. If no keyword is specified, all router information is enabled. If logging is enabled, results are sent to the logging system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] debug ip ospf router [ interface | redistribute ]
> no
> Disables the specified router debug information. If no keyword is specified, all router information is disabled.
> interface
> Enables router interface information.
> redistribute
> Enables router redistribute information.
> Usage
> Use this command to output debug information for the OSPF router.
> Example
> To enable all router debug information, enter the following command;
> debug ip ospf router
> To disable all router debug information, enter the following command;
> no debug ip ospf router
> default terminal
> Restores the system default value for the terminal options.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> default terminal { length | width }
> length | width
> length: reset the terminal length to the system default.
> width: restores the system default terminal width.
> Usage
> Restore the default terminal settings when the current paging and display wraps inappropriately or pages to soon.
> Example
> The following sets the default length then width in two commands.
> default terminal length
> default terminal width
> delete
> Removes the specified file(s) permanently from the local.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> delete filepath [ -noconfirm ]
> filepath
> Specifies the location of the file to delete. The path must be formatted according to the following format:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [ file: ] { /flash | /pcmcia1 | /hd }[ /directory ] /file_name

> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name
> filename is the actual file of interest
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Important: Use of the -noconfirm option should be done with extra care to ensure the file is specified accurately as there is no method of recovering a file that has been deleted.
> Usage
> Deleting files is a maintenance activity which may be part of periodic routine procedures to reduce system space utilization.
> Example
> The following removes files from the local /flash/pub directory.
> delete /flash/pub/june03.cfg
> dhcp force
> Tests the lease-renewal for DHCP-assigned IP addresses for a particular subscriber.
> Product
> GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> dhcp force lease-renewal { callid id | imsi imsi [ nsapi nsapi ] | msid msid }
> callid id
> Clears the call specified by call_id. The call ID must be specified as a 4-byte hexadecimal number.
> imsi msid
> Disconnects the subscriber with the specified msid. The IMSI (International Mobile Subscriber Identity) ID is a 50-bit field which identifies the subscriber’s home country and carrier. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
> nsapi nsapi
> A specific Network Service Access Point Identifier (NSAPI).
> nsapi is an integer value from 5 to 15.
> msid id
> Disconnects the mobile user identified by ms_id. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as a wildcard enclose them in single quotes ( ‘ ). For example; ‘$’.
> Usage
> Use this command tests a forced IP address lease renewal for a specific subscriber.
> Example
> The following command tests DHCP lease renewal for a subscriber with an MSID of 1234567:
> dhcp force lease-renewal msid 1234567
> dhcp test
> Tests DHCP (Dynamic Host Configuration Protocol) functions for a particular DHCP service.
> Product
> GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> dhcp test dhcp-service svc_name [ all | server ip_address ]
> dhcp-service svc_name
> The name of the DHCP service. It can be from 1 to 63 alphanumeric characters in length and is case sensitive.
> all
> Tests DHCP functionality for all servers.
> server ip_address
> Tests DHCP functionality for the server.
> ip_address is the IP address of the DHCP server in dotted-decimal notation.
> Usage
> Once DHCP functionality is configured on the system, this command can be used to verify that it is configured properly and that it can successfully communicate with the DHCP server.
> Executing this command causes the system to request and allocate an IP address and then release it.
> If a specific DHCP server is not specified, then each server configured in the service is tested.
> Example
> The following command tests the systems ability to get an IP address from all servers a DHCP service called DHCP-Gi is configured to communicate with:
> dhcp test dhcp-service DHCP-Gi all
> diameter disable endpoint
> This command disables a Diameter endpoint without removing the peer’s configuration.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter disable endpoint endpoint_name peer peer_id
> endpoint endpoint_name
> Specifies the endpoint in which the peer is configured.
> endpoint_name the name of the endpoint, an alphanumeric string of 1 to 63 characters.
> peer peer_id
> Specifies the peer to be disabled.
> peer_id the Diameter peer host name a string of 1 to 63 characters.
> Usage
> Use this command to administratively disable a Diameter peer without removing the peer configuration. This command will tear down all connections on the specified peer (by sending a DPR if the configuration demands the same at peer level configuration). The peer will remain in disabled state until it is enabled again. Also see the diameter enable endpoint command.
> Example
> This command disables the Diameter peer peer12:
> diameter disable endpoint endpoint1 peer peer12
> diameter enable endpoint
> This command enables a Diameter endpoint that is disabled.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter enable endpoint endpoint_name peer peer_id
> endpoint endpoint_name
> Specifies the endpoint in which the peer is configured.
> endpoint_name the endpoint name, a string of 1 to 63 characters.
> peer peer_id
> Specifies the peer to be enabled.
> peer_id the Diameter peer host name, a string of 1 to 63 characters.
> Usage
> Use this command to administratively enable a Diameter peer. Also see the diameter disable endpoint command.
> Example
> This command enables the Diameter peer peer12:
> diameter enable endpoint endpoint1 peer peer12
> diameter reset connection
> This command resets individual TCP/SCTP connections for a specified Diameter endpoint.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> diameter reset connection { endpoint endpoint_name peer peer_id }
> endpoint endpoint_name
> Resets connection to the specified endpoint.
> endpoint_name the endpoint name, an alphanumeric string of 1 to 63 characters.
> peer peer_id
> Resets connection to the specified peer.
> peer_id the Diameter peer host name, an alphanumeric string of 1 to 63 characters.
> Usage
> Use this command to reset the TCP/SCTP connections for the specified endpoint/peer. With this command, the connection will be closed temporarily after DPR/DPA. If there is any traffic to be sent to the particular peer, then the connection will be re-established.
> This command overrides the endpoint configured in any other configuration mode.
> This command is applicable only when the specified peer is enabled.
> Example
> This command resets connection to the endpoint named test123:
> diameter reset connection endpoint test123
> diameter reset route failure
> This command resets the failed route status of a Diameter destination-host combination via peer to AVAILABLE status.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> diameter reset route failure [ endpoint endpoint_name ] [ host host_name ] [ peer peer_id ]
> endpoint endpoint_name
> Resets paths to the specified endpoint.
> endpoint_name must be a string of 1 to 63 characters.
> host host_name
> Resets the FAILED status of all Diameter destination-host combination routes via peer for every Diameter client within the chassis having a specific host name to AVAILABLE.
> host_name the Diameter host name, a string of 1 to 63 characters.
> peer peer_id
> Resets the FAILED status of all Diameter destination-host combination routes via a peer having specific peer-Id for every Diameter client within the chassis to AVAILABLE.
> peer_id the Diameter peer host name, a string of 1 to 63 characters.
> Usage
> Use this command to reset the FAILED status of all Diameter destination-host combination routes via peer for every Diameter client within the chassis to AVAILABLE status.
> This command also resets the failure counts used to determine the AVAILABLE/FAILED status of a destination-host combination.
> When executed from local context, this command matches all contexts. If an optional keyword is not supplied, a wildcard is used for the value.
> The status of every matching combination of destination-host via peer for every matching Diameter client within the chassis will be reset to AVAILABLE. The failure counts that are used to determine AVAILABLE/FAILED status will also be reset.
> Also see the route-entry and route-failure CLI commands in the Diameter Endpoint Configuration Mode.
> Default value: N/A
> Example
> The following command resets the FAILED status of all Diameter destination-host combination routes via peer for every Diameter client within the chassis for specified endpoint name to AVAILABLE.
> diameter reset route failure endpoint endpoint_name
> directory
> Lists the files in a specified location.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> directory filepath [ -size ] [ -reverse ] [ -time ]
> filepath
> Specifies the directory path to list the contained files. The path must be formatted according to the following format:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [ file: ] { /flash | /pcmcia1 | /hd }[ /directory ] /file_name

> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name
> filename is the actual file of interest
> -size
> Indicates the size of each file should be displayed in the output.
> -reverse
> Indicates the order of files listed should be in descending order (z-aZ-A9-0). Default is to sort in ascending order (0-9A-Za-z).
> -time
> Indicates the last modification timestamp of each file should be displayed in the output.
> Usage
> Lists such things as log and crash files from multiple nodes within the network.
> The optional arguments may be specified individually or in any combination.
> Example
> The following command will list the files in the local /flash/pub directory sorted in reverse order.
> directory /flash/pub -reverse
> disable
> Prevents the system from making requests of a selected RADIUS server.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> disable radius [ accounting | charging [ accounting ] ] server address [ port num ] [ group name ]
> accounting | charging | charging accounting
> Specifies the type of RADIUS server to disable.
> server address
> Identifies the RADIUS server by IP address.
> address is specified using the standard IPv4 or IPv6 dotted decimal notation.
> port num
> Default: 1812 (authentication) 1813 (accounting)
> Specifies the port number of the RADIUS server being disabled.
> num must be the configured port number of the RADIUS server being disabled and be 0 to 65535 numeric characters in length.
> group name
> Default: default
> Specifies the RADIUS group to which the server belongs. Use this option in the event that the RADIUS server belongs to multiple groups and you only want to disable the server within the specific group.
> name must be the name of a configured RADIUS Server group and be 1 to 63 characters in length.
> Usage
> Use this command to gracefully stop the system from making requests of a specific RADIUS server.
> Example
> The following command disables a RADIUS accounting server with an IP address of 1.2.3.4, the default accounting server port number, and that resides in the “Group5” server group:
> disable radius accounting server 1.2.3.4 group Group5
> dns-client
> This command performs DNS (Domain Name System) query on the basis of specified DNS client name, DNS query domain name, and type of query criteria.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> dns-client dns_client_name [ query-type { A | AAAA | NAPTR | SRV } ] query-name query_domain_name
> dns-client dns_client_name
> Defines the name of the DNS client whose cache and/or statistics are to be queried. dns_client_name is an existing DNS client and must be from alphanumeric string of 1 through 64 characters.
> query-type { A | NAPTR | SRV } ]
> Default: A
> This keyword specifies that the type of query to perform for the defined DNS client is to be displayed.

> • | A: Filters DNS results based on domain IPv4 address records (A records). This is the default query type.

> • | AAAA: Filters DNS results based on domain IPv6 address records (AAAA records).

> • | NAPTR: Filters DNS results based on Naming Authority Pointer records (NAPTR).

> • | SRV: Filters DNS results based on service host records (SRV records).

> query-name query_domain_name
> This keyword filters the DNS results based on the query domain name.
> query_domain_name must be from 1 to 255 characters in length. query_domain_name is the domain name used to perform the DNS query and is different from the actual domain name which is resolved. For example, to resolve the SIP server for service.com, the query name is _sip._udp.service.com and the query type is SRV.
> Usage
> Use this command to perform DNS query on the basis of DNS Client name and filters the query results based on query type and query name. This command also populates the result into DNS Cache. This command used the current context to DNS request.
> Example
> The following command displays statistics for a DNS client named test_dns with query type for IP address as A and query name as domain1.com:
> dns-client test_dns query-type A query-name domain1.com
> enable
> Allows the system to start making requests of a selected RADIUS server.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> enable radius [ accounting | charging | [ accounting ] ] server address [ port num ] [ group name ]
> accounting | charging | charging accounting
> Specifies the type of RADIUS server to enable.
> server address
> Identifies the RADIUS server by IP address.
> address is specified using the standard IPv4 or IPv6 dotted decimal notation.
> port num
> Default: 1812 (authentication) 1813 (accounting)
> Specifies the port number of the RADIUS server being enabled.
> num the configured port number of the RADIUS server being enabled, 0 to 65535 numeric characters.
> group name
> Default: default
> Specifies the RADIUS group to which the server belongs. Use this option in the event that the RADIUS server belongs to multiple groups and you only want to disable the server within the specific group.
> name the name of a configured RADIUS Server group (1 to 63 characters).
> Usage
> Use this command to allow the system to start making requests of a specific RADIUS server.
> Example
> The following command enables a RADIUS accounting server with an IP address of 1.2.3.4, the default accounting server port number, and that resides in the “Group5” server group:
> enable radius accounting server 1.2.3.4 group Group5
> filesystem
> Used this command to check, format, or repair the PCMCIA, the Compact Flash on the SMC, or the HD Raid storage device.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> filesystem { check | format | repair } { /flash | /pcmcia1 | /hd-raid } [ card card_num ]
> Format the file system on the specified device.
> Usage
> Check, format, or repair all directories and files from the PCMCIA card(s), the Compact Flash and/or the HD Raid storage device and re-establish the file system.
> Example
> The following command formats the PCMCIA card located in slot 1 on the SMC:
> filesystem format /pcmcia1
> filesystem synchronize
> Use this command to manage the Switch Processor Cards (SPCs) and their active/standby status, and to synchronize the filesystem between the active device and the standby device.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> filesystem synchronize [ /flash | /pcmcia1 | all ] [ checkonly ] [ from card_num | to card_num ] [ -noconfirm ]
> Synchronize the file system on the specified device.
> Usage
> Synchronize the file system between the active device and the standby device.
> gtpc test echo
> Tests the ability of a GGSN service to exchange GTP-C echo request messages with the specified SGSN(s).
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> gtpc test echo src-address gn_address { all | sgsn-address ip_address }
> src-address gn_address
> Specifies the IP address of a Gn interface configured on the system.
> gn_address must be expressed in dotted decimal notation.
> Important: The IP address of the system’s Gn interface must be bound to a configured GGSN service prior to executing this command.
> all
> Specifies that GTP-C echo requests will be sent to all SGSNs that currently have sessions with the GGSN service.
> sgsn-address ip_address
> Specifies that GTP-C echo requests will be sent to a specific SGSN.
> ip_address is the address of the SGSN to send the requests to and must be expressed in dotted decimal notation.
> Usage
> This command tests the GGSN’s ability to exchange GPRS Tunneling Protocol control plane (GTP-C) packets with the specified SGSNs. This command is useful for troubleshooting and/or monitoring.
> This command must be executed from within the context in which the GGSN service is configured.
> Refer also to the gtpu test command.
> Example
> The following command issues GTP-C echo packets from a GGSN service bound to address 192.168.157.32 to an SGSN with an address of 192.168.157.2:
> gtpc test echo src-address 192.168.157.32 sgsn-address 192.168.157.2
> gtpp interim now
> Check points current GTPP accounting messages and identifies which types of interim CDRs are to be generated and sent to the external charging/storage servers (e.g., a CFG or a GSS). The impact of this command is immediate.
> Product
> GGSN, SGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> gtpp interim now [ active-charging egcdr | apn apn_name | callid call_id | cdr-types { gcdr | mcdr | scdr } | dhcp-server ip_address | gprs-service svc_name| ggsn-address ggsn_ip_addr | ggsn-service svc_name | imsi imsi [ ip-address sub_address [ username name ] now | nsapi nsapi [ ip-address sub-address [ username name ] | username name ] ] | ip-address sub_address [ username name ] | ip-pool pool_name | mcc mcc_number mnc mnc_number | msisdn msisdn_num | sgsn-address ip_address | sgsn-service svc_name | username name ] +
> active-charging
> This feature is specific to the GGSN and is documented separately. See .
> apn apn_name
> Initiates GTPP interim accounting for all PDP contexts accessing the specified APN.
> apn_name can be from 1 to 62, case sensitive, alphanumeric characters.
> callid call_id
> Identifies a specific call.
> call_id must be followed by an 8-digit HEX number.
> cdr-types { mcdr | scdr }
> Specifies the CDR types to be generated by the SGSN:
> This keyword is specific to the SGSN.
> gcdr - Instructs the GGSN to only generate G-CDRs.
> mcdr - Instructs the SGSN to only generate M-CDRs
> scdr - Instructs the SGSN to only generate S-CDRs.
> dhcp-server ip_address
> Identifies the DHCP server where the IP address (defined with the ip address keyword) was allocated. Must be followed by the IP address of the DHCP server.
> ip_address: Must be specified using dotted decimal notation.
> ggsn-address ggsn_ip_addr
> This keyword is specific to the GGSN.
> Specifies the IP address of the interface to the GGSN.
> ggsn_ip_addr must be specified using dotted decimal notation.
> ggsn-service svc_name
> This keyword is specific to the GGSN.
> Initiates GTPP interim accounting for all PDP contexts currently being facilitated by the specified GGSN service.
> svc_name can be from 1 to 63, case sensitive, alphanumeric characters.
> gprs-service svc_name
> This keyword is specific to the SGSN.
> Initiates GTPP interim accounting for all PDP contexts currently being facilitated by the specified GPRS service.
> This keyword is specific to the SGSN.
> svc_name can be from 1 to 63, case sensitive, alphanumeric characters. Must be an already defined GPRS service name.
> imsi imsi [ ip-address sub_address [ username name ] | nsapi nsapi [ ip-address sub-address [ username name ] | username name ] ]
> Initiates GTPP interim accounting for a specific International Mobile Subscriber Identity (IMSI) number. The request could be further filtered using any of the following keywords:

> • | ip-address: Interim accounting will be performed for the address specified by sub_address. The command can be further filtered by specifying a specific username ( name ) with that address.

> • | nsapi: Interim accounting will be performed for a specific Network Service Access Point Identifier (NSAPI). nsapi is an integer value from 5 to 15. The command can be further filtered by specifying a specific ip address (sub_address) and/or a username (name) with that address, or just a specific username.

> ip-address sub_address [ username name ]
> Initiates GTPP interim accounting for the address specified.
> sub_address is the IP address of the subscriber and must be expressed in dotted decimal notation.
> The command can be further filtered by specifying username with that address.
> name is the subscriber’s name and can be a sequence of characters and/or wildcard characters ('$' and '*') from 1 to 127 characters in length. The * wildcard matches multiple characters and the $ wildcard matches a single character. If you do not want the wildcard characters interpreted as wildcard enclose them in single quotes ( ‘). For example; ‘$’.
> ip-pool pool_name
> This keyword is applicable to the GGSN only.
> Initiates GTPP interim accounting for all PDP contexts that were allocated IP addresses from the specified pool.
> pool_name can be from 1 to 31 alphanumeric characters and is case sensitive.
> mcc mcc_number mnc mnc_number
> mcc_number Specifies the mobile country code (MCC) portion of the PLMN identifier and can be configured to any 3-digit integer value between 100 and 999.
> mnc_number Specifies the mobile network code (MNC) portion of the PLMN identifier and can be configured to any 2 or 3 digit integer value between 00 and 999.
> msisdn msisdn_num
> This keyword configures the SGSN to include the Mobile Subscribers Integrated Services Digital Network identifier in generated CDRs (M-CDRs and/or the S-CDRs).
> This keyword is applicable for SGSN only.
> msisdn_number - Must be followed by a valid MSISDN number, consisting of 1 to 15 digits.
> sgsn-address ip_address
> This keyword is specific to the GGSN.
> Initiates GTPP interim accounting for all PDP contexts currently being facilitated by the specified SGSN.
> ip_address is the IP address of the SGSN and must be expressed in dotted decimal notation.
> sgsn-service svc_name
> Initiates GTPP interim accounting for all PDP contexts currently being facilitated by the specified SGSN service.
> This keyword is specific to the SGSN.
> svc_name can be from 1 to 63, case sensitive, alphanumeric characters. Must be an already defined SGSN service name.
> username name
> Initiates GTPP interim accounting for all PDP contexts for the subscriber specified.
> name is the subscriber’s name and can be from 1 to 127 alphanumeric characters and is case sensitive.
> +
> More than one of the above keywords can be entered within a single command.
> Usage
> This command causes GTPP accounting CDRs to immediately be generated for all active sessions that are in the current context. If executed within the local context, CDRs will be generated for all active sessions regardless of context.
> The sending of the CDRs is paced so as not to overload the accounting server.
> Example
> The following command causes CDRs to immediately be generated:
> gtpp interim now
> gtpp interim now active-charging egcdr
> Check points current GTPP accounting messages for active charging immediately.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> gtpp interim now active-charging egcdr [ callid call_id | imsi imsi | msid msid | rulebase rbase_name | session-id sess_id | username name ]
> callid call_id
> Initiates GTPP interim accounting for a session with the specific call ID. call_id must be an 8-digit hexadecimal number.
> imsi imsi
> Initiates GTPP interim accounting for a specific International Mobile Subscriber Identity (IMSI) number. imsi must be a sequence of hexadecimal digits and wildcard characters - $ matches a single character and * matches multiple characters
> msid msid
> Initiates GTPP interim accounting for a specific Mobile Station Identifier (MSID) number. msid must be a sequence of up to 24 digits and wildcard characters - $ matches a single character and * matches multiple characters
> rulebase rbase_name
> Initiates GTPP interim accounting for sessions that use the named active charging rulebase. rbase_name must be an alphanumeric string of from 1 through 24 characters.
> session-id sess_id
> Initiates GTPP interim accounting for a specific active charging session. sess_id must be the name of a current active charging session.
> username name
> Initiates GTPP interim accounting for all PDP contexts for the subscriber specified.
> name is the subscriber’s name and can be from 1 to 127 alphanumeric characters and is case sensitive.
> Usage
> This command causes GTPP accounting eG-CDRs to immediately be generated for active charging sessions that meet the specified criteria.
> The sending of the CDRs is paced so as not to overload the accounting server.
> Example
> The following command causes eG-CDRs to immediately be generated for active charging sessions using the rulebase named rulbase1:
> gtpp interim now active-charging egcdr rulebase rulebase1
> gtpp storage-server commit
> Causes the GTPP storage server to save all buffered packets to the hard drive.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> gtpp storage-server commit now [ group name group_name ]
> group name group_name
> Commits Storage Server for the specified group name to be used.
> name is the group name and can be from 1 to 63 alphanumeric characters.
> Usage
> Upon execution, this command is relayed by the system to the GTPP Storage Server (GSS) causing the GSS to save all buffered packets to the hard drive. It also causes the GSS to delete all CDRs that have been acknowledged by the CGF. The deleted CDRs are saved in a separate file.
> Note that this command must be executed from within the context in which the GSS is configured.
> Refer to the gtpp storage-server command in the Context Configuration Mode for more information.
> gtpp test
> Tests the system’s ability to communicate with configured charging gateway function (CGF) severs or a GTPP Storage-Server (GSS).
> Product
> GGSN
> Privilege
> Operator, Config-Administrator, Administrator
> Syntax
> gtpp test { accounting { all | cgf-server cgf_address | group name group_name } | storage-server [ address ip-addr port udp-port | group name group_name ] }
> all
> Tests all CGFs configured within the given context.
> cgf-server cgf_address
> Tests a specific CGF configured within the given context.
> ip_address is the IP address of the CGF expressed in dotted decimal notation.
> group name group_name
> Tests the storage server for a specific group.
> group_name enter a name of 1 to 63 alphanumeric characters to identify the group.
> storage-server [ address ip-address port udp-port]
> Test the connectivity and provide round trip time for the echo request sent to the GTPP Storage-Server configured in the requested context.
> ip_address is the IP address of the GSS expressed in dotted decimal notation and udp-port is the port defined for the GTPP Storage Server.
> Usage
> This command is used to verify the configuration of and test the system’s ability to communicate with one or all configured GSS/CGFs for monitoring or troubleshooting purposes.
> When executed, this command causes the system to send GTPP echo packets to the specified GSS/CGF(s). The command’s response will display whether the GSS/CGF is active or unreachable.
> Example
> The following command tests communication with a CGF having an IP address of 192.168.1.5:
> gtpp test accounting cgf-server 192.168.1.5
> The following command tests communication with a GSS configured in requested context
> gtpp test storage-server
> The following command verify communication with a GSS, having IP address 192.156.12.10 and port 50000, without configuring it in a context
> gtpp test storage-server address 192.156.12.10 port 50000
> gtpu test echo
> Tests the ability of a GGSN service to exchange GTP-U echo request messages with the specified SGSN(s).
> Product
> GGSN
> Privilege
> Operator, Config-Administrator, Administrator
> Syntax
> gtpu test echo src-address gn_address { all | sgsn-address ip_address }
> src-address gn_address
> Specifies the IP address of a Gn interface configured on the system.
> gn_address must be expressed in dotted decimal notation.
> Important: The IP address of the system’s Gn interface must be bound to a configured GGSN service prior to executing this command.
> all
> Specifies that GTP-U echo requests will be sent to all SGSNs that currently have sessions with the GGSN service.
> sgsn-address ip_address
> Specifies that GTP-U echo requests will be sent to a specific SGSN.
> ip_address is the address of the SGSN to send the requests to and must be expressed in dotted decimal notation.
> Usage
> This command tests the GGSN’s ability to exchange GPRS Tunneling Protocol user plane (GTP-U) packets with the specified SGSNs. This command is useful for troubleshooting and/or monitoring.
> This command must be executed from within the context in which the GGSN service is configured.
> Refer also to the gtpc test command.
> Example
> The following command issues GTP-U echo packets from a GGSN service bound to address 192.168.157.43 to an SGSN with an address of 192.168.1.52:
> gtpu test echo src-address 192.168.157.43 sgsn-address 192.168.157.2
> gtpv0 test echo
> Tests the ability of a GGSN service to exchange GTPv0 echo request messages with the specified SGSN(s).
> Product
> GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> gtpv0 test echo src-address gn_address { all | sgsn-address ip_address }
> src-address gn_address
> Specifies the IP address of a Gn interface configured on the system.
> gn_address must be expressed in dotted decimal notation.
> Important: The IP address of the system’s Gn interface must be bound to a configured GGSN service prior to executing this command.
> all
> Specifies that GTPv0 echo requests will be sent to all SGSNs that currently have sessions with the GGSN service.
> sgsn-address ip_address
> Specifies that GTPv0 echo requests will be sent to a specific SGSN.
> ip_address is the address of the SGSN to send the requests to and must be expressed in dotted decimal notation.
> Usage
> This command tests the GGSN’s ability to exchange GPRS Tunneling Protocol version 0 (GTPv0) packets with the specified SGSNs which can be useful troubleshooting and/or monitoring.
> This command must be executed from within the context in which the GGSN service is configured.
> Refer also to the gtpc test and gtpu test commands.
> Example
> The following command issues GTPv0 echo packets from a GGSN service bound to address 192.168.1.33 to an SGSN with an address of 192.168.1.42:
> gtpv0 test echo src-address 192.168.1.33 sgsn-address 192.168.1.42
> hd raid
> Performs RAID management operations on the hard drives of redundant SMCs.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> hd raid { check | { create { local1 | remote1 } [ -force ] [ -noconfirm ] } | { overwrite { local1 | remote1 } [ -force ] [ -noconfirm ] } | { select { local1 | remote1 } [ -force ] [ -noconfirm ] } | { insert { local1 | remote1 } [ -force ] [ -noconfirm ] } | { remove { local1 | remote1 } [ -force ] [ -noconfirm ] } }
> check
> Starts a background check on RAID disks unless the RAID is running in degraded mode.
> -noconfirm: instructs system not to display “are you sure” prompts. -force: instructs the system to enforce the action and override warnings.
> create local1 | remote1
> Overwrites the specified disk to create a new RAID that could run in degraded mode on the specified drive:
> local1: specifies the RAID is to be established on the primary SMC. remote1: specifies the RAID is to be established on the backup SMC.
> -noconfirm: instructs system not to display “are you sure” prompts.. -force: instructs the system to enforce the action and override warnings.
> overwrite local1 | remote1
> Overwrites the specified disk and adds it to the current running RAID to construct a fully mirrored array.
> local1: specifies the primary SMC is to be added to the current RAID. remote1: specifies the backup SMC is to be added to the current RAID.
> -noconfirm: instructs system not to display “are you sure” prompts. -force: instructs the system to enforce the action and override warnings.
> select local1 | remote1
> Selects the specified disk to assemble a RAID when two unrelated RAID disks are present in the system. The resulting RAID runs in degraded mode.
> local1: specifies the primary SMC is to assemble the RAID. remote1: specifies the backup SMC is to assemble the RAID.
> -noconfirm: instructs system not to display “are you sure” prompts. -force: instructs the system to enforce the action and override warnings.
> insert local1 | remote1
> Inserts the specified disk to the running RAID causing it to recover from degraded mode.
> local1: specifies the primary SMC is to be inserted into the RAID. remote1: specifies the backup SMC is to be inserted into the RAID.
> -noconfirm: instructs system not to display “are you sure” prompts. -force: instructs the system to enforce the action and override warnings.
> remove local1 | remote1
> Removes the specified disk from the running RAID causing it to run in degraded mode or to fail.
> local1: specifies the primary SMC is to be removed from the RAID. remote1: specifies the backup SMC is to be removed from the RAID.
> -noconfirm: instructs system not to display “are you sure” prompts. -force: instructs the system to enforce the action and override warnings.
> Usage
> All commands need confirmation unless the -noconfirm is included in the command. If the result will bring down a running RAID, you have to force the command using -force.
> RAID commands are needed to intervene in the following situations:

> • | the hard disk controller task can not determine the correct operation,

> • | administrator action is required by policy

> • | the administrator wants to wipe out an unused disk.

> In an automated system, the policies created with this CLI address the possibility of a manually partitioned disk, a disk resulting from a different version of software, a partially constructed disk, or the case of two unrelated disks in the system.
> To reduce administrator intervention, a set of policies can be configured to set the default action using the commands in the HD RAID configuration mode. These hd raid commands are described in the HD RAID Configuration Mode chapter of this guide.
> Example
> The following instructs the system to setup a RAID on the primary SMC hard drive.
> hd raid create local1 -force
> host
> Used to resolve the IP address or logical host name information via a DNS query.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> host { host_name | host_ip_address }
> host_name | host_ip_address
> Specifies the host for which IP information is to be displayed.
> host_name: specifies the logical host name for which the IP address is to be displayed (via DNS lookup).
> host_ip_address: specifies the IP address for which the associated logical host name(s) are to be displayed (via reverse DNS lookup).
> Usage
> Verify DNS information which affects connections and packet routing.
> Example
> The following will resolve the host information for remoteABC and 1.2.3.4.
> host remoteABC
> host 1.2.3.4
> interface
> Use this command to configure the system to generate gratuitous ARP (G-ARP) requests in case of a failure during an inter-node online upgrade. If the chassis is not active, an error message displays.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, or Inspector with li-administrator permissions
> Syntax
> interface name send gratuitous-arp ip-address
> Usage
> This command generates a G-ARP for the IP address specified and sends it over the interface.
> Example
> The following generate a G-ARP for IP address 192.168.100.10.
> interface interface_1 send gratuitous-arp 192.168.100.10
> lawful-intercept
> Refer to the Lawful Intercept Configuration Guide for a description of this command.
> lawful-intercept packet-cable
> Refer to the Lawful Intercept Configuration Guide for a description of this command.
> lawful-intercept ssdf
> Refer to the Lawful Intercept Guide for a description of this command.
> link-aggregation port switch to
> When a link aggregation group (LAG) contains two sets of ports, each connecting to a different Ethernet switch, this command allows you to change the status of the active distributing ports.
> Default: none.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> link-aggregation port switch to slot# / port#
> slot#
> Identifies the physical chassis slot where the line card is installed.
> port#
> Identifies the physical port on the line card to automatically switch to.
> Usage
> This command is subject to the following restrictions:

> • | slot#/port# must support LAG.

> • | slot#/port# must be configured with LAG.

> • | slot#/port# must not be actively distributing.

> • | slot#/port# must have negotiated a partner while in standard mode.

> • | slot#/port#’s partner must have a priority equal to or greater than itself.

> • | slot#/port#’s partner bundle must have bandwidth in standard mode equal to or greater than itself.

> • | Switching to slot#/port# must not violate preference within hold-time in standard mode.

> Example
> link-aggregation port switch to 17/2
> logging active
> Enables/disables logging for active internal log files.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> logging active [ copy runtime filters ] [ event-verbosity event_level ] [ pdu-data format ] [ pdu-verbosity pdu_level ]
> no logging active
> no
> Indicates the internal logging is to be disabled.
> copy runtime filters
> When this command is issued, it makes a copy of the runtime filters and uses that copy to filter the current logging session.
> event-verbosity event_level
> Specifies the level of verboseness to use in logging of events as one of:

> • | min - displays minimal information about the event. Information includes event name, facility, event ID, severity level, date, and time.

> • | concise - displays detailed information about the event, but does not provide the event source within the system.

> • | full - displays detailed information about event, including source information, identifying where within the system the event was generated.

> pdu-data format
> Specifies output format for packet data units when logged as one of:

> • | none - output is in raw format (unformatted).

> • | hex - output is in hexadecimal format.

> • | hex-ascii - output is in hexadecimal and ASCII similar to a main-frame dump.

> pdu-verbosity pdu_level
> Specifies the level of verboseness to use in logging of packet data units as a value from 1 to 5 where 5 is the most detailed.
> Usage
> Adjust the active logging levels when excessive log file sizes are being generated or, conversely, not enough information is being sent to the active log files for adequate troubleshooting support. The no keyword is used to disable internal logging.
> Important: A maximum of 50,000 events may be stored in each log. Enabling more events for logging may cause the log to be filled in a much shorter time period. This may reduce the effectiveness of the log data as a shorter time period of event data may make troubleshooting more difficult.
> Important: Once a log has reached the 50,000 event limit the oldest events will be discarded as new log entries are created.
> Example
> The following sets the active logging for events to the maximum.
> logging active event-verbosity full
> The following command sets the active logging for packet data units to level 3 and sets the output format to the main-frame style hex-ascii.
> logging active pdu-data hex-ascii pdu-verbosity 3
> The following disables internal logging.
> no logging active
> logging filter
> Sets the logging filtering options for all or individual facilities.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> logging filter active facility facility level severity_level [ critical-info | no-critical-info ]
> active
> Indicates only active processes are to have logging options set.
> facility facility
> Specifies the facility to modify the filtering of logged information. Valid facilities for this command are:

> • | a10: A10 interface facility

> • | a11: A11 interface facility

> • | a11mgr: A11 Manager facility

> • | aaa-client: AAA client facility

> • | aaamgr: AAA manager logging facility

> • | aaaproxy: AAA Proxy facility

> • | aal2: AAL2 protocol logging facility

> • | acl-log: Access Control List logging facility

> • | acsctrl: Active Charging Service (ACS) Controller facility

> • | acsmgr: Active Charging Service (ACS) Manager facility

> • | alarmctrl: Alarm Controller facility

> • | alcap: ALCAP protocol logging facility

> • | alcapmgr: ALCAPMgr logging facility

> • | all: All facilities

> • | asngwmgr: ASN Gateway Manager facility

> • | asnpcmgr: ASN Paging Controller Manager facility

> • | bfd: BFD protocol logging facility

> • | bgp: Border Gateway Protocol (BGP) facility

> • | bindmux: IPCF BindMux-De-mux Manager logging facility

> • | bssap+: Base Station Sub-system Application Part+ protocol facility for loggin interface between the SGSN and the MSC/VLR (2.5G and 3G)

> • | bssgp: Base Station Sub-system GPRS Protocol logging facility handles exchange information between the SGSN and the BSS (2.5G only)

> • | callhome: Call home application logging facility

> • | cap: CAMEL Application Part (CAP) logging facility for protocol used in prepaid applications (2.5G and 3G)

> • | cli: CLI logging facility

> • | credit-control: Credit Control facility

> • | cscf: IMS/MMD CSCF

> • | cscfmgr: SIP CSCF Manager facility

> • | cscfttmgr: SIP CSCFTT Manager facility

> • | csp: Card Slot Port controller facility

> • | css: Content Service Selection (CSS) facility

> • | css-sig: Content Service Selection (CSS) RADIUS Signaling facility

> • | cx-diameter: Cx Diameter Messages facility

> • | dcardctrl: IPSEC Daughtercard Controller logging facility

> • | dcardmgr: IPSEC Daughtercard Manager logging facility

> • | demuxmgr: Demux Manager API facility

> • | dgmbmgr: Diameter Gmb Application Manager logging facility

> • | dhcp: Dynamic Host Configuration Protocol logging facility

> • | dhcpv6: DHCPv6

> • | dhost: Distributed Host logging facility

> • | diabase: Diabase messages facility

> • | diameter: Diameter endpoint logging facility

> • | diameter-acct: Diameter Accounting

> • | diameter-auth: Diameter Authentication

> • | diameter-dns: Diameter DNS subsystem

> • | diameter-ecs: ACS Diameter signaling facility

> • | diameter-hdd: Diameter HDD Interface facility

> • | diameter-svc: Diameter Service

> • | diamproxy: DiamProxy logging facility

> • | dpath: IPSEC Data Path facility

> • | drvctrl: Driver Controller facility

> • | eap-ipsec: EAP

> • | eap-sta-s6a-s13-s6b-diameter: EAP/STA/S6A/S13/S6B Diameter messages facility

> • | ecs-css: ACSMGR <-> Session Manager Signalling Interface facility

> • | egtpc: eGTP-C logging facility

> • | egtpmgr: eGTP manager logging facility

> • | egtpu: eGTP-U logging facility

> • | epdg: ePDG logging facility

> • | evlog: Event log facility

> • | famgr: Foreign Agent manager logging facility

> • | firewall: Firewall logging facility

> • | fng: FNG logging facility

> • | gmm:

> • | For 2.5G: Logs the GPRS Mobility Management (GMM) layer (above LLC layer)

> • | For 3G: Logs the access aplication layer (above the RANAP layer)

> • | gprs-app: GPRS Application logging facility

> • | gprs-ns: GPRS Network Service Protocol (layer between SGSN and the BSS) logging facility

> • | gq-rx-tx-diameter: Gq/Rx/Tx Diameter messages facility

> • | gss-gcdr: GTPP Storage Server GCDR facility

> • | gtpc: GTP-C protocol logging facility

> • | gtpcmgr: GTP-C protocol Manager logging facility

> • | gtpp: GTP-PRIME protocol logging facility

> • | gtpu: GTP-U protocol logging facility

> • | gtpumgr: GTPU Demux manager

> • | gx-ty-diameter: Gx/Ty Diameter messages facility

> • | gy-diameter: Gy Diameter messages facility

> • | hamgr: Home Agent manager logging facility

> • | hat: High Availability Task (HAT) process facility

> • | hdctrl: HD Controller logging facility

> • | hnb-gw: HNB-GW (3G Femto GW) logging facility

> • | hnbmgr: HNBMGR (3G Femto GW DemuxMgr) logging facility

> • | hss-peer-service: HSS Peer Service facility

> • | igmp: IGMP

> • | ikev2: IKEv2

> • | ims-authorizatn: IMS Authorization Service facility

> • | ims-sh: HSS SH Service facility

> • | imsimgr: SGSN IMSI Manager facility

> • | imsue: IMSUE

> • | ip-arp: IP Address Resolution Protocol facility

> • | ip-interface: IP interface facility

> • | ip-route: IP route facility

> • | ipms: IPMS logging facility

> • | ipsec: IP Security logging facility

> • | ipsg: IP Service Gateway interface logging facility

> • | ipsgmgr: IP Services Gateway facility

> • | ipsp: IP Pool Sharing Protocol logging facility

> • | kvstore: KV Store facility

> • | l2tp-control: L2TP control logging facility

> • | l2tp-data: L2TP data logging facility

> • | l2tpdemux: L2TP Demux Manager logging facility

> • | l2tpmgr: L2TP Manager logging facility

> • | lagmgr: LAGMGR logging facility

> • | ldap: Lightweight Directory Access Protocol (LDAP) messages logging facility

> • | li: Refer to the ASR 5000 Lawful Intercept Interface Reference for a description of this command.

> • | linkmgr: SGSN/BSS SS7 Link Manager logging facility (2.5G only)

> • | llc: Logical Link Control (LLC) Protocol logging facility; for SGSN: logs the LLC layer between the GMM and the BSSGP layers for logical links between the MS and the SGSN

> • | local-policy: Local Policy Service facility

> • | m3ua: M3UA Protocol logging facility

> • | magmgr: Mobile Access Gateway manager logging facility

> • | map: MAP Protocol logging facility

> • | megadiammgr: Megadiameter Manager (SLF Service) logging facility

> • | mme-app: Mobility Management Entity Application logging facility

> • | mme-misc: MME miscellaneous logging facility

> • | mmedemux: Mobility Management Entity Demux Manager logging facility

> • | mmemgr: MME Manager facility

> • | mmgr: Master Manager logging facility

> • | mobile-ip: Mobile IP processes

> • | mobile-ip-data: Mobile IP data facility

> • | mobile-ipv6: Mobile IPv6 logging facility

> • | mpls: MPLS protocol logging facility

> • | mseg-app: MSEG application logging facility

> • | mseg-gtpc: MSEG GTPC application logging facility

> • | mseg-gtpu: MSEG GTPU application logging facility

> • | msegmgr: MSEGMgr (MSEG DemuxMgr) logging facility

> • | mtp2: MTP2 Service logging facility

> • | mtp3: MTP3 Protocol logging facility

> • | multicast-proxy: Multicast Proxy logging facility

> • | npuctrl: Network Processor Unit Control facility

> • | npumgr: Network Processor Unit Manager facility

> • | npumgr-acl: NPUMGR ACL logging facility

> • | npumgr-flow: NPUMGR FLOW logging facility

> • | npumgr-fwd: NPUMGR FWD logging facility

> • | npumgr-init: NPUMGR INIT logging facility

> • | npumgr-port: NPUMGR PORT logging facility

> • | npumgr-recovery: NPUMGR RECOVERY logging facility

> • | ntfy-intf: Notification Interface logging facility

> • | orbs: Object Request Broker System logging facility

> • | ospf: OSPF protocol logging facility

> • | ospfv3: OSPFv3 protocol logging facility

> • | p2p: Peer-to-Peer Detection logging facility

> • | pccmgr: IPCF PCC Manager library

> • | pdg: PDG logging facility

> • | pdgdmgr: PDG Demux Manager logging facility

> • | pdif: PDIF logging facility

> • | pgw: PDN Gateway logging facility

> • | phs: Payload Header Suppression

> • | phs-control: PHS X1/X5 and X2/X6 Interface logging facility

> • | phs-data: PHS Data logging facility

> • | phs-eapol: PHS EAPOL logging facility

> • | phsgwmgr: PHS Gateway Manager facility

> • | phspcmgr: PHS Paging Controller Manager facility

> • | pmm-app: PMM application logging facility

> • | ppp: PPP link and packet facilities

> • | pppoe: PPPOE logging facility

> • | push: VPNMGR CDR push logging facility

> • | radius-acct: RADIUS accounting logging facility

> • | radius-auth: RADIUS authentication logging facility

> • | radius-coa: RADIUS change of authorization and radius disconnect

> • | ranap:Radio Access Network Application Part (RANAP) Protocol facility logging info flow between SGSN and RNS (3G)

> • | rct: Recovery Control Task logging facility

> • | rdt: Redirect Task logging facility

> • | resmgr: Resource Manager logging facility

> • | rf-diameter: Rf Diameter messages facility

> • | rip: RIP logging facility (RIP is not supported at this time.)

> • | rohc: RObust Header Compression facility

> • | rsvp: Reservation Protocol logging facility

> • | rua: RUA (3G Femto GW - RUA messages) logging facility

> • | s1ap: S1AP Protocol logging facility

> • | sccp: SCCP Protocol logging connection-oriented messages between RANAP and TCAP layers.

> • | sct: Shared Configuration Task logging facility

> • | sctp: SCTP Protocol logging facility

> • | sessctrl: Session Controller logging facility

> • | sessmgr: Session Manager logging facility

> • | sesstrc: session trace logging facility

> • | sft: Switch Fabric Task logging facility

> • | sgs: SGs protocol logging facility

> • | sgsn-app: SGSN-APP logging various SGSN ‘glue’ interfaces, e.g., between PMM, MAP,. GPRS-FSM, SMS.

> • | sgsn-failures: SGSN call failures (attach/activate rejects) logging facility (2.5G)

> • | sgsn-gtpc: SGSN GTP-C Protocol logging control messages between the SGSN and the GGSN

> • | sgsn-gtpu: SGSN GTP-U Protocol logging user data messages between the SGSN and GGSN

> • | sgsn-mbms-bearer:SGSN MBMS Bearer app (SMGR) logging facility

> • | sgsn-misc: Used by stach manager to log binding and removing between layers

> • | sgsn-system: SGSNs System Components logging facility; used infrequently

> • | sgsn-test: SGSN Tests logging facility; used infrequently

> • | sgtpcmgr: SGSN GTPC Manager logging information exchange through SGTPC and the GGSN

> • | sgw: Serving Gateway facility

> • | sh-diameter: Sh Diameter messages facility

> • | sitmain: System Initialization Task main logging facility

> • | sm-app: SM Protocol logging facility

> • | sms: Short Message Service (SMS) logging messages between the MS and the SMSC

> • | sndcp: SNDCP Protocol logging facility

> • | snmp: SNMP logging facility

> • | sprmgr: IPCF SPR Manager logging facility

> • | srdb: Static Rating Database

> • | srp: Service Redundancy Protocol (SRP) logging facility

> • | sscfnni: SSCFNNI Protocol logging facility

> • | sscop: SSCOP Protocol logging facility

> • | ssh-ipsec: SSH IP Security logging facility

> • | ssl: SSL (Secure socket layer messages) logging facility

> • | stat:: Statistics logging facility

> • | system: System logging facility

> • | tacacsplus: TACACS+ Protocol logging facility

> • | tcap: TCAP Protocol logging facility

> • | testctrl: Test Controller logging facility

> • | testmgr: Test Manager logging facility

> • | threshold: threshold logging facility

> • | ttg: TTG logging facility

> • | tucl: TUCL logging facility

> • | udr: User detail record facility (used with the Charging Service)

> • | user-data: User data logging facility

> • | user-l3tunnel: User layer-3 tunnel logging facility

> • | usertcp-stack: User Tcp Stack

> • | vpn: Virtual Private Network logging facility

> • | wimax-data: WiMAX DATA

> • | wimax-r6: WiMAX R6

> level severity_level
> Specifies the level of information to be logged from the following list which is ordered from highest to lowest:

> • | critical - display critical events

> • | error - display error events and all events with a higher severity level

> • | warning - display warning events and all events with a higher severity level

> • | unusual - display unusual events and all events with a higher severity level

> • | info - display info events and all events with a higher severity level

> • | trace - display trace events and all events with a higher severity level

> • | debug - display all events

> critical-info | no-critical-info
> Default: critical-info enabled.
> critical-info: specifies that events with a category attribute of critical information are to be displayed. Examples of these types of events can be seen at bootup when system processes and tasks are being initiated.
> no-critical-info: specifies that events with a category attribute of critical information are not to be displayed.
> Usage
> Apply filters for logged data to collect only that data which is of interest.
> Important: A maximum of 50,000 events may be stored in each log. Enabling more events for logging may cause the log to be filled in a much shorter time period. This may reduce the effectiveness of the log data as a shorter time period of event data may make troubleshooting more difficult.
> Important: Once a log has reached the 50,000 event limit the oldest events will be discarded as new log entries are created.
> Caution: Issuing this command could negatively impact system performance depending on the amount of system activity at the time of execution and/or the type of facility(ies) being logged.
> Example
> The following are selected examples used to illustrate the various options. Not all facilities will be explicitly shown as each follows the same syntax for options.
> The following sets the level to log only warning information for all facilities.
> logging filter active facility all level warning
> The following enables the logging of critical information for the SNMP facility while setting the level to error.
> logging filter active facility snmp level error critical-info
> logging trace
> Enables/disables the logging of trace information for specific calls, mobiles, or network addresses.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> logging trace { callid call_id | ipaddr ip_address | msid ms_id | username user_name }
> no logging trace { callid call_id | ipaddr ip_address | msid ms_id | username user_name }
> no
> Indicates the logging of trace information is to be disabled.
> callid call_id | ipaddr ip_address | msid ms_id | username user_name
> callid call_id: specifies the exact call instance ID which is to have trace data logged. call_id is specified as a 4-byte hexadecimal number.
> ipaddr ip_address: specifies the IP address for which trace information is to be logged. ip_address must be specified using the standard IPv4 dotted decimal notation.
> msid ms_id: specifies the mobile subscriber ID for which trace information is to be logged. ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> username user_name: specifies a user who is to have trace information logged. user_name must refer to a previously configured user.
> Usage
> A trace log is useful in troubleshooting subscriber problems as well as for system verification by using a test subscriber. The no keyword is used to stop the logging of trace information.
> Important: A maximum of 50,000 events may be stored in each log. Enabling more events for logging may cause the log to be filled in a much shorter time period. This may reduce the effectiveness of the log data as a shorter time period of event data may make troubleshooting more difficult.
> Important: Once a log has reached the 50,000 event limit the oldest events will be discarded as new log entries are created.
> Caution: Issuing this command could negatively impact system performance depending on the number of subscribers connected and the amount of data being passed.
> Example
> The following commands enables/disables trace information for user user1.
> logging trace username user1 no logging trace username user1
> The following commands will enable/disable trace information logging for the user assigned IP address 1.2.3.4.
> logging trace ipaddr 1.2.3.4 no logging trace ipaddr 1.2.3.4
> The following enables/disables logging of trace information for call ID FE80AA12.
> logging trace callid fe80aa12 no logging trace callid fe80aa12
> logs checkpoint
> Performs check pointing operations on log data. Check pointing identifies logged data as previously viewed or marked. Check pointing results in only the log information since the last check point being displayed; check pointed log data is not available for viewing.
> Individual logs may have up to 50,000 events in the active log. Check pointing the logs will then result in at most 50,000 events being in the inactive log files. This gives a maximum of 100,000 events in total which are available for each facility logged.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> logs checkpoint
> Usage
> Check point log data to a set the log contents to a well know point prior to special activities taking place. This command may also be a part of periodic regular maintenance to manage log data.
> The check pointing of logs moves the current log data to the inactive logs. Only the most recently check pointed data is retained in the inactive logs. A subsequent check pointing of the logs will result in the prior check pointed inactive log data being cleared and replaced with the newly check pointed data.
> The check pointing of log data moves the active log data to be retained as the inactive log data. This results in the active log data, if displayed, having no data earlier than the point in time when the check pointing occurred.
> Important: Check pointing of logs should be done periodically to avoid the logs becoming full. Logs which have 50,000 events logged will discard the oldest events first when new events are to be logged.
> Example
> logs checkpoint
> lsp-ping
> Checks Multi Protocol Label Switching (MPLS) label switch path (LSP) connectivity for the specified forwarding equivalence class (FEC). It must be followed by an IPv4 FEC prefix.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> lsp-ping ip_prefix_FEC [ count ping_packets ] [ | verbose ] [ | grep grep_options ]
> ip_prefix_FEC
> is an IPv4 prefix FEC with or without mask represented as ##.##.##.## or ##.##.##.##/x, where x is mask value.
> count
> sets the number of ping packets to be sent. ping_packets is an integer value that ranges from 1 to 16. The default value for the number of ping packets is 4.
> Important: The timeout interval for the packets is 5 seconds by default.
> verbose
> sets the verbose (detailed) output mode.
> grep grep_options
> indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Usage
> This command is used to verify the MPLS LSP connectivity for the specified FEC.
> Example
> Following are the examples for using this command with all possible options for IPv4 address 13.13.13.1 and mask 32:
> lsp-ping 13.13.13.1/32
> lsp-ping 13.13.13.1/32 count 15
> lsp-ping 13.13.13.1/32 verbose
> lsp-traceroute
> Discovers MPLS LSP routes that packets actually take when traveling to their destinations. It must be followed by an IPv4 FEC prefix.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> lsp-traceroute ip_prefix_FEC [ maxttl time_to_live ] [ | verbose ] [ | grep grep_options ]
> ip_prefix_FEC
> specifies the destination IPv4 address in decimal notation with or without mask. Without mask it is represented as ##.##.##.##, while with mask it is #.##.##.##/x where x is the mask value.
> maxttl
> sets the maximum time to live in hops. time_to_live is an integer value that ranges from 1 to 255. The default value for maxttl is 30.
> verbose
> sets the verbose (detailed) output mode.
> grep grep_options
> indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Usage
> This command is used or the router to discover the MPLS LSP routes through which the packets will travel to their IPv4 destinations.
> Example
> The following example specifies the destination IP address 13.13.13.13 for which the MPLS routes will be discovered for packets to traverse:
> lsp-traceroute 13.13.13.13/32
> mkdir
> Creates a new directory in the local file system or in remote locations as specified.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> mkdir filepath
> filepath
> Specifies the directory path to create. The path must be formatted as follows:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [file: ] { /flash | /pcmcia1 | /hd } [ /directory ]/file_name

> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name
> filename is the actual file of interest
> Usage
> Create new directories as part of periodic maintenance activities to better organize stored files.
> Example
> The following creates the directory /flash/pub in the local flash storage.
> mkdir /flash/pub
> mme offload
> Initiates or stops the offload of UEs associated with a specified MME service.
> Product
> MME
> Privilege
> Inspector
> Syntax
> mme offload mme-service name { start mme-init-release-timeout seconds paging-init-timeout seconds | stop }
> mme-service name
> Specifies the name of the MME service from which UEs will be offloaded. name must be an existing MME service and be from 1 to 63 alphanumeric characters.
> start mme-init-release-timeout seconds paging-init-timeout seconds | stop } [ -noconfirm ]
> Sets the timeout for the initial release procedure and the paging procedure.
> start mme-init-release-timeout seconds: Configures the timeout for triggering the IDLE MODE ENTRY procedure for UEs that are in the ECM_CONNECTED state. The cause of the IDLE MODE ENTRY will be “Load balancing TAU required”. seconds must be an integer value from 1 to 120.
> paging-init-timeout seconds: Configures the timeout for triggering the PAGING procedure for UEs in the ECM_IDLE state. seconds must be an integer value from 1 to 120.
> After returning the UEs to the ECM_CONNECTED state, the IDLE MODE ENTRY procedure is triggered with the “Load balancing TAU required” cause.
> stop: Ends the offload process.
> -noconfirm
> Execute the command without any additional prompts or confirmation from the user.
> Usage
> Use this command to initiate or stop the offloading of UEs associated with a specified MME service.
> Example
> The following command sets the trigger to start offloading UEs from a service named mme3 at 60 seconds and the paging trigger at 90 seconds:
> mme offload mme-service mme3 start mme-init-release-timeout 60 paging-init-timeout 90
> mme reset
> Sends an S1 RESET message to a designated EnodeB to reset all UE-associated S1 connections.
> Product
> MME
> Privilege
> Inspector
> Syntax
> mme reset s1-peer peer_ID
> s1-peer peer-ID
> Specifies the EnodeB peer ID to which the REST message is to be sent. peer_ID must be an existing EnodeB peer ID and be an integer value from 1 to 4294967295.
> Usage
> Use this command to send an S1 RESET message to a designated EnodeB to reset all UE-associated S1 connections.
> The S1 peer ID for an EnodeB can be identified by executing the show mme-service enodeb-association command available in this mode. The peer ID is presented in the “Peerid” field.
> Example
> The following command initiates the sending of an S1-peer reset message to an EnodeB with a peer ID of 22315734:
> mme rest s1-peer 22315734
> monitor protocol
> Enters the system’s protocol monitoring utility.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> monitor protocol
> Usage
> Useful for troubleshooting, this command provides a tool for monitoring protocol transactions between the system and other network nodes including the mobile station(s).
> The following protocols can be monitored:

> • | SNMP

> • | RADIUS Authentication

> • | RADIUS Accounting

> • | A11 (R-P Interface) (PDSN only)

> • | Mobile IPv4

> • | A11MGR

> • | PPP

> • | A10

> • | User L3 (User Layer 3 protocols)

> • | USERTCP STACK

> • | L2TP

> • | L2TPMGR

> • | L2TP Data

> • | GTPC

> • | GTPCMGR

> • | GTPU

> • | GTPP

> Important: If the hard disk drive (HDD) is used for CDR storage, the CDR option must be used and not GTPP option (27).

> • | DHCP (GGSN only)

> • | CDR

> • | DHCPV6

> • | RADIUS COA

> • | MIP Tunnel

> • | L3 Tunnel (Layer 3 Tunnel Protocols)

> • | CSS Data

> • | CSS Signaling

> Important: In StarOS 9.0 and later releases the CSS Data Signaling option is not supported.

> • | EC Diameter (Diameter Enhanced Charging)

> • | SIP (IMS)

> • | IPSec IKE Inter-Node

> • | IPSec IKE Subscriber

> • | IPSG RADIUS Signal

> • | ROHC (Robust Header Compression)

> • | WiMAX R6

> • | WiMAX Data

> • | SRP

> • | BCMCS SERV AUTH

> • | RSVP

> • | Mobile IPv6

> • | ASNGWMGR

> • | STUN

> • | SCTP: Enabling this option will display the SCTP protocol message packets on HNB-GW node.

> • | M3UA

> • | SCCP

> • | TCAP

> • | MAP

> • | RANAP

> • | GMM

> • | GPRS-NS

> • | BSSGP

> • | CAP

> • | SSCOP

> • | SSCFNNI

> • | MTP3

> • | LLC

> • | SNDCP

> • | BSSAP+

> • | SMS

> • | PHS (Payload Header Compression)

> • | PHS-Data

> • | DNS Client

> • | MTP2

> • | HNBAP: Enabling this option will display the HNB Application Part (HNBAP) protocol packets.

> • | RUA: Enabling this option will display the RANAP User Adaptation (RUA) protocol packets.

> • | EGTPC

> • | App Specific Diameter

> • | PHS-EAPOL

> • | ICAP

> • | Micro-Tunnel

> • | ALCAP: Enabling this option will display the Access Link Control Application Part (ALCAP) protocol message packets on HNB-GW node.

> • | SSL

> • | S1-AP

> • | NAS

> • | LDAP

> • | SGS

> • | AAL2: Enabling this option will display the ATM Adaptation Layer 2 (AAL2) protocol message packets on HNB-GW node.

> • | PHS (Payload Header Suppression)

> • | PPPOE

> • | RTP (IMS)

> • | RTCP (IMS)

> Once the protocol has been selected, the utility monitors and displays every relative protocol message transaction.
> Protocol monitoring is performed on a context-by-context-basis. Therefore, the messages displayed are only those that are transmitted/received within the system context from which the utility was executed.
> Caution: Protocol monitoring can be intrusive to subscriber sessions and could impact system performance. Therefore, it should only be used as a troubleshooting tool.
> Example
> The following command opens the protocol monitoring utility:
> monitor protocol
> monitor subscriber
> Enables the system’s subscriber monitoring utility.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> monitor subscriber [ asn-peer-address bs_peer_address | callid call_id fng-peer-address ipv4_address | imsi imsi_value | ipaddr ip_address | ipv6addr ipv6_address | ipsg-peer-address ipsg_peer_address | msid ms_id | msisdn msisdn | next-call | pcf pcf_address | pdif-peer-address pdif_peer_address | peer-fa peer_fa_address | peer-lac lac_peer_address | sgsn-address sgsn_address | type { 1xrtt | asngw | asnpc | closedrp | evdorev0 | evdoreva | interrogating-cscf | ggsn [ Next-Call By APN ] | ha | ipsg | lns | mme | pdif | proxy-cscf | rfc3261-proxy | serving-cscf } next-call | type bcmcs { next-call | next-service-request } | username user_name| Next-Call By APN ]
> asn-peer-address bs_peer_address
> Specifies the peer ASN Base Station IP address. Must be followed by IPv4 address in dotted decimal notation.
> callid call_id
> Specifies the call identification number assigned to the subscriber session by the system to be monitored.
> call_id is specified as a 4-byte hexadecimal number.
> fng-peer-address ipv4_address
> The specific FNG WLAN IP address.
> ipv4_address must be entered in standard IPv4 notation.
> imsi imsi_value
> Specifies the International Mobile Subscriber Identity (IMSI) of the subscriber session to be monitored.
> imsi_value is an integer value from 1 to 15 characters.
> ipaddr ip_address
> Specifies the IP address of the subscriber session to be monitored.
> ip_address must be specified using dotted decimal notation.
> ipv6addr ipv6_address
> Specifies the IPv6 address of the subscriber session to be monitored.
> ipv6_address must be an IPv6 IP address entered using colon ( : ) separated notation.
> ipsg-peer-address ipsg_peer_address
> Specifies the peer IPSG IP address. Must be followed by IPv4 address in dotted decimal notation.
> msid ms_id
> Specifies the mobile subscriber identification number to be monitored.
> ms_id must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> msisdn msisdn
> Specifies the Mobile Subscriber ISDN number to be monitored.
> msisdn must be from 7 to 16 digits specified as an IMSI, MIN, or RMI.
> next-call
> Specifies that the system will monitor the next incoming subscriber session.
> Entering this keyword will display the available options of protocols to select. For list of supported protocols with this keyword, refer monitor protocol command.
> pcf pcf_address
> Specifies the PCF IP address. Must be followed by IPv4 address in dotted decimal notation.
> pdif-peer-address pdif_peer_address
> Specifies the peer PDIF IP address. Must be followed by IPv4 address in dotted decimal notation.
> peer-fa peer_fa_address
> Specifies the peer FA IP address. Must be followed by IPv4 address in dotted decimal notation.
> peer-lac lac_peer_address
> Specifies the peer LAC IP address. Must be followed by IPv4 address in dotted decimal notation.
> sgsn-address sgsn_address
> Specifies the SGSN IP address. Must be followed by IPv4 address in dotted decimal notation.
> type { 1xrtt | asngw | asnpc | evdorev0 | evdoreva | | fng | interrogating-cscf | ggsn [ Next-Call By APN ] | ha | ipsg | lns | mme | openrp | | pdif | proxy-cscf | rfc3261-proxy | serving-cscf } next-call
> Allows monitoring for specific subscriber types established in the system when next call occurs.

> • | 1xrtt: Displays logs for cdma2000 1xRTT call session subscriber

> • | asngw: Displays logs for ASN GW call session subscriber

> • | asnpc: Displays logs for ASN PC/LR call session subscriber

> • | evdorev0: Displays logs for cdma2000 EVDO Rev0 call session subscriber

> • | evdoreva: Displays logs for cdma2000 EVDO RevA call session subscriber

> • | fng: Displays logs for the FNG session subscriber

> • | interrogating-cscf: Displays logs for Interrogating CSCF subscriber

> • | ggsn: Displays logs for UMTS GGSN call session subscriber

> • | Next-Call By APN: Display logs for next call on APN basis, where APN name can be any Gi or Gn APN.

> • | ha: Displays logs for Home Agent call session subscriber

> • | ipsg: Displays logs for IPSG call session subscriber

> • | lns: Displays logs for LNS call session subscriber

> • | mme: Displays logs for MME session subscribers.

> • | openrp: Displays logs for OpenRP subscriber

> • | pdif: Displays logs for PDIF call session subscriber

> • | proxy-cscf: Displays logs for Proxy CSCF subscriber

> • | rfc3261-proxy-cscf: Displays logs for non-ims-proxy (RFC-3261 proxy) subscriber

> • | serving-cscf: Displays logs for Serving CSCF subscriber

> type bcmcs {next-call | next-service-request}
> Specifies the type of BCMCS call for the subscriber.
> username user_name
> Specifies the username of the subscriber to be monitored.
> user_name refers to a previously configured user.
> Usage
> The monitor subscriber utility provides a useful tool for monitoring information about and the activity of either a single subscriber or all subscribers with active sessions within a given context.
> The following items can be monitored:

> • | Control events

> • | Data events

> • | Event ID information

> • | Inbound events

> • | Outbound events

> • | Protocols (identical to those monitored by command)

> Once the criteria has been selected, the utility will monitor and display every relative piece of information on the subscriber(s).
> Important: Option Y for performing multi-call traces is only supported for use with the GGSN. This option is available when monitoring is performed using the “Next-Call” option. It allows you monitor up to 11 primary PDP contexts for a single subscriber.
> Subscriber monitoring is performed on a context-by-context-basis. Therefore, the information displayed will be only that which is collected within the system context from which the utility was executed.
> Caution: Subscriber monitoring can be intrusive to subscriber sessions and could impact system performance. Therefore, it should only be used as a troubleshooting tool.
> Example
> The following command enables monitoring for user user1.
> monitor subscriber username user1
> The following command will enable monitoring for the user assigned IP address 1.2.3.4.
> monitor subscriber ip-address 1.2.3.4
> The following enables monitoring for call ID FE80AA12.
> monitor subscriber callid fe80aa12
> newcall policy
> This command configures new call policies for busy-out conditions.
> Product
> PDSN, GGSN,, HNB-GW, IPCF, MME, HA, LNS, P-CSCF, ASN GW, ASN PC/LR, SGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> newcall policy { asngw-service | asnpc-service | sgsn-service } { all | name service_name } reject
> newcall policy cscf-service { all | name service_name } { redirect target_ip_address [ weight weight_num ] [ target_ipaddress2 [ weight weight_num ] ... target_ip_address16 [ weight weight_num ] | reject }
> newcall policy { fa-service | lns-service | mipv6ha-service } { all | name service_name } reject
> newcall policy { ha-service | pdsn-service} { all | name service_name } { redirect target_ip_address [ weight weight_num ] [ target_ipaddress2 [ weight weight_num ] ... target_ip_address16 [ weight weight_num ] | reject }
> newcall policy ggsn-service {apn name apn_name | all | name service_name}reject
> newcall policy hnbgw-service {all | name service_name}reject
> newcall policy {pcc-af-service | pcc-policy-service} {all | name service_name}reject
> newcall policy mme-service {all | name service_name } reject
> no newcall policy { fa-service | ggsn-service | ha-service | mipv6ha-service | pdsn-service| pdsnclosedrp-service| lns-service } { all | name service_name }
> no newcall policy { ha-service | pdsn-service } { all | name service_name } redirect target_ip_address [ weight weight_num ] [ target_ip_address2 [ weight weight_num ] ... target_ip_address16 [ weight weight_num ]
> no newcall policy ggsn-service { apn apn_name | all | name service_name} reject
> no newcall policy { asngw-service | asnpc-service } { all | name service_name }
> no newcall policy hnbgw-service {all | name service_name}
> no newcall policy mme-service { all | name service_name }
> no newcall policy {pcc-af-service | pcc-policy-service} {all | name service_name}
> no
> Disables the new call policy for all or specified service of a service type.
> newcall policy { asngw-service | asnpc-service } { all | name service_name } reject
> Creates a new call policy to reject the calls based on the specified ASN GW or ASN PC/LR service name or all services of this type.
> asngw-service: Specifies the type of service as ASN GW for which new call policy is configured.
> asnpc-service: Specifies the type of service as ASN PC/LR for which new call policy is configured.
> name service_name: Specifies the name of the service for which new call policy is configured. service_name is name of a configured ASN GW or ASN PC/LR service.
> reject: Specifies that the policy rejects new incoming calls. Depending on the type of service that the policy is applied to, the reason codes are reported as part of the reply to indicate the rejection. For ASN GW and ASN PC/LR service rejection code is 81H (Registration Denied - administratively prohibited).
> newcall policy { cscf-service | fa-service | lns-service | mipv6ha-service } { all | name service_name } reject
> Creates a new call policy that rejects calls based on the specified access point name.
> no newcall policy { cscf-service | fa-service | ggsn-service| ha-service | mipv6ha-service | pdsn-service | } { all | name service_name }
> Removes a previously configured new call policy for the specified service
> no newcall policy { ha-service | pdsn-service } { all | name service_name } redirect target_ip_address [ weight weight_num ] [ target_ip_address2 [ weight weight_num ] ... target_ip_address16 [ weight weight_num ]
> Deletes up to 16 IP addresses from the redirect policy. The IP addresses must be expressed in IP v4 dotted decimal notation
> cscf-service | fa-service | ha-service | lns-service | mipv6ha-service | mme-service | pdsn-service | pdsnclosedrp-service
> Specifies the type of service for which to configure a new call policy. The following services are supported:

> • | cscf-service: A Call/Session Control Function service

> • | fa-service: A Foreign Agent service

> • | ha-service: A Home Agent service

> • | lns-service: An L2TP Network Server service

> • | mipv6ha-service: A Mobile IPv6 Home Agent service

> • | pdsn-service: A Packet Data Serving Node service

> { all | name service_name }
> Specifies a filter for the new call policy. Whether the new call policy will be applied to all configured services or a specific one.

> • | all: Specifies that the new call policy will be applied to all instances of the selected service type.

> • | name: service_name: Specifies the name of a specific instance of the selected service type. service_name can be between 1 and 63 alphanumeric characters and is case sensitive.

> redirect target_ip_address [ weight weight_num ] [ target_ip_address2 [ weight weight_num ] ... target_ip_address16 [ weight weight_num ]
> Configures the busy-out action. When a redirect policy is invoked, the service rejects new sessions and provides the IP address of an alternate destination. This command can be issued multiple times.
> address: The IP address of an alternate destination expressed in IP v4 dotted decimal notation. Up to 16 IP addresses can be specified either in one command or by issuing the redirect command multiple times. If you try to add more than 16 IP addresses to the redirect policy the CLI issues an error message. If you specify an IP address and weight that already exists in the redirect policy the new values override the existing values.
> weight weight_num: When multiple addresses are specified, they are selected in a weighted round-robin scheme. Entries with higher weights are more likely to be chosen. If a weight is not specified the entry is automatically assigned a weight of 1. weight_num must be an integer from 1 through 10.
> Depending on the type of service that the policy is applied to, the following reason codes are reported as part of the reply:

> • | ha service: 88H (Registration Denied - unknown home agent address)

> • | pdsn service: 88H (Registration Denied - unknown PDSN address)

> Important: The redirect option is not supported for use with FA and GGSN services.
> newcall policy hnbgw-service { all | name service_name} reject
> Creates a new call policy to reject the calls in specified HNB-GW service name instance or all HNB-GW services on the system.
> name service_name: Specifies the name of the HNB-GW service for which new call policy is configured. service_name is name of a configured HNB-GW service.
> reject: Specifies that the policy rejects all new incoming calls. Depending on the type of service that the policy is applied to, the reason codes are reported as part of the reply to indicate the rejection. For HNB-GW service rejection code is 81H (Registration Denied - administratively prohibited).
> newcall policy mme-service { all | name service_name } reject
> Creates a new call policy to reject the calls based on the specified MME service name or all MME services on the system.
> name service_name: Specifies the name of the MME service for which new call policy is configured. service_name is name of a configured MME service.
> reject: Specifies that the policy rejects new incoming calls. Depending on the type of service that the policy is applied to, the reason codes are reported as part of the reply to indicate the rejection. For MME service rejection code is 81H (Registration Denied - administratively prohibited).
> newcall policy {pcc-af-service | pcc-policy-service} {all | name service_name}reject
> Creates a new call policy to reject the calls for PCC services on the system. newcall policy can be configured for following PCC services:

> • | pcc-af-service name service_name: Specifies the Policy and Charging Control-Application Function (PCC-AF) service for which new call policy is to be configure on the system.

> name service_name: Specifies the name of the PCC-AF service for which new call policy is configured. service_name is name of a configured PCC-AF service.

> • | pcc-policy-service name service_name: Specifies the Policy and Charging Control-Policy (PCC-Policy) service for which new call policy is to be configure on the system.

> name service_name: Specifies the name of the PCC-Policy service for which new call policy is configured. service_name is name of a configured PCC-Policy service.
> reject: Specifies that the policy rejects new incoming calls. Depending on the type of service that the policy is applied to, the reason codes are reported as part of the reply to indicate the rejection. For PCC services rejection code is 81H (Registration Denied - administratively prohibited).
> reject
> Specifies that the policy rejects new incoming calls. Depending on the type of service that the policy is applied to, the following reason codes are reported as part of the reply to indicate the rejection:

> • | asngw service: 81H (Registration Denied - administratively prohibited)

> • | fa service: 41H (administratively prohibited)

> Important: When newcall policy is set to reject for the FA service, the Busy Bit is set in the Agent Advertisement. Any further RRQs will be rejected with this code value.

> • | ggsn service: C7H (Rejected - no resources available)

> • | ha service: 81H (Registration Denied - administratively prohibited)

> • | mipv6ha-service: 81H (Registration Denied - administratively prohibited)

> • | mme service: 81H (Registration Denied - administratively prohibited)

> • | pdsn service: 81H (Registration Denied - administratively prohibited)

> Usage
> This command is used to busy-out specific system services prior to planned maintenance or for troubleshooting. This is required when operator find out that the system is somehow overloaded, or needs some kind of maintenances or so.
> Example
> The following command creates a new call policy to re-direct all new calls for all PDSN services to a device having an IP address of 192.168.1.23:
> newcall policy pdsn-service all redirect 192.168.1.23
> The following command creates a new call policy to reject all new calls for a GGSN service called ggsn1:
> newcall policy ggsn-service name ggsn1 reject
> The following command creates a new call policy to reject all new calls for an MME service called MME1:
> newcall policy mme-service name MME1 reject
> The following command creates a new call policy to reject all new calls for an HNB-GW service called hnbgw1:
> newcall policy hnbgw-service name hnbgw1 reject
> The following command creates a new call policy to reject all new calls for a PCC Policy service called pcrf1:
> newcall policy pcc-policy-service name pcrf1 reject
> password change
> Provides a mechanism for local-user administrative users to change their passwords.
> Product
> All
> Privilege
> All local-user administrative levels except as noted below
> Syntax
> password change [ local-user name ]
> local-user name
> Specifies the name of the local-user administrative user for which to change the password.
> name can be from 3 to 16 alphanumeric characters in length and is case sensitive.
> Important: This keyword is only available to local-users with an authorization level of security-administrator.
> Usage
> This command provides a mechanism for local-user administrative users to change their passwords. In addition, it also provides a mechanism for security-administrator local-users to change the password for other local-user accounts.
> If the local-user keyword is not entered, the system prompts the user for their current password and for the new password. New passwords take effect at the next login. Users that have had their password changed by a security-administrator are prompted to change their passwords at their next login.
> New passwords must meet the criteria dictated by the local-user password command options in the Global Configuration Mode.
> Important: The system does not allow the changing of passwords unless the time limit specified by the local-user password min-change-interval has been reached.
> Example
> The following command, executed by a security-administrator, resets the password for a local-user name operator12:
> password change local-user operator12
> ping
> Verifies ability to communicate with a remote node in the network by passing data packets between and measuring the response. This is accomplished by sending Internet Control Message Protocol (ICMP) echo request packets to the target node (pinging) and waiting for an ICMP response.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Important: Inspector privileges are granted for all variables except count. To initiate a ping count, you must have a minimum privilege level of Operator.
> Syntax
> ping host_ip_address [ broadcast ] [ count num_packets ] [ pattern packet_pattern ] [ size octet_count ] [ src { src_host_name | src_host_ip_address } ] [ | { grep grep_options | more } ]
> host_ip_address
> Identifies the remote node to which the ability to communicate with is to be verified.
> host_ip_address: specifies the remote node using the node’s assigned IP address specified using the standard IPv4 dotted decimal notation.
> broadcast
> Sends ping packets to broadcast addresses.
> count num_packets
> Default: 5
> Specifies the number of packets to send to the remote host for verification. num_packets must be within the range 1 through 10000.
> pattern packet_pattern
> Default: each octet of the packet is encoded with the octet number of the packet.
> Specifies a pattern to use to fill the internet control message protocol packets with. packet_pattern must be specified in hexadecimal format with a value in the range hexadecimal 0x0000 through 0xFFFF. packet_pattern must begin with a ‘0x’ followed by up to 4 hexadecimal digits.
> size octet_count
> Default: 56
> Specifies the number of bytes each IP datagram. octet_count must be a value in the range 40 through 18432.
> src { src_host_name | src_host_ip_address }
> Default: originating system’s IP address
> Specifies an IP address to use in the packets as the source node.
> src_host_name: specifies the source node using the node’s logical host name which must be resolved via DNS lookup.
> src_host_ip_address: specifies the source node using the node’s assigned IP address specified using the standard IPv4 dotted decimal notation.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in Command Line Interface Reference.
> Usage
> This command is useful in verifying network routing and if a remote node is able to respond at the IP layer.
> Example
> The following command is the most basic and will report the results of trying to communication with remote node remoteABC.
> ping remoteABC
> The following will verify communication with the remote node 1.2.3.4 using 1000 packets.
> ping 1.2.3.4 count 1000
> The following verifies communication with remote node remoteABC while making it appears as though the source is remote node with IP address 1.2.3.4.
> ping remoteABC src 1.2.3.4
> Important: It is important to note that the responses from the remote host to the ping packets will be rerouted to the host specified as the source.
> ping6
> Ping options for IPv6 addresses
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> ping6 { hostname | ipv6 address } [ count num ] [ flood ] [ pattern val ] [ size val ] [ src val ] [ interface string ]
> hostname
> Name of the host to be pinged.
> ipv6 address
> IPv6 address of host to be pinged.
> count num
> Sets the number of ping packets to be sent. num must be an integer between 1 - 10,000.
> flood
> Configures ping6 to send packets as quickly as possible, or 100 per second, whichever is faster.
> pattern val
> Specifies hex pattern to fill ICMP packets. val is in the range 0x0 - 0ffff
> size val
> Size of ICMP datagram in bytes. val is an integer from 40 - 18432. Default is 56.
> src val
> Specifies the source IP address.
> interface string
> Specifies the originating source interface name.
> Usage
> Ping command for IPv6. Note that the command is just “ping6, and not “pingv6.”
> Example
> Use this command to ping the IPv6 address 2001:0db8:85a3:0000:0000:8a2e:0370:7334
> ping6 2001:0db8:85a3:0000:0000:8a2e:0370:7334
> port switch to
> Performs a manual switchover to an available redundant/standby line card or SPIO port.
> Default: none.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> port switch to slot# / port#
> slot#
> Identifies the physical chassis slot where the line card or SPIO card is installed.
> port#
> Identifies the physical port on the line card or SPIO to automatically switch to.
> Usage
> This command is used to specify the redundant port on a Line Card (LC). When port redundancy is enabled, if an external network device or cable failure occurs that causes a link down failure on the port, then the redundant port is used.
> Important: This command is not supported on all platforms.
> Example
> port switch to 17/1
> ppp echo-test
> This command sends link control protocol (LCP) keep-alive echo packet to the peer point-to-point protocol (PPP) connection to verify proper communication between PPP connections, and awaits a response.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> ppp echo-test { callid call_id | imsi imsi_id | ipaddr ip_address | msid ms_id | username user_name } [num_packets ] [ | { grep grep_options | more } ]
> callid call_id
> Specifies the call instance ID for which the PPP link must be verified.
> call_id is specified as a 4-byte hexadecimal number.
> imsi imsi_id
> Specifies the International Mobile Subscriber Identifier (IMSI) for which the PPP link must be verified.
> ipaddr ip_address
> Specifies the IP address for which the PPP link must be verified.
> ip_address must be specified using the standard IPv4 dotted decimal notation.
> msid ms_id
> Specifies the mobile subscriber ID for which the PPP link must be verified.
> ms_id must be from 7 to 16 digits specified as an MIN, or RMI.
> username user_name
> Specifies a user for which the PPP link must be verified.
> user_name must refer to a previously configured user.
> num_packets
> Default 1
> Specifies the number of test packets to generate.
> num_packets must be a value in the range from 1 through 1000000.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in Command Line Interface Reference.
> Usage
> Use this command to verify the point-to-point protocol communications. This command sends LCP keep-alive echo packet to the peer PPP connection to verify proper communication between PPP connections. ppp echo-test command waits for LCP echo response for configured numbers of tries, if response is not received it will retry configured no of times with an interval of 5 seconds. This command accepts the parameters call ID, IMSI, IP address, MSID, and user name to specify which active PPP session to consider.
> ppp echo-test command makes the dormant session active.
> Caution: Issuing this command could negatively impact system performance depending on the number of subscribers using the same name and/or if the number of packets used in the test is large.
> LCP includes Echo-Request and Echo-Reply codes in order to provide a Data Link Layer loopback mechanism for use in exercising both directions of the link. This is useful as an aid in debugging, link quality determination, performance testing, and for numerous other functions. Upon reception of an Echo-Request in the LCP Opened state, an Echo-Reply is transmitted.
> Example
> The following command tests the PPP link to user user1.
> ppp echo-test username user1
> The following command tests the PPP link to the user assigned IP address 1.2.3.4.
> ppp echo-test ipaddr 1.2.3.4
> The following tests the PPP link associated with call ID FE80AA12.
> ppp echo-test callid fe80aa12
> radius interim
> Check points current RADIUS accounting messages immediately.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> radius interim accounting now
> Usage
> The interim command may be part of a regiment of periodic activities to maintain the chassis.
> This command may also be useful in preparation for system monitoring or troubleshooting to set the list of messages to be displayed at a well known time.
> radius test
> Verifies the RADIUS servers functions for accounting and authentication.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> radius test { accounting | admin authentication | authentication | probe authentication server ip_addr port port_no [ username username password password ] } { all | [ on ] | off ] | radius group group_name user_name | server server_name port server_port } user_name password
> accounting
> Test accounting server functionality.
> admin authentication name_admin admin_password
> Test the RADIUS admin authentication.
> name_admin is an string of up to 127 alphanumeric characters to define the name of the administrator.
> admin_password is a string of up to 63 alphanumeric characters to define the password for the administrator.
> authentication
> Test authentication server functionality.
> all | radius group group_name user_name | server server_name port server_port
> all: indicates all configured servers are to be tested.
> server server_name port server_port: indicates only the server specified as server_name and server_port is to be tested. The server must have been previously configured.
> radius group group_name user_name: tests all configured authentication servers in a specific RADIUS group for specific user. Must be followed by the RADIUS group name and user name.
> group_name will be a string of size 1 to 63 characters and specifies the name of server group configured in specific context for authentication/accounting.
> on/off
> Allows the user to turn RADIUS test accounting on or off.
> user_name
> Specifies the RADIUS user who is to be verified. The user must have been previously configured.
> password
> Specifies the RADIUS user who is to have authentication verified. password is only applicable when the authentication keyword is specified.
> Usage
> Test the RADIUS accounting for troubleshooting the system for specific users or to verify all the system RADIUS accounting functions.
> Example
> The following verifies all RADIUS servers.
> radius test accounting all
> radius test authentication all
> The following verifies the RADIUS accounting and authentication for user user1 for the sampleServer.
> radius test accounting server sampleServer port 5000 user1
> radius test authentication server sampleServer port 5000 user1 dummyPwd
> The following commands will verify the RADIUS accounting and authentication for RADIUS server group star1 for the current context:
> radius test accounting server sampleServer port 5000 user1
> radius test authentication server sampleServer port 5000 user1 dummyPwd
> radius test authentication all
> The following verifies the RADIUS authentication server group star1 for user user1.
> radius test authentication radius group star1 user1
> reload
> Invokes a full system reboot.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> reload [ -noconfirm ]
> -noconfirm
> Execute the command without any additional prompts or confirmation from the user.
> Usage
> The system performs a hardware reset and reloads the highest priority boot image and configuration file specified in the boot.sys file. Refer to the boot system priority command in the Global Configuration Mode for additional information on configuring boot images, configuration files and priorities.
> Important: To avoid the abrupt termination of subscriber sessions, it is recommended that a new call policy be configured and executed prior to invoking the reload command. This sets busy-out conditions for the system and allows active sessions to terminate gracefully. Refer to the newcall command in the Exec Mode for additional information.
> Caution: Issuing this command causes the system to become unavailable for session processing until the reboot process is complete.
> Example
> The following command performs a hardware reset on the system:
> reload
> rename
> Changes the name of an existing local file.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> rename from_filepath to_filepath [ -noconfirm ]
> from_filepath
> Specifies the path to the file/directory to be renamed. The path must be formatted according to the following format:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [file: ] { /flash | /pcmcia1 | /hd } [ /directory ]/file_name

> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name
> filename is the actual file of interest
> to_filepath
> Specifies the new name of file/directory. The path must be formatted according to the following formats:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [file: ] { /flash | /pcmcia1 | /hd } [ /directory ]/file_name

> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name
> filename is the actual file of interest
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Important: Extreme caution should be taken when using the -noconfirm option. The paths to the source and the destination should be verified prior to performing the command.
> Usage
> Rename files as part of regular system maintenance in conjunction with the delete command.
> Example
> The following renames the directory /pub in the local PCMCIA1 device.
> rename /pcmcia1/pub /pcmcia1/pub_old
> reveal disabled commands
> Enables the input of commands for features that do not have license keys installed. The output of the command show cli indicates when this is enabled. This command effects the current CLI session only and is disabled by default.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> [ no ] reveal disabled commands
> no
> Do not show disabled commands.
> Usage
> When this command is enabled and a disabled command is entered, a message is displayed that informs you that the required feature is not enabled and also lists the name of the feature that you need to support the command.
> When this command is disabled and a disabled command is entered, the CLI does not acknowledge the existence of the command and displays a message that the keyword is unrecognized.
> Example
> Set the CLI to accept disabled commands and display the required feature for the current CLI session with the following command:
> reveal disabled commands
> Set the CLI to reject disabled commands and return an error message for the current CLI session:
> no reveal disabled commands
> rlogin
> Attempts to connect to a remote host.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> rlogin { host_name | host_ip_address } [ user user_name ]
> host_name | host_ip_address
> Identifies the remote node to attempt to connect to.
> host_name: specifies the remote node using the node’s logical host name which must be resolved via DNS lookup.
> host_ip_address: specifies the remote node using the node’s assigned IP address specified using the standard IPv4 dotted decimal notation.
> user user_name
> Specifies a user name to attempt to connect as. user_name must be from 1 to 1023 alphanumeric characters.
> Usage
> Connect to remote network elements using rlogin.
> Important: rlogin is not a secure method of connecting to a remote host. ssh should be used whenever possible for security reasons.
> Example
> The following connects to remote host remoteABC as user user1.
> rlogin remoteABC user user1
> The following connects to remote host 1.2.3.4 without any default user.
> rlogin 1.2.3.4
> rmdir
> Removes (deletes) a local directory.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> rmdir path [ force ]
> path
> Specifies the directory path to remove. The must be formatted according to the following formats:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:
> directory is the directory name
> filename is the actual file of interest
> force
> Over-rides any warnings to force deletion of the directory and any files contained therein.
> Important: Use of the force keyword should be done with care to ensure the directory is specified accurately as there is no method to recover a directory which has been removed.
> Usage
> Remove old directories as part of regular maintenance.
> Example
> The following removes the local directory /pcmcia1/pub.
> rmdir /pcmcia1/pub
> rotate-hd-file
> This command rotates the Diameter files stored on the hard disk drive.
> Product
> SGW, PGW, HSGW
> Privilege
> Security Administrator, Administrator
> Syntax
> rotate-hd-file diameter [ name policy_name ]
> [ name policy_name ]
> Specifies the hd-storage policy name. policy_name must be and existing HD Storage Policy name and must be an alphanumeric string of 0 through 63 characters in length.
> Usage
> Use this command to manually rotate the Diameter HD stored files.
> Example
> The following command rotates Diameter files that were stored using the HD storage policy named CDR1:
> rotate-hd-file diameter name CDR1
> save configuration
> Saves the configuraiton of current contexts to a local or remote location.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> save configuration url [ -redundant ] [ -noconfirm ] [ showsecrets ] [ verbose ]
> url
> Default: saves to the location of the active configuration currently loaded.
> Specifies the location to store the configuration file(s). url may refer to a local or a remote file. url must be entered using one of the following formats:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [file: ] { /flash | /pcmcia1 | /hd } [ /directory ]/file_name

> • | tftp://{ host[ :port# ] } [ /directory ]/file_name

> • | [ ftp: | sftp: ]//[ username[ :password ]@ ] { host } [ :port# ] [ /directory ]/file_name

> directory is the directory name.
> filename is the actual file of interest.
> Important: Configuration files should be named with a .cfg extension.
> username is the user to be authenticated.
> password is the password to use for authentication.
> host is the IP address or host name of the server.
> Important: hostname can only be used if the networkconfig parameter is configured for DHCP and the DHCP server returns a valid nameserver.
> port# is the logical port number that the communication protocol is to use.
> -redundant
> This keyword directs the system to save the CLI configuration file to the local device, defined by the url variable, and then automatically copy that same file to the like device on the standby processing card, if available.
> Important: This keyword will only work for local devices that are located on both the active and standby processing cards. For example, if you save the file to the /pcmcia1 device on the active processing card, that same type of device (card in Slot 1 of the standby processing card) must be available. Otherwise, a failure message is displayed. If saving the file to an external network (non-local) device, the system disregards this keyword.
> Important: This keyword does not synchronize the local file system. If you have added, modified, or deleted other files or directories to or from a local device for the active processing card, then you must synchronize the local file system on both SMC cards.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Important: Caution should be exercised when using the -noconfirm option as this may cause the accidental over-write of data if the URL refers to an existing file.
> showsecrets
> This keyword causes the CLI configuration file to be saved with all passwords in plain text, rather than their default encrypted format.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> Usage
> Backup the current configuration as part of periodic maintenance activities in case of emergencies.
> Important: The saving of a configuration does not save the boot options as configured via the global configuration mode boot commands.
> Example
> The following saves the configuration data to the local file /flash/pub/juneconfig.cfg with no confirmation from the user:
> save configuration /flash/pub/juneconfig.cfg -noconfirm
> The following saves the configuration data to remote hoist remoteABC as /pub/juneconfig.cfg:
> save configuration tftp://remoteABC/pub/juneconfig.cfg
> save logs
> Saves the current log file to a local or remote location.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> save logs { url } [ active ] [ inactive ] [ callid call_id ] [ event-verbosity evt_verboseness ] [ facility facility ] [ level severity_level ] [ pdu-data pdu_format ] [ pdu-verbosity pdu_verboseness ] [ since from_date_time [ until to_date_time ] ] [ | { grep grep_options | more } ]
> url
> Specifies the location to store the log file(s). url may refer to a local or a remote file. url must be entered using one of the following formats:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:
> Important: Use of the SMC hard drive is not supported in this release.
> directory is the directory name.
> filename is the actual file of interest.
> username is the user to be authenticated.
> password is the password to use for authentication.
> host is the IP address or host name of the server.
> Important: hostname can only be used if the networkconfig parameter is configured for DHCP and the DHCP server returns a valid nameserver.
> port# is the logical port number that the communication protocol is to use.
> active
> Indicates output is to display data from active logs.
> inactive
> Indicates output is to display data from inactive logs.
> callid call_id
> Specifies a call ID for which log information is to be displayed. call_id must be specified as a 4-byte hexadecimal number.
> event-verbosity evt_verboseness
> Specifies the level of verboseness to use in displaying of event data as one of:

> • | min - displays minimal information about the event. Information includes event name, facility, event ID, severity level, date, and time.

> • | concise - displays detailed information about the event, but does not provide the event source within the system.

> • | full - displays detailed information about event, including source information, identifying where within the system the event was generated.

> facility facility
> Specifies the facility to modify the filtering of logged information. Valid facilities for this command are:

> • | a10: A10 interface facility

> • | a11: A11 interface facility

> • | a11mgr: A11 Manager facility

> • | aaa-client: AAA client facility

> • | aaamgr: AAA manager logging facility

> • | aaaproxy: AAA Proxy facility

> • | aal2: AAL2 protocol logging facility

> • | acl-log: Access Control List logging facility

> • | acsctrl: Active Charging Service (ACS) Controller facility

> • | acsmgr: Active Charging Service (ACS) Manager facility

> • | alarmctrl: Alarm Controller facility

> • | alcap: ALCAP protocol logging facility

> • | alcapmgr: ALCAPMgr logging facility

> • | all: All facilities

> • | asngwmgr: ASN Gateway Manager facility

> • | asnpcmgr: ASN Paging Controller Manager facility

> • | bfd: BFD protocol logging facility

> • | bgp: Border Gateway Protocol (BGP) facility

> • | bindmux: IPCF BindMux-De-mux Manager logging facility

> • | bssap+: Base Station Sub-system Application Part+ protocol facility for loggin interface between the SGSN and the MSC/VLR (2.5G and 3G)

> • | bssgp: Base Station Sub-system GPRS Protocol logging facility handles exchange information between the SGSN and the BSS (2.5G only)

> • | callhome: Call home application logging facility

> • | cap: CAMEL Application Part (CAP) logging facility for protocol used in prepaid applications (2.5G and 3G)

> • | cli: CLI logging facility

> • | credit-control: Credit Control facility

> • | cscf: IMS/MMD CSCF

> • | cscfmgr: SIP CSCF Manager facility

> • | cscfttmgr: SIP CSCFTT Manager facility

> • | csp: Card Slot Port controller facility

> • | css: Content Service Selection (CSS) facility

> • | css-sig: Content Service Selection (CSS) RADIUS Signaling facility

> • | cx-diameter: Cx Diameter Messages facility

> • | dcardctrl: IPSEC Daughtercard Controller logging facility

> • | dcardmgr: IPSEC Daughtercard Manager logging facility

> • | demuxmgr: Demux Manager API facility

> • | dgmbmgr: Diameter Gmb Application Manager logging facility

> • | dhcp: Dynamic Host Configuration Protocol logging facility

> • | dhcpv6: DHCPv6

> • | dhost: Distributed Host logging facility

> • | diabase: Diabase messages facility

> • | diameter: Diameter endpoint logging facility

> • | diameter-acct: Diameter Accounting

> • | diameter-auth: Diameter Authentication

> • | diameter-dns: Diameter DNS subsystem

> • | diameter-ecs: ACS Diameter signaling facility

> • | diameter-hdd: Diameter HDD Interface facility

> • | diameter-svc: Diameter Service

> • | diamproxy: DiamProxy logging facility

> • | dpath: IPSEC Data Path facility

> • | drvctrl: Driver Controller facility

> • | eap-ipsec: EAP

> • | eap-sta-s6a-s13-s6b-diameter: EAP/STA/S6A/S13/S6B Diameter messages facility

> • | ecs-css: ACSMGR <-> Session Manager Signalling Interface facility

> • | egtpc: eGTP-C logging facility

> • | egtpmgr: eGTP manager logging facility

> • | egtpu: eGTP-U logging facility

> • | epdg: ePDG logging facility

> • | evlog: Event log facility

> • | famgr: Foreign Agent manager logging facility

> • | firewall: Firewall logging facility

> • | fng: FNG logging facility

> • | gmm:

> • | For 2.5G: Logs the GPRS Mobility Management (GMM) layer (above LLC layer)

> • | For 3G: Logs the access aplication layer (above the RANAP layer)

> • | gprs-app: GPRS Application logging facility

> • | gprs-ns: GPRS Network Service Protocol (layer between SGSN and the BSS) logging facility

> • | gq-rx-tx-diameter: Gq/Rx/Tx Diameter messages facility

> • | gss-gcdr: GTPP Storage Server GCDR facility

> • | gtpc: GTP-C protocol logging facility

> • | gtpcmgr: GTP-C protocol Manager logging facility

> • | gtpp: GTP-PRIME protocol logging facility

> • | gtpu: GTP-U protocol logging facility

> • | gtpumgr: GTPU Demux manager

> • | gx-ty-diameter: Gx/Ty Diameter messages facility

> • | gy-diameter: Gy Diameter messages facility

> • | hamgr: Home Agent manager logging facility

> • | hat: High Availability Task (HAT) process facility

> • | hdctrl: HD Controller logging facility

> • | hnb-gw: HNB-GW (3G Femto GW) logging facility

> • | hnbmgr: HNBMGR (3G Femto GW DemuxMgr) logging facility

> • | hss-peer-service: HSS Peer Service facility

> • | igmp: IGMP

> • | ikev2: IKEv2

> • | ims-authorizatn: IMS Authorization Service facility

> • | ims-sh: HSS SH Service facility

> • | imsimgr: SGSN IMSI Manager facility

> • | imsue: IMSUE

> • | ip-arp: IP Address Resolution Protocol facility

> • | ip-interface: IP interface facility

> • | ip-route: IP route facility

> • | ipms: IPMS logging facility

> • | ipsec: IP Security logging facility

> • | ipsg: IP Service Gateway interface logging facility

> • | ipsgmgr: IP Services Gateway facility

> • | ipsp: IP Pool Sharing Protocol logging facility

> • | kvstore: KV Store facility

> • | l2tp-control: L2TP control logging facility

> • | l2tp-data: L2TP data logging facility

> • | l2tpdemux: L2TP Demux Manager logging facility

> • | l2tpmgr: L2TP Manager logging facility

> • | lagmgr: LAGMGR logging facility

> • | ldap: Lightweight Directory Access Protocol (LDAP) messages logging facility

> • | li: Refer to the ASR 5000 Lawful Intercept Interface Reference for a description of this command.

> • | linkmgr: SGSN/BSS SS7 Link Manager logging facility (2.5G only)

> • | llc: Logical Link Control (LLC) Protocol logging facility; for SGSN: logs the LLC layer between the GMM and the BSSGP layers for logical links between the MS and the SGSN

> • | local-policy: Local Policy Service facility

> • | m3ua: M3UA Protocol logging facility

> • | magmgr: Mobile Access Gateway manager logging facility

> • | map: MAP Protocol logging facility

> • | megadiammgr: Megadiameter Manager (SLF Service) logging facility

> • | mme-app: Mobility Management Entity Application logging facility

> • | mme-misc: MME miscellaneous logging facility

> • | mmedemux: Mobility Management Entity Demux Manager logging facility

> • | mmemgr: MME Manager facility

> • | mmgr: Master Manager logging facility

> • | mobile-ip: Mobile IP processes

> • | mobile-ip-data: Mobile IP data facility

> • | mobile-ipv6: Mobile IPv6 logging facility

> • | mpls: MPLS protocol logging facility

> • | mseg-app: MSEG application logging facility

> • | mseg-gtpc: MSEG GTPC application logging facility

> • | mseg-gtpu: MSEG GTPU application logging facility

> • | msegmgr: MSEGMgr (MSEG DemuxMgr) logging facility

> • | mtp2: MTP2 Service logging facility

> • | mtp3: MTP3 Protocol logging facility

> • | multicast-proxy: Multicast Proxy logging facility

> • | npuctrl: Network Processor Unit Control facility

> • | npumgr: Network Processor Unit Manager facility

> • | npumgr-acl: NPUMGR ACL logging facility

> • | npumgr-flow: NPUMGR FLOW logging facility

> • | npumgr-fwd: NPUMGR FWD logging facility

> • | npumgr-init: NPUMGR INIT logging facility

> • | npumgr-port: NPUMGR PORT logging facility

> • | npumgr-recovery: NPUMGR RECOVERY logging facility

> • | ntfy-intf: Notification Interface logging facility

> • | orbs: Object Request Broker System logging facility

> • | ospf: OSPF protocol logging facility

> • | ospfv3: OSPFv3 protocol logging facility

> • | p2p: Peer-to-Peer Detection logging facility

> • | pccmgr: IPCF PCC Manager library

> • | pdg: PDG logging facility

> • | pdgdmgr: PDG Demux Manager logging facility

> • | pdif: PDIF logging facility

> • | pgw: PDN Gateway logging facility

> • | phs: Payload Header Suppression

> • | phs-control: PHS X1/X5 and X2/X6 Interface logging facility

> • | phs-data: PHS Data logging facility

> • | phs-eapol: PHS EAPOL logging facility

> • | phsgwmgr: PHS Gateway Manager facility

> • | phspcmgr: PHS Paging Controller Manager facility

> • | pmm-app: PMM application logging facility

> • | ppp: PPP link and packet facilities

> • | pppoe: PPPOE logging facility

> • | push: VPNMGR CDR push logging facility

> • | radius-acct: RADIUS accounting logging facility

> • | radius-auth: RADIUS authentication logging facility

> • | radius-coa: RADIUS change of authorization and radius disconnect

> • | ranap:Radio Access Network Application Part (RANAP) Protocol facility logging info flow between SGSN and RNS (3G)

> • | rct: Recovery Control Task logging facility

> • | rdt: Redirect Task logging facility

> • | resmgr: Resource Manager logging facility

> • | rf-diameter: Rf Diameter messages facility

> • | rip: RIP logging facility (RIP is not supported at this time.)

> • | rohc: RObust Header Compression facility

> • | rsvp: Reservation Protocol logging facility

> • | rua: RUA (3G Femto GW - RUA messages) logging facility

> • | s1ap: S1AP Protocol logging facility

> • | sccp: SCCP Protocol logging connection-oriented messages between RANAP and TCAP layers.

> • | sct: Shared Configuration Task logging facility

> • | sctp: SCTP Protocol logging facility

> • | sessctrl: Session Controller logging facility

> • | sessmgr: Session Manager logging facility

> • | sesstrc: session trace logging facility

> • | sft: Switch Fabric Task logging facility

> • | sgs: SGs protocol logging facility

> • | sgsn-app: SGSN-APP logging various SGSN ‘glue’ interfaces, e.g., between PMM, MAP,. GPRS-FSM, SMS.

> • | sgsn-failures: SGSN call failures (attach/activate rejects) logging facility (2.5G)

> • | sgsn-gtpc: SGSN GTP-C Protocol logging control messages between the SGSN and the GGSN

> • | sgsn-gtpu: SGSN GTP-U Protocol logging user data messages between the SGSN and GGSN

> • | sgsn-mbms-bearer:SGSN MBMS Bearer app (SMGR) logging facility

> • | sgsn-misc: Used by stach manager to log binding and removing between layers

> • | sgsn-system: SGSNs System Components logging facility; used infrequently

> • | sgsn-test: SGSN Tests logging facility; used infrequently

> • | sgtpcmgr: SGSN GTPC Manager logging information exchange through SGTPC and the GGSN

> • | sgw: Serving Gateway facility

> • | sh-diameter: Sh Diameter messages facility

> • | sitmain: System Initialization Task main logging facility

> • | sm-app: SM Protocol logging facility

> • | sms: Short Message Service (SMS) logging messages between the MS and the SMSC

> • | sndcp: SNDCP Protocol logging facility

> • | snmp: SNMP logging facility

> • | sprmgr: IPCF SPR Manager logging facility

> • | srdb: Static Rating Database

> • | srp: Service Redundancy Protocol (SRP) logging facility

> • | sscfnni: SSCFNNI Protocol logging facility

> • | sscop: SSCOP Protocol logging facility

> • | ssh-ipsec: SSH IP Security logging facility

> • | ssl: SSL (Secure socket layer messages) logging facility

> • | stat:: Statistics logging facility

> • | system: System logging facility

> • | tacacsplus: TACACS+ Protocol logging facility

> • | tcap: TCAP Protocol logging facility

> • | testctrl: Test Controller logging facility

> • | testmgr: Test Manager logging facility

> • | threshold: threshold logging facility

> • | ttg: TTG logging facility

> • | tucl: TUCL logging facility

> • | udr: User detail record facility (used with the Charging Service)

> • | user-data: User data logging facility

> • | user-l3tunnel: User layer-3 tunnel logging facility

> • | usertcp-stack: User Tcp Stack

> • | vpn: Virtual Private Network logging facility

> • | wimax-data: WiMAX DATA

> • | wimax-r6: WiMAX R6

> level severity_level
> Specifies the level of information to be logged, severity_level, from the following list which is ordered from highest to lowest:

> • | critical - display critical events

> • | error - display error events and all events with a higher severity level

> • | warning - display warning events and all events with a higher severity level

> • | unusual - display unusual events and all events with a higher severity level

> • | info - display info events and all events with a higher severity level

> • | trace - display trace events and all events with a higher severity level

> • | debug - display all events

> pdu-data pdu_format
> Specifies output format for the display of packet data units as one of:

> • | none - output is in raw format (unformatted).

> • | hex - output is in hexadecimal format.

> • | hex-ascii - output isd in hexadecimal and ASCII similar to a main-frame dump.

> pdu-verbosity pdu_verboseness
> Specifies the level of verboseness to use in displaying of packet data units as a value from 1 to 5 where 5 is the most detailed.
> since from_date_time [ until to_date_time ]
> Default: no limit.
> since from_date_time: indicates only the log information which has been collected more recently than from_date_time is to be displayed.
> until to_date_time: indicates no log information more recent than to_date_time is to be displayed. until defaults to current time when omitted.
> from_date_time and to_date_time must be formatted as YYYY:MM:DD:HH:mm or YYYY:MM:DD:HH:mm:ss. Where YYYY is a 4-digit year, MM is a 2-digit month in the range 01 through 12, DD is a 2-digit day in the range 01 through 31, HH is a 2-digit hour in the range 00 through 23, mm is a 2-digit minute in the range 00 through 59, and ss is a 2 digit second in the range 00 through 59.
> to_date_time must be a time which is more recent than from_date_time.
> The use of the until keyword allows for a time range of log information while only using the since keyword will display all information up to the current time.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter in Command Line Interface Reference.
> Usage
> Backup the current log file as part of periodic maintenance activities.
> Example
> The following saves the log to the local file /flash/pub/junelogs.logs with no confirmation from the user:
> save logs /flash/pub/junelogs.logs -noconfirm
> The following saves the configuration data to remote host remoteABC as /pub/junelogs.logs:
> save logs tftp://remoteABC/pub/junelogs.logs
> session trace
> This command enable/disables the subscriber session trace functionality based on a specified subscriber device or ID on one or all instance of session on a specified UMTS/EPS network elements. It also clears/resets the statistics collected for subscriber session trace on a system.
> Product
> GGSN, MME, P-GW, S-GW
> Privilege
> Operator
> Syntax
> session trace { reset statistics | subscriber network-element { mme | pgw | sgw | ggsn } { imei id | imsi id | interface { all | interface } } trace-ref id collection-entity ip_address}
> no session trace subscriber network-element [ mme | pgw | sgw | ggsn ] [ trace-ref id ]
> no
> Disables the entire session trace or for a specific network element and/or trace reference.
> reset statistics
> Clears/resets the entire session trace statistical data collected on a system.
> Caution: This is a system wide command that affects all statistical data.
> session trace subscriber network-element { mme | pgw | sgw | ggsn }
> Identifies the network element that, in turn, identifies the interfaces where the session trace is to occur. Specific interfaces can be specified using the interface keyword described below.
> ggsn: Specifies that the session trace is to occur on one or all interfaces on the GGSN.
> mme: Specifies that the session trace is to occur on one or all interfaces on the MME.
> pgw: Specifies that the session trace is to occur on one or all interfaces on the P-GW.
> sgw: Specifies that the session trace is to occur on one or all interfaces on the S-GW.
> imei id
> Specifies the International Mobile Equipment Identification number of the subscribers UE. id must be the 8-digit TAC (Type Allocation Code) and 6-digit serial number. Only the first 14 digits of the IMEI/IMEISV are used to find the equipment ID.
> imsi id
> Specifies the International Mobile Subscriber Identification (IMSI). id must be the 3-digit MCC (Mobile Country Code), 2- or 3- digit MNC (Mobile Network Code), and the MSIN (Mobile Subscriber Identification Number). The total should not exceed 15 digits.
> interface { all | interface }
> Specifies the interfaces where the session trace application will collect data.
> all: Specifies that all interfaces associated with the selected network element
> interface: Specifies the interface type where the session trace application will collect trace data. The following interfaces are applicable for the network element type:

> • | GGSN:

> • | gi: Specifies that the interface where the trace will be performed is the Gi interface between the GGSN and RADIUS server.

> • | gmb: Specifies that the interface where the trace will be performed is the Gmb interface between the GGSN and BM-SC.

> • | gn: Specifies that the interface where the trace will be performed is the Gn interface between the GGSN and the SGSN.

> • | gx: Specifies that the interface where the trace will be performed is the Gx interface between the GGSN and PCRF.

> • | MME:

> • | s1mme: Specifies that the interface where the trace will be performed is the S1-MME interface between the MME and the eNodeB.

> • | s3: Specifies that the interface where the trace will be performed is the S3 interface between the MME and an SGSN.

> • | s6a: Specifies that the interface where the trace will be performed is the S6a interface between the MME and the HSS.

> • | s10: Specifies that the interface where the trace will be performed is the S10 interface between the MME and another MME.

> • | s11: Specifies that the interface where the trace will be performed is the S11 interface between the MME and the S-GW.

> • | P-GW:

> • | gx: Specifies that the interface where the trace will be performed is the Gx interface between the P-GW and the PCRF.

> • | s2a: Specifies that the interface where the trace will be performed is the S2a interface between the P-GW and the HSGW.

> • | s2b: Specifies that the interface where the trace will be performed is the S2b interface between the P-GW and an ePDG.

> • | s2c: Specifies that the interface where the trace will be performed is the S2c interface between the P-GW and a trusted, non-3GPP access device.

> • | s5: Specifies that the interface where the trace will be performed is the S5 interface between the P-GW and the S-GW.

> • | s6b: Specifies that the interface where the trace will be performed is the S6b interface between the P-GW and the 3GPP AAA server.

> • | s8b: Specifies that the interface where the trace will be performed is the S8b interface between the P-GW and the S-GW.

> • | sgi: Specifies that the interface where the trace will be performed is the SGi interface between the P-GW and the PDN.

> • | S-GW:

> • | gxc: Specifies that the interface where the trace will be performed is the Gxc interface between the S-GW and the PCRF.

> • | s11: Specifies that the interface where the trace will be performed is the S11 interface between the S-GW and the MME.

> • | s4: Specifies that the interface where the trace will be performed is the S4 interface between the S-GW and an SGSN.

> • | s5: Specifies that the interface where the trace will be performed is the S5 interface between the S-GW and the P-GW.

> • | s8b: Specifies that the interface where the trace will be performed is the S8b interface between the S-GW and the P-GW.

> trace-ref id
> Specifies the trace reference for the trace being initiated. id must be the MCC (3 digits), followed by the MNC (3 digits), then the trace ID number (3-byte octet string).
> collection-entity ip_address
> Specifies the IP address of the collection entity where session trace data is pushed. ip_address must be a valid IPv4 address and is specified in dotted decimal notation.
> Usage
> Use this command to initiate a session trace for a specified subscriber device or ID on one or all interfaces on a specified network element.
> Important: Session trace configuration is performed in the Global Configuration Mode using the session trace command. Refer to the Global Configuration Mode Commands chapter for more information.
> Example
> The following command initiates a session trace on a P-GW S5 interface for a subscriber with an IMSI of 322233123456789 and sets the trace reference as 322233987654 and the collection entity IP address as 1.2.3.4:
> session trace subscriber network-element pgw imsi 322233123456789 interface s5 trace-ref 322233987654 collection-entity 1.2.3.4
> The following command initiates a session trace on an MME S6a interface for a subscriber with an IMSI of 322233123456789 and sets the trace reference as 322233987654 and the collection entity IP address as 1.2.3.4:
> session trace subscriber network-element mme imsi 322233123456789 interface s6a trace-ref 322233987654 collection-entity 1.2.3.4
> The following command initiates a session trace on a Gn interface on GGSN between GGSN and SGSN for a subscriber with an IMSI of 322233123456789 and sets the trace reference as 322233987654 and the collection entity IP address as 1.2.3.4:
> session trace subscriber network-element ggsn imsi 322233123456789 interface gn trace-ref 322233987654 collection-entity 1.2.3.4
> setup
> Enters the system setup wizard which guides the user through a series of questions regarding the system basic configuration options, such as initial context-level administrative users, host name, etc.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> setup
> Usage
> The setup wizard provides a user friendly interface for initial system configuration.
> Important: If the configuration script generated by the setup wizard is applied when an existing configuration is in use, the options which are common to both are updated and all remaining options are left unchanged.
> Example
> setup
> sgsn clear-detached-subscriptions
> Clear subscription data belonging to a subscriber who has already detached.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn clear-detached-subscriptions imsi imsi
> imsi imsi
> Specifies the international mobile subscriber identity (IMSI) of the subscriber session identifying the subscription data to be cleared.
> imsi : Enter 1 to 15 digits.
> Usage
> This command can be issued on either a 2G or 3G SGSN to clear subscription data (including subscription information, and information for P-TMSI allocated, received authorization vectors, and NGAF flag values). This command is only effective if the subscriber has already detached.
> After the data is purged, the SGSN sends an appropriate message to the HLR.
> Related Commands:

> • | To clear subscription data for subscribers that are currently attached, refer to the admin-disconnect-behavior clear-subscription commands described in the chapters for GPRS Service Configuration Mode or the SGSN Service Configuration Mode.

> Example
> sgsn clear-detached-subscriptions imsi 040501414199978
> sgsn imsimgr
> Enter commands to initiate an audit to enable managing the SGSN’s IMSI manager’s (IMSIMgr) IMSI table.
> Important: These commands are used primarily for troubleshooting purposes and are intended for the use of specially trained service representatives.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn imsimgr { add-record imsi sessmgr instance sessmgr# | audit-with sessmgr { all | instance sessmgr# } | remove-record imsi }
> add-record imsi
> Adds a record for an IMSI to the IMSI manager’s table and associates a specific session manager (SessMgr) with the IMSI.
> imsi : Enter up to 15 digits. An IMSI consists of the 3-digit MCC (mobile country code) + the 2- or 3-digit MNC (mobile network code) + the MSIN (mobile station identification number) for the remaining 10 or 9 digits (depending on the length of the MNC).
> sessmgr instance sessmgr#
> Identifies a specific Session Manager (SessMgr) associated with the IMSI.
> sessmgr# : Enter up to 4 digits, 0 to 4095.
> audit-with sessmgr { all | instance sessmgr# }
> Initiate an IMSI audit with a specific Session Manager (SessMgr) or with all SessMgrs.
> sessmgr# : Enter up to 4 digits, 0 to 4095.
> remove-record imsi
> Delete a specific IMSI from the IMSI table.
> imsi : Enter up to 15 digits. An IMSI consists of the 3-digit MCC (mobile country code) + the 2- or 3-digit MNC (mobile network code) + the MSIN (mobile station identification number) for the remaining 10 or 9 digits (depending on the length of the MNC).
> Usage
> Use this command to manage the IMSIMgr’s IMSI table, and to initiate an audit of one or more SessMgrs with the IMSIMgr so that the IMSI table has the correct IMSI-SessMgr association. After this audit, any IMSI in the IMSIMGR which is not found in any Sessmgr is deleted and similarly any missing entries at the IMSIMgr are created.
> Example
> Delete IMSI 044133255524211 from the audit table:
> sgsn imsimgr remove-record 044133255524211
> sgsn offload
> This command instructs the SGSN to begin the offloading procedure and actually starts and stops the offloading of subscribers which is part of the SGSN’s Gb (2G) or Iu (3G) Flex load redistribution functionality.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn offload [ gprs-service srvc_name | sgsn-service srvc_name } srvc_name { activating [ nri-value nri_value | stop nri-value nri_value ] | connecting [ nri-value nri_value | stop [ nri-value nri_value | target-nri target_nri target-count target_count ] | t3312-timeout seconds | target-nri target_nri target-count target_count ] }
> gprs-service srvc_name
> A unique string of 1 to 63 alphanumeric characters that identifies a specific GPRS service that has already been defined for the 2G SGSN configuration.
> sgsn-service srvc_name
> A unique string of 1 to 63 alphanumeric characters that identifies a specific SGSN service that has already been defined for the 3G SGSN configuration.
> activating
> Instructs the SGSN to off load any subscribers sending an ‘activate request’ message.
> connecting
> Instructs the SGSN to off load any subscribers sending either an ‘attach request’ or a ‘RAU request’ message.
> nri-value nri-value
> Sets the local NRI. Including this keyword in the configuration instructs the SGSN to check the P-TMSI and use the SGSN matching the configured NRI value to off load subscribers.
> Important: nri-value and target-nri are mutually exclusive.
> nri-value: Must be an integer from 1 to 63 to identify a specific, already defined, SGSN in a pool. (NRI defined in the service configuration.)
> Use of 0 (zero) value is not recommended.
> stop
> Instructs the SGSN to stop offloading subscribers from the pool area.
> target-nri target_nri
> Including this keyword instructs the SGSN to begin dynamically load balancing across a network of pooled SGSNs.
> target_nri: Enter an integer from 0 to 63. Identifies an already defined target NRI (SGSN) to which the subscribers are to be offloaded. (NRI previously defined in the service configuration.)
> Use of 0 (zero) value is not recommended.
> target-count target_count
> Identifies the number of subscribers to be offloaded.
> target_count: Enter an integer from 0 to 4000000.
> t3312-timeout seconds
> Configures the timer for sending period RAUs to the MS. Default is 4 seconds.
> seconds: Must be an integer from 2 to 60.
> Usage
> Use this command to configure the offloading of subscribers which is a part of the SGSN’s load redistribution operation. This command can be used anytime an SGSN is to be taken out of service.
> Commands, with different NRI values, are repeated to expand/contract the radius of the offloading.
> When targeted offloading is to be used, you should choose an algorithm to control offloading from the perspective of the IMSIMGR and SESSMGR. This is done with the target-offloading command in the SGSN-Global configuration mode.
> Example
> Command 1: The following command instructs the SGSN to begin offloading for the local NRI id 1 in the gprs1 GPRS service configuration:
> sgsn offload gprs-service gprs1 connecting nri-value 1
> Command 2: Enter this second command to add offloading for NRI 2 to the offloading already occurring for NRI 1:
> sgsn offload gprs-service gprs1 connecting nri-value 2
> Command 1: The following command instructs the SGSN to begin offloading for all local NRIs to the target NRIs 5 and 6 for 100000 and 200000 subscribers respectively:
> sgsn offload sgsn-service sgsnserv4 connecting target-nri 5 target-count 100000 target-nri 6 target-count 200000
> Command 2: The following command instructs the SGSN to add target NRI 4 to the offloading and also to change the subscriber offload number for target NRI 5:
> sgsn offload sgsn-service sgsnserv4 connecting target-nri 4 target-count 100000 target-nri 5 target-count 300000
> sgsn op
> These commands instruct the SGSN to begin specific operations or functions.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn op { auth-ptmsi-counters imsi imsi | convert | nse { fr | ip | sgsn-invoke-trace } | show | ss7-rd ss7-rd_id { destination | link | linkset | peer } }
> auth-ptmsi-counters imsi imsi
> Displays the authentication, P-TMSI reallocation, and P-TMSI signature reallocation counters for the specified IMSI.
> imsi: Enter a unique 15-digit number associated with a mobile phone.
> convert point-code pt_code variant variant
> This command accesses a built-in conversion tool to convert SS7 point codes, according to identified variants, from dotted-decimal format to decimal format and vice versa.
> point-code pt_code: Enter an SS7 point code in either dotted-decimal format or decimal format.
> variant variant: Identify the appropriate variant for the point code:

> • | ansi

> • | itu

> • | ttc

> nse { fr operation | ip operation | sgsn-invoke-trace nse-id nse_id }
> The nse command enables the operator to perform a range of live control functions (e.g, reset, block, unblock) for various types of virtual connections based on the signalling type of the NSE:
> fr : Identifies a Frame Relay NSE.
> ip : Identifies an IP NSE.
> operation: Identifies the operation to be performed for the NSE connection (if available for the selected signalling type):

> • | block nse-id nse_id - Blocks signal flow through all network service virtual connections (NSVC) for the specified NSE:

> • | nse_id : Enter an integer from 0 to 65535.

> • | bvc-flc-limit rate rate bvc-id bvc_id nse-id nse_id - SGSN initiates flow control at the defined percentage rate to limit the flow through the BSSGP virtual connection (BVC) for the specified NSE and optionally for a specified BVC.

> • | rate : Enter an integer from 0 to 100.

> • | bvc_id : Enter an integer from 0 to 65000.

> • | nse_id : Enter an integer from 0 to 65535.

> • | bvc-reset bvc-id bvc_id nse-id nse_id - SGSN initiates a BVC-Reset on the specified BVC and NSE:

> • | bvc_id : Enter an integer from 0 to 65000.

> • | nse_id : Enter an integer from 0 to 65535.

> • | nsvc nsvc_id { block | enable | disable | unblock }nse_id - SGSN initiates NS-Block or NS-Unblock for the specified NSVC of the specified NSE:

> • | nsvc_id : Enter an integer from 0 to 65535.

> • | nse_id : Enter an integer from 0 to 65535.

> • | reset nse-id nse_id - SGSN initiates NS-Reset for all NSVC configured in the NSE.

> • | nse_id : Enter an integer from 0 to 65535.

> • | unblock nse-id nse_id - SGSN initiates NS-Unblock for all NSVC configured for the specified NSE.

> • | nse_id : Enter an integer from 0 to 65535.

> sgsn-invoke-trace nse-id nse_id record-type record_type trace-reference reference [ mobile-id type id_type | trace-transaction-id trace_id ] :
> Important: This command can be used for troubleshooting/debugging purposes and is primarily intended for the use of specially trained service representatives.
> Instructs the SGSN (1) to send the BSSGP message SGSN-INVOKE-TRACE to the BSC to initiate a BSC trace of a particular MS and (2) to define the type and triggering of the trace.

> • | nse_id : Identify the peer NSE, enter an integer from 0 to 65535.

> • | record_type : Select the type of trace to be performed:

> • | basic

> • | handover

> • | no-bss-trace

> • | radio

> • | trace-reference reference : Enter the trace reference ID - an integer from 0 to 65535.

> • | mobile-id type id_type : Select the appropriate mobile ID type for the MS that is to be traced:

> • | imei value value - Specifies the mobile ID type as the unique International Mobile Equipment Identity.

> value : Enter the 15-digit IMEI value.

> • | imeisv value value - Specifies the mobile ID type as the unique International Mobile Equipment Identity - with the two-digit software version number.

> value : Enter the 16-digit IMEISV value.

> • | imsi value value - Specifies the mobile ID type as a network unique International Mobile Subscriber Identity.

> value : Enter the 15-digit IMSI value.

> • | trace-transaction-id trace_id : Enter the trace transaction ID - an integer from 0 to 65535.

> show plmn-list smgr-inst sessmgr#
> Important: This function is only available in release 8.1.
> SGSN displays the configured PLMN list for the specified session manager (SessMgr):
> sessmgr# : Enter up to 4 digits, 0 to 4095.
> ss7-rd ss7-rd_id { destination | link | linkset | peer }
> The ss7-rd commands assist with troubleshooting connections between the SGSN and the peer server.
> ss7-rd_id : Enter a value between 1 and 12 that identifying the configured SS7 routing domain.

> • | destination audit asp-instance asp_id peer-server-id peer_id psp-instance-id psp_id

> Initiate destination audit (DAUD) messages for all point codes reachable via the identified peer-server, which is in restricted/unavailable/congested state due to DRST/DUNA/SCON messages respectively from the far end.

> • | asp_id : Enter the relevant ASP configuration ID, an integer between 1 and 4.

> • | peer_id : Enter the relevant peer server configuration ID, an integer between 1 and 144.

> • | psp_id : Enter the relevant PSP configuration ID, an integer between 1 and 4

> • | link procedure linkset-id linkset_id link-id link_id

> Initiates MTP3 network link management procedures for the specified link:

> • | activate -- activates the deactivated link.

> • | deactivate -- deactivates specified link.

> • | deactivate-l2-only -- deactivates the link only at the MTP3 layer.

> • | inhibit -- inhibits the link only if it does not make any destination unreachable.

> • | uninhibit -- uninhibits the inhibited link.

> • | linkset_id : Enter an integer between 1 and 144.

> • | link_id : Enter an integer between 1 and 16.

> • | linkset-id procedure linkset-id linkset_id

> Initiates MTP3 network link management procedures for all the links in the specified linkset:

> • | activate -- activates the deactivated linkset.

> • | deactivate -- deactivates the linkset.

> • | deactivate-l2-only -- deactivates the linkset only at MTP3 layer.

> • | linkset_id : Enter an integer between 1 and 144.

> • | peer message asp-instance asp_id peer-server-id peer_id psp-instance-id psp_id :

> Initiates one of the following SCTP/M3UA management messages from the identified link:

> • | abort - Sends an SCTP Abort message which aborts the SCTP association ungracefully.

> • | activate - Sends an M3UA ASP Active message to activate the link.

> • | down - Sends an M3UA ASP Down message to bring down the M3UA link.

> • | establish - Sends an SCTP INIT message to start the SCTP association establishment.

> • | inactivate - Sends an M3UA ASP Inactive message to deactivate the link.

> • | inhibit - Inhibits the M3UA link locally when the operator wants to lockout the link.

> • | terminate - Sends SCTP Shutdown message which closes the SCTP association gracefully.

> • | un-inhibit - Uninhibits the M3UA link.

> • | up - Sends an M3UA ASP UP message to bring up the M3UA link.

> • | asp_id : Enter the relevant ASP configuration ID, an integer between 1 and 4.

> • | peer_id : Enter the relevant peer server configuration ID, an integer between 1 and 144.

> • | psp_id : Enter the relevant PSP configuration ID, an integer between 1 and 4

> Usage
> In most cases, an operator will block/unblock/reset from the BSC-side. The nse commands cause the SGSN to initiate actions, usually for one of the following reasons:

> • | to resolve issues on the BSC-side,

> • | as part of an upgrade to the BSC,

> • | as part of link expansion,

> • | to resolve NSVC/BVC status mismatches observed between the SGSN and BSC.

> The sgsn-invoke-trace command initiates the trace procedure where the BSC begins a trace record on a specified MS.
> Example
> Instruct the SGSN to initiate an NS-Block for all NSVC associated with Frame Relay NSE ID 2422:
> sgsn op nse fr unblock nse-id 2422
> Activate linkset 1 configured in SS7 routing domain 1:
> sgsn op ss7-rd 1 linkset activate linkset-id 1
> sgsn retry-unavailable-ggsn
> Marks the GGSN as available for further activation.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn retry-unavailable-ggsn IP_address
> IP_address
> Specifies the IP address or a specific GGSN. Enter either an IPv4 or IPv6 according to standard format.
> Usage
> This command allows the operator to directly inform both the session manager and the SGTPC manager that the GGSN has been removed from a blacklist and is now available for activations. This action would override the GGSN blacklist timer configuration with ggsn-fail-retry-timer in the SGTP service configuration mode.
> Example
> The following command indicates that the GGSN identified by its IP address is now available for activation:
> sgsn retry-unavailable-ggsn 198.168.128.8
> sgtpc test echo sgsn-address
> Initiates SGTPC echo test procedure.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgtpc test echo sgsn-address sgsn_ip_address { all | ggsn-address ggsn_ip_address }
> sgsn-address sgsn_ip_address
> Identify the IP address of the SGSN issuing the test.
> sgsn_ip_address : Enter a standard IPv4 dotted decimal format.
> all
> Instruct the SGSN to send the GTPC echo request to all GGSNs having current sessions with the SGTP service.
> ggsn-address ggsn_ip_address
> Instructs the SGSN to send the GTPC echo request to the specified GGSN whether or not the GGSN has active sessions with the SGTP service.
> ggsn_ip_address: Enter a standard IPv4 dotted decimal format.
> Usage
> This command initiates a test for the GTPC echo procedure -- echo from the specified SGSN to a specified GGSN or to all GGSNs that have sessions with the SGTP service. Issue the command from the Exec Mode within the context in which the SGTP service is configured.
> Note that if the GGSN does not respond to the initial echo request, the echo requests will be retried for the max-retransmissions times.
> Example
> This SGSN with IP address of 1.1.1.1 sends an echo test to all GGSNs attached to the SGTP service:
> sgtpc test echo sgsn-address 1.1.1.1 all
> shutdown
> Terminates all processes within the chassis.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> shutdown [ -noconfirm ]
> -noconfirm
> Execute the command without any additional prompts or confirmation from the user.
> Usage
> The system performs a hardware reset and reloads the highest priority boot image and configuration file specified in the boot.sys file. Refer to the boot system priority command in the Global Configuration Mode for additional information on configuring boot images, configuration files and priorities.
> Important: To avoid the abrupt termination of subscriber sessions, it is recommended that a new call policy be configured and executed prior to invoking the shutdown command. This sets busy-out conditions for the system and allows active sessions to terminate gracefully. Refer to the newcall command in the Exec Mode for additional information.
> Caution: Issuing this command causes the system to become unavailable for session processing until the reboot process is complete.
> Example
> The following command performs a hardware reset on the system:
> shutdown
> sleep
> Pauses the command line interface (CLI).
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> sleep seconds
> seconds
> Specifies the number of seconds to pause. The number of seconds must be a value in the range from 1 through 3600.
> Usage
> Sleep is a command delay which is only useful when creating command line interface scripts such as predefined configuration files/scripts.
> Example
> The following will cause the CLI to pause for 30 seconds.
> sleep 30
> srp initiate-switchover
> This command changes the device status on the primary and backup systems configured for Interchassis Session Recovery (ICSR) support.
> Product
> All products that support ICSR
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> srp initiate-switchover [ post-processing-timeout | reset-route-modifier | timeout seconds ] [ -noconfirm ]
> post-processing-timeout
> Specifies the timeout value in seconds to initiate the post-switchover process. The value must be an integer from 0 through 3600.
> reset-route-modifier
> During a switchover, reset the route-modifier to the initial value.
> timeout seconds
> Default: 300
> Specifies the number of seconds before a forced switchover occurs. seconds must be a value in the range from 0 through 65535.
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Usage
> This command executes a forced switchover from active to inactive. The command must be executed on the active system and switches the active system to the inactive state and the inactive system to an active state.
> Example
> The following initiates a switchover in 30 seconds.
> srp initiate-switchover timeout 30
> srp reset-auth-probe-fail
> This command resets the authentication probe monitor failure information.
> Product
> All products that support Interchassis Session Recovery (ICSR)
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> srp reset-auth-probe-fail
> Usage
> This command resets the auth probe monitor failure information to 0.
> srp terminate-post-process
> This command forcibly terminates the post-switchover of primary and backup systems configured for Interchassis Session Recovery (ICSR) support.
> Product
> All products that support ICSR
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> srp terminate-post-process [ -noconfirm ]
> -noconfirm
> Indicates that the command is to execute without any additional prompt and confirmation from the user.
> Usage
> Use this command to force the termination of post-switchover process.
> Example
> srp terminate-post-process
> srp validate-configuration
> Initiates a configuration validation check from the ACTIVE chassis.
> Product
> All products that support Interchassis Session Recovery (ICSR)
> Privilege
> Security Administrator, Administrator
> Syntax
> srp validate-configuration
> Usage
> Validates the configuration for an active chassis.
> ssh
> Connects to a remote host using a secure interface.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> ssh { host_name | host_ip_address } [ port port_num ] [ user user_name ]
> host_name | host_ip_address
> Identifies the remote node to attempt to connect to.
> host_name: specifies the remote node using the node’s logical host name which must be resolved via DNS lookup.
> host_ip_address: specifies the remote node using the node’s assigned IP address specified using the standard IPv4 dotted decimal notation.
> port port_num
> Specifies a specific port to connect to where port_num must be a value in the range 1025 through 10000.
> user user_name
> Specifies a user name to attempt to connect as.
> Usage
> SSH connects to a remote network element using a secure interface.
> Example
> The following connects to remote host remoteABC as user user1.
> ssh remoteABC user user1
> The following connects to remote host 1.2.3.4 without any default user.
> ssh 1.2.3.4
> The following connects to remote host 1.2.3.4 via port 2047 without any default user.
> ssh 1.2.3.4 port 2047
> start crypto security-association
> Initiates Internet Key Exchange (IKE) negotiations.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> start crypto security-association cryptomap
> cryptomap
> This is the name of the crypto map policy to use when starting the IKE negotiations. cryptomap must be the name of an existing crypto map entered as an alphanumeric string from 1 to 127 characters.
> Usage
> Use this command to start IKE negotiations for IPSEC.
> Example
> The following command starts the IKE negotiations using the parameters set in the crypto map named crytpomap1:
> start crypto security-association cryptomap1
> system
> These commands configure information about the system, accessible by the SNMP agent.
> Product
> P-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> system { carrier-id mcc mcc_num mnc mnc_num | contact name | description description | hostname name | location location }
> default system { contact | description | hostname | location }
> no system carrier-id
> carrier-id mcc mcc_num mnc mnc_num
> Specifies the system’s Carrier ID via the three-digit MCC (mobile country code) and three-digit MNC (mobile network code).
> contact name
> Specifies the system’s contact name. name must be an alphanumeric string from 0 to 255 characters.
> description description
> System description that will accept both text and some parameters, to include:

> • | %version% - software version

> • | %build% - software build number

> • | %chassis% - chassis type (“asr5000”)

> • | %staros% - ID of the kernel revision

> • | %ostype% - os type

> • | %hostname% - system name

> • | %release% - release

> • | %kerver% - kernel version

> • | %machine% - machine hardware name

> description must be an alphanumeric string from 1 to 255 characters.
> Default: “%ostype% %hostname% %release% %kerver% %machine%”
> After replacing the parameters with values, the string will be truncated if the length is greater than 255.
> hostname name
> Specifies the system’s host name (name of system). name must be an alphanumeric string from 1 to 63 characters.
> location location
> Specifies the system’s geographic or referenced location. location must be an alphanumeric string from 0 to 255 characters.
> default system { contact | description | hostname | location }
> Sets/restores the default value assigned for specified parameter.
> no system carrier-id
> Removes the Carrier ID identified for the system.
> Usage
> Use this command to configure information about the system that is accessible by the SNMP agent.
> Example
> The following command identifies the system’s location as boston:
> system location boston

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883