> show ims-authorization
> This chapter describes the outputs of the show ims-authorization command.
> show ims-authorization policy-control statistics
> show ims-authorization policy-control statistics Command Output Descriptions

> Field | Description
> DPCA Session Stats
> Total Current Sessions | The total number of DPCA session currently running on this system.
> Total IMSA Adds | The total number of IP multimedia subsystem applications (IMSAs) added to service.
> Total DPCA Starts | The total number of Diameter Policy Control Applications (DPCAs) started.
> Total Secondary Create | The total number of secondary contexts created.
> Total Secondary Terminate | The total number of secondary contexts deleted.
> Total Session Updates | The total number of updates applied for session/s.
> Total Terminated | The total number of Diameter Policy Control Application sessions terminated.
> DPCA Sessions Failovers | The total number of Diameter Policy Control Application sessions failed.
> DPCA Message Stats
> Total messages Received | Total policy control messages received for IMS authorization policy control.
> Total Messages Sent | Total messages sent to IMS authorization policy control server.
> Total CCR | Total Credit Control Request (CCR) messages received.
> Total CCA | Total Credit Control Answer (CCA) messages sent in response to CCRs.
> CCR-Initial | Total number of initial CCR messages received.
> CCA-Initial | Total number of initial CCA messages sent in response to initial CCR messages.
> CCA-Initial Accept | Total number of initial CCA messages accepted in response to initial CCR messages.
> CCA-Initial Reject | Total number of initial CCA messages rejected in response to initial CCR messages.
> CCA-Initial Timeouts | Total number of initial CCA messages timed out in response to initial CCR messages.
> CCR-Update | Total number of Credit Control Request (CCR) messages received after initial CCR for update.
> CCA-Update | Total Credit Control Answer (CCA) messages sent in response to update CCRs.
> CCA-Update Timeouts | Total Credit Control Answer (CCA) messages sent in response to update CCRs but timed out.
> CCA-Update Errors | Total number of errors in parsing the CCA-Update Message.
> CCR-Final | Total number of final CCR messages received to end application.
> CCA-Final | Total number of final CCA messages sent in response to final CCR messages to end session/s.
> CCA-Final Timeouts | Total number of final CCA messages sent in response to final CCR messages to end session/s but timed out.
> CCA-Final Errors | Total number of errors in parsing the CCA-Terminate Message.
> ASR | Total number of Abort-Session-Requests (ASRs) received.
> ASA | Total number of Abort-Session-Accept (ASA) messages sent in response to Abort-Session-Requests (ASRs).
> RAR | Total number of Re-Auth-Requests (RARs) received for re-authorization.
> RAA | Total number of Re-Auth-Requests (RARs) answered with Re-Auth-Answer (RAA) message.
> DPCA Message Error Stats
> Diameter Protocol Errs | Total number of errors related to Diameter protocol.
> Bad Answers | Total number of errors related to invalid response/answers.
> Unknown Session Reqs | Total number of errors related to unknown session requests.
> Unknown Command Code | Total number of errors related to unknown command codes.
> Unsupported Command Code | Total number of errors related to unsupported command codes.
> Unk Failure Handling | Total number of errors related to unknown handling of failures.
> DPCA Termination Cause Stats
> Diameter Logout | Total number of DPCA session termination due to Diameter logout.
> Service Not Provided | Total number of DPCA session termination due to unavailability of service.
> Bad Answer | Total number of DPCA sessions terminated due to invalid/bad response reason.
> Administrative | Total number of DPCA sessions terminated due to administrative reasons.
> Link Broken | Total number of DPCA sessions terminated due to link broken.
> Auth Expired | Total number of DPCA sessions terminated due to authorization expired.
> User moved | Total number of DPCA sessions terminated as subscriber/user moved to unknown/non-service area.
> Session Timeout | Total number of DPCA sessions terminated due to timed out reason.
> Auth Rejected | Total number of DPCA sessions terminated due to authorization rejected.
> Other Errors | Total number of DPCA sessions terminated due to unknown reasons or reasons not listed in this list.
> DPCA Experimental Result Code Stats: | Statistics of the number of times the specific Experimental-Result-Code value was received in the Diameter Gx Credit-Control-Answer (CCA) from the PCRF per IMSA service.
> Error Initial Parameters | The number of times DIAMETER_ERROR_INITIAL_PARAMETERS (5140) Experimental-Result-Code value was received in the Diameter Gx CCA.
> Error Trigger Event | The number of times DIAMETER_ERROR_TRIGGER_EVENT (5141) Experimental-Result-Code value was received in the Diameter Gx CCA.
> Bearer Not Authorized | The number of times DIAMETER_ERROR_BEARER_NOT_AUTHORIZED (5143) Experimental-Result-Code value was received in the Diameter Gx CCA.
> Traffic Mapping Rejected | The number of times DIAMETER_ERROR_TRAFFIC_MAPPING_INFO_REJECTED (5144) Experimental-Result-Code value was received in the Diameter Gx CCA.
> PCC Rule Event | The number of times DIAMETER_PCC_RULE_EVENT (5142) Experimental-Result-Code value was sent in the Diameter Gx Re-Auth-Request (RAR).
> Confecting Request | This error is used when the PCRF cannot accept the UE-initiated resource request as a network-initiated resource allocation is already in progress with packet filters that cover the packet filters in the received UE-initiated resource request.
> Bearer Event | This error is used when a PCC rule for some reason cannot be enforced or modified successfully in a network initiated procedure.
> Base Result Code | The number of times an unknown Experimental-Result-Code value (apart form the ones recognized in CCA that are listed above PCC Rule Event) was received in the Diameter CCA.
> Session Release Cause
> Unspecified Reason | The total number of sessions released due to unspecified reasons.
> UE Subscription Changed | The total number of sessions released due to a change in the UE subscription.
> Insuffcnt Srvr Resource | The total number of sessions released due to insufficient server resources.
> DPCA Failure Handling Stats
> Connection Based FH
> Total Message Timeouts | Total number of response message timeouts, i.e. PCRF failed to respond within the configured timeout value.
> CCA-Initial | Response to the CCR-I message was timed out.
> CCA-Update | Response to the CCR-U message was timed out.
> CCA-Terminate | Response to the CCR-T message was timed out.
> Total Message Send Errs | Total number of requests failed to be sent due to socket based send errors.
> CCR-Initial | CCR-I failed to be sent due to socket based errors.
> CCR-Update | CCR-U failed to be sent due to socket based errors.
> CCR-Terminate | CCR-T failed to be sent due to socket based errors.
> Result Code Based FH |
> Configured Result Code | Failure handling being undertaken due to configured result code range.
> CCA-Initial | Failure handling being undertaken due to configured result code range for CCA-Initial messages.
> CCA-Update | Failure handling being undertaken due to configured result code range for CCA-Update messages.
> CCA-Terminate | Failure handling being undertaken due to configured result code range for CCA-Terminate messages.
> Unh and Unk Result Code | Failure handling being undertaken due to a result code which is neither defined in the diameter or customer specs.
> CCA-Initial | Failure handling being undertaken due to unknown result code for CCA-Initial messages.
> CCA-Update | Failure handling being undertaken due to unknown result code for CCA-Update messages.
> CCA-Terminate | Failure handling being undertaken due to unknown result code for CCA-Terminate messages.
> FH Behavior
> Continue | Total number of times the failure handling action continue has been undertaken.
> Retry-And-Terminate | Total number of times the failure handling action retry-and-terminate has been undertaken.
> Terminate | Total number of times the failure handling action terminate has been undertaken.
> Peer Switches
> Attempted Switches | Total number of peer switches attempted.
> Successful Switches | Total number of peer switches successful.

> ‌
> show ims-authorization policy-gate status full
> Important: This command is no longer an option in StarOS release 11.0 and beyond.
> show ims-authorization policy-gate status full Command Output Descriptions

> Field | Description
> CallID | Specifies Call Identifier.
> IMSI | Specifies International Mobile Subscriber Identity (IMSI) of subscriber.
> NSAPI | Specifies Network Service Access Point Identifier (NSAPI) to a single PDP context of the subscriber.
> Charging Rule | Specifies dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Precedence | Displays the precedence of the dynamic charging rule applicable to specific flow.
> Flow Status | Specifies the status of flow with specific charging rule. Possible states are:
> • | Open
> • | Closed
> • | Dormant
> Flow Dir | Specifies the direction of flow with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service. Possible states are:
> • | Uplink
> • | Downlink
> Source Addr | Specifies the source IP address of flow with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Source Addr Mask | Specifies the masking of source IP address of flow with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Destination Addr | Specifies the destination IP address of flow with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Destination Addr Mask | Specifies the masking of destination IP address of flow with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Source Port | Specifies the IP port of flow origin with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Destination Port | Specifies the destination IP port of flow end with specific dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.

> ‌
> show ims-authorization policy-gate counters all
> Important: This command is no longer an option in StarOS release 11.0 and beyond.
> show ims-authorization policy-gate counters all Command Output Descriptions

> Field | Description
> CallID | Specifies Call Identifier.
> IMSI | Specifies International Mobile Subscriber Identity (IMSI) of subscriber.
> NSAPI | Specifies Network Service Access Point Identifier (NSAPI) to a single PDP context of the subscriber.
> Charging Rule | Specifies dynamic charging rule applicable for specific flow through a policy gate in IMS authorization service.
> Gate State changed | Displays the change state of policy gate for specific subscriber flow. Possible values are:
> • | 0: No change
> • | 1: Changed
> Uplink Pkts Statistics | Displays the statistics of packets in uplink direction.
> Downlink Pkts Statistics | Displays the statistics of packets in downlink direction.
> Pkts processed | Displays the total number of packets received and processed.
> Bytes processed | Displays the total number of bytes received and processed.
> Pkts dropped | Displays the total number of packets received but dropped.
> Bytes dropped | Displays the total number of bytes received but dropped.

> ‌
> show ims-authorization servers
> show ims-authorization servers ims-auth-service Command Output Descriptions

> Field | Description
> Service Name | IMS authorization service name.
> IMS Authorization Server | IMS authorization server name.
> Server Type | IMS Authorization server type. It may be Policy, Charging, or both.
> PCRF host | Identifies the Policy Control and Charging Rules Function (PCRF) host.
> Operational State | Indicates operational state of the authorization server.
> Server Session State | Indicates authorization server session state.
> Server Statistics | Indicates authorization server session statistics.
> Session Active | Total number of active authorization server sessions.
> Session Opened | Total number of opened authorization server sessions.
> Session Closed | Total number of closed authorization server sessions.
> Sessions switched due to Tx Expiry | Total number of sessions switched due to transmission expiry.
> Sessions switched due to reselection | Total number of sessions switched due to re-selection of authorization servers.
> Server Up -> down indications | Total number of servers going to down state from up state.
> Total servers matching specified criteria | Total number of servers matching the specified criteria.

> ‌
> show ims-authorization service name
> show ims-authorization service name Command Output Descriptions

> Field | Description
> IMS Authorization Service Name | Name of IMS authorization service name.
> Context | Name of the context in which IMS authorization service is configured.
> Service State | State of the IMS authorization service.
> Service mode | Mode of IMS authorization service for policy and charging.
> Binding Mechanism | Describes the mechanism on the control of bearer resources based on a binding mechanism that binds one or more service to a bearer.
> QoS Update Timeout | Specifies the timeout duration in seconds to discard QoS update request. NOTE: QoS Update Timeout is no longer shown in StarOS release 11.0 and beyond.
> Reauth Trigger | Specifies the Re-authorization trigger’s status.
> P-CSCF Discovery | Specifies the configured route-table applicable for Proxy-Call Session Control Function (P-CSCF) discovery.
> P-CSCF Selection Table[ n ] | Specifies the configured selection table information for Proxy-Call Session Control Function (P-CSCF) server selection. [n] indicates the selection table number.
> Diameter Policy Control Specifies Diameter Policy Control related configuration and information.
> Endpoint | Specifies Diameter endpoint name for Diameter Policy Control.
> Origin-Realm | Specifies Diameter origin domain name for Diameter Policy Control.
> Dictionary | Specifies the configured applicable dictionary for Diameter Policy Control.
> Update-Dictionary-Avps | Indicates whether the 3GPP Rel. 8 AVPs or 3GPP Rel. 9 AVPs are selected for encoding.
> Request Timeout | Indicates the configured request timeout value.
> Reauth Trigger | Indicates the re-authorization trigger status.
> Custom Reauth Trigger | Indicates enabled custom reauth event triggers.
> Failure Handling | Specifies the configured mechanism for failure handling in Diameter Policy Control.
> Peer Switch | Specifies the status of Peer switching for in Diameter Policy Control.
> Host Selection | Specifies host selection mechanism with selection table.
> Host Reselection Subscriber Limit | Specifies the limit of subscriber bind to specific host origin to trigger re-selection of host.
> Host Reselection Interval | Specifies time interval to trigger host re-selection for subscriber.
> Host Selection Table[ n ] | Specifies the configured selection table information for host server selection. [n] indicates the selection table number.
> Precedence | Specifies the precedence applicable.
> Primary Host | Specifies the primary name/IP address the host.
> Secondary Host | Specifies the secondary name/IP address of the host.

> ‌
> show ims-authorization sessions full all
> show ims-authorization sessions full all Command Output Descriptions

> Field | Description
> CallId | The call identifier.
> Service Name | The IMS authorization service name.
> IMSI | The International Mobile Subscriber Identity (IMSI) of subscriber.
> Session ID | The session ID is of type UTF8String and is used to identify a specific session.
> NSAPI | The Network Service Access Point Identifier (NSAPI) to a single PDP context of the subscriber.
> Bearer Usage | Indicates the bearer usage for this session.
> Bearer Type | Indicates the bearer type.
> Bearer ID | Indicates the bearer identifier.
> Context Type | Indicates the PDP context Type: Primary or Secondary.
> SGSN IP-Addr | IP address of the SGSN node.
> APN | Indicates the Access Point Name (APN) for this service.
> Bearer Control Mode | The bearer control mode: UE/NW
> State | Indicates the session state.
> Primary PCRF Server | The primary Policy Control and Charging Rules Function (PCRF) server host name.
> Secondary PCRF Server | The secondary PCRF server host name.
> Primary P-CSCF | The primary Proxy-Call Session Control Function gateway address.
> Secondary P-CSCF | The secondary P-CSCF gateway address.
> UE IP Address
> UE IP Session Type | Specifies the type of the address assigned to the user. The possible valid values are IPv4, IPv6 and IPv4_IPv6.
> IPv4 Address | Displays the IPv4 address assigned to the user.
> IPv6 Address | Displays the IPv6 address assigned to the user.
> Primary OCS
> Hostname | Specifies the Primary-Event-Charging-Function-Name of type DiameterURI, or the address of primary online charging system.
> Port | The port associated with the primary OCS.
> Protocol | The protocol associated with the primary OCS.
> Secondary OCS
> Hostname | Specifies the Secondary-Event-Charging-Function-Name of type DiameterURI, or the address of secondary online charging system.
> Port | The port associated with the secondary OCS.
> Protocol | The protocol associated with the secondary OCS.
> Primary CCF
> Hostname | Specifies the Primary-Charging-Collection-Function-Name of type DiameterURI or the address of primary offline charging system for the bearer.
> Port | The port associated with the primary CCF.
> Protocol | The protocol associated with the primary CCF.
> Secondary CCF
> Hostname | Specifies the Secondary-Charging-Collection-Function-Name of type DiameterURI or the address of secondary offline charging system for the bearer.
> Port | The port associated with the secondary CCF.
> Protocol | The protocol associated with the secondary CCF.
> Auth Decision | Parameters configured for authorization decision.
> Event Triggers | Triggers for different events for Authorization decision.
> Event Report Indication | Specifies which type of changes will trigger an event report from the PCRF.
> QoS Policy | Specifies QoS policy for specific session.
> QoS Class | The QoS class applicable to this session.
> Max Uplink Bw(in bps) | The maximum bandwidth for uplink direction, in bps.
> Max Downlink Bw(in bps) | The maximum bandwidth for downlink direction, in bps.
> Guaranteed Uplink Bw(in bps) | The guaranteed bandwidth for uplink direction, in bps.
> Guaranteed Downlink Bw(in bps) | The guaranteed bandwidth for downlink direction, in bps.
> Apn Uplink AMBR(in bps) | The APN uplink AMBR, in bps.
> Apn Downlink AMBR(in bps) | The APN downlink AMBR, in bps.
> Charging Rules | Dynamic charging rule applicable for specific session in IMSA service. NOTE: Charging Rules are no longer shown in StarOS release 11.0 and beyond.
> Rule Name | Name of the applicable dynamic charging rule.
> Precedence | Precedence of the applicable dynamic charging rule.
> Revalidation Time | Specifies the time at which the next CCR-U will be sent out for the Re-validation Timeout EVENT TRIGGER.
> Session Packet Statistics | Specifies the session data statistics. NOTE: Session Packet Statistics are no longer shown in StarOS release 11.0 and beyond.
> Uplink Pkt Processed | Total number of packets processed in uplink direction.
> Uplink Bytes Processed | Total number of bytes processed in uplink direction.
> Uplink Pkt Dropped | Total number of packets dropped or not processed in uplink direction.
> Uplink Bytes Dropped | Total number of bytes dropped or not processed in uplink direction.
> Downlink Pkt Processed | Total number of packets processed in downlink direction.
> Downlink Bytes Processed | Total number of bytes processed in downlink direction.
> Downlink Pkt Dropped | Total number of packets dropped or not processed in downlink direction.
> Downlink Bytes Dropped | Total number of bytes dropped or not processed in downlink direction.
> Total sessions matching specified criteria | The total number of sessions matching the specified criteria.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883