> CSCF Diameter Selection Configuration Mode Commands
> The Diameter Selection Configuration Mode is used to configure AAA group selection criteria that will be used for all HSS interactions for a subscriber.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> aaa-group
> Configures AAA group selection criteria.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> [ no ] aaa-group name criteria { source aor aor_prefix | subscriber-capability { audio [ only ] | text | video } | subscriber-ip-type { v4 | v6 } } +
> no
> Removes configured criteria.
> name
> Specifies a name for the AAA group criteria.
> name must be from 1 to 63 alpha and/or numeric characters.
> criteria
> Specifies AAA group selection criteria.
> source aor aor_prefix
> Filters based on the source AoR.
> aor_prefix must be an existing AoR from 1 to 79 characters in length.
> Important: AoR regular expressions are supported. Refer to the SCM Engineering Rules Appendix in the Cisco ASR 5000 Series Session Control Manager Administration Guide for more information about regular expressions.
> subscriber-capability { audio [ only ] | text | video }
> Filters based on the capability of the subscriber.
> audio [ only ]: audio capability only
> text: text capability type
> video: video capability type
> subscriber-ip-type { v4 | v6 }
> Filters based on the IP type of the subscriber.
> v4: IPv4 type
> v6: IPv6 type
> +
> This symbol indicates that the keywords can be entered multiple times within a single command.
> Usage
> This command configures matching criteria for selecting a AAA group name. When a subscriber registers, the selection criteria are compared and the AAA group name from the matching entry will be picked up. The selected AAA group will be used for all HSS interactions for that subscriber.
> Example
> The following command creates AAA group criteria named aaa1 with a destination AoR of $.@abc123.com:
> aaa-group aaa1 criteria source aor $.@abc123.com
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883