> Closed R-P Schema Statistics
> The Closed R-P schema provides operational statistics that can be used for monitoring and troubleshooting the following products: PDSN
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the Closed R-P Service Schema

> Variables | Description | Data Type
> vpnname | Description: The name of the context configured on the system that is currently facilitating the Closed R-P PDSN service. This is a key variable. | String
> vpnid | Description: The identification number of the context configured on the system that is currently facilitating the Closed R-P PDSN service. This is an internal reference number. This is a key variable. | Int32
> servname | Description: Displays the name of the Closed R-P PDSN service for which the statistics are displayed. This is a key variable. | String
> tun-conn-attempt | Description: This proprietary counter indicates the total number of tunnel connection attempts. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-conn-success | Description: This proprietary counter indicates the total number of successful tunnel connections Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-conn-fail | Description: This proprietary counter indicates the total number of failed tunnel connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-conn-curactive | Description: This proprietary counter indicates the total number of currently active tunnel connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-attempts | Description: This proprietary counter indicates the total number of session connection attempts. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-successful | Description: This proprietary counter indicates the total number of successful session connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-failed | Description: This proprietary counter indicates the total number of failed session connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-curactive | Description: This proprietary counter indicates the total number of currently active session connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | int2
> sess-intrapdsnho-attempt | Description: This proprietary counter indicates the total number of Intra-PDSN Hand-Offs connection attempts Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-intrapdsnho-success | Description: This proprietary counter indicates the total number of successful Intra-PDSN Hand-Offs connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-intrapdsnho-failed | Description: This proprietary counter indicates the total number of failed Intra-PDSN Hand-Offs connections. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-interpdsnho-attempt | Description: This proprietary counter indicates the total number of Inter-PDSN Hand-Offs connection attempts. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-malformed | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to malformed packets. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-ctrlfield | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to control field errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-pktlen | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to packet length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-avplen | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to AVP length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-protover | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to protocol version errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-md5 | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to MD5 errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-invattr | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to invalid attribute errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-unkattr | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to unknown attribute errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-invsessid | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to invalid session ID errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-invstate | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to invalid state errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-unkmsg | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to unknown message errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-unmatchpktlen | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to unmatched packet length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> recv-err-invtunid | Description: This proprietary counter indicates the total number of Tunnel Receive Control Packet errors experienced due to invalid tunnel length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-genclear | Description: This proprietary counter indicates the total number of tunnels cleared normally. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-ctrlconnexists | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to a pre-existing control connection. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-unauth | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to unauthorized errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-badproto | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to bad protocol errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-reqshutdown | Description: This proprietary counter indicates the total number of tunnel disconnects experienced due to requester shutdown. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-statemacherr | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to state machine errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-badlen | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to wrong length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-oor | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to out-of-range errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-noresource | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to insufficient resources. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-vendspec | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to vendor-specific errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-tryanotherlns | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced resulting in “Try Another LNS” message generation. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-unkavp | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to unknown AVP with M-bit errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-ipsecdisc | Description: This proprietary counter indicates the total number of tunnel disconnects experienced due to IPSEC. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-ipsecfail | Description: This proprietary counter indicates the total number of tunnel failures experienced due to IPSEC. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-license | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to license exceeded errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-newcallpoldisc | Description: This proprietary counter indicates the total number of tunnel disconnects experienced due to new call policies. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-maxretry | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to the maximum number of retries being exceeded. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-syslimit | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to reaching the system tunnel limit. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> tun-miscerr | Description: This proprietary counter indicates the total number of tunnel disconnects/failures experienced due to miscellaneous errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-nogeneral | Description: This proprietary counter indicates the total number of sessions for which there were no general errors experienced. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-admin | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to administrative reasons. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-lossofcarr | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to loss of carrier. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-remoteadmin | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to remote administrative reasons. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-nofactemp | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to temporary no facility available errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-nofacperm | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to permanent no facility available errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-invdest | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to invalid destination errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-nocarrier | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due no carrier being detected. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-busysig | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to receipt of a busy signal. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-nodialtime | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to receipt of no dial tone. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-lactimeout | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to LAC timeout. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-noframing | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to no appropriate framing. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-noctrlconn | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to no control connection existing. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-badlen | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to wrong length errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-oor | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to out-of-range errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-noresource | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to insufficient resources. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-invsessid | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to an invalid session ID. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-vendspec | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to vendor specific errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-tryanotherlns | Description: This proprietary counter indicates the total number of session disconnects/failures experienced resulting in “Try Another LNS” message generation. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-unkavp | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to unknown AVP with M-bit errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-maxtunnel | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to reaching the maximum tunnel limit. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-ipsecfail | Description: This proprietary counter indicates the total number of session failures experienced due to IPSEC. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-ipsecdisc | Description: This proprietary counter indicates the total number of session disconnects experienced due to IPSEC. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-newcallpoldisc | Description: This proprietary counter indicates the total number of session disconnects experienced due to new call policies. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-license | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to license exceeded errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-servmismatch | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to service mismatch errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-miscerr | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to miscellaneous errors. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-hocomplete | Description: This proprietary counter indicates the total number of session disconnects experienced due to handoff completions. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-invho | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to invalid handoffs. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> sess-duplsess | Description: This proprietary counter indicates the total number of session disconnects/failures experienced due to duplicate sessions. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> ttlprepaid | Description: This proprietary counter indicates the total number of Prepaid calls facilitated by the service. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> curprepaid | Description: This proprietary counter indicates the total number of Prepaid calls currently being facilitated by the service. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> ttlonlineauthsucc | Description: This proprietary counter indicates the total number of successful Online Authentications for the service. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> ttlonlineauthfail | Description: This proprietary counter indicates the total number of successful Online Authentications for the service. Availability: per Closed-RP PDSN service, per PCF, per session Type: Counter | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883