> MME Service Configuration Mode Commands
> The MME Service Configuration Mode is used to create and manage the LTE Mobility Management Entity (MME) services for the LTE/SAE network. This service works in conjunction with MME-HSS Service and eGTP Service.
> associate
> This command associates/disassociates the supportive services and policies like an Evolved GPRS Tunnelling Protocol (eGTP) service, an HSS peer service, or an MME policy subscriber map with an MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> associate { { egtp-service egtp_svc_name | egtp-sv-service egtp_sv_svc_name | hss-peer-service hss_svc_name | lte-emergency-profile profile_name | network-global-mme-id-mgmt-db | sctp-param-template template_name | sgs-service sgs_svc_name | sgtpc-service sgtpc_svc_name } [ context ctx_name ] | subscriber-map map_name | tai-mgmt-db database_name }
> no associate { egtp-service | egtp-sv-service | hss-peer-service | lte-emergency-profile | network-global-mme-id-mgmt-db | sctp-param-template | sgs-service | sgtpc-service | subscriber-map | tai-mgmt-db }
> no
> Disassociates a previously associated service with this MME service.
> egtp-service egtp_svc_name
> Associates an eGTP service with MME service.
> egtp_svc_name specifies the name for a pre-configured eGTP service to associate with the MME service. For more information on the eGTP service, refer to the egtp-service command in the Context Configuration Mode Commands chapter.
> egtp-sv-service egtp_sv_svc_name
> Associates an eGTP Sv service with MME service.
> egtp_sv_svc_name specifies the name for a pre-configured eGTP Sv service to associate with the MME service. For more information on the eGTP Sv service, refer to the egtp-service command in the Context Configuration Mode Commands chapter.
> hss-peer-service hss_svc_name
> Associates an HSS peer service with this MME service.
> hss_svc_name specifies the name for a pre-configured HSS peer service to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information about the HSS peer service, refer to the hss-peer-service command in the Context Configuration Mode Commands chapter and refer to the HSS Peer Service Configuration Mode Commands chapter.
> lte-emergency-profile profile_name
> Associates an LTE emergency profile with this MME service.
> profile_name specifies the name for a pre-configured LTE emergency profile to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information about the LTE emergency profile, refer to the lte-emergency-profile command in the LTE Policy Configuration Mode Commands chapter and refer to the LTE Emergency Profile Configuration Mode Commands chapter.
> network-global-mme-id-mgmt-db
> Associates the configured global MME ID management database with the MME service. The global MME ID management database is configured through the LTE Policy Configuration Mode using the network-global-mme-id-mgmt-db command.
> sctp-param-template template_name
> Associates an SCTP parameter template with the MME service.
> template_name specifies the name for a pre-configured SCTP parameter template to associate with this MME service and must be from 1 to 63 alpha and/or numeric characters. For more information on the SCTP parameter template, refer to the sctp-param-template command in the Global Configuration Mode Commands chapter and refer to the SCTP Parameter Template Configuration Mode Commands chapter.
> sgs-service sgs_svc_name
> Associates an SGs service with this MME service.
> sgs_svc_name specifies the name for a pre-configured SGs service to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information on the SGs service, refer to the sgs-service command in the Context Configuration Mode Commands chapter and refer to the MME SGs Service Configuration Mode Commands chapter.
> sgtpc-service sgtpc_svc_name
> Associates an SGTPC service with this MME service.
> sgtpc_svc_name specifies the name for a pre-configured SGTPC service to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information on the SGTPC service, refer to the sgtp-service command in the Context Configuration Mode Commands chapter and/or refer to the SGTP Service Configuration Mode Commands chapter.
> context ctx_name
> Identifies a specific context name where the named service is configured. If this keyword is omitted, the named service must exist in the same context as the MME service.
> ctx_name is name of the configured context of the named service. This can be from 1 to 63 alpha and/or numeric characters and is case sensitive.
> subscriber-map map_name
> Associates this MME service with a pre-configured subscriber map.
> map_name specifies the name of a pre-configured subscriber map to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information on subscriber maps, refer to the subscriber-map command in the LTE Policy Configuration Mode Commands chapter and refer to the LTE Subscriber Map Configuration Mode Commands chapter.
> tai-mgmt-db database_name
> Associates this MME service with a pre-configured TAI Management Database.
> database_name specifies the name of a pre-configured TAI Management Database to associate with the MME service and must be from 1 to 64 alpha and/or numeric characters. For more information on subscriber maps, refer to the tai-mgmt-db command in the LTE Policy Configuration Mode Commands chapter and refer to the LTE TAI Management Database Configuration Mode Commands chapter.
> Usage
> Use this command to associate a pre-configured service or policy with an MME service.
> The eGTP service provides eGTP-C protocol interface support between EPS nodes. For more information on the eGTP service and the supported interface type, refer to the eGTP Service Configuration Mode Commands chapter.
> Important: Only one eGTP service can be associated with a service. The eGTP service should be configured prior to issuing this command.
> The HSS peer service provides S6a and S13 interface support via the Diameter protocol between the MME and an HSS (S6a) or EIR (S13). For more information on HSS peer service and other parameters, refer to the HSS Peer Service Configuration Mode Commands chapter.
> Important: Only one HSS peer service can be associated to a service in this release. The HSS peer service should be configured prior to issuing this command.
> Caution: This is a critical configuration. The MME service can not be started without this configuration. Any change to this configuration would lead to restarting the MME service. Removing or disabling this configuration will stop the MME service.
> Example
> The following command associates a pre-configured eGTP service called egtp1 in the dst_ctx context to an MME service:
> associate egtp-service egtp1 context dst_ctx
> The following command associates a pre-configured HSS peer service called hss1 in the same context as MME service to an MME service:
> associate hss-peer-service hss1
> bind s1-mme
> This command binds the MME service to a logical IP interface serving as the S1-MME interface.
> Product
> MME
> Privilege
> Administrator
> Syntax
> bind s1-mme { ipv4-address address [ ipv4-address secondary_address ] | ipv6-address address [ ipv6-address secondary_address ] } [ crypto-template name ] [ max-subscribers number ]
> no bind s1-mme
> no
> Removes a previously configured IP address used for binding the SCTP (local bind address) to communicate with the eNodeBs using an S1-MME interface.
> { ipv4-address address [ ipv4-address secondary_address ] | ipv6-address address [ ipv6-address secondary_address ] }
> Specifies the IP address in IPv4 or IPv6 notation for the interface configured as an S1-MME interface. For IPv4, address must be specified in dotted decimal notation. For IPv6, address must be specified in colon separated notation. Optionally configure a secondary IP address for either address type.
> crypto-template name
> Specifies the crypto template name used when implementing IP Security (IPSec) on the S1-MME interface. name must be an existing crypto template name and be from 1 to 104 alpha and/or numeric characters.
> max-subscribers number
> Specifies the maximum number of subscribers that can access this service on this interface. number must be an integer from 0 and 4,000,000.
> Usage
> Use this command to associate or tie the MME service to a specific logical IP address that will be used for binding the SCTP socket to communicate with the eNodeB using S1AP. A maximum of one IP address can be configured with this command for one MME service.
> The MME passes the IP address during setting up the SCTP association with the eNodeB.
> Caution: This is a critical configuration. The MME service can not be started without this configuration. Any change to this configuration would lead to restarting the MME service and removing or disabling this configuration will stop the MME service.
> Important: Up to two IPv4 or IPv6 addresses can be configured to support SCTP multi-homing.
> Example
> The following command would bind the logical IP interface with the address of 192.168.3.1 to the MME service to interact with eNodeB:
> bind s1-mme ipv4-address 192.168.3.1
> The following command disables a binding that was previously configured:
> no bind s1-mme ipv4address
> dns
> This command associates/disassociates the Domain Name System (DNS) client service configured for DNS query in a context to select P-GW and S-GW in an MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> dns { peer-mme | peer-sgsn | pgw | sgw } [ context ctx_name ]
> no dns { peer-mme | pgw | sgw }
> no
> Disassociates a previously associated context having DNS client service configured for DNS query to select peer MME, P-GW or S-GW with this MME service.
> peer-mme
> This keyword associates the named context with a DNS client service for DNS query for selecting a peer MME and associating it with this MME service for inter-MME handovers.
> peer-sgsn
> This keyword associates the named context with a DNS client service for DNS query for selecting a peer SGSN and associating it with this MME service for inter-RAT handovers.
> pgw
> This keyword associates the named context with a DNS client service for DNS query for selecting a P-GW and associating it with this MME service.
> sgw
> This keyword associates the named context with a DNS client service for DNS query for selecting an S-GW and associating it with this MME service.
> context ctx_name
> This optional keyword associates the specific context name where DNS client service is configured to select a peer MME, a P-GW and/or an S-GW for this MME service. If this keyword is omitted DNS client service must be configured in the same context as this MME service.
> ctx_name is name of the configured context of the DNS client service. This can be from 1 to 63 alpha and/or numeric characters and is case sensitive.
> Usage
> Use this command to associate a pre-configured context where a DNS client service is configured with an MME service.
> The DNS Client service configured in a context provides the DNS query support to locate peer MMEs, peer-SGSNs, P-GWs, or S-GWs from an MME service. For more information on DNS Client service and support, refer to the DNS Client Service Configuration Mode Commands chapter in the Command Line Interface Reference.
> A maximum of one DNS client service for a peer MME, one DNS client service for a peer SGSN, one DNS client service for a P-GW, and one DNS client service for S-GW can be associated with an MME service.
> Example
> The following command associates a pre-configured context dns_ctx1 where a DNS client service is configured for DNS query to P-GW from an MME service:
> dns pgw context dns_ctx1
> The following command associates a pre-configured context dns_ctx2 where a DNS client service is configured for DNS query to S-GW from an MME service:
> dns sgw context dns_ctx2
> emm
> This command defines the Evolved Mobility Management timer parameters like timeout durations for timers for the NAS message retransmission in MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> emm { implicit-detach-timeout detach_dur | mobile-reachable-timeout mob_reach_dur | t3412-timeout t3412_dur | t3413-timeout t3413_dur | t3422-timeout t3422_dur | t3423-timeout t3423_dur | t3450-timeout t3450_dur | t3460-timeout t3460_dur | t3470-timeout t3470_dur }
> default emm { mobile-reachable-timeout | t3412-timeout | t3413-timeout | t3422-timeout | t3423-timeout | t3450-timeout | t3460-timeout | t3470-timeout }
> no emm implicit-detach-timeout
> default
> Resets the specified timer timeout to the system default value.
> no
> Removes the specified EMM timeout definition from the configuration.
> implicit-detach-timeout detach_dur
> Default: 3480
> Sets the timer timeout duration after which subscriber will implicitly detached from the network if there is no activity. Generally this timer value is 240 seconds (4 minutes) more than the timeout value of T3423 timer.
> This timer starts when mobile reachable timer expires while the network is in EMM-IDLE mode and ISR is activated and stops when NAS signalling connection established.
> detach_dur is timeout duration in seconds and must be an integer from 1 through 12000.
> mobile-reachable-timeout mob_reach_dur
> Default: 3480
> Sets the timeout timer duration after which reachability procedure will be discarded and reattempt starts.
> mob_reach_dur is timeout duration in seconds and must be an integer from 1 through 12000.
> t3412-timeout t3412_dur
> Default: 3240
> Sets the timeout duration for T3412 timer. This timer is used for periodic tracking area update (P-TAU). When this timer expires, the periodic tracking area updating procedure starts and the timer is set to its initial value for the next start.
> This timer starts when the UE goes from EMM-CONNECTED to EMM-IDLE mode and stops when the UE enters EMM-CONNECTED mode.
> t3412_dur is timeout duration in seconds and must be an integer from 1 through 11160.
> t3413-timeout t3413_dur
> Default: 6
> Sets the timeout duration for T3413 timer. The timer starts when MME initiates the EPS paging procedure to the EMM entity in the network and requests the lower layer to start paging. This timer stops for the paging procedure when a response received from the UE.
> t3413_dur is timeout duration in seconds and must be an integer from 1 through 20.
> t3422-timeout t3422_dur
> Default: 6
> Sets the timeout duration for T3422 timer. This timer starts when MME initiates the detach procedure by sending a DETACH REQUEST message to the UE and stops upon receipt of the DETACH ACCEPT message.
> t3422_dur is timeout duration in seconds and must be an integer from 1 through 20.
> t3423-timeout t3423_dur
> Default: 3240
> Sets the timeout duration for T3423 timer. This timer starts when UE enters the EMM-DEREGISTERED state or when entering EMM-CONNECTED mode. It stops while the UE is in EMM-REGISTERED.NO-CELL-AVAILABLE state and Idle mode Signalling Reduction (ISR) is activated.
> t3423_dur is timeout duration in seconds and must be an integer from 1 through 11160.
> t3450-timeout t3450_dur
> Default: 6
> Sets the timeout duration for T3450 timer. This timer starts when MME initiates the Globally Unique Temporary Identifier (GUTI) reallocation procedure by sending a GUTI REALLOCATION COMMAND message to the UE and stops upon receipt of the GUTI REALLOCATION COMPLETE message.
> This timer is also used for Tracking area update procedure.
> t3450_dur is timeout duration in seconds and must be an integer from 1 through 20.
> t3460-timeout t3460_dur
> Default: 6
> Sets the timeout duration for T3460 timer. The timers starts when the network initiates the authentication procedure by sending an AUTHENTICATION REQUEST message to the UE and stops upon receipt of the AUTHENTICATION RESPONSE message.
> t3460_dur is timeout duration in seconds and must be an integer from 1 through 20.
> t3470-timeout t3470_dur
> Default: 6
> Sets the timeout duration for T3470 timer. The MME starts this timer when the network initiates the identification procedure by sending an IDENTITY REQUEST message to the UE and stops upon receipt of the IDENTITY RESPONSE message.
> t3470_dur is timeout duration in seconds and must be an integer from 1 through 20.
> Usage
> Use this command to set EMM timers.
> The following tables describe the triggers and states for timers:
> EPS mobility management timers – UE side

> Timer | State | Cause of Start | Normal Stop | On Expiry
> T3402 |
> • | EMM-DEREGISTERED
> • | EMM-REGISTERED
> • | At attach failure and the attempt counter is equal to 5.
> • | At tracking area updating failure and the attempt counter is equal to 5.
> • | ATTACH REQUEST sent
> • | TRACKING AREA UPDATE REQUEST sent
> | Initiation of the attach procedure or TAU procedure
> T3410 | EMM-REGISTERED-INITIATED | ATTACH REQUEST sent |
> • | ATTACH ACCEPT received
> • | ATTACH REJECT received
> | Start T3411 or T3402 as described in subclause 5.5.1.2.6
> T3411 |
> • | EMM-DEREGISTERED. ATTEMPTING-TO-ATTACH
> • | EMM-REGISTERED. ATTEMPTING-TO-UPDATE
> • | At attach failure due to lower layer failure, T3410 timeout or attach rejected with other EMM cause values than those treated in subclause 5.5.1.2.5.
> • | At tracking area updating failure due to lower layer failure, T3430 timeout or TAU rejected with other EMM cause values than those treated in subclause 5.5.3.2.5.
> • | ATTACH REQUEST sent
> • | TRACKING AREA UPDATE REQUEST sent
> | Retransmission of the ATTACH REQUEST or TRACKING AREA UPDATE REQUEST
> T3412 | EMM-REGISTERED | In EMM-REGISTERED, when EMM-CONNECTED mode is left. |
> • | When entering state EMM-DEREGISTERED or
> • | When entering EMM-CONNECTED mode.
> | Initiation of the periodic TAU procedure
> T3416 |
> • | EMM-REGISTERED-INITIATED
> • | EMM-REGISTERED
> • | EMM-DEREGISTERED-INITIATED
> • | EMM-TRACKING-AREA-UPDATING-INITIATED
> • | EMM-SERVICE-REQUEST-INITIATED
> | RAND and RES stored as a result of a UMTS authentication challenge |
> • | SECURITY MODE COMMAND received
> • | SERVICE REJECT received
> • | TRACKING AREA UPDATE ACCEPT received
> • | AUTHENTICATION REJECT received
> • | AUTHENTICATION FAILURE sent
> • | EMM-DEREGISTERED or EMM-NULL entered
> | Delete the stored RAND and RES
> T3417 | EMM-SERVICE-REQUEST-INITIATED |
> • | SERVICE REQUEST sent
> • | EXTENDED SERVICE REQUEST sent in case f and g in subclause 5.6.1.1
> • | Bearers have been set up
> • | SERVICE REJECT received
> | Abort the procedure
> T3417ext | EMM-SERVICE-REQUEST-INITIATED |
> • | EXTENDED SERVICE REQUEST sent in case d in subclause 5.6.1.1
> • | EXTENDED SERVICE REQUEST sent in case e in subclause 5.6.1.1 and the CSFB response was set to “CS fallback accepted by the UE”.
> • | Inter-system change from S1 mode to A/Gb mode or Iu mode is completed
> • | Inter-system change from S1 mode to A/Gb mode or Iu mode is failed
> • | SERVICE REJECT received
> | Abort the procedure
> T3418 |
> • | EMM-REGISTERED-INITIATED
> • | EMM-REGISTERED
> • | EMM-TRACKING-AREA-UPDATING-INITIATED
> • | EMM-DEREGISTERED-INITIATED
> • | EMM-SERVICE-REQUEST-INITIATED
> | AUTHENTICATION FAILURE (EMM cause = #20 “MAC failure” or #26 “Non-EPS authentication unacceptable”) sent | AUTHENTICATION REQUEST received | On first expiry, the UE should consider the network as false
> T3420 |
> • | EMM-REGISTERED-INITIATED
> • | EMM-REGISTERED
> • | EMM-DEREGISTERED-INITIATED
> • | EMM-TRACKING-AREA-UPDATING-INITIATED
> • | EMM-SERVICE-REQUEST-INITIATED
> | AUTHENTICATION FAILURE (cause = #21 “synch failure”) sent | AUTHENTICATION REQUEST received | On first expiry, the UE should consider the network as false
> T3421 | EMM-DEREGISTERED-INITIATED | DETACH REQUEST sent | DETACH ACCEPT received | Retransmission of DETACH REQUEST
> T3423 | EMM-REGISTERED | T3412 expires while the UE is in EMM-REGISTERED.NO-CELL-AVAILABLE and ISR is activated. |
> • | When entering state EMM-DEREGISTERED or
> • | When entering EMM-CONNECTED mode.
> | Set TIN to “P‑TMSI”
> T3430 | EMM-TRACKING-AREA-UPDATING-INITIATED | TRACKING AREA UPDATE REQUEST sent |
> • | TRACKING AREA UPDATE ACCEPT received
> • | TRACKING AREA UPDATE REJECT received
> | Start T3411 or T3402 as described in subclause 5.5.3.2.6
> T3440 |
> • | EMM-REGISTERED-INITIATED
> • | EMM-TRACKING-AREA-UPDATING-INITIATED
> • | EMM-DEREGISTERED-INITIATED
> • | EMM-SERVICE-REQUEST-INITIATED
> • | EMM-REGISTERED
> • | ATTACH REJECT, DETACH REQUEST, TRACKING AREA UPDATE REJECT with any of the EMM cause values #11, #12, #13, #14 or #15
> • | SERVICE REJECT received with any of the EMM cause values #11, #12, #13 or #15
> • | TRACKING AREA UPDATE ACCEPT received after the UE sent TRACKING AREA UPDATE REQUEST in EMM-IDLE mode with no “active” flag
> • | Signalling connection released
> • | Bearers have been set up
> | Release the signalling connection and proceed as described in subclause 5.3.1.2
> T3442 | EMM-REGISTERED | SERVICE REJECT received with EMM cause #39 | TRACKING AREA UPDATE REQUEST sent | None
> NOTE 1: The default value of this timer is used if the network does not indicate another value in an EMM signalling procedure.
> NOTE 2: The value of this timer is provided by the network operator during the attach and tracking area updating procedures.
> NOTE 3: The value of this timer may be provided by the network in the ATTACH ACCEPT message and TRACKING AREA UPDATE ACCEPT message. The default value of this timer is identical to the value of T3412.
> NOTE 4: The value of this timer is provided by the network operator when a service request for CS fallback is rejected by the network with EMM cause #39 “CS domain temporarily not available”.

> ‌
> EPS mobility management timers – network side

> Timer | State | Cause of Start | Normal Stop | On Expiry1st, 2nd, 3rd, 4th EXPIRY (NOTE 1)
> T3413 | EMM-REGISTERED | Paging procedure initiated | Paging procedure completed | Network dependent
> T3422 | EMM-DEREGISTERED-INITIATED | DETACH REQUEST sent | DETACH ACCEPT received | Retransmission of DETACH REQUEST
> T3450 | EMM-COMMON-PROC-INIT |
> • | ATTACH ACCEPT sent
> • | TRACKING AREA UPDATE ACCEPT sent with GUTI
> • | GUTI REALLOCATION COMMAND sent
> • | ATTACH COMPLETE received
> • | TRACKING AREA UPDATE COMPLETE received
> • | GUTI REALLOCATION COMPLETE received
> | Retransmission of the same message type, i.e. ATTACH ACCEPT, TRACKING AREA UPDATE ACCEPT or GUTI REALLOCATION COMMAND
> T3460 | EMM-COMMON-PROC-INIT |
> • | AUTHENTICATION REQUEST sent
> • | SECURITY MODE COMMAND sent
> • | AUTHENTICATION RESPONSE received
> • | AUTHENTICATION FAILURE received
> • | SECURITY MODE COMPLETE received
> • | SECURITY MODE REJECT received
> | Retransmission of the same message type, i.e. AUTHENTICATION REQUEST or SECURITY MODE COMMAND
> T3470 | EMM-COMMON-PROC-INIT | IDENTITY REQUEST sent | IDENTITY RESPONSE received | Retransmission of IDENTITY REQUEST
> Mobile reachable timer | All except EMM-DEREGISTERED | Entering EMM-IDLE mode | NAS signalling connection established | Network dependent, but typically paging is halted on 1st expiry
> Implicit detach timer | All except EMM-DEREGISTERED | The mobile reachable timer expires while the network is in EMM-IDLE mode and ISR is activated | NAS signalling connection established | Implicitly detach the UE on 1st expiry
> NOTE 1: Typically, the procedures are aborted on the fifth expiry of the relevant timer. Exceptions are described in the corresponding procedure description.
> NOTE 2: The value of this timer is network dependent.

> ‌
> EPS session management timers – UE side

> Timer | State | Cause of Start | Normal Stop | On Expiry1st, 2nd, 3rd, 4th EXPIRY (NOTE 1)
> T3480 | PROCEDURE TRANSACTION PENDING | BEARER RESOURCE ALLOCATION REQUEST sent | ACTIVATE DEDICATED EPS BEARER CONTEXT REQUEST received or MODIFY EPS BEARER CONTEXT REQUEST received or BEARER RESOURCE ALLOCATION REJECT received | Retransmission of BEARER RESOURCE ALLOCATION REQUEST
> T3481 | PROCEDURE TRANSACTION PENDING | BEARER RESOURCE MODIFICATION REQUEST sent | ACTIVATE DEDICATED EPS BEARER CONTEXT REQUEST received or MODIFY EPS BEARER CONTEXT REQUEST received or DEACTIVATE EPS BEARER CONTEXT REQUEST received or BEARER RESOURCE MODIFICATION REJECT received | Retransmission of BEARER RESOURCE MODIFICATION REQUEST
> T3482 | PROCEDURE TRANSACTION PENDING | An additional PDN connection is requested by the UE which is not combined in attach procedure | ACTIVE DEFAULT EPS BEARER CONTEXT REQUEST received or PDN CONNECTIVITY REJECT received | Retransmission of PDN CONNECTIVITY REQUEST
> T3492 | PROCEDURE TRANSACTION PENDING | PDN DISCONNECT REQUEST sent | DEACTIVATE EPS BEARER CONTEXT REQUEST received or PDN DISCONNECT REJECT received | Retransmission of PDN DISCONNECT REQUEST
> NOTE 1: Typically, the procedures are aborted on the fifth expiry of the relevant timer. Exceptions are described in the corresponding procedure description.

> ‌
> This command can be repeated to set each timer as needed.
> The retransmission of all type of NAS messages can be configured through nas-max-retransmissions command.
> Example
> The following command sets the timeout value for EPS paging procedure timer T3413 for 10 seconds.
> emm t3413-timeout 10
> enb-cache-timeout
> Configures the amount of time eNodeB information is stored in cache after the eNodeB terminates the connection.
> Product
> MME
> Privilege
> Administrator
> Syntax
> enb-cache-timeout min
> default enb-cache-timeout
> default
> Returns the command to it’s default value of 10.
> min
> Default: 10
> Specifies the amount of time, in minutes that the MME stores eNodeB information after the eNodeB terminates the connection. min must be an integer value from 1 to 60.
> Usage
> Use this command to set the amount of time the MME stores eNodeB information in cache after the eNodeB terminates the connection.
> Example
> The following command sets the amount of time the MME stores eNodeB information to 15 minutes:
> enb-cache-timeout 15
> encryption-algorithm-lte
> This command configures the precedence for LTE encryption algorithms to use for security procedures through this MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> encryption-algorithm-lte priority1 { 128-eea0 | 128-eea1 | 128-eea2 } [ priority2 { 128-eea0 | 128-eea1 | 128-eea2 } ] [ priority3 { 128-eea0 | 128-eea1 | 128-eea2 } ]
> default encryption-algorithm-lte
> default
> Sets the default LTE encryption algorithm for security procedures with configured priority value. Default configuration of LTE encryption algorithm is:

> • | priority1 with 128-eea0 encryption algorithm

> • | priority2 with 128-eea1 encryption algorithm

> • | priority3 with 128-eea2 encryption algorithm

> priority1
> Specifies the preference of integrity algorithm for security procedures on this MME service as priority 1.
> Least value has highest preference.
> priority2
> Specifies the preference of integrity algorithm for security procedures on this MME service as priority 2.
> Least value has highest preference.
> priority3
> Specifies the preference of integrity algorithm for security procedures on this MME service as priority 3.
> Least value has highest preference.
> 128-eea0
> Default: Enabled
> This keyword sets the Null ciphering algorithm (128-EEA0) for LTE encryption as the encryption algorithm for security procedures.
> 128-eea1
> Default: priority2
> This keyword sets the SNOW 3G synchronous stream ciphering algorithm (128-EEA1) for LTE encryption as the encryption algorithm for security procedures. SNOW 3G is a stream cipher that forms the base of the 3GPP confidentiality algorithm UEA2 and the 3GPP integrity algorithm UIA2.
> 128-eea2
> Default: priority3
> This keyword sets the Advance Encryption Standard (AES) ciphering algorithm (128-EEA2) for LTE encryption as the encryption algorithm for security procedures.
> Usage
> Use this command to set the LTE encryption algorithms for security procedures to use with this MME service.
> Caution: When this command is executed, all the existing priority to algorithm mappings will be removed and the newly configured ones will be applicable for security procedures.
> Caution: Configuration of same algorithm to multiple priorities is prohibited.
> Example
> The following command sets the 128-EEA1 as the LTE encryption algorithm with priority 2 for security procedures with an MME service:
> encryption-algorithm-lte priority2 128-eea1
> end
> Exits the current mode and returns to the Exec Mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> end
> Usage
> Change the mode back to the Exec mode.
> esm
> This command defines the Evolved Session Management timer parameters like timeout durations for timers for the retransmission of NAS messages in MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> esm { t3485-timeout t3485_dur | t3486-timeout t3486_dur | t3489-timeout t3489_dur | t3495-timeout t3495_dur }
> default esm { t3485-timeout | t3486-timeout | t3489-timeout | t3495-timeout }
> default
> Resets the specified Evolved Session Management timer timeout to the system default value.
> t3485-timeout t3485_dur
> Default: 8
> Sets the timeout duration for T3485 timer. This timer is used for default EPS bearer context activation procedure.
> This timer starts when the MME sends ACTIVATE DEFAULT EPS BEARER CONTEXT REQUEST message to UE and stops when receives ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT or ACTIVATE DEFAULT EPS BEARER CONTEXT REJECT message from UE.
> t3485_dur is timeout duration in seconds and must be an integer from 1 through 60.
> t3486-timeout t3486_dur
> Default: 8
> Sets the timeout duration for T3486 timer. This timer is used for the default EPS bearer context modification procedure.
> This timer starts when the MME sends a MODIFY EPS BEARER CONTEXT REQUEST message to the UE and stops whenit receives a MODIFY EPS BEARER CONTEXT ACCEPT received or a MODIFY EPS BEARER CONTEXT REJECT message from UE.
> t3485_dur is timeout duration in seconds and must be an integer from 1 through 60.
> t3489-timeout t3489_dur
> Default: 4
> Sets the timeout duration for T3489 timer. This timer is used for the default EPS bearer context deactivation procedure.
> This timer starts when the MME sends an ESM INFORMATION REQUEST message to the UE and stops when receives a ESM INFORMATION RESPONSE message from the UE.
> t3495_dur is timeout duration in seconds and must be an integer from 1 through 60.
> t3495-timeout t3495_dur
> Default: 8
> Sets the timeout duration for T3495 timer. This timer is used for default EPS bearer context deactivation procedure.
> This timer starts when the MME sends a DEACTIVATE EPS BEARER CONTEXT REQUEST message to UE and stops when receives DEACTIVATE EPS BEARER CONTEXT ACCEPT or DEACTIVATE EPS BEARER CONTEXT REJECT message from UE.
> t3495_dur is timeout duration in seconds and must be an integer from 1 through 60.
> Usage
> Use this command to set Evolved Session Management timers.
> Following tables describe the triggers and states for timers:
> EPS session management timers – Network side

> Timer | State | Cause of Start | Normal Stop | On Expiry1st, 2nd, 3rd, 4th EXPIRY (NOTE 1)
> T3485 | BEARER CONTEXT ACTIVE PENDING |
> • | ACTIVATE DEFAULT EPS BEARER CONTEXT REQUEST sent
> • | ACTIVATE DEDICATED EPS BEARER CONTEXT REQUEST sent
> • | ACTIVATE DEFAULT EPS BEARER CONTEXT ACCEPT received or
> • | ACTIVATE DEFAULT EPS BEARER CONTEXT REJECT received or
> • | ACTIVATE DEDICATED EPS BEARER CONTEXT ACCEPT received or
> • | ACTIVATE DEDICATED EPS BEARER CONTEXT REJECT received
> | Retransmission of the same message
> T3486 | BEARER CONTEXT MODIFY PENDING | MODIFY EPS BEARER CONTEXT REQUEST sent |
> • | MODIFY EPS BEARER CONTEXT ACCEPT received or
> • | MODIFY EPS BEARER CONTEXT REJECT received
> | Retransmission of MODIFY EPS BEARER CONTEXT REQUEST
> T3489 | PROCEDURETRANSACTION PENDING | ESM INFORMATION REQUEST sent | ESM INFORMATION RESPONSE received | Retransmission of ESM INFORMATION REQUEST on 1st and 2nd expiry only
> T3495 | BEARER CONTEXT INACTIVE PENDING | DEACTIVATE EPS BEARER CONTEXT REQUEST sent | DEACTIVATE EPS BEARER CONTEXT ACCEPT received | Retransmission of DEACTIVATE EPS BEARER CONTEXT REQUEST
> NOTE 1: Typically, the procedures are aborted on the fifth expiry of the relevant timer. Exceptions are described in the corresponding procedure description.

> ‌
> This command can be repeated to set each timer as needed.
> The retransmission of all type of NAS messages can be configured through nas-max-retransmissions command.
> Example
> The following command sets the timeout value for default EPS bearer context activation procedure timer T3485 for 10 seconds.
> esm t3485-timeout 10
> exit
> Exits the current mode and returns to the previous mode.
> Product
> All
> Privilege
> Administrator
> Syntax
> exit
> Usage
> Return to the previous mode.
> gtpv2
> Configures GTPv2 piggybacking support from the MME to the P-GW. A piggybacking flag is sent by the MME to a P-GW in the S11 “Create Session Request” message and determines whether dedicated bearer creation (Create Bearer Request) is piggybacked onto the “Create Session Response” message or not.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ default | no ] gtpv2 piggybacking
> default
> Returns the command to it’s default setting of enabled.
> no
> Disables the feature.
> piggybacking
> Specifies that piggybacking is to be performed by the P-GW.
> Usage
> Use this command to enable the sending of a piggybacking flag to the P-GW over the S11 interface requesting that the Create Bearer Request message is piggybacked on the Create Session Response message (sent from the P-GW to the MME.
> Example
> The following command disables this feature:
> no gtpv2 piggybacking
> heuristic-paging
> Enables/disables the heuristic or optimized paging feature for the service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ default | no ] heuristic-paging
> default
> Returns the command to it’s default setting of disabled.
> no
> Disables the feature.
> Usage
> Use this command to enable or disable the heuristic paging feature for the service. Also known as idle-mode paging, enabling this feature prompts the MME service to keep track of the eNodeBs to which the access terminal (AT) most commonly attaches, thus reducing the signalling otherwise associated with continuous paging.
> Important: Optimized Paging is a licensed feature and will not appear as a command option unless the proper licensed is installed.
> integrity-algorithm-lte
> This command configures the precedence of LTE integrity algorithms to use for security procedures through this MME service. By default integrity algorithm is enabled on MME service, which cannot be disabled.
> Product
> MME
> Privilege
> Administrator
> Syntax
> integrity-algorithm-lte priority1 { 128-eia1 | 128-eia2 } [ priority2 { 128-eia1 | 128-eia2 } ]
> default integrity-algorithm-lte
> default
> Removes the preconfigured integrity algorithm and sets the default LTE integrity algorithm for security procedures. Default configuration of LTE integrity algorithm is:

> • | priority1 with 128-eia1 integrity algorithm

> • | priority2 with 128-eia2 integrity algorithm

> priority1
> Specifies the preference of integrity algorithm for security procedures on this MME service as priority 1.
> This is the mandatory and default priority keyword.
> priority2
> Specifies the preference of integrity algorithm for security procedures on this MME service as priority 2.
> 128-eia1
> Default: priority1
> This keyword sets the SNOW 3G synchronous stream ciphering algorithm (128-EIA1) for LTE integrity as the integrity algorithm for security procedures. SNOW 3G is a stream cipher that forms the base of the 3GPP confidentiality algorithm UEA2 and the 3GPP integrity algorithm UIA2.
> 128-eia2
> Default: Enabled
> This keyword sets the Advance Encryption Standard (AES) ciphering algorithm (128-EIA2) for LTE integrity as the integrity algorithm for security procedures.
> Usage
> Use this command to set the LTE integrity algorithms for security procedures to use with this MME service.
> Warning: Integrity algorithm is a mandatory aspect and can not be disabled in MME service.
> Caution: When this command is executed, all the existing priority to algorithm mappings will be removed and the newly configured ones will be applicable for security procedures.
> Caution: Configuration of same algorithm to multiple priorities is prohibited.
> Example
> The following command sets the AES ciphering algorithms (128-EIA2) as the LTE integrity algorithm with priority as 1 for security procedures with an MME service:
> integrity-algorithm-lte priority1 128-eia2
> location-reporting
> This command enables the UE location reporting function on the MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no | default ] location-reporting
> default
> Disables the location reporting feature on MME service.
> no
> Disables the location reporting feature on MME service.
> Usage
> Use this command to enable/disable the UE location reporting feature on the MME service. The MME forwards a location report request, for a specific UE, from the P-GW to the eNodeB.
> Important: Location reporting, also known as User Location Information (ULI) Reporting, is a licensed feature and requires the purchase of the ULI Reporting feature license.
> Example
> The following command sets the MME service to allow for location reporting for UEs:
> location-reporting
> max-bearers per-subscriber
> This command specifies the maximum number of EPS bearers that a subscriber may simultaneously use to access this MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> max-bearers per-subscriber max_bearer
> default max-bearers per-subscriber
> default
> Configures the maximum EPS bearers for a subscriber to use simultaneously to default value of 11.
> max_bearer
> Default: 11
> Specifies the maximum number of EPS bearers for a subscriber may simultaneously use to access this MME service.
> max_bearer can be configured to any integer value between 1 and 11.
> Usage
> Use this command to set the maximum number of EPS bearers that a subscriber may simultaneously use to access this MME service.
> Example
> The following command specifies that a maximum of 6 simultaneous EPS bearers can be facilitated for a subscriber at any given time:
> max-bearers per-subscriber 6
> max-paging-attempts
> This command configures the maximum number of paging attempt retransmission allowed for network requested service creation to a subscriber while first attempt failed.
> Product
> MME
> Privilege
> Administrator
> Syntax
> max-paging-attempts max_paging_retry
> default max-paging-attempts
> default
> Configures the maximum number of retransmission of paging request to default value of 3.
> max_paging_retry
> Default: 3
> Specifies the maximum number of paging attempt retransmission allowed for network requested service creation to a subscriber while first attempt failed.
> max_paging_retry can be configured to any integer value between 1 and 10.
> Usage
> Use this command to set the maximum number of paging attempt retransmission allowed for network requested service creation to a subscriber while first attempt failed.
> Example
> The following command specifies that a maximum of 6 paging attempt retransmission allowed for network requested service creation to a subscriber while first attempt failed for a subscriber at any given time:
> max-paging-attempts 6
> max-pdns per-subscriber
> This command specifies the maximum number of PDNs that a subscriber may simultaneously access through this MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> max-pdns per-subscriber max_pdn
> default max-pdns per-subscriber
> default
> Configures the maximum PDNs for a subscriber simultaneously access through this MME service to default value of 3 PDNs.
> max_pdn
> Default: 3
> Specifies the maximum number of PDNs that a subscriber may simultaneously access through this MME service.
> max_pdn can be configured to any integer value between 1 and 11.
> Usage
> Use this command to set the maximum number of PDNs that a subscriber may simultaneously access through this MME service.
> Example
> The following command specifies that a maximum of 2 simultaneous PDNs can be accessed by a subscriber at any given time through this MME service:
> max-pdns per-subscriber 2
> mme-id
> This command configures the MME identifier with an MME service. MME identifier is constructed with MME group ID and MME Code.
> Product
> MME
> Privilege
> Administrator
> Syntax
> mme-id group-id grp_id mme-code mme_code
> no mme-id
> no
> Removes the configured MME identifier for this MME service.
> Caution: Removing the MME identifier is a disruptive operation; the MME service shall be removed from the service.
> group-id grp_id
> Specifies the group identifier for the group of which this MME belongs.
> grp_id must be an integer value from 0g through 65535.
> mme-code mme_code
> Specifies the unique code for this MME service.
> mme_code must be an integer value from 0 through 255.
> Usage
> Use this command to set the MME identifier for this MME service. This MME identifier will be the identity of this MME in network.
> Caution: Changing or removing the MME identifier is a disruptive operation; the MME service shall be re-started or removed from service.
> Example
> The following command configures the MME identifier with group id as 41025 and MME code as 101 for this MME service:
> mme-id group-id 41025 mme-code 101
> mmemgr-recovery
> Configures the recovery action for the MME manager.
> Product
> MME
> Privilege
> Administrator
> Syntax
> mmemgr-recovery { no-reset | reset-s1-peers }
> default mmemgr-recovery
> default
> Resets the command to its default value.
> no-reset
> Specifies that the recovery action is to NOT reset S1 peers.
> reset-s1-peers
> Specifies that the recovery action is TO reset S1 peers.
> Usage
> Use this command to set a recovery action for the MME Manager.
> Example
> The following command configures the MME Manager recovery action to reset all S1 peers:
> mmemgr-recovery reset-s1-peers
> msc
> Specifies the IP address of the enhanced Mobile Switching Center (eMSC) server for the MME service. This parameter is used for communicating with the eMSC server over the Sv interface in support of the Single Radio Voice Call Continuity (SRVCC) feature.
> Product
> MME
> Privilege
> Administrator
> Syntax
> msc ip_address
> no msc
> no
> Removes the eMSC IP address configuration from the MME service.
> ip_address
> Specifies the IP address in IPv4 or IPv6 notation of the peer eMSC server. For an IPv4 address, ip_address must be specified in dotted decimal notation. For an IPv6 address, ip_address must be specified in colon separated notation.
> Usage
> Use this command to specify the IP address of the peer eMSC server used during SRVCC handovers.
> Example
> The following command specifies an IPv4 address for the peer eMSC server as 1.2.3.4:
> msc 1.2.3.4
> nas-max-retransmission
> This command sets the retransmission counter for all type of NAS messages in an MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> nas-max-retransmissions nas_retrans_count
> default nas-max-retransmissions
> default
> Resets the retransmission counter to the system default value of 4.
> nas_retrans_count
> Default: 4
> Sets the maximum number of retransmission of NAS messages permitted during any procedure after which activation procedure will be discarded.
> nas_retrans_count is number of retransmission allowed and must be an integer from 1 through 10.
> Usage
> Use this command to set maximum number of retries allowed for any type of NAS messages.
> NAS Messages send by the MME which require a response from the UE for procedure completion are retransmitted. Retransmission happens based on timer expiry. The timers are configured through emm and esm command. The NAS messages are retransmitted as per configuration, and if no response from the UE is received, the pending transaction is abandoned. If the transaction is a DETACH or PDN DISCONNECT REQUEST, the transaction is completed without further UE signaling.
> The timeout duration configured through emm and esm command will be applicable between two retries.
> Example
> The following command sets the maximum number of retries allowed as 4 for all type of NAS messages in an MME service.
> default nas-max-retransmissions
> nri
> Configures the network resource identifier (NRI) length used for source SGSN discovery via NRI-FQDN based DNS resolution.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] nri length length plmn-id mcc mcc_value mnc mnc_value
> no
> Removes a configured NRI length configuration.
> length length
> Specifies the number of bits to be used in the P-TMSI (bits 23 to 18) to define the NRI. length must be an integer value from 1 to 8.
> plmn-id mcc mcc_value mnc mnc_value
> Specifies the PLMN-ID of the SGSN pool.
> mcc mcc_value: Specifies the mobile country code (MCC) part of PLMN identifier. mcc_value must be an integer value from 100 through 999.
> mnc mnc_value: Specifies the mobile network code (MNC) part of PLMN identifier. mnc_value must be an integer value from 00 through 999.
> Usage
> Use this command to retrieve the NRI (identity of an SGSN) stored in bits 23 to 18 of the packet-temporary mobile subscriber identity (P-TMSI). Up to eight NRI length values can be configured.
> In the absence of this configuration, the MME treats the NRI as invalid. The MME will use plain RAI-based FQDN (and not NRI-based FQDN) for DNS queries made to resolve the source SGSN.
> Example
> The following command creates an NRI length of 5 and associates it with an SGSN pool with the PLMN-ID of 12323:
> nri length 5 plmnid mcc 123 mnc 23
> peer-mme
> Configures parameters that, when matched by another MME, specifies that MME as a peer for inter-MME relocations.
> Product
> MME
> Privilege
> Administrator
> Syntax
> peer-mme { gummei mcc number mnc number group-id id mme-code code address ipv4_address | tai-match priority value mcc number mnc number tac { area_code | any | start_area_code to end_area_code } address ipv4_address }
> no peer-mme { gummei mcc number mnc number group-id id mme-code code | tai-match priority value
> no
> Removes the configured peer MME GUMMEI or TAI match priority from this service.
> gummei mcc number mnc number group-id id mme-code code address ipv4_address
> Specifies that an MME with values matching those configured in this Globally Unique MME Identifier (GUMMEI) is to be considered a peer MME. This variable supports the lookup of an IP address for a peer MME based on the exact match of the supporting keyword below (which make up the GUMMEI).
> mcc number: Sets the mobile country code (MCC) for peer match. number must be an integer value between 100 and 999.
> mnc number: Sets the mobile network code (MNC) for this peer match. number must be an integer value between 00 and 999.
> group-id id: Specifies the group identifier for the group to which this MME belongs. id must be an integer value from 32768 through 65535.
> mme-code code: Specifies the unique code for an MME service. code must be an integer value from 0 through 255.
> address ipv4_address: Specifies the IPv4 address of the peer MME. ipv4_address must be entered in dotted decimal notation.
> tai-match priority value mcc number mnc number tac { area_code | any | start_area_code to end_area_code } address ipv4_address
> Specifies that an MME with values matching those configured in this Tracking Area Identifier (TAI) match, is to be considered a peer MME. This keyword provides a priority-ordered list of TAI descriptions where the TAC field may be either an exact value, a range of values, or a “wildcard” value. It also provides an IP address of the peer MME corresponding to the TAI description.
> priority value:
> mcc number: Sets the mobile country code (MCC) for peer match. number must be an integer value between 100 and 999.
> mnc number: Sets the mobile network code (MNC) for this peer match. number must be an integer value between 00 and 999.
> tac area_code: Sets a specific Tracking Area Code (TAC) for the peer MME match. area_code must be an integer value from 1 to 65535.
> tac any: Specifies that any TAC value can be considered for a peer MME.
> tac start_area_code to end_area_code: Specifies a range of TACs. MMEs within this range and matching the rest of the criteria in this command are to be considered peer MMEs. start_area_code and end_area_code must be integer values from 1 to 268435455.
> address ipv4_address: Sets a specific IPv4 address for this TAI peer MME match. ipv4_address must be entered in dotted decimal notation.
> Usage
> Use this command to configure parameters that, when matched by another MME, specifies that MME as a peer for inter-MME relocations.
> This command allows configuration for two relocation scenarios:

> • | gummei: an MME receives either an Attach or a TAU request with a GUTI that originated from another MME.

> • | tai-match: an MME receives an S1 Handover Required message and must select a new MME based on the TAI.

> Up to 32 peer-mme gummei or tai-match entries may be configured per MME service.
> Example
> The following command identifies a peer MME with GUMMEI parameters:
> peer-mme gummei mcc 123 mnc 12 group-id 40000 mme-code 100 address 1.2.3.4
> peer-sgsn
> Statically configures peer SGSN environments to facilitate MME-SGSN relocations over S3 or Gn/Gp interfaces.
> Product
> MME
> Privilege
> Administrator
> Syntax
> peer-sgsn rai mcc mcc_value mnc mnc_value [ nri value ] rac value lac value address ip_address capability [ gn ] [ gp ] [ s16 ] [ s3 ]
> no peer-sgsn rai mcc mcc_value mnc mnc_value [ nri value ] rac value lac value
> peer-sgsn rnc-id mcc mcc_value mnc mnc_value rnc value address ip_address capability [ gn ] [ gp ] [ s16 ] [ s3 ]
> no peer-sgsn rnc-id mcc mcc_value mnc mnc_value rnc value
> rai
> Configures Routing Area Identity (RAI) parameters used to facilitate a lookup for a specific peer SGSN.
> rnc-id
> Configures Radio Network Controller Identification (RNC-ID) parameters used to facilitate a lookup for a specific peer SGSN.
> mcc mcc_value
> Specifies the mobile country code (MCC) part of a PLMN identifier.
> mcc_value must be an integer value from 100 through 999.
> mnc mnc_value
> Specifies the mobile network code (MNC) part of a PLMN identifier.
> mnc_value must be an integer value from 00 through 999.
> nri value
> Specifies the Network Resource Identifier (NRI) value used as an additional identity along with the RAC within the RAI parameters. value must be an integer from 0 to 65535.
> rac value
> Specifies the Routing Area Code (RAC) used to facilitate a lookup for a specific peer SGSN. value must be an integer from 0 to 255.
> rnc value
> Specifies the Radio Network Controller (RNC) identification number used to facilitate a lookup for a specific peer SGSN. value must be an integer from 0 to 65535.
> lac value
> Specifies the Location Area Code (LAC) value used to facilitate a lookup for a specific peer SGSN. value must be an integer from 0 to 65535.
> address ip_address
> Specifies the IP address of the peer SGSN. ip_address must be an existing IPv4 or IPv6 address of an existing SGSN. For IPv4, ip_address must be specified in dotted decimal notation. For IPv6, ip_address must be specified in colon separated notation.
> capability [ gn ] [ gp ] [ s16 ] [ s3 ]
> Configures the GTP interface capability of the peer SGSN.
> gn: Specifies that the peer SGSN is capable of communication over the Gn interface.
> gp: Specifies that the peer SGSN is capable of communication over the Gp interface.
> s16: Specifies that the peer SGSN is capable of communication over the S16 interface.
> s3: Specifies that the peer SGSN is capable of communication over the S3 interface.
> Usage
> Use this command to configure parameters that, when matched by an SGSN, specifies that SGSN as a peer for inter-RAT relocations.
> This command allows configuration for two relocation scenarios:

> • | rai: the lookup of an IP address for a peer MME based on the exact match of the RAI (and optionally NRI).

> • | rnc-id: the lookup of an IP address for a peer SGSN based on the exact match of the RNC-ID.

> Up to 32 peer-SGSN RAI and RNC-ID entries may be configured per MME service.
> Example
> The following command configures an SGSN lookup using RNC-ID parameters with Gn interface capability:peer-sgsn rnc-id mcc 123 mnc 12 rnc 2000 address 1.2.3.4 capability gn
> pgw-address
> This command configures the PDN Gateway (P-GW) address to use P-MIP protocol for S5 and S8 interface and other parameters with MME service. By default S5 and S8 use GTP protocol for this.
> Product
> MME
> Privilege
> Administrator
> Syntax
> pgw-address address [ s5-s8-protocol pmip ] [ weight value ]
> no pgw-address address [ s5-s8-protocol pmip ]
> no
> Removes a previously configured IP address of P-GW along with S5 and S8 interface of P-MIP protocol type and other parameters from this MME service.
> address
> Specifies the IP address of the P-GW.
> address must be an IP address in IPv4 or IPv6 notation.
> s5-s8-protocol pmip
> Specifies that P-MIP type of protocol to use for S5 and S8 interfaces with P-GW. By default S5 and S8 interface uses GTP protocol.
> pmip Sets the protocol to Proxy-MIP for S5 and S8 interface as by default GTP is the applicable protocol.
> weight value
> Assigns the weight to P-GW address to use as a preferred P-GW.
> value must be an integer from 1 through 100. Lowest value has the least preference.
> Usage
> Use this command to configure the PDN Gateway (P-GW) addresses to use with MME service. This command also changes the default protocol or GTP to P-MIP for the S5 and S8 interface and weight to share the load between associated P-GWs. A maximum of 16 P-GW addresses can be configured with this command.
> This command only changes the use of protocol in S5 and S8 interface. By default P-GW uses GTP protocol for S5 and S8 interfaces. By this command user can change the protocol to P-MIP for S5 and S8 interface.
> When weight is used, the weights of the P-GW(s) (that are operational) are totaled and then weighted round-robin selection is used to distribute new default bearer context among the P-GW(s) according to their weights.
> Important: A maximum of 16 P-GW addresses can be configured per MME service.
> Example
> The following command associates the P-GW IP address of 192.168.3.1 to the MME service with S5 and S8 protocol as P-MIP and weight as 90:
> pgw-address 192.168.3.1 s5-s8-protocol pmip weight 90
> The following command removes the above configured P-GW IP address and other parameters:
> no pgw-address 192.168.3.1 s5-s8-protocol pmip
> plmn-id
> This command configures the Public Land Mobile Network (PLMN) identifier for this MME service. PLMN identifier is made of Mobile Country Code (MCC) and Mobile Network Code (MNC). A maximum of 16 PLMN id can be configured in an MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> plmn-id mcc mcc_value mnc mnc_value
> no plmn-id mcc mcc_value mnc mnc_value
> no
> Removes the configured PLMN identifier for this MME service.
> Caution: Removing the PLMN identifier is a disruptive operation; the MME service shall be re-started.
> mcc mcc_value
> Specifies the mobile country code (MCC) part of PLMN identifier.
> mcc_value must be an integer value from 100 through 999.
> mnc mnc_value
> Specifies the mobile network code (MNC) part of PLMN identifier.
> mnc_value must be an integer value from 00 through 999.
> Usage
> Use this command to set the PLMN identifier for this MME service.
> Caution: Changing or removing the PLMN identifier is a disruptive operation; the MME service shall be re-started.
> A maximum of 16 PLMN identifiers are supported for an MME service.
> Example
> The following command configures the PLMN identifier with MCC value as 102 and MNC value as 20 for this MME service:
> plmn-id mmc 102 mnc 20
> policy attach
> Configures parameters for the UE attach procedure.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy attach { imei-query-type { imei | imei-sv | none } [ verify-equipment-identity [ allow-on-eca-timeout | deny-greylisted | deny-unknown | verify-emergency ] ] | set-ue-time { disable | enable }
> default policy attach { imei-query-type | set-ue-time }
> default
> Returns the command to it’s default setting of none for imei-query-type and disabled for set-ue-time.
> imei-query-type { imei | imei-sv | none }
> Configures the IMEI query type for UE attach.
> imei: Specifies that the MME is required to query the UE for it’s International Mobile Equipment Identity (IMEI).
> imei-sv: Specifies that the MME is required to query the UE for it’s International Mobile Equipment Identity - Software Version (IMEI-SV).
> none: Specifies that the MME does not need to query fro IMEI or IMEI-SV.
> verify-equipment-identity [ allow-on-eca-timeout | deny-greylisted | deny-unknown | verify-emergency ]
> Specifies that the identification (IMEI or IMEI-SV) of the UE is to be performed by the Equipment Identity Register (EIR) over the S13 interface.
> allow-on-eca-timeout: Configures the MME to allow equipment that has timed-out on ECA during the attach procedure.
> deny-greylisted: Configures the MME to deny grey-listed equipment during the attach procedure.
> deny-unknown: Configures the MME to deny unknown equipment during the attach procedure.
> verify-emergency: Configures the MME to ignore the IMEI validation of the equipment during the attach procedure in emergency cases.
> This is the default for the equipment identity verification option.
> set-ue-time { disable | enable }
> Configures the MME to set the time in the UE during the attach procedure. Default: disabled.
> Usage
> Use this command to configure various MME settings used during the UE attach procedure.
> Example
> The following command configures the MME to query the UE for it’s IMEI and to verify the UEs equipment identity over the S13 interface with an EIR:
> policy attach imei-query-type imei verify-equipment-identity
> policy idle-mode
> This command configures the user-defined policies of session management for LTE subscriber in an MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy idle-mode detach { explicit | implicit }
> [ default ] policy idle-mode detach
> default
> Sets the policy of idle mode detach for a subscriber to its default behavior as implicit.
> idle-mode detach
> This keyword configures the IDLE mode detach behavior of a UE.
> detach
> This keyword defines the detach procedure while UE is in IDLE mode.
> explicit
> Default: disabled
> This keyword enables the explicit detach while a UE is in IDLE mode. System will page UE before detach procedure started and then perform explicit detach procedure.
> implicit
> Default: Enabled
> This keyword enables the implicit detach while a UE is in IDLE mode. System never send any message to UE before detach and performs explicit detach procedure immediately.
> Usage
> Use this command to set the user-defined policies for session management in this MME service.
> Example
> The following command sets the idle mode detach policy to explicit for a user in this MME service:
> policy idle-mode detach explicit
> policy inter-rat
> This command enables/disables establishment of indirect data forwarding tunnels for Gn/Gp-based SRNS relocations.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy inter-rat indirect-forwarding-tunnels always
> no policy inter-rat indirect-forwarding-tunnels
> no
> Disables the function.
> indirect-forwarding-tunnels always
> Enables establishment of indirect data forwarding tunnels for Gn/Gp-based SRNS relocations.
> Usage
> Use this command to enable or disable establishment of indirect data forwarding tunnels for Gn/Gp-based SRNS relocations.
> Example
> The following command enables establishment of indirect data forwarding tunnels for Gn/Gp-based SRNS relocations:
> policy inter-rat indirect-forwarding-tunnels always
> policy network
> This command configures the MME to indicate to the P-GW that all peer SGSNs support dual-addressing for bearers and, subsequently, dual-addressing must be supported for all IPv4 and IPv6 PDNs. Dual-addressing on SGSNs is based on UE capability to support inter-rat roaming.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ default | no ] policy network dual-addressing-supported
> default
> Returns the command to it’s default setting of disabled.
> no
> Removes the ability to send dual-addressing support messaging from the MME to the P-GW.
> dual-addressing-supported
> Specifies that the MME shall indicate to the P-GW that dual-addressing is supported.
> Usage
> Use this command to configure the MME to send messaging to the P-GW that indicate that all peer SGSNs support dual-addressing for bearers and, subsequently, dual-addressing must be supported for all IPv4 and IPv6 PDNs.
> Important: This command can be used for Pre-release 8 and Release 8 SGSNs.
> policy overload
> This command configures the traffic overload policy to control congestion in this service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy overload { drop | reject }
> default policy overload
> default
> Sets the traffic overload policy action to default behavior of reject.
> drop
> Default: Disabled
> Specifies that the system is to drop the incoming packets with new session requests to avoid overload on MME node.
> reject
> Default: Enabled
> This keyword configures the system to reject the new session/call request and responds with a reject message when threshold for allowed call session is crossed on MME node.
> Usage
> Use this command to set the user-defined policies for new call connection attempted during overload in an MME service.
> Congestion policies at the service-level can be configured for service. When congestion control functionality is enabled at service level, these policies dictate how services respond should the system detect that a congestion condition threshold has been crossed.
> Example
> The following command sets the nw call connect policy to reject the new session/call request in an MME service:
> policy overload reject
> policy pdn-reconnection
> This command configures the action by the MME when a PDN connection request to an already connected APN is being processed by the MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy pdn-reconnection { multiple | reject | restart }
> [ default ] policy pdn-reconnection
> default
> Sets the policy of PDN reconnection to its default behavior of reject.
> multiple
> Default: Disabled
> This keyword allows multiple connections to a PDN with same APN and PDN Type. In this case, the existing connection is left unchanged, and the MME attempts to establish an additional connection to the PDN.
> reject
> Default: Enabled
> This keyword configures set the action of MME to deny or reject the request, by sending a PDN connection reject command. This is the default behavior.
> restart
> Default: Disabled
> This keyword deletes the existing connection and initiate an attempt to establish a new connection.
> Usage
> Use this command to set the user-defined policies for PDN reconnection attempt procedures initiated by UE in an MME service.
> While a UE is attached, the UE can request connections to PDNs. The PDNs are identified by APN (Access Point Name) and PDN Type (ipv4, ipv6 or ipv4v6).
> If the UE requests connection to a PDN for which a connection with the same APN name and PDN type already exists, the MME can; 1) deny or Reject the request, by sending a PDN connection reject command; 2) allow multiple connections to a PDN with same APN and PDN Type; or 3) delete the existing connection, and attempt to establish a new connection.
> Example
> The following command sets the PDN reconnect policy to delete the existing PDN and start the attempt to establish a new connection in an MME service:
> policy pdn-reconnection restart
> policy s1-reset
> This command configures how the MME responds to an S1 interface reset.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy s1-reset { detach-ue | idle-mode-entry }
> default policy s1-reset
> default
> Returns the command to it’s default setting of idle-mode-entry.
> { detach-ue | idle-mode-entry }
> Specifies the action to perform when the S1 interface is reset.
> detach-ue: Specifies that UEs are to be detached from the service upon S1 interface reset.
> idle-mode-entry: Specifies that UEs are to be placed into an idle mode condition during S1 interface reset.
> Usage
> Use this command to configure how the MME reacts to an S1 interface reset condition.
> Example
> The following command configures the MME to place UEs into an idle state while the S1 interface is being reset:
> s1-reset idle-mode-entry
> policy sctp-down
> This command configures how the MME responds to a failure of the SCTP connection from the eNodeB.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy sctp-down { detach-ue | idle-mode-entry }
> default policy sctp-down
> default
> Returns the command to it’s default setting of idle-mode-entry.
> { detach-ue | idle-mode-entry }
> Specifies the action to perform when the SCTP connection from the eNodeB fails.
> detach-ue: Specifies that UEs are to be detached from the service upon SCTP failure.
> idle-mode-entry: Specifies that UEs are to be placed into an idle mode condition upon SCTP failure.
> Usage
> Use this command to configure how the MME reacts to an SCTP connection failure condition.
> Example
> The following command configures the MME to place UEs into an idle state while the SCTP connection from the eNodeB fails:
> sctp-down idle-mode-entry
> policy tau
> Configures parameters for the tracking area update (TAU) procedure.
> Product
> MME
> Privilege
> Administrator
> Syntax
> policy tau { imei-query-type { imei | imei-sv | none } [ verify-equipment-identity [ allow-on-eca-timeout | deny-greylisted | deny-unknown | verify-emergency ] ] | set-ue-time { disable | enable }
> default policy tau { imei-query-type | set-ue-time }
> default
> Returns the command to it’s default setting of none for imei-query-type and disabled for set-ue-time.
> imei-query-type { imei | imei-sv | none }
> Configures the IMEI query type for TAUs.
> imei: Specifies that the MME is required to query the UE for it’s International Mobile Equipment Identity (IMEI).
> imei-sv: Specifies that the MME is required to query the UE for it’s International Mobile Equipment Identity - Software Version (IMEI-SV).
> none: Specifies that the MME does not need to query for IMEI or IMEI-SV.
> verify-equipment-identity [ allow-on-eca-timeout | deny-greylisted | deny-unknown | verify-emergency ]
> Specifies that the identification (IMEI or IMEI-SV) of the UE is to be performed by the Equipment Identity Register (EIR) over the S13 interface.
> allow-on-eca-timeout: Configures the MME to allow equipment that has timed-out on ECA during the attach procedure.
> deny-greylisted: Configures the MME to deny grey-listed equipment during the attach procedure.
> deny-unknown: Configures the MME to deny unknown equipment during the attach procedure.
> verify-emergency: Configures the MME to ignore the IMEI validation of the equipment during the attach procedure in emergency cases.
> set-ue-time { disable | enable }
> Configures the MME to set the time in the UE during the TAU procedure. Default: disabled.
> Usage
> Use this command to configure various MME settings used during the tracking area update (TAU) procedure.
> Example
> The following command configures the MME to query the UE for it’s IMEI and to verify the UEs equipment identity over the S13 interface with an EIR:
> policy tau imei-query-type imei verify-equipment-identity
> relative-capacity
> Configures a relative capacity variable that is sent o the eNodeB for use in selecting an MME in order to load balance the pool.
> Product
> MME
> Privilege
> Administrator
> Syntax
> relative-capacity number
> default relative-capacity
> default
> Returns the command to it’s default setting of 255.
> number
> Specifies the relative capacity or weight of an MME compared to others in an MME pool. number must be an integer value from 0 to 255. Default: 255
> Usage
> Use this command to configure the relative capacity or weight of this MME in comparison to other MMEs in a pool. This value is sent to the eNodeB in the S1AP S1 SETUP RESPONSE message.
> If this value is changed after the S1 interface is initialized, the MME CONFIGURATION UPDATE message is used to update the eNodeB with the change.
> Example
> The following command sets this MME with a relative capacity or weight of 100:
> relative-capacity 100
> s1-mme ip
> Configures the quality of service (QoS) differentiated service code point (DSCP) used when sending data packets of a particular 3GPP QoS class over the S1-MME interface.
> Product
> MME
> Privilege
> Administrator
> Syntax
> s1-mme ip qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef }
> default s1-mme ip qos-dscp
> qos-dscp { af11 | af12 | af13 | af21 | af22 | af23 | af31 | af32 | af33 | af41 | af42 | af43 | be | ef }
> Default: af11
> Specifies the DSCP for the specified QoS traffic pattern. qos-dscp can be configured to any one of the following:
> af11: Assured Forwarding 11 per-hop-behavior (PHB)
> af12: Assured Forwarding 12 PHB
> af13: Assured Forwarding 13 PHB
> af21: Assured Forwarding 21 PHB
> af22: Assured Forwarding 22 PHB
> af23: Assured Forwarding 23 PHB
> af31: Assured Forwarding 31 PHB
> af32: Assured Forwarding 32 PHB
> af33: Assured Forwarding 33 PHB
> af41: Assured Forwarding 41 PHB
> af42: Assured Forwarding 42 PHB
> af43: Assured Forwarding 43 PHB
> be: Best effort forwarding PHB
> ef: Expedited forwarding PHB
> Usage
> DSCP levels can be assigned to specific traffic patterns in order to ensure that data packets are delivered according to the precedence with which they’re tagged. The diffserv markings are applied to the IP header of every subscriber data packet transmitted over the S1-MME interface(s).
> Example
> The following command sets the DSCP-level for data traffic sent over the S1-MME interface to af12:
> s1-mme ip qos-dscp af12
> s1-mme sctp port
> This command configures the source SCTP port that will be used for binding the SCTP socket to communicate with the eNodeB using S1AP with this MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> s1-mme sctp port port_num
> default s1-mme sctp port
> default
> Sets the SCTP port to default value of 36412 to communicate with the eNodeBs using S1-MME interface.
> port_num
> Default: 36412
> Specifies the SCTP port number to communicate with the eNodeBs using S1-MME interface.
> port_num must be an integer between 1 through 65535.
> Usage
> Use this command to assign the SCTP port with SCTP socket to communicate with the eNodeB using S1AP.
> A maximum of one SCTP port can be associated with one MME service.
> Example
> The following command sets the default SCTP port number 699 for to interact with eNodeB using S1AP on S1-MME interface:
> default s1-mme sctp port
> setup-timeout
> This command configures the timeout duration for call setup of MME calls in this MME service.
> Product
> MME
> Privilege
> Administrator
> Syntax
> setup-timeout dur
> default setup-timeout
> default
> Sets the call setup timeout duration to default value of 60 seconds.
> dur
> Default: 60
> Specifies the call setup timeout duration for MME calls after which attempt will be discarded.
> dur must be an integer between 1 through 10000.
> Usage
> Use this command to configured the timeout duration in seconds to setup an MME call with an MME service. One this duration exhausted Call setup procedure will be discarded with this MME service.
> Example
> The following command sets the default setup timeout duration of 60 seconds for MME calls:
> default setup-timeout
> snmp trap
> Enables or disables the SNMP trap for S1 interface connection establishment.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ default | no ] snmp trap { s1-initial-establishment | s1-path-establishment }
> default
> Returns the command to it’s default setting of disabled.
> no
> Disables the SNMP trap.
> s1-initial-establishment
> Specifies that the SNMP trap for the initial S1 interface connection establishment is to be enabled or disabled.
> s1-path-establishment
> Specifies that the SNMP trap for the S1 path establishment is to be enabled or disabled.
> Usage
> Use this command to enable or disabled the SNMP trap for S1 interface connection establishment.
> ue-db
> This command configures the UE database which is maintained by MME as cache of EPS context per UE keyed by IMSI/GUTI to allow UE to attach by GUTI and reuse previously established security parameters. This cache will be maintained in each session manager where the first attach occurred for an UE.
> Product
> MME
> Privilege
> Administrator
> Syntax
> ue-db purge-timeout dur_mins
> default ue-db purge-timeout
> default
> Resets the UE database purge timer timeout to the system default value of 10080 mins.
> purge-timeout dur_mins
> Default: 10080
> Sets the timeout duration for MME to store UE database in cache memory.
> This timer starts when UE goes in dormant.
> dur_mins is timeout duration in minutes and must be an integer from 1 through 20160.
> Usage
> Use this command to set timeout duration for MME to hold UE database information in cache memory.
> The MME DB acts as a cache for storing subscriber related information. This subscriber related information helps in reducing signaling traffic. The MME DB is a part of the Session Manager and interfaces between the Session Manager Application and Evolved Mobility Management Manager to provide access to the cached data.
> Example
> The following command configures the MME database cache timer to hold the UE information up to 7 days (10080 minutes) in MME Database:
> default ue-db purge-timeout

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883