> CS-Network-RTP Schema Statistics
> The CS-Network-RTP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HNB-GW.
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the CS-Network-RTP Schema

> Variables | Description | Data Type
> nwname | Indicates the name of the Circuit Switch (CS) Network connected with specific HNB-GW on which statistics are collected or displayed. This is a key variable. | String
> rtp-uplink-pkts-tx | Indicates the total number of RTP Uplink Packets transmitted. Trigger: When RTP Uplink Packets are transmitted by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-uplink-byts-tx | Indicates the total number of RTP Uplink Bytes transmitted. Trigger: When RTP Uplink Bytes are transmitted by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-pkts-rx | Indicates the total number of RTP Downlink Packets received. Trigger: When RTP Downlink Packets are received by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-byts-rx | Indicates the total number of RTP Downlink Bytes received. Trigger: When RTP Downlink Bytes are received by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-pkts-dropped | Indicates the total number of RTP Downlink Packets dropped. Trigger: When RTP Downlink Packets are dropped by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-pkts-drop-rab_not-in_conn_state | Indicates the total number of RTP Downlink Packets dropped with cause RAB not in CONNETED state. Trigger: When RTP Downlink Packets are dropped by CS Network with cause RAB not in CONNETED state. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-pkts-dropped-misc | Indicates the total number of RTP Downlink Packets dropped with cause Miscellaneous. Trigger: When RTP Downlink Packets are dropped by CS Network with cause Miscellaneous. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-byts-dropped | Indicates the total number of RTP Downlink Bytes dropped. Trigger: When RTP Downlink Bytes are dropped by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-byts-drop-rab_not-in_conn_state | Indicates the total number of RTP Downlink Bytes dropped with cause RAB not in CONNETED state. Trigger: When RTP Downlink Bytes are dropped by CS Network with cause RAB not in CONNETED state. Availability: Across all CS Networks. | Unsigned Int32
> rtp-downlink-byts-dropped-misc | Indicates the total number of RTP Downlink Bytes dropped with cause Miscellaneous. Trigger: When RTP Downlink Bytes are dropped by CS Network with cause Miscellaneous. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-uplink-pkts-tx | Indicates the total number of RTCP Uplink Packets transmitted. Trigger: When RTCP Uplink Packets are transmitted by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-uplink-byts-tx | Indicates the total number of RTCP Uplink Bytes transmitted. Trigger: When RTCP Uplink Bytes are transmitted by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-pkts-rx | Indicates the total number of RTCP Downlink Packets received. Trigger: When RTCP Downlink Packets are received by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-byts-rx | Indicates the total number of RTCP Downlink Bytes received. Trigger: When RTCP Downlink Bytes are received by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-pkts-dropped | Indicates the total number of RTCP Downlink Packets dropped. Trigger: When RTCP Downlink Packets are dropped by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-pkts-drop-rab_not-in_conn_state | Indicates the total number of RTCP Downlink Packets dropped with cause RAB not in CONNETED state. Trigger: When RTCP Downlink Packets are dropped by CS Network with cause RAB not in CONNETED state. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-pkts-dropped-misc | Indicates the total number of RTCP Downlink Packets dropped with cause Miscellaneous. Trigger: When RTCP Downlink Packets are dropped by CS Network with cause Miscellaneous. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-byts-dropped | Indicates the total number of RTCP Downlink Bytes dropped. Trigger: When RTCP Downlink Bytes are dropped by CS Network. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-byts-drop-rab_not-in_conn_state | Indicates the total number of RTCP Downlink Bytes dropped with cause RAB not in CONNETED state. Trigger: When RTCP Downlink Bytes are dropped by CS Network with cause RAB not in CONNETED state. Availability: Across all CS Networks. | Unsigned Int32
> rtcp-downlink-byts-dropped-misc | Indicates the total number of RTCP Downlink Bytes dropped with cause Miscellaneous. Trigger: When RTCP Downlink Bytes are dropped by CS Network with cause Miscellaneous. Availability: Across all CS Networks. | Unsigned Int32
> Important: See Bulk Statistics Overview chapter for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883