> Diameter Attribute Definitions
> This chapter presents Diameter attribute definitions.
> For the quick reference table, see the Diameter Attribute Quick Reference appendix.
> Diameter Dictionary Types
> DPCA
> To configure the Diameter dictionary for Policy Control Configuration, use the following configuration:
> configure
> context <context_name>
> ims-auth-service <ims_auth_service_name>
> policy-control
> diameter dictionary { Standard | dpca-custom1 | dpca-custom10 | dpca-custom11 | dpca-custom12 | dpca-custom13 | dpca-custom14 | dpca-custom15 | dpca-custom16 | dpca-custom17 | dpca-custom18 | dpca-custom19 | dpca-custom2 | dpca-custom20 | dpca-custom3 | dpca-custom4 | dpca-custom5 | dpca-custom6 | dpca-custom7 | dpca-custom8 | dpca-custom9 | gxa-3gpp2-standard | gxc-standard | pdsn-ty | r8-gx-standard | std-pdsn-ty | ty-plus | ty-standard }
> end

> Dictionary | Description
> Standard | Specifies standard attributes for the Rel 6 Gx interface.
> dpca-custom1...dpca-custom n | Custom-defined dictionaries.
> gxa-3gpp2-standard | Specifies standard Gxa 3GPP2 Standard attributes.
> gxc-standard | Specifies Gxc Standard attributes.
> pdsn-ty | Specifies the standard attributes for the PDSN Ty interface.
> r8-gx-standard | Specifies standard R8 Gx attributes.
> std-pdsn-ty | Specifies standard attributes for the Ty interface.
> ty-plus | Specifies customer-specific enhanced attributes for the Ty interface.
> ty-standard | Specifies standard Ty attributes.

> ‌
> Important: For information on custom-defined dictionaries, please contact your local service representative.
> DCCA
> To configure the DCCA dictionary for Active Charging service, use the following configuration:
> configure
> active-charging service <acs_service_name>
> credit-control
> diameter dictionary { dcca-custom1 | dcca-custom10 | dcca-custom11 | dcca-custom12 | dcca-custom13 | dcca-custom14 | dcca-custom15 | dcca-custom16 | dcca-custom17 | dcca-custom18 | dcca-custom19 | dcca-custom2 | dcca-custom20 | dcca-custom21 | dcca-custom22 | dcca-custom23 | dcca-custom24 | dcca-custom25 | dcca-custom26 | dcca-custom27 | dcca-custom28 | dcca-custom29 | dcca-custom3 | dcca-custom30 | dcca-custom4 | dcca-custom5 | dcca-custom6 | dcca-custom7 | dcca-custom8 | dcca-custom9 | standard }
> end

> Dictionary | Description
> dcca-custom1 ... dcca-custom n | Custom-defined dictionaries.
> standard | Specifies standard attributes for the Gy interface.

> ‌
> Important: For information on custom-defined dictionaries, please contact your local service representative.
> CSCF
> In Star OS 8.1 and later releases, to configure the Diameter Policy Control dictionary, use the following configuration:
> configure
> context <context_name>
> cscf service <cscf_service_name>
> proxy-cscf
> diameter policy-control dictionary { Gq-custom | Gq-standard | Rq-custom | Rx-rel8 | Rx-standard | Tx-standard | custom01 | custom02 | custom03 | custom04 | custom05 | custom06 | custom07 | custom08 | custom09 }
> end

> Dictionary | Description
> Cx-standard | Specifies standard attributes for the Cx interface.
> Gq-custom | Specifies customized attributes for the 3GPP Gq interface.
> Gq-standard | Specifies standard attributes for the 3GPP Gq interface.
> Rq-custom | Custom-defined dictionary.
> Rx-rel8 | Rel. 8 Rx dictionary.
> Rx-standard | Specifies standard attributes for the 3GPP Rx interface.
> Tx-standard | Specifies the standard attributes for the 3GPP2 Tx interface.
> custom01...custom n | Custom-defined dictionaries.

> ‌
> Important: For information on custom-defined dictionaries, please please contact your local service representative.
> Diameter AAA
> To specify the AAA dictionary to be used when Diameter is being used for accounting, in the AAA Server Group Configuration Mode or in the Context Configuration Mode, use the following command:
> diameter accounting dictionary { aaa-custom1 | aaa-custom10 | aaa-custom2 | aaa-custom3 | aaa-custom4 | aaa-custom5 | aaa-custom6 | aaa-custom7 | aaa-custom8 | aaa-custom9 | nasreq | rf-plus }
> To specify the AAA dictionary to be used when Diameter is being used for authentication, in the AAA Server Group Configuration Mode or in the Context Configuration Mode, use the following command:
> diameter authentication dictionary { aaa-custom1 | aaa-custom10 | aaa-custom11 | aaa-custom12 | aaa-custom13 | aaa-custom14 | aaa-custom15 | aaa-custom16 | aaa-custom17 | aaa-custom18 | aaa-custom19 | aaa-custom2 | aaa-custom20 | aaa-custom3 | aaa-custom4 | aaa-custom5 | aaa-custom6 | aaa-custom7 | aaa-custom8 | aaa-custom9 | nasreq }

> Dictionary | Description
> aaa-custom1... aaa-custom8, aaa-custom10 ... aaa-custom n | Custom-defined dictionaries.
> aaa-custom9 | Specifies standard attributes for the STa interface.
> nasreq | Specifies the NASREQ attributes defined by RFC 4005.
> rf-plus | Specifies customer-specific enhanced attributes for the Rf interface.

> ‌
> Important: For information on custom-defined dictionaries, please contact your local service representative.
> Attributes
> Important: Diameter attributes received by the system from the Diameter server always take precedence over local-subscriber attributes and parameters configured on the system.
> 3GPP-Called-Station-Id
> This AVP identifies the layer 2 addresses the user contacted in the request.
> AVP Header
> 30 10415
> Vendor ID
> 10415
> VSA Type
> 30
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> 3GPP-CAMEL-Charging-Info
> This AVP identifies the Customized Application for Mobile Enhanced Logic (CAMEL) charging information.
> AVP Header
> 24 10415
> Vendor ID
> 10415
> VSA Type
> 24
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> 3GPP-CF-IPv6-Address
> 3GPP-CF-IPv6-Address.
> AVP Header
> 14 10415
> Vendor ID
> 10415
> VSA Type
> 14
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-CG-Address
> This AVP contains the Charging Gateway address.
> AVP Header
> 846 10415
> Vendor ID
> 10415
> VSA Type
> 846
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Charging-Characteristics
> This AVP contains the charging characteristics for this PDP Context received in the Create PDP Context Request Message.
> AVP Header
> 13 10415
> Vendor ID
> 10415
> VSA Type
> 13
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Charging-Id
> This AVP contains the Charging ID for this PDP Context (this together with the GGSN-Address constitutes a unique identifier for the PDP context.
> AVP Header
> 2 10415
> Vendor ID
> 10415
> VSA Type
> 2
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Charging-Rule-Based-Name
> This AVP indicates the group name of charging rules residing in the TPF.
> AVP Header
> 1004 10415
> Vendor ID
> 10415
> VSA Type
> 1004
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Feature-List
> This AVP contains a bit mask indicating the supported features of an application.
> AVP Header
> 630 10415
> Vendor ID
> 10415
> VSA Type
> 630
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Feature-List-ID
> This AVP contains the identity of a feature list.
> AVP Header
> 629 10415
> Vendor ID
> 10415
> VSA Type
> 629
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-GGSN-Address
> This AVP contains the GGSN IP address used by the GTP control plane for the context establishment. It is the same as the GGSN IP address used in the GCDRs.
> AVP Header
> 7 10415
> Vendor ID
> 10415
> VSA Type
> 7
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-GGSN-MCC-MNC
> This AVP contains MCC-MNC of the network the GGSN belongs to.
> AVP Header
> 9 10415
> Vendor ID
> 10415
> VSA Type
> 9
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-GPRS-QoS-Negotiated-Profile
> This AVP contains QoS profile applied by GGSN.
> AVP Header
> 5 10415
> Vendor ID
> 10415
> VSA Type
> 5
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-IMEISV
> This AVP contains International Mobile Equipment ID and its Software Version.
> AVP Header
> 20 10415
> Vendor ID
> 10415
> VSA Type
> 20
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-IMSI
> This AVP contains an IMSI of the user.
> AVP Header
> 1 10415
> Vendor ID
> 10415
> VSA Type
> 1
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-IMSI-MCC-MNC
> MCC and MNC extracted from the user's IMSI (first 5 or 6 digits, as applicable from the presented IMSI).
> AVP Header
> 8 10415
> Vendor ID
> 10415
> VSA Type
> 8
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-MS-TimeZone
> Indicates the Mobile Station Time Zone.
> AVP Header
> 23 10415
> Vendor ID
> 10415
> VSA Type
> 23
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-NSAPI
> Identifies a particular PDP context for the associated PDN and MSISDN/IMSI from creation to deletion.
> AVP Header
> 10 10415
> Vendor ID
> 10415
> VSA Type
> 10
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-PDP-Type
> Type of PDP context, for example IP or PPP.
> AVP Header
> 3 10415
> Vendor ID
> 10415
> VSA Type
> 3
> AVP Type
> ENUM. Supported values are:
> IPv4 (0)
> PPP (1)
> IPv6 (2)
> IPv4v6 (3)
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Public-Identity
> This AVP contains the public identity of a user in the IMS.
> AVP Header
> 601 10415
> Vendor ID
> 10415
> VSA Type
> 601
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Quota-Consumption-Time
> This AVP contains an idle traffic threshold time in seconds.
> AVP Header
> 881 10415
> Vendor ID
> 10415
> VSA Type
> 881
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Quota-Holding-Time
> This AVP contains the quota holding time in seconds. The client starts the quota holding timer when quota consumption ceases. This is always when traffic ceases, i.e. the timer is re-started at the end of each packet. The Credit Control Client deems a quota to have expired when no traffic associated with the quota is observed for the value indicated by this AVP.
> AVP Header
> 871 10415
> Vendor ID
> 10415
> VSA Type
> 871
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-RAT-Type
> Indicates which Radio Access Technology is currently serving the UE.
> AVP Header
> 21 10415
> Vendor ID
> 10415
> VSA Type
> 21
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-RAT-Type-Enum
> Type of Radio Access Technology.
> AVP Header
> 21 10415
> Vendor ID
> 10415
> VSA Type
> 21
> AVP Type
> ENUM. Supported values are:
> UTRAN (1)
> GERAN (2)
> WLAN (3)
> GAN (4)
> HSPA (5)
> EUTRAN (6)
> 3GPP2_eHRPD (102)
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Reporting-Reason
> Specifies the reason for usage reporting for one or more types of quota for a particular category.
> AVP Header
> 872 10415
> Vendor ID
> 10415
> VSA Type
> 872
> AVP Type
> ENUM. Supported values are:
> THRESHOLD (0)
> QHT (1)
> FINAL (2)
> QUOTA_EXAUSTED (3)
> VALIDITY_TIME (4)
> OTHER_QUOTA_TYPE (5)
> RATING_CONDITION_CHANGE (6)
> FORCED_REAUTHORIZATION (7)
> POOL_EXAISTED (8)
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Selection-Mode
> This AVP contains the Selection mode for this PDP Context received in the Create PDP Context Request Message.
> AVP Header
> 12 10415
> Vendor ID
> 10415
> VSA Type
> 12
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Server-Name
> This AVP contains a SIP-URL of the S-CSCF server.
> AVP Header
> 602 10415
> Vendor ID
> 10415
> VSA Type
> 602
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Session-Stop-Indicator
> Indicates to the AAA server that the last PDP context of a session is released and that the PDP session has been terminated.
> AVP Header
> 11 10415
> Vendor ID
> 10415
> VSA Type
> 11
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-SGSN-Address
> This AVP contains the SGSN address used by the GTP control plane for the handling of control messages. It may be used to identify the PLMN to which the user is attached.
> AVP Header
> 6 10415
> Vendor ID
> 10415
> VSA Type
> 6
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-SGSN-IPv6-Address
> This AVP contains the SGSN IPv6 address used by the GTP control plane for the handling of control messages. It may be used to identify the PLMN to which the user is attached.
> AVP Header
> 15 10415
> Vendor ID
> 10415
> VSA Type
> 15
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-SGSN-MCC-MNC
> Specifies the MCC-MNC of the network the SGSN belongs to.
> AVP Header
> 18 10415
> Vendor ID
> 10415
> VSA Type
> 18
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Supported-Features
> This AVP contains a list of supported features of the origin host.
> AVP Header
> 628 10415
> Vendor ID
> 10415
> VSA Type
> 628
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID ]
> [ 3GPP_FEATURE_LIST_ID ]
> [ 3GPP_FEATURE_LIST ]
> AVP Flag
> M
> 3GPP-Time-Quota-Threshold
> This AVP contains a threshold value in seconds.
> AVP Header
> 868 10415
> Vendor ID
> 10415
> VSA Type
> 868
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Trigger-Type
> This AVP contains information about type of trigger, for example, CHANGE_IN_SGSN_IP_ADDRESS, CHANGE_IN_QOS, etc. for activation of the associated action.
> AVP Header
> 870 10415
> Vendor ID
> 10415
> VSA Type
> 870
> AVP Type
> ENUM. Supported values are:
> CHANGE_IN_SGSN_IP_ADDRESS (1)
> CHANGE_IN_QOS (2)
> CHANGE_IN_LOCATION (3)
> CHANGE_IN_RAT (4)
> CHANGEINQOS_TRAFFIC_CLASS (10)
> CHANGEINQOS_RELIABILITY_CLASS (11)
> CHANGEINQOS_DELAY_CLASS (12)
> CHANGEINQOS_PEAK_THROUGHPUT (13)
> CHANGEINQOS_PRECEDENCE_CLASS (14)
> CHANGEINQOS_MEAN_THROUGHPUT (15)
> CHANGEINQOS_MAXIMUM_BIT_RATE_FOR_UPLINK (16)
> CHANGEINQOS_MAXIMUM_BIT_RATE_FOR_DOWNLINK (17)
> CHANGEINQOS_RESIDUAL_BER (18)
> CHANGEINQOS_SDU_ERROR_RATIO (19)
> CHANGEINQOS_TRANSFER_DELAY (20)
> CHANGEINQOS_TRAFFIC_HANDLING_PRIORITY (21)
> CHANGEINQOS_GUARANTEED_BIT_RATE_FOR_UPLINK (22)
> CHANGEINQOS_GUARANTEED_BIT_RATE_FOR_DOWNLINK (23)
> CHANGEINLOCATION_MCC (30)
> CHANGEINLOCATION_MNC (31)
> CHANGEINLOCATION_RAC (32)
> CHANGEINLOCATION_LAC (33)
> CHANGEINLOCATION_CellId (34)
> CHANGE_IN_SERVING_NODE (61)
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Unit-Quota-Threshold
> This AVP contains a threshold value in service specific units.
> AVP Header
> 1226 10415
> Vendor ID
> 10415
> VSA Type
> 1226
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-User-Data
> This AVP contains the user data required to give service to a user.
> AVP Header
> 606 10415
> Vendor ID
> 10415
> VSA Type
> 606
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-User-Location-Info
> This AVP contains information about the users current geographical location.
> AVP Header
> 22 10415
> Vendor ID
> 10415
> VSA Type
> 22
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-Volume-Quota-Threshold
> This AVP contains a threshold value in octets.
> AVP Header
> 869 10415
> Vendor ID
> 10415
> VSA Type
> 869
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP-WLAN-APN-Id
> This AVP contains the W-APN for which the user will have services available.
> AVP Header
> 11003 10415
> Vendor ID
> 10415
> VSA Type
> 11003
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Allowed-Persistent-TFTS
> Maximum allowed persistent TFTs.
> AVP Header
> 6083 5535
> Vendor ID
> 5535
> VSA Type
> 6083
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-BSID
> 3GPP2 BSID.
> AVP Header
> 9010 5535
> Vendor ID
> 5535
> VSA Type
> 9010
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Correlation-Id
> Correlation ID in 3GPP2 networks.
> AVP Header
> 6071 5535
> Vendor ID
> 5535
> VSA Type
> 6071
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Information
> AVP Header
> 6077 5535
> Vendor ID
> 5535
> VSA Type
> 6077
> AVP Type
> GROUPED
> Group Value
> [ SUBSCRIBER_PRIORITY ]
> [ AUTH_PROFILE_ID_FORWARD ]
> [ AUTH_PROFILE_ID_REVERSE ]
> [ AUTH_PROFILE_ID_BI_DIRECTION ]
> AVP Flag
> M
> 3GPP2-Inter-User-Priority
> Inter user priority.
> AVP Header
> 139 5535
> Vendor ID
> 5535
> VSA Type
> 139
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-MEID
> This AVP contains the International Mobile Equipment Identity.
> AVP Header
> 1471 10415
> Vendor ID
> 10415
> VSA Type
> 1471
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Max-Auth-Aggr-BW-BET
> Maximum allowed bandwidth for best effort link.
> AVP Header
> 130 5535
> Vendor ID
> 5535
> VSA Type
> 130
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Max-Inst-Per-Service-Option
> Maximum service option instances.
> AVP Header
> 6082 5535
> Vendor ID
> 5535
> VSA Type
> 6082
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Max-Per-Flow-Priority-User
> Per flow priority for the user.
> AVP Header
> 6088 5535
> Vendor ID
> 5535
> VSA Type
> 6088
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Max-Svc-Inst-Link-Flow-Total
> Maximum allowed link flows per service instance.
> AVP Header
> 6084 5535
> Vendor ID
> 5535
> VSA Type
> 6084
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-RAT-Type
> 3GPP2-RAT type.
> AVP Header
> 1001 5535
> Vendor ID
> 5535
> VSA Type
> 1001
> AVP Type
> ENUM. Supported values are:
> 3G1X (0)
> HRPD (1)
> WLAN (2)
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-RP-Session-ID
> 3GPP2 RP Session Identifier.
> AVP Header
> 6074 5535
> Vendor ID
> 5535
> VSA Type
> 6074
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Service-Option
> 3GPP2 Service option number.
> AVP Header
> 16 5535
> Vendor ID
> 5535
> VSA Type
> 16
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-Service-Option-Profile
> 3GPP2-Service-Option-Profile.
> AVP Header
> 74 5535
> Vendor ID
> 5535
> VSA Type
> 74
> AVP Type
> GROUPED
> Group Value
> [ 3GPP2_SERVICE_OPTION ]
> [ 3GPP2_MAX_INST_PER_SERVICE_OPTION ]
> AVP Flag
> M
> 3GPP2-Serving-PCF
> 3GPP2 Serving PCF Address
> AVP Header
> 6073 5535
> Vendor ID
> 5535
> VSA Type
> 6073
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> 3GPP2-User-Zone
> 3GPP2 User Zone.
> AVP Header
> 6075 5535
> Vendor ID
> 5535
> VSA Type
> 6075
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Abort-Cause
> Determines the cause of a session abort request or of an RAR indicating a PDP context release.
> AVP Header
> 500 10415
> Vendor ID
> 10415
> VSA Type
> 500
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Acceptable-Service-Info
> The maximum bandwidth for an AF session and/or for specific media components that will be authorized by the PCRF.
> AVP Header
> 526 10415
> Vendor ID
> 10415
> VSA Type
> 526
> AVP Type
> GROUPED
> Group Value
> [ MEDIA_COMPONENT_DESCRIPTION ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> [ MAX_REQUESTED_BANDWIDTH ]
> AVP Flag
> M
> Access-Network-Charging-Address
> Indicates the IP address of the network entity within the access network performing charging (for example, the GGSN IP address).
> AVP Header
> 501 10415
> Vendor ID
> 10415
> VSA Type
> 501
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Charging-Identifier
> This AVP contains a charging identifier (for example, GCID) within the Access-Network-Charging-Identifier-Value AVP along with information about the flows transported within the corresponding bearer within the Flows AVP.
> AVP Header
> 502 10415
> Vendor ID
> 10415
> VSA Type
> 502
> AVP Type
> GROUPED
> Group Value
> [ ACCESS_NETWORK_CHARGING_IDENTIFIER_VALUE ]
> [ FLOWS ]
> AVP Flag
> M
> Access-Network-Charging-Identifier-Gx
> The PCRF may use this information for charging correlation towards the AF.
> AVP Header
> 1022 10415
> Vendor ID
> 10415
> VSA Type
> 1022
> AVP Type
> GROUPED
> Group Value
> [ ACCESS_NETWORK_CHARGING_IDENTIFIER_VALUE ]
> [ CHARGING_RULE_BASE_NAME ]
> [ CHARGING_RULE_NAME ]
> AVP Flag
> M
> Access-Network-Charging-Identifier-Ty
> This grouped AVP contains a charging identifier generated by the AGW within the Access-Network-Charging-Identifier-Value AVP and the related PCC rule name(s) within the Charging-Rule-Name AVP(s). The PCRF may use this information for charging correlation towards the AF.
> AVP Header
> 1022 10415
> Vendor ID
> 10415
> VSA Type
> 1022
> AVP Type
> GROUPED
> Group Value
> [ ACCESS_NETWORK_CHARGING_IDENTIFIER_VALUE ]
> [ CHARGING_RULE_BASE_NAME ]
> [ CHARGING_RULE_NAME ]
> AVP Flag
> M
> Access-Network-Charging-Identifier-Value
> This AVP contains a charging identifier (for example, GCID).
> AVP Header
> 503 10415
> Vendor ID
> 10415
> VSA Type
> 503
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Charging-Physical-Access-Id
> This AVP indicates the identifier for the physical device the user is connected for charging.
> AVP Header
> In 12.1 and earlier releases: 1472 10415
> In 12.2 and later releases: 1472 8164
> Vendor ID
> In 12.1 and earlier releases: 10415
> In 12.2 and later releases: 8164
> VSA Type
> 1472
> AVP Type
> GROUPED
> Group Value
> [ ACCESS_NETWORK_CHARGING_PHYSICAL_ACCESS_ID_VALUE ]
> [ ACCESS_NETWORK_CHARGING_PHYSICAL_ACCESS_ID_REALM ]
> AVP Flag
> M
> Access-Network-Charging-Physical-Access-Id-Realm
> This AVP indicates the domain of the physical device the user is connected for charging.
> AVP Header
> In 12.1 and earlier releases: 1474 10415
> In 12.2 and later releases: 1474 8164
> Vendor ID
> In 12.1 and earlier releases: 10415
> In 12.2 and later releases: 8164
> VSA Type
> 1474
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Charging-Physical-Access-Id-Value
> This AVP indicates the identifier value of the physical device the user is connected for charging.
> AVP Header
> In 12.1 and earlier releases: 1473 10415
> In 12.2 and later releases: 1473 8164
> Vendor ID
> In 12.1 and earlier releases: 10415
> In 12.2 and later releases: 8164
> VSA Type
> 1473
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Information
> This AVP indicates access network information, such as the information included in the SIP P-header “P-Access-Network-Information".
> AVP Header
> 1263 0
> Vendor ID
> 0
> VSA Type
> 1263
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Physical-Access-Id
> Conveys an identifier that represents the topological segment hosting the AT within the serving IP-CAN.
> AVP Header
> 1472 5535
> Vendor ID
> 5535
> VSA Type
> 1472
> AVP Type
> GROUPED
> Group Value
> [ ACCESS_NETWORK_PHYSICAL_ACCESS_ID_VALUE ]
> [ ACCESS_NETWORK_PHYSICAL_ACCESS_ID_REALM ]
> AVP Flag
> M
> Access-Network-Physical-Access-Id-Realm
> Access-Network-Physical-Access ID Realm.
> AVP Header
> 1474 5535
> Vendor ID
> 5535
> VSA Type
> 1474
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Physical-Access-Id-Value
> Access-Network-Physical-Access ID Value.
> AVP Header
> 1473 5535
> Vendor ID
> 5535
> VSA Type
> 1473
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Access-Network-Type
> This attribute specifies the type of access network over which IP connectivity is provided to the user equipment.
> AVP Header
> 306 0
> Vendor ID
> 0
> VSA Type
> 306
> AVP Type
> GROUPED
> Group Value
> N/A
> AVP Flag
> M
> Access-Restriction-Data
> Contains a bit mask indicating the services of a subscriber, that are barred by the operator.
> AVP Header
> 1426 10415
> Vendor ID
> 10415
> VSA Type
> 1426
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Accounting-EAP-Auth-Method
> Indicates the EAP method(s) used to authenticate the user.
> AVP Header
> 465 0
> Vendor ID
> 0
> VSA Type
> 465
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> N/A
> Accounting-Input-Octets
> This AVP contains the number of octets in IP packets received from the user.
> AVP Header
> 363 0
> Vendor ID
> 0
> VSA Type
> 363
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Input-Packets
> This AVP contains the number of IP packets received from the user.
> AVP Header
> 365 0
> Vendor ID
> 0
> VSA Type
> 365
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Output-Octets
> This AVP contains the number of octets in IP packets sent to the user.
> AVP Header
> 364 0
> Vendor ID
> 0
> VSA Type
> 364
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Output-Packets
> This AVP contains the number of IP packets sent to the user.
> AVP Header
> 366 0
> Vendor ID
> 0
> VSA Type
> 366
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Accounting-PCC-R3-P-Capability
> This AVP indicates the accounting capabilities in a CCR that are supported by the sender. CCA will not include this AVP.
> AVP Header
> 403 24757
> Vendor ID
> 24757
> VSA Type
> 403
> AVP Type
> ENUM. Supported values are:
> Online (0)
> Offline (1)
> Online_and_Offline (2)
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Record-Number
> This AVP identifies this record within one session.
> AVP Header
> 485 0
> Vendor ID
> 0
> VSA Type
> 485
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Record-Type
> This AVP contains the type of accounting record being sent.
> AVP Header
> 480 0
> Vendor ID
> 0
> VSA Type
> 480
> AVP Type
> ENUM. Supported values are:
> EVENT_RECORD (1)
> START_RECORD (2)
> INTERIM_RECORD (3)
> STOP_RECORD (4)
> Group Value
> N/A
> AVP Flag
> M
> Accounting-Sub-Session-Id
> This AVP contains the accounting sub-session identifier.
> AVP Header
> 287 0
> Vendor ID
> 0
> VSA Type
> 287
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Acct-Application-Id
> Advertise support of the Accounting portion of an application.
> AVP Header
> 259 0
> Vendor ID
> 0
> VSA Type
> 259
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Acct-Interim-Interval
> Sent from the Diameter Home Authorization Server to the Diameter client.
> AVP Header
> 85 0
> Vendor ID
> 0
> VSA Type
> 85
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Acct-Multi-Session-Id
> Link multiple related accounting sessions.
> AVP Header
> 50 0
> Vendor ID
> 0
> VSA Type
> 50
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Acct-Realtime-Required
> This AVP is used to decide the action to be performed when sending of accounting records to the accounting server has been temporarily prevented due to network problem.
> AVP Header
> 483 0
> Vendor ID
> 0
> VSA Type
> 483
> AVP Type
> ENUM. Supported values are:
> DELIVER_AND_GRANT (1)
> GRANT_AND_STORE (2)
> GRANT_AND_LOSE (3)
> Group Value
> N/A
> AVP Flag
> M
> Acct-Session-Id
> This AVP is only used when RADIUS/Diameter translation occurs. This AVP contains the contents of the RADIUS Acct-Session-Id attribute.
> AVP Header
> 44 0
> Vendor ID
> 0
> VSA Type
> 44
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Acct-Session-Time
> This AVP indicates the length of the current session in seconds. This AVP MUST be included in all Accounting-Request messages and MAY be present in the corresponding Accounting-Answer messages as well.
> AVP Header
> 46 10415
> Vendor ID
> 10415
> VSA Type
> 46
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Active-APN
> This AVP indicates the active APN.
> AVP Header
> 1612 10415
> Vendor ID
> 10415
> VSA Type
> 1612
> AVP Type
> GROUPED
> Group Value
> [ CONTEXT_IDENTIFIER ]
> [ SERVICE_SELECTION ]
> [ MIP6_AGENT_INFO ]
> [ VISITED_NETWORK_IDENTIFIER ]
> [ SPECIFIC_APN_INFO ]
> AVP Flag
> M
> Additional-MBMS-Trace-Info
> This AVP contains additional information such as Trace-Reference, Triggering Events in BMSC, List of interfaces in BMSC, Trace Activity Control, etc.
> AVP Header
> 910 10415
> Vendor ID
> 10415
> VSA Type
> 910
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Address-Realm
> This AVP contains the realm that the user belongs to.
> AVP Header
> 1005 0
> Vendor ID
> 0
> VSA Type
> 1005
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> AF-Application-Identifier
> This AVP contains information that identifies particular service that the Application Function (AF) service session belongs to.
> AVP Header
> 504 10415
> Vendor ID
> 10415
> VSA Type
> 504
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> AF-Charging-Identifier
> The Application Function (AF) charging identifier that may be used in charging correlation.
> AVP Header
> 505 10415
> Vendor ID
> 10415
> VSA Type
> 505
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> AF-Correlation-Information
> This grouped AVP includes the AF Charging Identifier (ICID for IMS) and associated flow identifiers generated by the AF and received by GGSN over Rx/Gx.
> AVP Header
> 1276 10415
> Vendor ID
> 10415
> VSA Type
> 1276
> AVP Type
> GROUPED
> Group Value
> [ AF_CHARGING_IDENTIFIER ]
> [ FLOWS ]
> AVP Flag
> M
> Age-Of-Location-Information
> Age-Of-Location-Information
> AVP Header
> 1611 10415
> Vendor ID
> 10415
> VSA Type
> 1611
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> AGW-IP-Address
> This AVP contains the IP address of Access Gateway (AGW) in IPv4 decimal notation format.
> AVP Header
> 806 5535
> Vendor ID
> 5535
> VSA Type
> 806
> AVP Type
> OctetString
> Group Value
> N/A
> AVP Flag
> M
> AGW-IPv6-Address
> This AVP contains the IP address of Access Gateway (AGW) in IPv6 colon notation format.
> AVP Header
> 807 5535
> Vendor ID
> 5535
> VSA Type
> 807
> AVP Type
> OctetString
> Group Value
> N/A
> AVP Flag
> M
> AGW-MCC-MNC
> This AVP indicates the Mobile Country Code (MCC) and Mobile Network Code (MNC) of the AGW.
> AVP Header
> 1002 5535
> Vendor ID
> 5535
> VSA Type
> 1002
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Alert-Reason
> This AVP indicates that the mobile subscriber is present or the MS has available memory.
> AVP Header
> 1434 10415
> Vendor ID
> 10415
> VSA Type
> 1434
> AVP Type
> ENUM. Supported values are:
> UE_PRESENT (0)
> UE_MEMORY_AVAILABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> All-APN-Configurations-Included-Indicator
> This AVP indicates addition/modification/deletion of APN configuration for MME/SGSN service.
> AVP Header
> 1428 10415
> Vendor ID
> 10415
> VSA Type
> 1428
> AVP Type
> ENUM. Supported values are:
> ALL_APN_CONFIGURATIONS_INCLUDED (0)
> MODIFIED_ADDED_APN_CONFIGURATIONS_INCLUDED (1)
> Group Value
> N/A
> AVP Flag
> M
> Allocation-Retention-Priority
> Allocation and retention priority.
> AVP Header
> 1034 10415
> Vendor ID
> 10415
> VSA Type
> 1034
> AVP Type
> GROUPED
> Group Value
> [ AVP_PRIORITY_LEVEL ]
> [ PRE_EMPTION_CAPABILITY ]
> [ PRE_EMPTION_VULNERABILITY ]
> AVP Flag
> M
> Alternative-APN
> This AVP contains the value of a new APN. BM-SC only includes it if the UE must use a different APN for the MBMS PDP Context from the one used in the Join message.
> AVP Header
> 905 10415
> Vendor ID
> 10415
> VSA Type
> 905
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> AMBR
> This AVP contains the UE Aggregate Maximum Bit Rate (AMBR) of the user. This will be present only if the non-3GPP access network is trusted.The Rf interface supports AMBR reporting for non-guaranteed bit rate (non-GBR) bearers in the Traffic-Data-Volumes (TDV) Grouped AVP.
> AVP Header
> 1435 10415
> Vendor ID
> 10415
> VSA Type
> 1435
> AVP Type
> GROUPED
> Group Value
> [ MAX_REQUESTED_BANDWIDTH_UL ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> AVP Flag
> M
> Anchor-Data-Path-Address
> This AVP is set to the IP address of the serving SFA and is included in the CCR message.
> AVP Header
> 401 24757
> Vendor ID
> 24757
> VSA Type
> 401
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> AN-GW-Address
> Access network gateway address.
> AVP Header
> 1050 10415
> Vendor ID
> 10415
> VSA Type
> 1050
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> AN-Trusted
> This AVP contains the 3GPP AAA Server's decision on handling the non-3GPP access network trusted or non-trusted.
> AVP Header
> 1503 10415
> Vendor ID
> 10415
> VSA Type
> 1503
> AVP Type
> ENUM. Supported values are:
> TRUSTED (0)
> UNTRUSTED (1)
> Group Value
> N/A
> AVP Flag
> M
> ANID
> Access Network Identity. This AVP contains the Access Network Identifier used for key derivation at the HSS.
> AVP Header
> 6112 10415
> Vendor ID
> 10415
> VSA Type
> In 10.2 and earlier releases: 6112
> In 11.0 and later releases: 1504
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> APN-Aggregate-Max-Bitrate-DL
> Maximum aggregate bit rate in bits per seconds for the downlink direction across all non-GBR bearers related with the same APN.
> AVP Header
> 1040 10415
> Vendor ID
> 10415
> VSA Type
> 1040
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> APN-Aggregate-Max-Bitrate-UL
> Maximum aggregate bit rate in bits per seconds for the uplink direction across all non-GBR bearers related with the same APN.
> AVP Header
> 1041 10415
> Vendor ID
> 10415
> VSA Type
> 1041
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> APN-Authorized
> APN-Authorized.
> AVP Header
> 6090 10415
> Vendor ID
> 10415
> VSA Type
> 6090
> AVP Type
> GROUPED
> Group Value
> [ CONTEXT_IDENTIFIER ]
> [ CALLED_STATION_ID ]
> [ APN_BARRING_TYPE ]
> [ FRAMED_IP_ADDRESS ]
> [ FRAMED_IPV6_PREFIX ]
> [ MIP6_AGENT_INFO ]
> [ PDN_GW_ALLOCATION_TYPE ]
> [ VPLMN_DYNAMIC_ADDRESS_ALLOWED ]
> [ EPS_SUBSCRIBED_QOS_PROFILE ]
> AVP Flag
> M
> APN-Barring-Type
> Allows operator to disable all APNs for a subscriber at one time.
> AVP Header
> 6091 10415
> Vendor ID
> 10415
> VSA Type
> 6091
> AVP Type
> ENUM. Supported values are:
> NON_3GPP_APNS_ENABLE (0)
> NON_3GPP_APNS_DISABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> APN-Configuration
> This AVP contains the information related to the user’s subscribed APN configurations.
> AVP Header
> 1430 10415
> Vendor ID
> 10415
> VSA Type
> 1430
> AVP Type
> GROUPED
> Group Value
> [ CONTEXT_IDENTIFIER ]
> [ PDN_TYPE ]
> [ SERVICE_SELECTION ]
> [ EPS_SUBSCRIBED_QOS_PROFILE ]
> [ VPLMN_DYNAMIC_ADDRESS_ALLOWED ]
> [ MIP6_AGENT_INFO ]
> [ PDN_GW_ALLOCATION_TYPE ]
> [ 3GPP_CHARGING_CHARACTERISTICS ]
> [ AMBR ]
> [ SERVED_PARTY_IP_ADDRESS ]
> [ SPECIFIC_APN_INFO ]
> AVP Flag
> M
> APN-Configuration-Profile
> This AVP contains the information related to the user's subscribed APN configurations for EPS.
> AVP Header
> 1429 10415
> Vendor ID
> 10415
> VSA Type
> 1429
> AVP Type
> GROUPED
> Group Value
> [ CONTEXT_IDENTIFIER ]
> [ ALL_APN_CONFIGURATIONS_INCLUDED_INDICATOR ]
> [ APN_CONFIGURATION ]
> AVP Flag
> M
> APN-OI-Replacement
> This AVP contains the domain name to replace the APN OI when constructing the PDN GW FQDN upon which to perform a DNS resolution.
> AVP Header
> 1427 10415
> Vendor ID
> 10415
> VSA Type
> 1427
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Application-Provided-Called-Party-Address
> This AVP holds the called party number (SIP URL, E.164), if it is determined by an application server.
> AVP Header
> 837 10415
> Vendor ID
> 10415
> VSA Type
> 837
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Application-Server
> This AVP holds the SIP URL(s) of the AS(s) addressed during the session.
> AVP Header
> 836 10415
> Vendor ID
> 10415
> VSA Type
> 836
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Application-Server-Information
> This AVP contains the list of application servers visited on the ISC interface.
> AVP Header
> 850 10415
> Vendor ID
> 10415
> VSA Type
> 850
> AVP Type
> GROUPED
> Group Value
> [ APPLICATION_SERVER ]
> [ APPLICATION_PROVIDED_CALLED_PARTY_ADDRESS ]
> AVP Flag
> M
> ARP
> Allocation and retention priority for the corresponding APN configuration.
> AVP Header
> 6039 10415
> Vendor ID
> 10415
> VSA Type
> 6039
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Associated-Identities
> This AVP contains the private user identities associated to an IMS subscription.
> AVP Header
> 632 10415
> Vendor ID
> 10415
> VSA Type
> 632
> AVP Type
> GROUPED
> Group Value
> [ USER_NAME ]
> AVP Flag
> M
> Associated-Registered-Identities
> Contains the Private User Identities registered with the Public User Identity received in the request command.
> AVP Header
> 647 10415
> Vendor ID
> 10415
> VSA Type
> 647
> AVP Type
> GROUPED
> Group Value
> [ USER_NAME ]
> AVP Flag
> N/A
> Associated-URI
> This AVP holds a non-barred public user identity (SIP URI or TEL URI) associated to the the public user identity under registration.
> AVP Header
> 856 10415
> Vendor ID
> 10415
> VSA Type
> 856
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Auth-Application-Id
> This AVP contains the Diameter supported authorization application ID.
> AVP Header
> 258 0
> Vendor ID
> 0
> VSA Type
> 258
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N
> Auth-Grace-Period
> This AVP contains the number of seconds the Diameter server will wait following the expiration of the Authorization-Lifetime AVP before cleaning up resources for the session.
> AVP Header
> 276 0
> Vendor ID
> 0
> VSA Type
> 276
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N
> Authentication-Info
> This AVP contains the Authentication Vectors.
> AVP Header
> 6016 10415
> Vendor ID
> 10415
> VSA Type
> 6016
> AVP Type
> GROUPED
> Group Value
> [ EPS_VECTOR ]
> [ UMTS_VECTOR ]
> [ GERAN_VECTOR ]
> AVP Flag
> M
> Authorised-QoS
> This AVP holds the authorized QoS.
> AVP Header
> 849 0
> Vendor ID
> 0
> VSA Type
> 849
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Authorization-Lifetime
> This AVP contains the maximum number of seconds of service to be provided to the user before the user is to be re-authenticated and/or re- authorized.
> AVP Header
> 291 0
> Vendor ID
> 0
> VSA Type
> 291
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N
> Authorization-Token
> This AVP contains the authorization token defined in RFC 3520.
> AVP Header
> 506 10415
> Vendor ID
> 10415
> VSA Type
> 506
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Authorized-QoS
> Used to carry the authorized QoS from the E-PDF to the IPC/GGSN.
> AVP Header
> 1016 10415
> Vendor ID
> 10415
> VSA Type
> 1016
> AVP Type
> GROUPED
> Group Value
> [ QoS-Class ]
> [ Max-Requested-Bandwidth-UL ]
> [ Max-Requested-Bandwidth-DL ]
> AVP Flag
> M
> Auth-Profile-Id-Bi-Direction
> 3GPP2 Auth profile ID bi-direction.
> AVP Header
> 6081 5535
> Vendor ID
> 5535
> VSA Type
> 6081
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Auth-Profile-Id-Forward
> 3GPP2 Auth profile ID forward.
> AVP Header
> 6079 5535
> Vendor ID
> 5535
> VSA Type
> 6079
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Auth-Profile-Id-Reverse
> 3GPP2 Auth profile ID reverse.
> AVP Header
> 6080 5535
> Vendor ID
> 5535
> VSA Type
> 6080
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Auth-Request-Type
> Includes authorization request type to inform the peers whether a user is to be authenticated only, authorized only or both.
> AVP Header
> 274 0
> Vendor ID
> 0
> VSA Type
> 274
> AVP Type
> ENUM. Supported values are:
> AUTHENTICATE_ONLY (1)
> AUTHORIZE_ONLY (2)
> AUTHORIZE_AUTHENTICATE (3)
> Group Value
> N/A
> AVP Flag
> M
> Auth-Session-State
> Specifies whether state is maintained for a particular session.
> AVP Header
> 277 0
> Vendor ID
> 0
> VSA Type
> 277
> AVP Type
> ENUM. Supported values are:
> STATE_MAINTAINED (0)
> NO_STATE_MAINTAINED (1)
> Group Value
> N/A
> AVP Flag
> M
> AUTN
> This AVP contains the Authentication token AUTN (EAP Authentication Vector).
> AVP Header
> 1449 10415
> Vendor ID
> 10415
> VSA Type
> 1449
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Base-Time-Interval
> This AVP contains the length of the base time interval for controlling the consumption of time quota, in seconds.
> AVP Header
> 1265 10415
> Vendor ID
> 10415
> VSA Type
> 1265
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> BCID
> This AVP holds the PacketCable 1.5 Billing Correlation ID as generated for a SIP session. This value is copied from the BCID field in the P-DCS-LAES header.
> AVP Header
> 200 4491
> Vendor ID
> 4491
> VSA Type
> 200
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Bearer-Control-Mode
> This AVP indicates the preferred bearer control mode.
> In 10.0 and later releases, if the Bearer-Control-Mode (BCM) AVP is not received from PCRF, the IP-CAN session is not terminated. The value negotiated between UE/SGSN/GGSN is considered as the BCM. In earlier releases, if the PCRF did not send a BCM in CCA-I, the PCEF terminated the session.
> The following values are considered for each of the service types.

> • | GGSN: The negotiated value between UE/SGSN/GGSN is considered.

> In the following scenarios UE_ONLY is chosen as the BCM:
> Scenario 1:

> • | UE-> UE_ONLY

> • | SGSN-> UE_ONLY

> • | GGSN-> UE_ONLY

> • | PCRF-> NO BCM

> Scenario 2:

> • | UE-> UE_ONLY

> • | SGSN-> UE_ONLY

> • | GGSN-> Mixed

> • | PCRF-> NO BCM

> • | GTP-PGW: BCM of UE_NW is considered.

> • | IPSG: BCM of UE_ONLY is considered.

> • | HSGW/SGW/PDIF/FA/PDSN/HA/MIPV6HA: BCM of NONE is considered.

> AVP Header
> 1023 10415
> Vendor ID
> 10415
> VSA Type
> 1023
> AVP Type
> ENUM. Supported values are:
> UE_ONLY (0)
> RESERVED (1)
> UE_NW (2)
> Group Value
> N/A
> AVP Flag
> M
> Bearer-Identifier
> This AVP indicates the bearer to which the information belongs.
> AVP Header
> 1020 10415
> Vendor ID
> 10415
> VSA Type
> 1020
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Bearer-Operation
> This AVP indicates the bearer event that causes the request for PCC rules.
> AVP Header
> 1021 10415
> Vendor ID
> 10415
> VSA Type
> 1021
> AVP Type
> ENUM. Supported values are:
> TERMINATION (0)
> ESTABLISHMENT (1)
> MODIFICATION (2)
> Group Value
> N/A
> AVP Flag
> M
> Bearer-Service
> This AVP holds the used bearer service for the application, for example, PSTN leg in the case of voice.
> AVP Header
> 854 10415
> Vendor ID
> 10415
> VSA Type
> 854
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Bearer-Usage
> This AVP indicates how the bearer is being used, for example, whether it is used as a dedicated IMS signaling context or not.
> AVP Header
> 1000 10415
> Vendor ID
> 10415
> VSA Type
> 1000
> AVP Type
> ENUM. Supported values are:
> GENERAL (0)
> IMS_SIGNALLING (1)
> DEDICATED (2) - This is specific to customer.
> Group Value
> N/A
> AVP Flag
> M
> Binding-Information
> Used to convey binding information required for NA(P)T, hosted NA(P)T, and NA(P)T-PT control.
> AVP Header
> 450 13019
> Vendor ID
> 13019
> VSA Type
> 450
> AVP Type
> GROUPED
> Group Value
> [ BINDING_INPUT_LIST ]
> [ BINDING_OUTPUT_LIST ]
> AVP Flag
> N/A
> Binding-Input-List
> Contains a list of transport addresses for which a binding is requested.
> AVP Header
> 451 13019
> Vendor ID
> 13019
> VSA Type
> 451
> AVP Type
> GROUPED
> Group Value
> [ V6_TRANSPORT_ADDRESS ]
> [ V4_TRANSPORT_ADDRESS ]
> AVP Flag
> N/A
> Binding-Output-List
> Contains a list of transport addresses which is the result of the binding operation performed by the transport plane functions.
> AVP Header
> 452 13019
> Vendor ID
> 13019
> VSA Type
> 452
> AVP Type
> GROUPED
> Group Value
> [ V6_TRANSPORT_ADDRESS ]
> [ V4_TRANSPORT_ADDRESS ]
> AVP Flag
> N/A
> BM-Correlation-ID
> Indicates unique correlation identifier for entire MIP session.
> AVP Header
> 527 10415
> Vendor ID
> 10415
> VSA Type
> 527
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> BM-Type
> Indicates home and visited Bearer Manager in current service flow.
> AVP Header
> 1454 10415
> Vendor ID
> 10415
> VSA Type
> 1454
> AVP Type
> ENUM. Supported values are:
> HBM (0)
> VBM (1)
> Group Value
> N/A
> AVP Flag
> M
> BSID
> BSID
> AVP Header
> 10003 0
> Vendor ID
> 0
> VSA Type
> 10003
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Callback-Id
> This AVP contains the name of a place to be called, to be interpreted by the NAS.
> AVP Header
> 20 0
> Vendor ID
> 0
> VSA Type
> 20
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Callback-Number
> This AVP contains a dialing string to be used for callback.
> AVP Header
> 19 0
> Vendor ID
> 0
> VSA Type
> 19
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Call-Barring-Info-List
> This AVP contains the service codes for the short message related call barring services for a subscriber.
> AVP Header
> 1488 10415
> Vendor ID
> 10415
> VSA Type
> 1488
> AVP Type
> GROUPED
> Group Value
> [ SS_CODE ]
> AVP Flag
> M
> Called-Asserted-Identity
> This AVP holds the address (Public User ID: SIP URI, E.164, etc.) of the finally asserted called party.
> AVP Header
> 1250 10415
> Vendor ID
> 10415
> VSA Type
> 1250
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Called-Party-Address
> This AVP holds the address of the party to whom a session is established.
> AVP Header
> 832 0
> Vendor ID
> 0
> VSA Type
> 832
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Called-Station-Id
> Describing the layer 2 addresses the user contacted in the request.
> AVP Header
> 30 0
> Vendor ID
> 0
> VSA Type
> 30
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Call-ID-SIP-Header
> Contains the information in the Call-ID header.
> AVP Header
> 643 10415
> Vendor ID
> 10415
> VSA Type
> 643
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Calling-Party-Address
> This AVP holds the address of the party initiating a session.
> AVP Header
> 831 10415
> Vendor ID
> 10415
> VSA Type
> 831
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Calling-Station-Id
> Allows the NAS to send the ASCII string describing the layer 2 address from which the user connected in the request.
> AVP Header
> 31 0
> Vendor ID
> 0
> VSA Type
> 31
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> Cancellation-Type
> Indicates the type of cancellation.
> AVP Header
> 1420 10415
> Vendor ID
> 10415
> VSA Type
> 1420
> AVP Type
> ENUM. Supported values are:
> MME_UPDATE_PROCEDURE (0)
> SGSN_UPDATE_PROCEDURE (1)
> SUBSCRIPTION_WITHDRAWAL (2)
> UPDATE_PROCEDURE_IWF (3)
> Group Value
> N/A
> AVP Flag
> M
> Carrier-Select-Routing-Information
> This AVP holds information on carrier selection performed by S-CSCF/AS.
> AVP Header
> 2023 10415
> Vendor ID
> 10415
> VSA Type
> 2023
> AVP Type
> UTF8 String
> Group Value
> N/A
> AVP Flag
> M
> Cause
> Cause
> AVP Header
> 860 10415
> Vendor ID
> 10415
> VSA Type
> 860
> AVP Type
> GROUPED
> Group Value
> [ CAUSE_CODE ]
> [ NODE_FUNCTIONALITY ]
> AVP Flag
> M
> Cause-Code
> This AVP includes the cause code value from IMS node. It is used in Accounting-Request[stop] and/or Accounting-Request[event] messages.
> AVP Header
> 861 0
> Vendor ID
> 0
> VSA Type
> 861
> AVP Type
> INT32
> Group Value
> N/A
> AVP Flag
> M
> CC-Correlation-Id
> Correlates credit control requests generated for different components of the service.
> AVP Header
> 411 0
> Vendor ID
> 0
> VSA Type
> 411
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> CC-Input-Octets
> This AVP contains the number of requested granted or used octets that can be/have been received from the end user.
> AVP Header
> 412 0
> Vendor ID
> 0
> VSA Type
> 412
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> CC-Money
> This AVP indicates the monetary amount in the given currency.
> AVP Header
> 413 0
> Vendor ID
> 0
> VSA Type
> 413
> AVP Type
> GROUPED
> Group Value
> N/A
> AVP Flag
> M
> CC-Output-Octets
> This AVP contains the number of requested, granted, or used octets that can be/have been sent to the end user.
> AVP Header
> 414 0
> Vendor ID
> 0
> VSA Type
> 414
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> CC-Request-Number
> This AVP contains the number of Credit Control request for mapping requests and answers.
> AVP Header
> 415 0
> Vendor ID
> 0
> VSA Type
> 415
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> CC-Request-Type
> This AVP contains the type of credit-control Request/Answer message.
> AVP Header
> 416 0
> Vendor ID
> 0
> VSA Type
> 416
> AVP Type
> ENUM. Supported values are:
> INITIAL_REQUEST (1)
> UPDATE_REQUEST (2)
> TERMINATION_REQUEST (3)
> EVENT_REQUEST (4)
> Group Value
> N/A
> AVP Flag
> M
> CC-Selection-Mode
> This AVP indicates how the applied Charging-Characteristics was selected.
> AVP Header
> 2066 10415
> Vendor ID
> 10415
> VSA Type
> 416
> AVP Type
> ENUM. Supported values are:
> SERVING_NODE_SUPPLIED (0)
> SUBSCRIPTION_SPECIFIC (1)
> APN_SPECIFIC (2)
> HOME_DEFAULT (3)
> ROAMING_DEFAULT (4)
> VISITING_DEFAULT (5)
> Group Value
> N/A
> AVP Flag
> M
> CC-Service-Specific-Units
> This AVP specifies the number of service-specific units (for example, number of events, points) given in a selected service.
> AVP Header
> 417 0
> Vendor ID
> 0
> VSA Type
> 417
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> CC-Session-Failover
> Information as to whether moving the credit-control message stream to a backup server during an ongoing credit-control session is supported.
> AVP Header
> 418 0
> Vendor ID
> 0
> VSA Type
> 418
> AVP Type
> ENUM. Supported values are:
> FAILOVER_NOT_SUPPORTED (0)
> FAILOVER_SUPPORTED (1)
> Group Value
> N/A
> AVP Flag
> M
> CC-Sub-Session-Id
> This AVP contains the credit-control sub-session identifier.
> AVP Header
> 419 0
> Vendor ID
> 0
> VSA Type
> 419
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> CC-Time
> This AVP indicates the length of the requested, granted, or used time in seconds.
> AVP Header
> 420 0
> Vendor ID
> 0
> VSA Type
> 420
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> CC-Total-Octets
> This AVP contains the total number of requested, granted, or used octets regardless of the direction.
> AVP Header
> 421 0
> Vendor ID
> 0
> VSA Type
> 421
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> CC-Unit-Type
> This AVP indicates the type of units.
> AVP Header
> 454 0
> Vendor ID
> 0
> VSA Type
> 454
> AVP Type
> ENUM. Supported values are:
> TIME (0)
> MONEY(1)
> TOTAL-OCTETS (2)
> INPUT-OCTETS (3)
> OUTPUT-OCTETS (4)
> SERVICE-SPECIFIC-UNITS(5)
> Group Value
> N/A
> AVP Flag
> M
> Cell-Global-Identity
> This attribute contains the cell global identification of the user.
> AVP Header
> 1604 10415
> Vendor ID
> 10415
> VSA Type
> 1604
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> CG-Address
> This AVP holds the IP-address of the charging gateway.
> AVP Header
> 846 10415
> Vendor ID
> 10415
> VSA Type
> 846
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Change-Condition
> This AVP indicates the change in charging condition.
> AVP Header
> 2037 10415
> Vendor ID
> 10415
> VSA Type
> 2037
> AVP Type
> ENUM. Supported values are:
> NORMAL_RELEASE (0)
> ABNORMAL_RELEASE(1)
> QOS_CHANGE(2)
> VOLUME_LIMIT(3)
> TIME_LIMIT(4)
> SERVING_NODE_CHANGE(5)
> SERVING_NODE_PLMN_CHANGE(6)
> USER_LOCATION_CHANGE(7)
> RAT_CHANGE(8)
> UE_TIME_ZONE_CHANGE(9)
> TARIFF_TIME_CHANGE(10)
> SERVICE_IDLED_OUT(11)
> SERVICE_SPECIFIC_UNIT_LIMIT(12)
> MAX_NUMBER_OF_CHARGING_CONDITIONS(13)
> MANAGEMENT_INTERVENTION(14)
> Group Value
> N/A
> AVP Flag
> M
> Change-Time
> This attribute holds the time in UTC format when the volume counts associated to the service data container is closed and reported due to Charging condition change.
> AVP Header
> 2038 10415
> Vendor ID
> 10415
> VSA Type
> 2038
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> CHAP-Auth
> CHAP-Authentication
> AVP Header
> 402 10415
> Vendor ID
> 10415
> VSA Type
> 402
> AVP Type
> GROUPED
> Group Value
> [ CHAP-IDENT ]
> [ CHAP-RESPONSE ]
> AVP Flag
> M
> CHAP-Challenge
> CHAP-Challenge
> AVP Header
> 60 10415
> Vendor ID
> 10415
> VSA Type
> 60
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> CHAP-Ident
> CHAP-Identifier
> AVP Header
> 404 10415
> Vendor ID
> 10415
> VSA Type
> 404
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> CHAP-Response
> CHAP-Response
> AVP Header
> 405 10415
> Vendor ID
> 10415
> VSA Type
> 405
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Chargeable-User-Id
> MN-NAI identfying the user in EPS network.
> AVP Header
> 89 0
> Vendor ID
> 0
> VSA Type
> 89
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Charging-Characteristics
> This AVP contains the charging mode to be applied.
> AVP Header
> 11006 10415
> Vendor ID
> 10415
> VSA Type
> 11006
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Charging-Characteristics-Selection-Mode
> Charging-Characteristics-Selection-Mode
> AVP Header
> 2066 10415
> Vendor ID
> 10415
> VSA Type
> 2066
> AVP Type
> ENUM. Supported values are:

> • | SERVING-NODE-SUPPLIED (0)

> • | SUBSCRIPTION-SPECIFIC (1)

> • | APN-SPECIFIC (2)

> • | HOME-DEFAULT (3)

> • | ROAMING-DEFAULT (4)

> • | VISITING-DEFAULT (5)

> Group Value
> N/A
> AVP Flag
> M
> Charging-Data
> This AVP contains addresses of the charging functions.
> AVP Header
> 11005 10415
> Vendor ID
> 10415
> VSA Type
> 11005
> AVP Type
> GROUPED
> Group Value
> [ CHARGING_CHARACTERISTICS ]
> AVP Flag
> M
> Charging-Information
> This AVP contains the addresses of the charging functions in the grouped AVPs.
> AVP Header
> 618 10415
> Vendor ID
> 10415
> VSA Type
> 618
> AVP Type
> GROUPED
> Group Value
> [ Primary-Event-Charging-Function-Name ]
> [ Secondary-Event-Charging-Function-Name ]
> [ Primary-Charging-Collection-Function-Name ]
> [ Secondary-Charging-Collection-Function-Name ]
> AVP Flag
> M
> Charging-Rule-Base-Name
> Indicates the name of a pre defined group of charging rules residing at the TPF.
> AVP Header
> 1004 10415
> Vendor ID
> 10415
> VSA Type
> 1004
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Charging-Rule-Definition
> Defines the charging rule for a service flow sent by the CRF to the TPF.
> AVP Header
> 1003 10415
> Vendor ID
> 10415
> VSA Type
> 1003
> AVP Type
> GROUPED
> Group Value
> [ CHARGING_RULE_NAME ]
> [ SERVICE_IDENTIFIER ]
> [ RATING_GROUP ]
> [ FLOW_DESCRIPTION ]
> [ REPORTING_LEVEL ]
> [ ONLINE ]
> [ OFFLINE ]
> [ FLOW_STATUS ]
> [ QOS_INFORMATION ]
> [ METERING_METHOD ]
> [ PRECEDENCE ]
> [ AF_CHARGING_IDENTIFIER ]
> [ FLOWS ]
> AVP Flag
> M
> Charging-Rule-Install
> Used to activate, install, or modify Charging/Firewall rules from the Policy server. Charging/Firewall ruledefs for a subscriber can be dynamically activated from gx server. If the incoming rule fails to match in the charging ruledefs of a rulebase, then there will be a lookup with the Firewall ruledefs of the rulebase.
> AVP Header
> 1001 10415
> Vendor ID
> 10415
> VSA Type
> 1001
> AVP Type
> GROUPED
> Group Value
> [ CHARGING_RULE_DEFINITION ]
> [ CHARGING_RULE_NAME ]
> [ CHARGING_RULE_BASE_NAME ]
> [ BEARER_IDENTIFIER ]
> [ RULE_ACTIVATION_TIME ]
> [ RULE_DEACTIVATION_TIME ]
> [ RESOURCE_ALLOCATION_NOTIFICATION ]
> AVP Flag
> M
> Charging-Rule-Name
> Specifies the charging rule name provided by the CRF. It uniquely identifies a charging rule for a bearer.
> AVP Header
> 1005 10415
> Vendor ID
> 10415
> VSA Type
> 1005
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Charging-Rule-Name-LI
> Charging rule name for LI-Indicator-Gx.
> AVP Header
> 1005 10415
> Vendor ID
> 10415
> VSA Type
> 1005
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Charging-Rule-Remove
> Specifies the deactivated or removed Charging/Firewall rules from the Policy server. Charging/Firewall ruledefs for a subscriber can be dynamically deactivated from gx server. If the incoming rule fails to match in the charging ruledefs of a rulebase, then there will be a lookup with the Firewall ruledefs of the rulebase.
> AVP Header
> 1002 10415
> Vendor ID
> 10415
> VSA Type
> 1002
> AVP Type
> GROUPED
> Group Value
> [ CHARGING_RULE_NAME ]
> [ CHARGING_RULE_BASE_NAME ]
> AVP Flag
> M
> Charging-Rule-Report
> This AVP is used to report the status of a Policy and Charging Control (PCC) rule for installation successful/removal. It is a reference for a specific PCC rule at the AGW that has been successfully installed, modified or removed because of trigger from the MS. The PCC-Rule-Status AVP indicates the action being performed on the PCC rule. Multiple instances of Charging-Rule-Report AVPs shall be used in the case it is required to report different PCCRule-Status values for different groups of rules within the same Diameter command.
> AVP Header
> 1018 5535
> Vendor ID
> 5535
> VSA Type
> 1018
> AVP Type
> GROUPED
> Group Value
> [ CHARGING_RULE_NAME ]
> [ CHARGING_RULE_BASE_NAME ]
> [ PCC_RULE_STATUS ]
> [ RULE_FAILURE_CODE ]
> [ FINAL_UNIT_INDICATION ]
> AVP Flag
> M
> Check-Balance-Result
> Result of the balance check. Applicable only when requested-Action AVP indicates CHECK_BALANCE.
> AVP Header
> 422 0
> Vendor ID
> 0
> VSA Type
> 422
> AVP Type
> ENUM. Supported values are:
> ENOUGH_CREDIT (0)
> NO_CREDIT (1)
> Group Value
> N/A
> AVP Flag
> M
> Civic-Location
> This attribute provides location information.
> AVP Header
> 355 13019
> Vendor ID
> 13019
> VSA Type
> 355
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Class
> Used by Diameter servers to return state information to the access device.
> AVP Header
> 25 0
> Vendor ID
> 0
> VSA Type
> 25
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Client-Identity
> This attribute contains the ISDN number of the external client.
> AVP Header
> 1480 10415
> Vendor ID
> 10415
> VSA Type
> 1480
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> CoA-Information
> This attribute contains care-of-address and the tunnel information related to the care of address.
> AVP Header
> 1039 10415
> Vendor ID
> 10415
> VSA Type
> 1039
> AVP Type
> GROUPED
> Group Value
> [ TUNNEL_INFORMATION ]
> [ COA_IP_ADDRESS ]
> AVP Flag
> M
> CoA-IP-Address
> Care of IP address for DSMIP6 access.
> AVP Header
> 1035 10415
> Vendor ID
> 10415
> VSA Type
> 1035
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Codec-Data
> This AVP contains CODEC-related information known at the AF.
> AVP Header
> 524 10415
> Vendor ID
> 10415
> VSA Type
> 524
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Complete-Data-List-Included-Indicator
> This attribute indicates addition/modification/deletion of PDP-Contexts at MME/SGSN.
> AVP Header
> 1468 10415
> Vendor ID
> 10415
> VSA Type
> 1468
> AVP Type
> ENUM. Supported values are:
> ALL_PDP_CONTEXTS_INCLUDED (0)
> MODIFIED_ADDED_PDP_CONTEXTS_INCLUDED (1)
> Group Value
> N/A
> AVP Flag
> M
> Confidentiality-Key
> This AVP contains the Confidentiality Key (CK).
> AVP Header
> 625 10415
> Vendor ID
> 10415
> VSA Type
> 625
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Configuration-Token
> Sent by a Diameter Server to a Diameter Proxy Agent or Translation Agent in an AA-Answer command to indicate a type of user profile to be used.
> AVP Header
> 78 0
> Vendor ID
> 0
> VSA Type
> 78
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Connect-Info
> Sent in the AA-Request message or ACR STOP message.
> AVP Header
> 77 0
> Vendor ID
> 0
> VSA Type
> 77
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Contact
> Contains the contact addresses and parameters in the Contact header.
> AVP Header
> 641 10415
> Vendor ID
> 10415
> VSA Type
> 641
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Content-Disposition
> This AVP indicates how the message body or a message body part is to be interpreted (for example, session, render).
> AVP Header
> 828 10415
> Vendor ID
> 10415
> VSA Type
> 828
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Content-Length
> This AVP holds the size of the message body.
> AVP Header
> 827 10415
> Vendor ID
> 10415
> VSA Type
> 827
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Content-Type
> This AVP holds the media type (for example, application/sdp, text/html) of the message-body.
> AVP Header
> 826 10415
> Vendor ID
> 10415
> VSA Type
> 826
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Context-Identifier
> Context identifier.
> AVP Header
> 1423 10415
> Vendor ID
> 10415
> VSA Type
> 1423
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Correlate-Reason
> Indicates the reason that the Correlate message was sent.
> AVP Header
> 202 4491
> Vendor ID
> 4491
> VSA Type
> 202
> AVP Type
> ENUM. Supported values are:
> UNKNOWN (0)
> B2BUA (1)
> INITIAL_SIP_MESSAGE (2) — Initial SIP Message sent by target's S-CSCF
> ADDITIONAL_TARGET_ENCOUNTERED (3)
> HAND_OFF_OCCURED (4)
> ORIGINATION_FROM_APP_SERVER (5) — Origination from an Application Server as a result of a termination on that Application Server.
> BCID (6) — BCID received in the P-DCS-LAES header.
> Group Value
> N/A
> AVP Flag
> M
> Cost-Information
> Cost information of service transferred by the credit-control client to the end user.
> AVP Header
> 423 0
> Vendor ID
> 0
> VSA Type
> 423
> AVP Type
> GROUPED
> Group Value
> [ Unit-Value ]
> [ Currency-Code ]
> [ Cost-Unit ]
> AVP Flag
> M
> Cost-Unit
> Specifies the applicable unit to the Cost-Information when the service cost is a cost per unit: can be minutes, hours, days and kilobytes.
> AVP Header
> 424 0
> Vendor ID
> 0
> VSA Type
> 424
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> CSG-Id
> Closed Subscriber Group Identity used to identify Closed Subscriber Group within a PLMN.
> AVP Header
> 1437 10415
> Vendor ID
> 10415
> VSA Type
> 1437
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> CSG-Subscription-Data
> This attribute contains the CSG-Id and optionally an associated expiration date.
> AVP Header
> 1436 10415
> Vendor ID
> 10415
> VSA Type
> 1436
> AVP Type
> GROUPED
> Group Value
> [ CSG_ID ]
> [ EXPIRATION_DATE ]
> AVP Flag
> M
> Credit-Control
> Included in AA requests when the service element has credit-control application.
> AVP Header
> 426 0
> Vendor ID
> 0
> VSA Type
> 426
> AVP Type
> ENUM. Supported values are:
> CREDIT_AUTHORIZATION (0)
> RE_AUTHORIZATION (1)
> Group Value
> N/A
> AVP Flag
> M
> Credit-Control-Failure-Handling
> The credit-control client uses this information to handle the credit control server failure.
> AVP Header
> 427 0
> Vendor ID
> 0
> VSA Type
> 427
> AVP Type
> ENUM. Supported values are:
> TERMINATE (0)
> CONTINUE (1)
> RETRY_AND_TERMINATE (2)
> Group Value
> N/A
> AVP Flag
> M
> Currency-Code
> Currency in which the values of AVPs containing monetary units were given.
> AVP Header
> 425 0
> Vendor ID
> 0
> VSA Type
> 425
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Current-Location
> Indicates whether an active location retrieval has to be initiated or not.
> AVP Header
> 707 0
> Vendor ID
> 0
> VSA Type
> 707
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Current-Location-Retrieved
> Current-Location-Retrieved
> AVP Header
> 1610 10415
> Vendor ID
> 10415
> VSA Type
> 1610
> AVP Type
> ENUM. Supported value is ACTIVE-LOCATION-RETRIEVAL (0)
> Group Value
> N/A
> AVP Flag
> M
> Customer-Id
> Customer ID; used in header enrichment scenarios.
> AVP Header
> 1146 8164
> Vendor ID
> 8164
> VSA Type
> 1146
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Data-Reference
> Indicates the type of the requested used data in the operation UDR and SNR.
> AVP Header
> 703 0
> Vendor ID
> 0
> VSA Type
> 703
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Default-EPS-Bearer-QoS
> Defines the QoS information for the EPS default bearer.
> AVP Header
> 1049 10415
> Vendor ID
> 10415
> VSA Type
> 1049
> AVP Type
> GROUPED
> Group Value
> [ QOS_CLASS_IDENTIFIER ]
> [ ALLOCATION_RETENTION_PRIORITY ]
> AVP Flag
> M
> Deregistration-Reason
> This AVP contains the reason for a de-registration operation.
> AVP Header
> 615 10415
> Vendor ID
> 10415
> VSA Type
> 615
> AVP Type
> GROUPED
> Group Value
> [ REASON_CODE ]
> [ REASON_INFO ]
> AVP Flag
> M
> Destination-Host
> The destination endpoint of the message. This attribute is present in all request messages.
> AVP Header
> 293 0
> Vendor ID
> 0
> VSA Type
> 293
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Destination-Realm
> The realm the message is to be routed to. It is present in all request messages sent from DCCA.
> AVP Header
> 283 0
> Vendor ID
> 0
> VSA Type
> 283
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Diagnostics
> This attribute provides a more detailed cause value for sending Accounting-request from PCN node.
> AVP Header
> 2039 10415
> Vendor ID
> 10415
> VSA Type
> 2039
> AVP Type
> ENUM. Supported values are:
> UNSPECIFIED (0)
> SESSION_TIMEOUT (1)
> RESOURCE_LIMITATION (2)
> ADMIN_DISCONNECT (3)
> IDLE_TIMEOUT (4)
> PCRF_UNREACHABLE (5)
> AAA_UNREACHABLE (6)
> AAA_INITIATED_SESSION_TERMINATION (7)
> REAUTHENTICATION_FAILED (8)
> PCRF_INITIATED_SESSION_TERMINATION (9)
> PCRF_INITIATED_FLOW_TERMINATION (10)
> PCRF_ACCOUNTING_PARAMETERS_CHANGED (11)
> PMIP_INITIATED_SESSION_TERMINATION (12)
> PPP_INITIATED_SESSION_TERMINATION (13)
> GTP_INITIATED_SESSION_TERMINATION (14)
> PMIP_REVOCATION (15)
> HANDOVER_ERROR (16)
> PMIP_LIFETIME_EXPIRED (17)
> Group Value
> N/A
> AVP Flag
> M
> Dialog-Id
> Contains the SIP dialog identifier in the form: Call-ID=x;FTag=y;TTag=z, where x is the value of the SIP Call-ID header, y is the contents of the From header tag, and z is the contents of the To header tag. If the To header tag value is not present in the SIP message then TTag field MUST not be present in the AVP.
> AVP Header
> 203 4491
> Vendor ID
> 4491
> VSA Type
> 203
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-Algorithm
> Holds the algorithm parameter that influences the HTTP Digest calculation.
> AVP Header
> 111 0
> Vendor ID
> 0
> VSA Type
> 111
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-Auth-Param
> This attribute is a placeholder for future extensions and corresponds to the "auth-param" parameter defined in section 3.2.1 of [RFC2617].
> AVP Header
> 117 0
> Vendor ID
> 0
> VSA Type
> 117
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-Domain
> Consists of a single URI that defines a protection space component.
> AVP Header
> 119 0
> Vendor ID
> 0
> VSA Type
> 119
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-HA1
> Contains the hexadecimal representation of H(A1) as described in [RFC2617].
> AVP Header
> 121 0
> Vendor ID
> 0
> VSA Type
> 121
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-QoP
> Holds the Quality of Protection parameter that influences the HTTP Digest calculation.
> AVP Header
> 110 0
> Vendor ID
> 0
> VSA Type
> 110
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Digest-Realm
> Describes a protection space component of the RADIUS server.
> AVP Header
> 104 0
> Vendor ID
> 0
> VSA Type
> 104
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> DIR
> AVP Header
> 11000 0
> Vendor ID
> 0
> VSA Type
> 11000
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Direct-Debiting-Failure-Handling
> Specifies the action to handle the failure of request message to the credit control server with DIRECT_DEBITING attribute.
> AVP Header
> 428 0
> Vendor ID
> 0
> VSA Type
> 428
> AVP Type
> ENUM. Supported values are:
> TERMINATE_OR_BUFFER (0)
> CONTINUE (1)
> Group Value
> N/A
> AVP Flag
> M
> Direction
> Indicates whether the reported message was sent “to" or "from" the intercept target.
> AVP Header
> 210 4491
> Vendor ID
> 4491
> VSA Type
> 210
> AVP Type
> ENUM. Supported values are:
> UNDEFINED (0)
> TO_TARGET (1)
> FROM_TARGET (2)
> Group Value
> N/A
> AVP Flag
> M
> Direct-Message
> Indicates if the reported message is exchanged directly between the IAP and the intercept target.
> AVP Header
> 211 4491
> Vendor ID
> 4491
> VSA Type
> 211
> AVP Type
> ENUM. Supported values are:
> FALSE (0)
> TRUE (1)
> Group Value
> N/A
> AVP Flag
> M
> Disconnect-Cause
> Specifies the reason or cause of disconnection with peer.
> AVP Header
> 273 0
> Vendor ID
> 0
> VSA Type
> 273
> AVP Type
> ENUM. Supported values are:
> REBOOTING (0)
> BUSY (1)
> DO_NOT_WANT_TO_TALK_TO_YOU (2)
> Group Value
> N/A
> AVP Flag
> N/A
> DSA-Flags
> This AVP contains a bit mask.
> AVP Header
> 1422 10415
> Vendor ID
> 10415
> VSA Type
> 1422
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> DSR-Flags
> This AVP contains a bit mask.
> AVP Header
> 1421 10415
> Vendor ID
> 10415
> VSA Type
> 1421
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Dynamic-Address-Flag
> This AVP indicates whether the PDP context/PDN address is statically or dynamically allocated. If not present, then it is statically allocated.
> AVP Header
> 2051 10415
> Vendor ID
> 10415
> VSA Type
> 2051
> AVP Type
> ENUM. Supported values are:
> STATIC (0)
> DYNAMIC (1)
> Group Value
> N/A
> AVP Flag
> M
> EAP-Key-Name
> This AVP contains an opaque key identifier (name) generated by the EAP method.
> AVP Header
> 102 0
> Vendor ID
> 0
> VSA Type
> 102
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> EAP-Master-Session-Key
> This AVP contains keying material for protecting the communications between the user and the NAS.
> AVP Header
> 464 0
> Vendor ID
> 0
> VSA Type
> 464
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> EAP-Payload
> Used to encapsulate the actual EAP packet that is being exchanged between the EAP client and the home Diameter server.
> AVP Header
> 462 0
> Vendor ID
> 0
> VSA Type
> 462
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> EAP-Reissued-Payload
> Sent in DEA for a non-fatal error, and encapsulates the previous EAP Request sent by the server
> AVP Header
> 463 0
> Vendor ID
> 0
> VSA Type
> 463
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Early-Media-Description
> This grouped AVP describes the SDP session, media parameters, and timestamps related to media components set to active according to SDP signalling exchanged during a SIP session establishment before the final successful or unsuccessful SIP answer to the initial SIP INVITE message is received.
> AVP Header
> 1272 10415
> Vendor ID
> 10415
> VSA Type
> 1272
> AVP Type
> GROUPED
> Group Value
> [ SDP_TIMESTAMPS ]
> [ SDP_MEDIA_COMPONENT ]
> [ SDP_SESSION_DESCRIPTION ]
> AVP Flag
> M
> Element-ID
> This AVP identifies the PacketCable IAP sending an intercept message to the DF.
> AVP Header
> 212 4491
> Vendor ID
> 4491
> VSA Type
> 212
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Element-Type
> This AVP identifies the type of node where the intercept message was generated.
> AVP Header
> 213 4491
> Vendor ID
> 4491
> VSA Type
> 213
> AVP Type
> ENUM. Supported values are:
> S_CSCF (0)
> P_CSCF (1)
> I_CSCF(2)
> MRFC (3)
> MGCF (4)
> BGCF (5)
> AS (6)
> UE (7)
> Group Value
> N/A
> AVP Flag
> M
> Envelope
> Reports the start and end time of one time envelope using the AttributeEnvelope-Start-Time and AttributeEnvelope-End-Time AVPs.
> AVP Header
> 1266 10415
> Vendor ID
> 10415
> VSA Type
> 1266
> AVP Type
> GROUPED
> Group Value
> [ ENVELOPE_START_TIME ]
> [ ENVELOPE_END_TIME ]
> [ CC_TOTAL_OCTETS ]
> [ CC_INPUT_OCTETS ]
> [ CC_OUTPUT_OCTETS ]
> [ CC_SERVICE_SPECIFIC_UNITS ]
> AVP Flag
> M
> Envelope-End-Time
> Time of the end of the time envelope.
> AVP Header
> 1267 10415
> Vendor ID
> 10415
> VSA Type
> 1267
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Envelope-Reporting
> Indicate whether the CLCI-C shall report the start and end of each time envelope, in those cases in which quota is consumed in envelopes.
> AVP Header
> 1268 10415
> Vendor ID
> 10415
> VSA Type
> 1268
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Envelope-Start-Time
> Time of the packet of user data which caused the time envelope to start.
> AVP Header
> 1269 10415
> Vendor ID
> 10415
> VSA Type
> 1269
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> EPS-Information
> EPS information.
> AVP Header
> 1041 10415
> Vendor ID
> 10415
> VSA Type
> 1041
> AVP Type
> GROUPED
> Group Value
> [ AF_CORRELATION_INFORMATION ]
> [ SGW_ADDRESS ]
> [ PGW_ADDRESS ]
> [ HSGW_ADDRESS ]
> [ 3GPP_CF_IPV6_ADDRESS ]
> [ PGW_MCC_MNC ]
> [ EPS_CAUSE_CODE ]
> [ NODE_FUNCTIONALITY ]
> [ CALLED_STATION_ID ]
> [ ACCOUNTING_INPUT_OCTETS ]
> [ ACCOUNTING_OUTPUT_OCTETS ]
> [ ACCOUNTING_INPUT_PACKETS ]
> [ ACCOUNTING_OUTPUT_PACKETS ]
> [ START_TIME ]
> [ STOP_TIME ]
> [ ACCT_SESSION_TIME ]
> [ OPERATOR_STRING ]
> [ ACCESS_NETWORK_CHARGING_IDENTIFIER_VALUE ]
> [ FIRST_PACKET_DIRECTION ]
> [ PSCID ]
> [ FID ]
> [ CHARGING_RULE_BASE_NAME ]
> [ CHARGING_RULE_NAME ]
> [ FLOW_DESCRIPTION ]
> [ QOS_INFORMATION ]
> [ PMIP_MOBILE_NODE_ADDRESS ]
> [ 3GPP2_BSID ]
> [ USER_EQUIPMENT_INFO ]
> AVP Flag
> M
> EPS-Loction-Information
> EPS-Location-Information
> AVP Header
> 1496 10415
> Vendor ID
> 10415
> VSA Type
> 1496
> AVP Type
> GROUPED
> Group Value
> [ MME_LOCATION_INFORMATION ]
> [ SGSN_LOCATION_INFORMATION ]
> AVP Flag
> M
> EPS-Subscribed-QoS-Profile
> This attribute contains the bearer-level QoS parameters associated to the default bearer for an APN.
> AVP Header
> 1431 10415
> Vendor ID
> 10415
> VSA Type
> 1431
> AVP Type
> GROUPED
> Group Value
> [ QOS_CLASS_IDENTIFIER ]
> [ ARP ]
> [ AMBR ]
> AVP Flag
> M
> EPS-User-State
> EPS-User-State
> AVP Header
> 1495 10415
> Vendor ID
> 10415
> VSA Type
> 1495
> AVP Type
> GROUPED
> Group Value
> [ MME_USER_STATE ]
> [ SGSN_USER_STATE ]
> AVP Flag
> M
> EPS-Vector
> This attribute contains Authentication Information for EPS.
> AVP Header
> 6017 10415
> Vendor ID
> 10415
> VSA Type
> 6017
> AVP Type
> GROUPED
> Group Value
> [ ITEM_NUMBER ]
> [ RAND ]
> [ XRES ]
> [ AUTN ]
> [ KASME ]
> AVP Flag
> M
> Equipment-Status
> This attribute contains the status of the mobile equipment.
> AVP Header
> 1445 10415
> Vendor ID
> 10415
> VSA Type
> 1445
> AVP Type
> ENUM. Supported values are:
> WHITELISTED (0)
> BLACKLISTED (1)
> GREYLISTED (2)
> Group Value
> N/A
> AVP Flag
> M
> ESN
> ESN.
> AVP Header
> 6109 10415
> Vendor ID
> 10415
> VSA Type
> 6109
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Error-Diagnostic
> Error-Diagnostic
> AVP Header
> 1614 10415
> Vendor ID
> 10415
> VSA Type
> 1614
> AVP Type
> ENUM. Supported values are:

> • | GPRS_DATA_SUBSCRIBED (0)

> • | NO_GPRS_DATA_SUBSCRIBED (1)

> Group Value
> N/A
> AVP Flag
> M
> Error-Message
> Human Readable Error Message.
> AVP Header
> 281 0
> Vendor ID
> 0
> VSA Type
> 281
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> Error-Reporting-Host
> This AVP contains the identity of the Diameter host that sent the Result Code AVP to a value other than 2001.
> AVP Header
> 294 0
> Vendor ID
> 0
> VSA Type
> 294
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> EUTRAN-Cell-Global-Identity
> E-UTRAN cell global identity of the user
> AVP Header
> 1602 10415
> Vendor ID
> 10415
> VSA Type
> 1602
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> EUTRAN-Vector
> EUTRAN Vector.
> AVP Header
> 1414 10415
> Vendor ID
> 10415
> VSA Type
> 1414
> AVP Type
> GROUPED
> Group Value
> [ ITEM_NUMBER ]
> [ RAND ]
> [ XRES ]
> [ AUTN ]
> [ KASME ]
> AVP Flag
> M
> Event
> This AVP holds the content of the "Event" header used in SUBSCRIBE and NOTIFY messages.
> AVP Header
> 825 10415
> Vendor ID
> 10415
> VSA Type
> 825
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Event-Message-Type
> Identifies the type of surveillance message.
> AVP Header
> 214 4491
> Vendor ID
> 4491
> VSA Type
> 214
> AVP Type
> ENUM. Supported values are:
> REPORT (0)
> CORRELATE (1)
> CARRIER_INFO (2)
> Group Value
> N/A
> AVP Flag
> M
> Event-Report-Indication
> Specifies which type of changes will trigger an event report from the PCRF. This attribute is used to report an event coming from BBERF/PCEF and also to provide information about some event-triggers to the PCRF.
> AVP Header
> 1033 10415
> Vendor ID
> 10415
> VSA Type
> 1033
> AVP Type
> GROUPED
> Group Value
> [ EVENT_TRIGGER ]
> [ RAT_TYPE ]
> [ QOS_INFORMATION ]
> [ RAI ]
> [ 3GPP_USER_LOCATION_INFO ]
> [ TRACE_DATA ]
> [ TRACE_REFERENCE ]
> [ 3GPP2_BSID ]
> [ 3GPP_MS_TIMEZONE ]
> [ 3GPP_SGSN_ADDRESS ]
> [ 3GPP_SGSN_IPV6_ADDRESS ]
> AVP Flag
> M
> Event-Timestamp
> Records the time the event was reported.
> AVP Header
> 55 0
> Vendor ID
> 0
> VSA Type
> 55
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Event-Trigger
> Indicates an event that shall cause a re-request of charging rules.
> AVP Header
> 1006 10415
> Vendor ID
> 10415
> VSA Type
> 1006
> AVP Type
> ENUM. Supported values are:
> SGSN_CHANGE (0)
> QOS_CHANGE (1)
> RAT_CHANGE (2)
> TFT_CHANGE (3)
> PLMN_CHANGE (4)
> LOSS_OF_FLOW (5)
> RECOVERY_OF_FLOW (6)
> IP_CAN_CHANGE (7)
> GW_PCEF_MALFUNCTION (8) — obsolete; must not be used
> RESOURCES_LIMITATION (9) — obsolete; must not be used
> MAX_NR_BEARERS_REACHED (10) — obsolete; must not be used
> QOS_CHANGE_EXCEEDING_AUTHORIZATION (11)
> RAI_CHANGE (12)
> USER_LOCATION_CHANGE (13)
> NO_EVENT_TRIGGERS (14)
> OUT_OF_CREDIT (15)
> REALLOCATION_OF_CREDIT (16)
> REVALIDATION_TIMEOUT (17)
> UE_IP_ADDRESS_ALLOCATE (18)
> UE_IP_ADDRESS_RELEASE (19)
> DEFAULT_EPS_BEARER_QOS_CHANGE (20)
> AN_GW_CHANGE (21)
> SUCCESSFUL_RESOURCE_ALLOCATION (22)
> RESOURCE_MODIFICATION_REQUEST (23)
> PGW_TRACE_CONTROL (24)
> UE_TIME_ZONE_CHANGE (25)
> USAGE_REPORT (26)
> USAGE_THRESHOLD_REACHED (33)
> SERVICE_FLOW_DETECTION (34)
> PRESERVATION_CHANGED (2000)
> REACTIVATION_CHANGED (2001)
> TFT_DELETED (1000)
> LOSS_OF_BEARER (1001)
> RECOVERY_OF_BEARER (1002)
> POLICY_ENFORCEMENT_FAILED (1003)
> Group Value
> N/A
> AVP Flag
> M
> Event-Type
> This grouped AVP contains information about the type of chargeable telecommunication service/event for which the accounting-request message is generated.
> AVP Header
> 823 10415
> Vendor ID
> 10415
> VSA Type
> 823
> AVP Type
> GROUPED
> Group Value
> [ SIP_METHOD ]
> [ EVENT ]
> [ EXPIRES ]
> AVP Flag
> M
> Experimental-Result
> This AVP contains the Result code of SUCCESS or FAILURE. The exact value is specific to Vendor-Id.
> AVP Header
> 297 0
> Vendor ID
> 0
> VSA Type
> 297
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID ]
> [ EXPERIMENTAL_RESULT_CODE ]
> AVP Flag
> M
> Experimental-Result-Code
> This AVP contains vendor specific result codes to indicate temporary or permanent failures.
> AVP Header
> 298 0
> Vendor ID
> 0
> VSA Type
> 298
> AVP Type
> ENUM. Supported values are:
> DIAMETER_MULTI_ROUND_AUTH (1001)
> DIAMETER_SUCCESS (2001)
> DIAMETER_LIMITED_SUCCESS (2002)
> DIAMETER_PDP_CONTEXT_DELETION_INDICATION (2021)
> DIAMETER_UNREGISTERED_SERVICE (2003)
> DIAMETER_SUCCESS_NOT_SUPPORTED_USER_DATA (2004)
> DIAMETER_SUCCESS_SERVER_NAME_NOT_STORED (2005)
> DIAMETER_COMMAND_UNSUPPORTED (3001)
> DIAMETER_UNABLE_TO_DELIVER (3002)
> DIAMETER_REALM_NOT_SERVED (3003)
> DIAMETER_TOO_BUSY (3004)
> DIAMETER_LOOP_DETECTED (3005)
> DIAMETER_REDIRECT_INDICATION (3006)
> DIAMETER_APPLICATION_UNSUPPORTED (3007)
> DIAMETER_INVALID_HDR_BITS (3008)
> DIAMETER_INVALID_AVP_BITS (3009)
> DIAMETER_UNKNOWN_PEER (3010)
> DIAMETER_AUTHENTICATION_REJECTED (4001)
> DIAMETER_OUT_OF_SPACE (4002)
> ELECTION_LOST (4003)
> DIAMETER_END_USER_SERVICE_DENIED (4010)
> DIAMETER_CREDIT_CONTROL_NOT_APPLICABLE (4011)
> DIAMETER_CREDIT_LIMIT_REACHED (4012)
> INSUFFICIENT-RESOURCES (4041)
> COMMIT-FAILURE (4043)
> REFRESH-FAILURE (4044)
> QOS-PROFILE-FAILURE (4045)
> ACCESS-PROFILE-FAILURE (4046)
> PRIORITY-NOT-GRANTED (4047)
> DIAMETER_USER_DATA_NOT_AVAILABLE (4100)
> DIAMETER_PRIOR_UPDATE_IN_PROGRESS (4101)
> DIAMETER_ERROR_OUT_OF_RESOURCES (4121)
> DIAMETER_PCC_BEARER_EVENT (4141)
> AUTHENTICATION_DATA_UNAVAILABLE (4181)
> DIAMETER_AVP_UNSUPPORTED (5001)
> DIAMETER_UNKNOWN_SESSION_ID (5002)
> DIAMETER_AUTHORIZATION_REJECTED (5003)
> DIAMETER_INVALID_AVP_VALUE (5004)
> DIAMETER_MISSING_AVP (5005)
> DIAMETER_RESOURCES_EXCEEDED (5006)
> DIAMETER_CONTRADICTING_AVPS (5007)
> DIAMETER_AVP_NOT_ALLOWED (5008)
> DIAMETER_AVP_OCCURS_TOO_MANY_TIMES (5009)
> DIAMETER_NO_COMMON_APPLICATION (5010)
> DIAMETER_UNSUPPORTED_VERSION (5011)
> DIAMETER_UNABLE_TO_COMPLY (5012)
> DIAMETER_INVALID_BIT_IN_HEADER (5013)
> DIAMETER_INVALID_AVP_LENGTH (5014)
> DIAMETER_INVALID_MESSAGE_LENGTH (5015)
> DIAMETER_INVALID_AVP_BIT_COMBO (5016)
> DIAMETER_NO_COMMON_SECURITY (5017)
> BINDING-FAILURE (5021)
> DIAMETER_USER_UNKNOWN (5030)
> DIAMETER_RATING_FAILED (5031)
> MODIFICATION-FAILURE (5041)
> INVALID_SERVICE_INFORMATION (5061)
> FILTER_RESTRICTIONS (5062)
> REQUESTED_SERVICE_NOT_AUTHORIZED (5063)
> DUPLICATED_AF_SESSION (5064)
> IP_CAN_SESSION_NOT_AVAILABLE (5065)
> DIAMETER_ERROR_USER_DATA_NOT_RECOGNIZED (5100)
> DIAMETER_ERROR_OPERATION_NOT_ALLOWED (5101)
> DIAMETER_ERROR_USER_DATA_CANNOT_BE_READ (5102)
> DIAMETER_ERROR_USER_DATA_CANNOT_BE_MODIFIED (5103)
> DIAMETER_ERROR_USER_DATA_CANNOT_BE_NOTIFIED (5104)
> DIAMETER_ERROR_SUBS_DATA_ABSENT (5106)
> DIAMETER_ERROR_NO_SUBSCRIPTION_TO_DATA (5107)
> DIAMETER_ERROR_DSAI_NOT_AVAILABLE (5108)
> DIAMETER_ERROR_START_INDICATION (5120)
> DIAMETER_ERROR_STOP_INDICATION (5121)
> DIAMETER_ERROR_UNKNOWN_MBMS_BEARER_SERVICE (5122)
> DIAMETER_ERROR_SERVICE_AREA (5123)
> DIAMETER_ERROR_INITIAL_PARAMETERS (5140)
> DIAMETER_ERROR_TRIGGER_EVENT (5141)
> DIAMETER_PCC_RULE_EVENT (5142)
> DIAMETER_ERROR_BEARER_NOT_AUTHORIZED (5143)
> DIAMETER_ERROR_TRAFFIC_MAPPING_INFO_REJECTED (5144)
> DIAMETER_QOS_RULE_EVENT (5145)
> DIAMETER_BEARER_EVENT (5146) — in 10.2 and earlier releases
> DIAMETER_BEARER_EVENT (4142) — in 11.0 and later releases
> DIAMETER_ERROR_CONFLICTING_REQUEST (5147)
> ERROR_UNKNOWN_EPS_SUBSCRIPTION (5420)
> ERROR_RAT_NOT_ALLOWED (5421)
> ERROR_ROAMING_NOT_ALLOWED (5402)
> ERROR_EQUIPMENT_UNKNOWN (5422)
> Group Value
> N/A
> AVP Flag
> M
> Expiration-Date
> This attribute contains the information on when the subscription to the CSG-Id expires.
> AVP Header
> 1439 10415
> Vendor ID
> 10415
> VSA Type
> 1439
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Expires
> This AVP holds the content of the "Expires" header.
> AVP Header
> 888 10415
> Vendor ID
> 10415
> VSA Type
> 888
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Exponent
> Exponent AVP contains the exponent value to be applied for the Value-Digit AVP within the Unit-Value AVP.
> AVP Header
> 429 0
> Vendor ID
> 0
> VSA Type
> 429
> AVP Type
> INT32
> Group Value
> N/A
> AVP Flag
> M
> Extended-QoS-Filter-Rule
> Defines one or more traffic flows together with a set of QoS parameters that should be applied to the flow(s) by the Resource Management Function.
> AVP Header
> 6066 0
> Vendor ID
> 0
> VSA Type
> 6066
> AVP Type
> INT32
> Group Value
> N/A
> AVP Flag
> M
> External-Client
> This attribute contains the identities of the external clients that are allowed to locate a target UE for a MT-LR.
> AVP Header
> 1479 10415
> Vendor ID
> 10415
> VSA Type
> 1479
> AVP Type
> GROUPED
> Group Value
> [ CLIENT_IDENTITY ]
> [ GMLC_RESTRICTION ]
> [ NOTIFICATION_TO_UE_USER ]
> AVP Flag
> M
> Failed-AVP
> This AVP contains the missing and/or unsupported AVPs that caused the failure.
> AVP Header
> 279 0
> Vendor ID
> 0
> VSA Type
> 279
> AVP Type
> GROUPED
> Group Value
> N/A
> AVP Flag
> M
> FDR-Reason
> Indicates the reason for FDR cut.
> AVP Header
> 1501 10415
> Vendor ID
> 10415
> VSA Type
> 1501
> AVP Type
> ENUM. Supported values are:
> END_FLOW (0)
> IPGW_HO (1)
> FORCED_CLOSURE (2)
> Group Value
> N/A
> AVP Flag
> M
> Feature-List
> This AVP contains a bit mask indicating the supported features of an application.
> AVP Header
> 630 10415
> Vendor ID
> 10415
> VSA Type
> 630
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Feature-List-ID
> This AVP contains the identity of the featured list.
> AVP Header
> 629 10415
> Vendor ID
> 10415
> VSA Type
> 629
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Feature-List-ID-Resp
> Contains the identity of the featured list.
> AVP Header
> 629 10415
> Vendor ID
> 10415
> VSA Type
> 629
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Feature-List-Resp
> Contains a bit mask indicating the supported features of an application.
> AVP Header
> 630 10415
> Vendor ID
> 10415
> VSA Type
> 630
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> FID
> Contains the Flow Correlation ID.
> AVP Header
> 7003 10415
> Vendor ID
> 10415
> VSA Type
> 7003
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Filter-Id
> The name of the filter list for this user.
> AVP Header
> 11 0
> Vendor ID
> 0
> VSA Type
> 11
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Final-Unit-Action
> The Final-Unit-Action AVP defines the behavior of the service element when the user's account cannot cover the cost of the service.
> AVP Header
> 449 0
> Vendor ID
> 0
> VSA Type
> 449
> AVP Type
> ENUM. Supported values are:
> TERMINATE(0)
> REDIRECT(1)
> RESTRICT_ACCESS (2)
> Group Value
> N/A
> AVP Flag
> M
> Final-Unit-Indication
> Indicates that the Granted-Service-Unit AVP in the Credit-Control-Answer, or in the AA answer, contains the final units for the service.
> AVP Header
> 430 0
> Vendor ID
> 0
> VSA Type
> 430
> AVP Type
> GROUPED
> Group Value
> [ FINAL_UNIT_ACTION ]
> [ RESTRICTION_FILTER_RULE ]
> [ FILTER_ID ]
> [ REDIRECT_SERVER ]
> AVP Flag
> M
> Firmware-Revision
> Support for Vendor Specific Applications.
> AVP Header
> 267 0
> Vendor ID
> 0
> VSA Type
> 267
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Flow-Description
> Defines the service flow filter parameters for a charging rule.
> AVP Header
> 507 10415
> Vendor ID
> 10415
> VSA Type
> 507
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> Flow-Description-Info
> This grouped AVP is used within the Flow-Info AVP to identify a flow and associated precedence value from the AGW to the PCRF.
> AVP Header
> 1022 5535
> Vendor ID
> 5535
> VSA Type
> 1022
> AVP Type
> GROUPED
> Group Value
> [ FLOW_DESCRIPTION ]
> [ PRECEDENCE ]
> AVP Flag
> M
> Flow-Direction
> This AVP indicates the direction/directions that a filter is applicable, downlink only, uplink only or both down- and uplink (bidirectional).
> AVP Header
> 1080 10415
> Vendor ID
> 10415
> VSA Type
> 1080
> AVP Type
> ENUM. Supported values are:

> • | UNSPECIFIED (0)

> • | DOWNLINK (1)

> • | UPLINK (2)

> • | BIDIRECTIONAL (3)

> Group Value
> N/A
> AVP Flag
> M
> Flow-Grouping
> Indicates that no other IP Flows shall be transported together with the listed IP Flows in the same PDP context(s).
> AVP Header
> 508 10415
> Vendor ID
> 10415
> VSA Type
> 508
> AVP Type
> GROUPED
> Group Value
> [ FLOWS ]
> AVP Flag
> M
> Flow-Identifier
> This AVP contains the identifier of the IP flow(s) of a given Flow-Info to which specific information refers.
> AVP Header
> 810 5535
> Vendor ID
> 5535
> VSA Type
> 810
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Flow-Info
> This AVP contains the customized information of the IP flow(s). This is a unique identifier within the context of an IP-CAN session for the IP flow(s) given within the same Flow-Info AVP. The flow identifier is selected by AGW. The Flow-Description AVP(s) describe the flow using an IPFilterRule. If two Flow-Description AVPs are included, one shall represent the uplink and the other the downlink.
> AVP Header
> 809 5535
> Vendor ID
> 5535
> VSA Type
> 809
> AVP Type
> GROUPED
> Group Value
> [ FLOW_IDENTIFIER ]
> [ FLOW_DESCRIPTION_INFO ]
> [ REQUESTED_QOS ]
> [ GRANTED_QOS ]
> [ FLOW_STATUS ]
> AVP Flag
> M
> Flow-Information
> This AVP contains the information from a single IP flow packet filter including the flow description.
> AVP Header
> 1058 10415
> Vendor ID
> 10415
> VSA Type
> 1058
> AVP Type
> GROUPED
> Group Value
> [ FLOW_DESCRIPTION ]
> [ PACKET_FILTER_IDENTIFIER ]
> [ TOS_TRAFFIC_CLASS ]
> [ SECURITY_PARAMETER_INDEX ]
> [ FLOW_LABEL ]
> [ FLOW_DIRECTION ]
> AVP Flag
> M
> Flow-Label
> Contains the IPv6 flow label header field.
> AVP Header
> 1057 10415
> Vendor ID
> 10415
> VSA Type
> 1057
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Flow-Number
> This AVP contains the ordinal number of the IP flow(s).
> AVP Header
> 509 10415
> Vendor ID
> 10415
> VSA Type
> 509
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Flow-Operation
> This APV indicates the IP-CAN flow event that causes a request for PCC rules.
> AVP Header
> 800 5535
> Vendor ID
> 5535
> VSA Type
> 800
> AVP Type
> ENUM. Supported values are:
> TERMINATION (0)
> ESTABLISHMENT (1)
> MODIFICATION (2)
> Group Value
> N/A
> AVP Flag
> M
> Flows
> The flow identifiers of the IP flows related to a charging rule as provided by the Application Function (AF).
> AVP Header
> 510 10415
> Vendor ID
> 10415
> VSA Type
> 510
> AVP Type
> GROUPED
> Group Value
> [ MEDIA_COMPONENT_NUMBER ]
> [ FLOW_NUMBER ]
> AVP Flag
> M
> Flow-Status
> Describes whether the IP flow(s) are enabled or disabled.
> AVP Header
> 511 10415
> Vendor ID
> 10415
> VSA Type
> 511
> AVP Type
> ENUM. Supported values are:
> ENABLED-UPLINK (0)
> ENABLED-DOWNLINK (1)
> ENABLED (2)
> DISABLED (3)
> REMOVED (4)
> TERMINATE (5)
> Group Value
> N/A
> AVP Flag
> M
> Flow-Usage
> Provides information about the usage of IP Flows.
> AVP Header
> 512 10415
> Vendor ID
> 10415
> VSA Type
> 512
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Framed-Appletalk-Link
> This AVP contains the AppleTalk network number that should be used for the serial link to the user, which is another AppleTalk router.
> AVP Header
> 37 0
> Vendor ID
> 0
> VSA Type
> 37
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Framed-Appletalk-Network
> This AVP contains the AppleTalk Network number that the NAS should probe to allocate an AppleTalk node for the user.
> AVP Header
> 38 0
> Vendor ID
> 0
> VSA Type
> 38
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Framed-Appletalk-Zone
> This AVP contains the AppleTalk Default Zone to be used for the user.
> AVP Header
> 39 0
> Vendor ID
> 0
> VSA Type
> 39
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-Compression
> This AVP contains the compression protocol to be used for the link.
> AVP Header
> 13 0
> Vendor ID
> 0
> VSA Type
> 13
> AVP Type
> ENUM. Supported values are:
> None (0)
> VJ_TCP-IP_header_compression (1)
> IPX-header-compression (2)
> Stac-LZS-compression (3)
> Group Value
> N/A
> AVP Flag
> M
> Framed-Interface-Id
> This AVP contains the IPv6 interface identifier to be configured for the user.
> AVP Header
> 96 0
> Vendor ID
> 0
> VSA Type
> 96
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> Framed-IP-Address
> This AVP contains an IPv4 address of the type specified in the attribute value to be configured for the user.
> AVP Header
> 8 0
> Vendor ID
> 0
> VSA Type
> 8
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-IP-Netmask
> This AVP contains the four octets of the IPv4 netmask to be configured for the user when the user is a router to a network.
> AVP Header
> 9 0
> Vendor ID
> 0
> VSA Type
> 9
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-IPv6-Pool
> This AVP contains the name of an assigned pool that must be used to assign an IPv6 prefix for the user.
> AVP Header
> 100 0
> Vendor ID
> 0
> VSA Type
> 100
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-IPv6-Prefix
> This AVP contains the IPv6 prefix to be configured for the user. One or more AVPs MAY be used in authorization requests as a hint to the server that a specific IPv6 prefixes are desired.
> AVP Header
> 97 0
> Vendor ID
> 0
> VSA Type
> 97
> AVP Type
> OctetString
> Group Value
> N/A
> AVP Flag
> M
> Framed-IPv6-Route
> This AVP contains the ASCII routing information to be configured for the user on the NAS.
> AVP Header
> 99 0
> Vendor ID
> 0
> VSA Type
> 99
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> Framed-IPX-Network
> This AVP contains the IPX network number to be configured for the user.
> AVP Header
> 23 0
> Vendor ID
> 0
> VSA Type
> 23
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Framed-MTU
> This AVP contains the Maximum Transmission Unit to be configured for the user, when it is not negotiated by some other means (such as PPP).
> AVP Header
> 12 0
> Vendor ID
> 0
> VSA Type
> 12
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Framed-Pool
> This AVP contains the name of an assigned address pool that SHOULD be used to assign an address for the user.
> AVP Header
> 88 0
> Vendor ID
> 0
> VSA Type
> 88
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-Protocol
> This AVP contains the framing to be used for framed access.
> AVP Header
> 7 0
> Vendor ID
> 0
> VSA Type
> 7
> AVP Type
> ENUM. Supported values are:
> PPP (1)
> SLIP (2)
> AppleTalk-Remote-Access-Protocol_ARAP (3)
> Gandalf-proprietary-SingleLink_MultiLink-protocol (4)
> Xylogics-proprietary_IPX-SLIP (5)
> X75-Synchronous (6)
> Group Value
> N/A
> AVP Flag
> M
> Framed-Route
> This AVP contains the ASCII routing information to be configured for the user on the NAS.
> AVP Header
> 22 0
> Vendor ID
> 0
> VSA Type
> 22
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Framed-Routing
> This AVP contains the routing method for the user when the user is a router to a network.
> AVP Header
> 10 0
> Vendor ID
> 0
> VSA Type
> 10
> AVP Type
> ENUM. Supported values are:
> None (0)
> Send-routing-packets (1)
> Listen-for-routing-packets (2)
> Send-and-Listen (3)
> Group Value
> N/A
> AVP Flag
> M
> From-SIP-Header
> This AVP contains the information in the From header
> AVP Header
> 644 10415
> Vendor ID
> 10415
> VSA Type
> 644
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Geodetic-Information
> This AVP provides geodetic location information of the user.
> AVP Header
> 1609 10415
> Vendor ID
> 10415
> VSA Type
> 1609
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Geographical-Information
> This AVP provides geographical location information of the user.
> AVP Header
> 1608 10415
> Vendor ID
> 10415
> VSA Type
> 1608
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Geospatial-Location
> This AVP provides location information using the Location Configuration Information (LCI) format.
> AVP Header
> 356 13019
> Vendor ID
> 13019
> VSA Type
> 356
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> GERAN-Vector
> This AVP contains Authentication Information for GERAN.
> AVP Header
> 6019 10415
> Vendor ID
> 10415
> VSA Type
> 6019
> AVP Type
> GROUPED
> Group Value
> [ ITEM_NUMBER ]
> [ RAND ]
> [ SRES ]
> [ KC_KEY ]
> AVP Flag
> M
> GGSN-Address
> GGSN IP address used by the GTP control plane for the context establishment. It is the same as the IP-address of the GGSN that generated the GPRS Charging ID used in the GCDRs.
> AVP Header
> 847 10415
> Vendor ID
> 10415
> VSA Type
> 847
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Globally-Unique-Address
> This AVP represents the UE's address.
> AVP Header
> 300 13019
> Vendor ID
> 13019
> VSA Type
> 300
> AVP Type
> GROUPED
> Group Value
> [ Framed_IP_Address ]
> [ Address_Realm ]
> AVP Flag
> M
> GMLC-Address
> This AVP contains the IPv4 or IPv6 address of the V-GMLC associated with the serving node.
> AVP Header
> 1474 10415
> Vendor ID
> 10415
> VSA Type
> 1474
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> GMLC-Number
> This AVP contains the ISDN number of the GMLC.
> AVP Header
> 1474 10415
> Vendor ID
> 10415
> VSA Type
> 1474
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> GMLC-Restriction
> This attritbue contains GMLC Restriction List.
> AVP Header
> 1481 10415
> Vendor ID
> 10415
> VSA Type
> 1481
> AVP Type
> ENUM. Supported values are:
> GMLC_LIST (0)
> HOME_COUNTRY (1)
> Group Value
> N/A
> AVP Flag
> M
> GPRS-Subscription-Data
> This AVP contains the information related to the user profile relevant for GPRS.
> AVP Header
> 1467 10415
> Vendor ID
> 10415
> VSA Type
> 1467
> AVP Type
> GROUPED
> Group Value
> [ COMPLETE_DATA_LIST_INCLUDED_INDICATOR ]
> [ PDP_CONTEXT ]
> AVP Flag
> M
> Granted-QoS
> It is used within the Flow-Info AVP to indicate the QoS granted to the UE for a particular IP flow in the high rate packet data radio access network.
> AVP Header
> 811 5535
> Vendor ID
> 5535
> VSA Type
> 811
> AVP Type
> GROUPED
> Group Value
> [ QoS-Class ]
> [ Min-Bandwidth-UL ]
> [ Min-Bandwidth-DL ]
> AVP Flag
> M
> Granted-Service-Unit
> This AVP contains the amount of units that the Diameter credit-control client can provide to the end user until the service must be released or the new Credit-Control-Request must be sent.
> AVP Header
> 431 0
> Vendor ID
> 0
> VSA Type
> 431
> AVP Type
> GROUPED
> Group Value
> [ TARIFF_TIME_CHANGE ]
> [ TARIFF_CHANGE_USAGE ]
> [ CC_TIME ]
> [ CC_MONEY ]
> [ CC_TOTAL_OCTETS ]
> [ CC_INPUT_OCTETS ]
> [ CC_OUTPUT_OCTETS ]
> [ CC_SERVICE_SPECIFIC_UNITS ]
> AVP Flag
> M
> G-S-U-Pool-Identifier
> Specifies the credit pool from which credit is drawn for this unit type.
> AVP Header
> 453 0
> Vendor ID
> 0
> VSA Type
> 453
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> G-S-U-Pool-Reference
> This AVP contains a reference to a credit pool, a unit-type and a multiplier (using the Unit-Value AVP). It is used within Granted-Service-Units AVP to indicate that credit Service-Units AVP to indicate that credit of a particular type is pooled.
> AVP Header
> 457 0
> Vendor ID
> 0
> VSA Type
> 457
> AVP Type
> GROUPED
> Group Value
> [ G_S_U_POOL_IDENTIFIER ]
> [ CC_UNIT_TYPE ]
> [ UNIT_VALUE ]
> AVP Flag
> M
> Guaranteed-Bitrate-DL
> Defines the guaranteed bit rate allowed for the downlink direction.
> AVP Header
> 1025 10415
> Vendor ID
> 10415
> VSA Type
> 1025
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Guaranteed-Bitrate-UL
> Defines the guaranteed bit rate allowed for the uplink direction.
> AVP Header
> 1026 10415
> Vendor ID
> 10415
> VSA Type
> 1026
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> HBM-Address
> HBM-Address.
> AVP Header
> 1462 10415
> Vendor ID
> 10415
> VSA Type
> 1462
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Home-Agent
> Used to convey the HA IPv4 address that the MS requests or the HA IPv4 address that the H-AAA assigns.
> AVP Header
> 3 5535
> Vendor ID
> 5535
> VSA Type
> 3
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Host-IP-Address
> This attribute indicates the Mobile station IP address.
> AVP Header
> 257 0
> Vendor ID
> 0
> VSA Type
> 257
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> HPLMN-ODB
> This AVP contains a bit mask indicating the HPLMN specific services of a subscriber that are barred by the operator.
> AVP Header
> 1418 10415
> Vendor ID
> 10415
> VSA Type
> 1418
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> HSGW-Address
> HSGW IP address. In 12.2 and later releases, this attribute is deprecated.
> AVP Header
> 1415 10415
> Vendor ID
> 10415
> VSA Type
> 1415
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> ICS-Indicator
> ICS-Indicator
> AVP Header
> 1491 10415
> Vendor ID
> 10415
> VSA Type
> 1491
> AVP Type
> ENUM. Supported values are:

> • | FALSE (0)

> • | TRUE (1)

> Group Value
> N/A
> AVP Flag
> M
> IDA-Flags
> The IDA-Flags AVP contains a bit mask.
> AVP Header
> 1441 10415
> Vendor ID
> 10415
> VSA Type
> 1441
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Identity-Set
> Indicates the requested set of IMS Public identities.
> AVP Header
> 708 0
> Vendor ID
> 0
> VSA Type
> 708
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> N/A
> Idle-Timeout
> Sets the maximum number of consecutive seconds of idle connection allowable to the user before termination of the session or before a prompt is issued.
> AVP Header
> 28 0
> Vendor ID
> 0
> VSA Type
> 28
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> IDR-Flags
> Contains a bit mask.
> AVP Header
> 1490 10415
> Vendor ID
> 10415
> VSA Type
> 1490
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> IMEI
> This AVP contains the International Mobile Equipment Identity.
> AVP Header
> 6003 10415
> Vendor ID
> 10415
> VSA Type
> 6003
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Immediate-Response-Preferred
> Indicates which type of AV is requested for immediate use in the MME/SGSN.
> AVP Header
> 6015 10415
> Vendor ID
> 10415
> VSA Type
> 6015
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> IMS-3GPP-Charging-Id
> IMS-3GPP-Charging ID.
> AVP Header
> 2 10415
> Vendor ID
> 10415
> VSA Type
> 2
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> IMS-Charging-Identifier
> This AVP holds the IMS Charging Identifier (ICID) as generated by an IMS node for a SIP session.
> AVP Header
> 841 10415
> Vendor ID
> 10415
> VSA Type
> 841
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> IMS-Communication-Service-Identifier
> Holds the IMS Communication Service Identifier (ICSI) as contained in the P-Asserted-Service header of a SIP request to identify an IMS Communication Service as defined in TS 24.229.
> AVP Header
> 1281 10415
> Vendor ID
> 10415
> VSA Type
> 1281
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> IMS-Information
> This grouped AVP allows the transmission of additional IMS service specific information elements.
> AVP Header
> 876 10415
> Vendor ID
> 10415
> VSA Type
> 876
> AVP Type
> GROUPED
> Group Value
> [ EVENT_TYPE ]
> [ ROLE_OF_NODE ]
> [ NODE_FUNCTIONALITY ]
> [ USER_SESSION_ID ]
> [ CALLING_PARTY_ADDRESS ]
> [ CALLED_PARTY_ADDRESS ]
> [ CALLED_ASSERTED_IDENTITY ]
> [ ASSOCIATED_URI ]
> [ TIME_STAMPS ]
> [ APPLICATION_SERVER_INFORMATION ]
> [ INTER_OPERATOR_IDENTIFIER ]
> [ IMS_CHARGING_IDENTIFIER ]
> [ SDP_SESSION_DESCRIPTION ]
> [ SDP_MEDIA_COMPONENT ]
> [ MESSAGE_BODY ]
> [ CAUSE_CODE ]
> [ ACCESS_NETWORK_INFORMATION ]
> [ EARLY_MEDIA_DESCRIPTION ]
> AVP Flag
> M
> IMS-Voice-Over-PS-Sessions-Supported
> IMS-Voice-Over-PS-Sessions-Supported
> AVP Header
> 1492 10415
> Vendor ID
> 10415
> VSA Type
> 1492
> AVP Type
> ENUM. Supported values are:

> • | NOT_SUPPORTED (0)

> • | SUPPORTED (1)

> Group Value
> N/A
> AVP Flag
> M
> IMSI-Unauthenticated-Flag
> This attribute indicates whether or not the served IMSI is authenticated.
> AVP Header
> 2308 10415
> Vendor ID
> 10415
> VSA Type
> 2308
> AVP Type
> ENUM. Supported values are:
> AUTHENTICATED (0)
> UNAUTHENTICATED (1)
> Group Value
> N/A
> AVP Flag
> M
> Inband-Security-Id
> Advertise support of the Security portion of the application.
> AVP Header
> 299 0
> Vendor ID
> 0
> VSA Type
> 299
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Incoming-Trunk-Group-ID
> This AVP identifies the incoming PSTN leg.
> AVP Header
> 852 0
> Vendor ID
> 0
> VSA Type
> 852
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Integrity-Key
> This AVP contains the Integrity Key (IK).
> AVP Header
> 626 10415
> Vendor ID
> 10415
> VSA Type
> 626
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Inter-Operator-Identifier
> This AVP contains the identification of the network neighbors (originating and terminating) as exchanged via SIP signalling. The Inter-Operator-Identifier AVP contains the CIC code present in the Carrier-info message.
> AVP Header
> 838 10415
> Vendor ID
> 10415
> VSA Type
> 838
> AVP Type
> GROUPED
> Group Value
> [ ORIGINATING_IOI ]
> [ TERMINATING_IOI ]
> AVP Flag
> M
> IP-CAN-Type
> This AVP indicate the type of Connectivity Access Network in which the user is connected.
> AVP Header
> 1027 10415
> Vendor ID
> 10415
> VSA Type
> 1027
> AVP Type
> ENUM. Supported values are:
> 3GPP (0)
> DOCSIS (1)
> xDSL (2)
> WiMAX (3)
> 3GPP2 (4)
> 3GPP-EPS (5)
> NON-3GPP-EPS (6)
> Group Value
> N/A
> AVP Flag
> M
> IP-MMS
> IP mobility selector.
> AVP Header
> 6076 10415
> Vendor ID
> 10415
> VSA Type
> 6076
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> IP-Version-Authorized
> Used to indicate whether the MS is authorised for using IPv4 and/or IPv6.
> AVP Header
> 11 5535
> Vendor ID
> 5535
> VSA Type
> 11
> AVP Type
> ENUM. Supported values are:
> IPv4_or_IPv6 (0)
> IPv4_ONLY (1)
> IPv6_ONLY (2)
> Group Value
> N/A
> AVP Flag
> M
> Item-Number
> If more than one EPS Vector is included within one Authentication-Info AVP, the Item-Number AVP shall be present within each EPS Vector.
> AVP Header
> 1419 10415
> Vendor ID
> 10415
> VSA Type
> 1419
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> KASME
> This AVP contains the KASME (EAP Authentication Vector).
> AVP Header
> 1450 10415
> Vendor ID
> 10415
> VSA Type
> 1450
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> KC-Key
> This AVP contains the Ciphering Key.
> AVP Header
> 1453 10415
> Vendor ID
> 10415
> VSA Type
> 1453
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Last-CellSector-ID
> String contains last Cell ID and Sector ID.
> AVP Header
> 1420 10415
> Vendor ID
> 10415
> VSA Type
> 1420
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Last-CellSector-Location
> Indicates subscriber last cell/sector location.
> AVP Header
> 536 10415
> Vendor ID
> 10415
> VSA Type
> 536
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Last-UE-Activity-Time
> Last-UE-Activity-Time
> AVP Header
> 1494 10415
> Vendor ID
> 10415
> VSA Type
> 1494
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Latching-Indication
> This AVP contains the latching indication.
> AVP Header
> 457 13019
> Vendor ID
> 13019
> VSA Type
> 457
> AVP Type
> ENUM. Supported values are:
> LATCH (0)
> RELATCH (1)
> Group Value
> N/A
> AVP Flag
> N/A
> LCS-Info
> This AVP contains LCS related information for a subscriber.
> AVP Header
> 1473 10415
> Vendor ID
> 10415
> VSA Type
> 1473
> AVP Type
> GROUPED
> Group Value
> [ GMLC_ADDRESS ]
> [ LCS_PRIVACYEXCEPTION ]
> [ MO_LR ]
> AVP Flag
> M
> LCS-PrivacyException
> This AVP contains the classes of LCS Client that are allowed to locate any target UE.
> AVP Header
> 1475 10415
> Vendor ID
> 10415
> VSA Type
> 1475
> AVP Type
> GROUPED
> Group Value
> [ SS_CODE ]
> [ SS_STATUS ]
> [ NOTIFICATION_TO_UE_USER ]
> [ EXTERNAL_CLIENT ]
> [ PLMN_CLIENT ]
> [ SERVICE_TYPE ]
> AVP Flag
> M
> LI-Information
> This AVP holds all the other surveillance AVPs.
> AVP Header
> 218 4491
> Vendor ID
> 4491
> VSA Type
> 218
> AVP Type
> GROUPED
> Group Value
> [ EVENT_MESSAGE_TYPE ]
> [ ELEMENT_TYPE ]
> [ ELEMENT_ID ]
> [ TAP_ID ]
> [ SIP_MESSAGE ]
> [ DIRECT_MESSAGE ]
> [ DIRECTION ]
> [ DIALOG_ID ]
> [ NEW_DIALOG_ID ]
> [ CORRELATE_REASON]
> [ BCID ]
> AVP Flag
> M
> Line-Identifier
> This AVP contains a fixed broadband access line identifier associated with the user.
> AVP Header
> 500 13019
> Vendor ID
> 13019
> VSA Type
> 500
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Local-Sequence-Number
> This AVP holds the service data container sequence number; incremented by 1 for each service data container closed.
> AVP Header
> 2063 10415
> Vendor ID
> 10415
> VSA Type
> 2063
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Location-Area-Identity
> This AVP contains the location area identification of the user.
> AVP Header
> 1606 10415
> Vendor ID
> 10415
> VSA Type
> 1606
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Location-Information
> This AVP contains the location information (or a pointer to such information) in a form that is suitable for the requesting application.
> AVP Header
> 350 13019
> Vendor ID
> 13019
> VSA Type
> 350
> AVP Type
> GROUPED
> Group Value
> [ LINE_IDENTIFIER ]
> [ CIVIC_LOCATION ]
> [ GEOSPATIAL_LOCATION ]
> AVP Flag
> M
> Logical-Access-Id
> This specifies the identity of the logical access where the user equipment is connected.
> AVP Header
> 302 0
> Vendor ID
> 0
> VSA Type
> 302
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Loose-Route-Indication
> Indicates to the S-CSCF whether or not the loose route mechanism is required to serve the registered Public User Identities.
> AVP Header
> 638 10415
> Vendor ID
> 10415
> VSA Type
> 638
> AVP Type
> ENUM. Supported values are:
> LOOSE_ROUTE_NOT_REQUIRED (0)
> LOOSE_ROUTE_REQUIRED (1)
> Group Value
> N/A
> AVP Flag
> N/A
> Mandatory-Capability
> This AVP contains single determined mandatory capability of an S-CSCF.
> AVP Header
> 604 10415
> Vendor ID
> 10415
> VSA Type
> 604
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Max-Requested-Bandwidth
> Indicates the maximum subscriber requested bandwidth.
> AVP Header
> 313 10415
> Vendor ID
> 10415
> VSA Type
> 313
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Max-Requested-Bandwidth-DL
> Indicates the maximum requested bandwidth in bits per second for a downlink IP flow.
> AVP Header
> 515 10415
> Vendor ID
> 10415
> VSA Type
> 515
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Max-Requested-Bandwidth-UL
> Indicates the maximum requested bandwidth in bits per second for an uplink IP flow.
> AVP Header
> 516 10415
> Vendor ID
> 10415
> VSA Type
> 516
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> MBMS-2G-3G-Indicator
> Indicates whether the MBMS bearer service will be delivered in 2G only, 3G only of both coverage areas.
> AVP Header
> 907 10415
> Vendor ID
> 10415
> VSA Type
> 907
> AVP Type
> ENUM. Supported values are:
> 2G (0)
> 3G (1)
> 2G_AND_3G (2)
> Group Value
> N/A
> AVP Flag
> M
> MBMS-BMSC-SSM-IP-Address
> Contains the value of BM-SCs IPv4 address for Source Specific Multicasting.
> AVP Header
> 918 10415
> Vendor ID
> 10415
> VSA Type
> 918
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-BMSC-SSM-IPv6-Address
> Contains the value of BM-SCs IPv6 address for Source Specific Multicasting.
> AVP Header
> 919 10415
> Vendor ID
> 10415
> VSA Type
> 919
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Counting-Information
> Contains explicit information about whether the MBMS Counting procedures are applicable for the MBMS Service that is about to start.
> AVP Header
> 914 10415
> Vendor ID
> 10415
> VSA Type
> 914
> AVP Type
> ENUM. Supported values are:
> COUNTING_NOT_APPLICABLE (0)
> COUNTING_APPLICABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> MBMS-GGSN-Address
> Contains the value of GGSN’s IPv4 address for user plane data.
> AVP Header
> 916 10415
> Vendor ID
> 10415
> VSA Type
> 916
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-GGSN-IPv6-Address
> Contains the value of GGSN’s IPv6 address for user plane data.
> AVP Header
> 917 10415
> Vendor ID
> 10415
> VSA Type
> 917
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Required-QoS
> Indicates the quality of service required for the MBMS bearer service.
> AVP Header
> 913 10415
> Vendor ID
> 10415
> VSA Type
> 913
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Service-Area
> Indicates the area over which the MBMS bearer service has to be distributed
> AVP Header
> 903 10415
> Vendor ID
> 10415
> VSA Type
> 903
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Service-Type
> Contains explicit information about the type of service that the BM-SC Start Procedure is about to start.
> AVP Header
> 906 10415
> Vendor ID
> 10415
> VSA Type
> 906
> AVP Type
> ENUM. Supported values are:
> MULTICAST (0)
> BROADCAST (1)
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Session-Duration
> Indicates the estimated session duration, if available.
> AVP Header
> 904 10415
> Vendor ID
> 10415
> VSA Type
> 904
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Session-Identity
> Identifies a transmission of a specific MBMS session along with TMGI.
> AVP Header
> 908 10415
> Vendor ID
> 10415
> VSA Type
> 908
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Session-Repetition-number
> Contains the session identity repetition number of the MBMS transmission session on the Gmb interface.
> AVP Header
> 912 10415
> Vendor ID
> 10415
> VSA Type
> 912
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-StartStop-Indication
> Indicates whether it is session start or stop procedure.
> AVP Header
> 902 10415
> Vendor ID
> 10415
> VSA Type
> 902
> AVP Type
> ENUM. Supported values are:
> START (0)
> STOP (1)
> UPDATE (2)
> Group Value
> N/A
> AVP Flag
> M
> MBMS-Time-To-Data-Transfer
> Indicates the expected time between reception of the MBMS Session Start and the commencement of the MBMS Data flow.
> AVP Header
> 911 10415
> Vendor ID
> 10415
> VSA Type
> 911
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MBMS-User-Data-Mode-Indication
> Specifies whether the sending entity supports unicast or multicast mode of operation.
> AVP Header
> 915 10415
> Vendor ID
> 10415
> VSA Type
> 915
> AVP Type
> ENUM. Supported values are:
> UNICAST (0)
> MULTICAST_AND_UNICAST (1)
> Group Value
> N/A
> AVP Flag
> M
> Media-Component-Description
> This AVP contains service information for a single media component within an Application Function (AF) session.
> AVP Header
> 517 10415
> Vendor ID
> 10415
> VSA Type
> 517
> AVP Type
> GROUPED
> Group Value
> [ MEDIA_COMPONENT_NUMBER ]
> [ MEDIA_SUB_COMPONENT ]
> [ AF_APPLICATION_IDENTIFIER ]
> [ MEDIA_TYPE ]
> [ MAX_REQUESTED_BANDWIDTH_UL ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> [ FLOW_STATUS ]
> [ RS_BANDWIDTH ]
> [ RR_BANDWIDTH ]
> AVP Flag
> M
> Media-Component-Number
> This AVP contains the ordinal number of the media component.
> AVP Header
> 518 10415
> Vendor ID
> 10415
> VSA Type
> 518
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Media-Initiator-Flag
> This AVP indicates which party has requested the session modification.
> The default value is "0" indicating the called party initiated the modification

> • | [0] called party

> • | [1] calling party

> • | [2] unknown

> AVP Header
> 882 10415
> Vendor ID
> 10415
> VSA Type
> 882
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Media-Initiator-Party
> This AVP enumerated in IMS charging, holds the address (SIP URI or TEL URI) of the party (Public User ID or Public Service ID) who initiates the media action, like adding/removing, connecting/disconnecting the media.
> AVP Header
> 1288 10415
> Vendor ID
> 10415
> VSA Type
> 1288
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Media-Sub-Component
> The requested QoS and filters for the set of IP flows identified by their common Flow-Identifier.
> AVP Header
> 519 10415
> Vendor ID
> 10415
> VSA Type
> 519
> AVP Type
> GROUPED
> Group Value
> [ FLOW_NUMBER ]
> [ FLOW_DESCRIPTION ]
> [ FLOW_STATUS ]
> [ FLOW_USAGE ]
> [ MAX_REQUESTED_BANDWIDTH_UL ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> AVP Flag
> M
> Media-Type
> The media types indicate the type of media in the same way as the SDP media types with the same names like AUDIO, VIDEO.
> AVP Header
> 520 10415
> Vendor ID
> 10415
> VSA Type
> 520
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> MEID
> This AVP contains the International Mobile Equipment Identity.
> AVP Header
> 6110 10415
> Vendor ID
> 10415
> VSA Type
> 6110
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Message-Body
> This grouped AVP holds information about the message bodies including user-to-user data.
> AVP Header
> 889 10415
> Vendor ID
> 10415
> VSA Type
> 889
> AVP Type
> GROUPED
> Group Value
> [ CONTENT_TYPE ]
> [ CONTENT_LENGTH ]
> [ CONTENT_DISPOSITION ]
> [ ORIGINATOR ]
> AVP Flag
> M
> Metering-Method
> Defines what parameters shall be metered for offline charging.
> AVP Header
> 1007 10415
> Vendor ID
> 10415
> VSA Type
> 1007
> AVP Type
> ENUM. Supported values are:
> DURATION (0)
> VOLUME (1)
> DURATION_VOLUME (2)
> Group Value
> N/A
> AVP Flag
> M
> Min-Bandwidth-DL
> This AVP contains the requested/granted data rate information in bits per second for the mobile in the downlink direction for the associated IP flow.
> AVP Header
> 1012 5535
> Vendor ID
> 5535
> VSA Type
> 1012
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Min-Bandwidth-UL
> This AVP contains the requested/granted data rate information in bits per second for the mobile in the uplink direction for the associated IP flow.
> AVP Header
> 1013 5535
> Vendor ID
> 5535
> VSA Type
> 1013
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> MIP-Feature-Vector
> Is added with flag values set by the foreign agent or by the AAAF owned by the same administrative domain as the foreign agent. The foreign agent SHOULD include MIP-Feature-Vector AVP within the AMR message it sends to the AAAF.
> AVP Header
> 337 10415
> Vendor ID
> 10415
> VSA Type
> 337
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> MIP-Home-Agent-Address
> This AVP contains the mobile node's home agent IP address.
> AVP Header
> 334 10415
> Vendor ID
> 10415
> VSA Type
> 334
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> MIP-Home-Agent-Address-IETF
> This specifies the IPv6 or IPv4 address of the MIPv6 HA.
> AVP Header
> 334 0
> Vendor ID
> 0
> VSA Type
> 334
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> MIP-Home-Agent-Host
> This AVP contains the identity of the assigned MIPv6 HA.
> AVP Header
> 348 0
> Vendor ID
> 0
> VSA Type
> 348
> AVP Type
> GROUPED
> Group Value
> [ DESTINATION_REALM ]
> [ DESTINATION_HOST ]
> AVP Flag
> M
> MIP-Mobile-Node-Address
> This AVP contains the mobile node's home IP address.
> AVP Header
> 333 10415
> Vendor ID
> 10415
> VSA Type
> 333
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> MIP6-Agent-Info
> This AVP contains necessary information to assign a HA to the MN. It can be an IP address or Fully Qualified Domain Name (FQDN).
> AVP Header
> 486 0
> Vendor ID
> 0
> VSA Type
> 486
> AVP Type
> GROUPED
> Group Value
> [ MIP_HOME_AGENT_ADDRESS_IETF ]
> [ MIP_HOME_AGENT_HOST ]
> [ MIP6_HOME_LINK_PREFIX ]
> AVP Flag
> M
> MIP6-Feature-Vector
> This is the subset of the MIPv6 Features supported.
> AVP Header
> 6062 0
> Vendor ID
> 0
> VSA Type
> 6062
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> M
> MIP6-Home-Link-Prefix
> This AVP contains the Mobile IPv6 home network prefix information in a network byte order.
> AVP Header
> 6061 0
> Vendor ID
> 0
> VSA Type
> 6061
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> MME-Location-Information
> This attribute contains the location information of the MME user.
> AVP Header
> 1600 10415
> Vendor ID
> 10415
> VSA Type
> 1600
> AVP Type
> GROUPED
> Group Value
> [ EUTRAN_CELL_GLOBAL_IDENTITY ]
> [ TRACKING_AREA_IDENTITY ]
> [ GEOGRAPHICAL_INFORMATION ]
> [ GEODETIC_INFORMATION ]
> [ CURRENT_LOCATION_RETRIEVED ]
> [ AGE_OF_LOCATION_INFORMATION ]
> AVP Flag
> M
> MME-Service-Type
> MME service type.
> AVP Header
> 1483 10415
> Vendor ID
> 10415
> VSA Type
> 1483
> AVP Type
> GROUPED
> Group Value
> [ SERVICETYPEIDENTITY ]
> [ GMLC_RESTRICTION ]
> [ NOTIFICATION_TO_UE_USER ]
> AVP Flag
> M
> MME-User-State
> This attribute contains the location information of the MME user.
> AVP Header
> 1497 10415
> Vendor ID
> 10415
> VSA Type
> 1497
> AVP Type
> GROUPED
> Group Value
> [ USER_STATE ]
> AVP Flag
> M
> MO-LR
> This AVP defines the classes of Mobile Originating Location Request (MO-LR) for which a subscription exists for a particular MS.
> AVP Header
> 1485 10415
> Vendor ID
> 10415
> VSA Type
> 1485
> AVP Type
> GROUPED
> Group Value
> [ SS_CODE ]
> [ SS_STATUS ]
> AVP Flag
> M
> Mobile-Node-Identifier
> Contains MN-NAI identifying the user in EPS network.
> AVP Header
> 89 0
> Vendor ID
> 0
> VSA Type
> 89
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Monitoring-Key
> This attribute serves as an identifier to a usage monitoring control instance. This AVP is used for usage monitoring control purposes.
> AVP Header
> 1066 10415
> Vendor ID
> 10415
> VSA Type
> 1066
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> MSISDN
> This AVP contains an MSISDN, in international number format as described in ITU-T.
> AVP Header
> 701 0
> Vendor ID
> 0
> VSA Type
> 701
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Multiple-Auth-Profile
> This attribute indicates Multiple Authentication requirements for a particular user.
> AVP Header
> 30 5535
> Vendor ID
> 5535
> VSA Type
> 30
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Multiple-Auth-Support
> This AVP indicates the support of the Multiple Authentication at the SRNC and AGW.
> AVP Header
> 29 5535
> Vendor ID
> 5535
> VSA Type
> 29
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Multiple-Registration-Indication
> Indicates to the HSS whether or not the request is related to a multiple registration
> AVP Header
> 648 10415
> Vendor ID
> 10415
> VSA Type
> 648
> AVP Type
> ENUM. Supported values are:
> NOT_MULTIPLE_REGISTRATION (0)
> MULTIPLE_REGISTRATION (1)
> Group Value
> N/A
> AVP Flag
> N/A
> Multiple-Services-Credit-Control
> This AVP contains the AVPs related to the independent credit-control of multiple services feature.
> AVP Header
> 456 0
> Vendor ID
> 0
> VSA Type
> 456
> AVP Type
> GROUPED
> Group Value
> [ REQUESTED_SERVICE_UNIT ]
> [ GRANTED_SERVICE_UNIT ]
> [ USED_SERVICE_UNIT ]
> [ TARIFF_CHANGE_USAGE ]
> [ SERVICE_IDENTIFIER ]
> [ RATING_GROUP ]
> [ G_S_U_POOL_REFERENCE ]
> [ VALIDITY_TIME ]
> [ RESULT_CODE ]
> [ FINAL_UNIT_INDICATION ]
> AVP Flag
> M
> Multiple-Services-Indicator
> Indicates support for independent credit-control of multiple services within the session.
> AVP Header
> 455 0
> Vendor ID
> 0
> VSA Type
> 455
> AVP Type
> ENUM. Supported values are:
> MULTIPLE_SERVICES_NOT_SUPPORTED (0)
> MULTIPLE_SERVICES_SUPPORTED (1)
> Group Value
> N/A
> AVP Flag
> M
> Multi-Round-Time-Out
> Present in application-specific authorization answer messages whose Result-Code AVP is set to “DIAMETER_MULTI_ROUND_AUTH”.
> AVP Header
> 272 0
> Vendor ID
> 0
> VSA Type
> 272
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> NAS-Filter-Rule
> Provides filter rules that need to be configured on the NAS for the user.
> AVP Header
> 400 0
> Vendor ID
> 0
> VSA Type
> 400
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> NAS-Identifier
> This AVP contains the identity of the NAS providing service to the user.
> AVP Header
> 32 0
> Vendor ID
> 0
> VSA Type
> 32
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> NAS-IP-Address
> This AVP contains the IP address of the NAS providing service to the user.
> AVP Header
> 4 0
> Vendor ID
> 0
> VSA Type
> 4
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> NAS-IPv6-Address
> This AVP contains the IPv6 address of the NAS providing service to the user.
> AVP Header
> 95 0
> Vendor ID
> 0
> VSA Type
> 95
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> NAS-Port
> This AVP contains the physical or virtual port number of the NAS which is authenticating the user.
> AVP Header
> 5 0
> Vendor ID
> 0
> VSA Type
> 5
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> NAS-Port-Id
> Consists of ASCII text identifying the port of the NAS authenticating the user.
> AVP Header
> 87 0
> Vendor ID
> 0
> VSA Type
> 87
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> NAS-Port-Type
> This AVP contains the type of the port on which the NAS is authenticating the user.
> AVP Header
> 61 0
> Vendor ID
> 0
> VSA Type
> 61
> AVP Type
> ENUM. Supported values are:
> Async (0)
> Sync (1)
> ISDN_Sync (2)
> ISDN_Async_V120 (3)
> ISDN_Async_V110 (4)
> Virtual (5)
> PIAFS (6)
> HDLC_Clear_Channel (7)
> X25 (8)
> X75 (9)
> G3_Fax (10)
> ADSL-CAP-AsymmetricDSL_Carrierless-Amplitude-Phase-Modulation (12)
> ADSL-DMT-AsymmetricDSL-Discrete-Multi-Tone (13)
> IDSL-ISDN-Digital-Subscriber-Line (14)
> Ethernet (15)
> xDSL-Digital-Subscriber-Line-of-unknown-type (16)
> Cable (17)
> Wireless-Other (18)
> Wireless-IEEE802_11 (19)
> Token-Ring_RAD802_1X (20)
> FDDI_RAD802_1X (21)
> Wireless-CDMA2000 (22)
> Wireless-UMTS (23)
> Wireless-1X-EV (24)
> IAPP_IEEE-802_11f (25)
> Group Value
> N/A
> AVP Flag
> M
> Network-Access-Mode
> Defines whether the subscriber is registered to get access to the CS, PS network or to both networks.
> AVP Header
> 1417 10415
> Vendor ID
> 10415
> VSA Type
> 1417
> AVP Type
> ENUM. Supported values are:
> PACKET_AND_CIRCUIT (0)
> ONLY_CIRCUIT (1)
> ONLY_PACKET(2)
> Group Value
> N/A
> AVP Flag
> M
> Network-Element-Type
> Network element type.
> AVP Header
> 1461 10415
> Vendor ID
> 10415
> VSA Type
> 1461
> AVP Type
> ENUM. Supported values are:
> MME (0)
> SGSN (1)
> Serving-GW (2)
> PDN-GW (3)
> eNodeB (4)
> RNC (5)
> Group Value
> N/A
> AVP Flag
> M
> Network-Request-Support
> Indicates the UE and network support of the network requested bearer control mode.
> AVP Header
> 1024 10415
> Vendor ID
> 10415
> VSA Type
> 1024
> AVP Type
> ENUM. Supported values are:
> NETWORK_REQUEST_NOT_SUPPORTED (0)
> NETWORK_REQUEST_SUPPORTED (1)
> Group Value
> N/A
> AVP Flag
> M
> New-Dialog-Id
> Contains the SIP dialog identifier in the form: Call-ID=x;FTag=y;TTag=z, where x is the value of the SIP Call-ID header, y is the contents of the From header tag, and z is the contents of the To header tag. If the To header tag value is not present in the SIP message then TTag field MUST not be present in the AVP.
> AVP Header
> 219 4491
> Vendor ID
> 4491
> VSA Type
> 219
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Node-Functionality
> This AVP includes the functionality identifier of the node where the cause code was generated.
> AVP Header
> 862 0
> Vendor ID
> 0
> VSA Type
> 862
> AVP Type
> ENUM. Supported values are:
> S-CSCF (0)
> P-CSCF (1)
> I-CSCF (2)
> Group Value
> N/A
> AVP Flag
> M
> Node-Id
> This AVP contains the operator configurable identifier string for the node that had generated the ACR.
> AVP Header
> 2064 10415
> Vendor ID
> 10415
> VSA Type
> 2064
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> NOR-Flags
> The NOR-Flags AVP contains a bit mask.
> AVP Header
> 1443 10415
> Vendor ID
> 10415
> VSA Type
> 1443
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Nortel-Data-Reference
> Indicates the type of the Nortel-specific user data requested or updated in the UDR and PUR operation.
> AVP Header
> 301 0
> Vendor ID
> 0
> VSA Type
> 301
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Notification-To-UE-User
> Notification-To-UE-User
> AVP Header
> 1478 10415
> Vendor ID
> 10415
> VSA Type
> 1478
> AVP Type
> ENUM. Supported values are:
> NOTIFY_LOCATION_ALLOWED (0)
> NOTIFYANDVERIFY_ALLOWED_IF_NO_RESPONSE (1)
> NOTIFYANDVERIFY_NOT_ALLOWED_IF_NO_RESPONSE (2)
> LOCATION_NOT_ALLOWED (3)
> Group Value
> N/A
> AVP Flag
> M
> Number-Of-Requested-Vectors
> Contains the number of AVs the MME is prepared to receive.
> AVP Header
> 6013 10415
> Vendor ID
> 10415
> VSA Type
> 6013
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Number-Portability-Routing-Information
> This AVP contains information on routing number received by S-CSCF during number portability look-up (ENUM/DNS).
> AVP Header
> 2024 10415
> Vendor ID
> 10415
> VSA Type
> 2024
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Offline
> Defines whether the offline charging interface from the TPF for the associated charging rule shall be enabled.
> AVP Header
> 1008 10415
> Vendor ID
> 10415
> VSA Type
> 1008
> AVP Type
> ENUM. Supported values are:
> DISABLE (0)
> ENABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> Offline-Charging
> Holds the parameters required for offline charging.
> AVP Header
> 1278 10415
> Vendor ID
> 10415
> VSA Type
> 1278
> AVP Type
> GROUPED
> Group Value
> [ RULEBASE_ID ]
> [ QUOTA_CONSUMPTION_TIME ]
> [ TIME_QUOTA_MECHANISM ]
> [ ENVELOPE_REPORTING ]
> [ MULTIPLE_SERVICES_CREDIT_CONTROL ]
> AVP Flag
> M
> Online
> Defines whether the online charging interface from the TPF for the associated charging rule shall be enabled.
> AVP Header
> 1009 10415
> Vendor ID
> 10415
> VSA Type
> 1009
> AVP Type
> ENUM. Supported values are:
> DISABLE (0)
> ENABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> OMC-Id
> OMC ID.
> AVP Header
> 1466 10415
> Vendor ID
> 10415
> VSA Type
> 1466
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Operator-Determined-Barring
> Contains a bit mask indicating the services of a subscriber that are barred by the operator.
> AVP Header
> 1425 10415
> Vendor ID
> 10415
> VSA Type
> 1425
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Optional-Capability
> This AVP contains single determined optional capability of an S-CSCF.
> AVP Header
> 605 10415
> Vendor ID
> 10415
> VSA Type
> 605
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Originating-IOI
> This AVP holds the Inter Operator Identifier for the originating network as generated by the S-CSCF in the home network of the originating end user.
> AVP Header
> 839 0
> Vendor ID
> 0
> VSA Type
> 839
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Originating-Line-Info
> Sent by the NAS system to convey information about the origin of the call from an SS7 system.
> AVP Header
> 94 0
> Vendor ID
> 0
> VSA Type
> 94
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Originating-Request
> Indicates that the request is related to an AS originating SIP request in the Location-Information-Request operation.
> AVP Header
> 633 10415
> Vendor ID
> 10415
> VSA Type
> 633
> AVP Type
> ENUM. Supported values are:
> ORIGINATING (0)
> Group Value
> N/A
> AVP Flag
> M
> Originator
> This AVP indicates the originating party of the message body.
> The following values are defined:

> • | Calling Party (0)

> • | Called Party (1)

> AVP Header
> 864 10415
> Vendor ID
> 10415
> VSA Type
> 864
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Origin-Host
> The endpoint that originated the Diameter message.
> AVP Header
> 264 0
> Vendor ID
> 0
> VSA Type
> 264
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Origin-Realm
> The realm of the originator of any Diameter message, and is present in all messages.
> AVP Header
> 296 0
> Vendor ID
> 0
> VSA Type
> 296
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Origin-State-Id
> The Origin-State-Id AVP is a monotonically increasing value that is advanced whenever a Diameter entity restarts with loss of previous state, for example upon reboot. Origin-State-Id MAY be included in any Diameter message, including CER.
> AVP Header
> 278 0
> Vendor ID
> 0
> VSA Type
> 278
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Outgoing-Trunk-Group-ID
> This AVP identifies the outgoing PSTN leg.
> AVP Header
> 853 0
> Vendor ID
> 0
> VSA Type
> 853
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Packet-Filter-Content
> Contains the content of the packet filter as requested by the UE and required by the PCRF to create the PCC rules.
> AVP Header
> 1059 10415
> Vendor ID
> 10415
> VSA Type
> 1059
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> Packet-Data-Flow-Info
> This AVP is unique within the context of an IP-CAN session for the IP flow(s) given within the same Packet-Data-Flow-Info AVP.
> AVP Header
> 405 24757
> Vendor ID
> 24757
> VSA Type
> 405
> AVP Type
> GROUPED
> Group Value
> [ PDFID ]
> [ PRECEDENCE ]
> [ FLOW_DESCRIPTION ]
> [ WIMAX_QOS_INFORMATION ]
> AVP Flag
> M
> Packet-Filter-Identifier
> Indicates identity of the packet filter. The packet filter identifier is assigned by the PCRF and within the scope of the PCRF is unique per UE.
> AVP Header
> 1060 10415
> Vendor ID
> 10415
> VSA Type
> 1060
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Packet-Filter-Information
> This AVP contains the information from a single packet filter sent from the PCEF to the PCRF.
> AVP Header
> 1061 10415
> Vendor ID
> 10415
> VSA Type
> 1061
> AVP Type
> GROUPED
> Group Value
> [ PACKET_FILTER_IDENTIFIER ]
> [ PRECEDENCE ]
> [ PACKET_FILTER_CONTENT ]
> [ TOS_TRAFFIC_CLASS ]
> [ SECURITY_PARAMETER_INDEX ]
> [ FLOW_LABEL ]
> AVP Flag
> M
> Packet-Filter-Operation
> Indicates a UE initiated resource operation that causes a request for PCC rules.
> AVP Header
> 1062 10415
> Vendor ID
> 10415
> VSA Type
> 1062
> AVP Type
> ENUM. Supported values are:
> DELETION (0)
> ADDITION (1)
> MODIFICATION (2)
> Group Value
> N/A
> AVP Flag
> M
> Packet-Interval
> This AVP indicates the packetization time in millisecond which should be used to calculate the polling or grant interval.
> AVP Header
> 414 24757
> Vendor ID
> 24757
> VSA Type
> 414
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Packet-Size
> This AVP indicates the length in bytes of the IP Packet including the IP-header in case of IP-flows where packets have a fixed size.
> AVP Header
> 415 24757
> Vendor ID
> 24757
> VSA Type
> 415
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Paging-Group-Id
> AVP Header
> 1001 0
> Vendor ID
> 0
> VSA Type
> 1001
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Path
> This AVP contains a comma separated list of SIP proxies in the Path header.
> AVP Header
> 640 10415
> Vendor ID
> 10415
> VSA Type
> 640
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> PCC-Rule-Status
> This AVP describes the status of a Policy and Charging Control (PCC) Rule.
> AVP Header
> 1019 5535
> Vendor ID
> 5535
> VSA Type
> 1019
> AVP Type
> ENUM. Supported values are:
> ACTIVE (0) - This value is used to indicate that the PCC rule(s) are successfully installed (for those provisioned from Policy and Charging Rule Functions (PCRF)) or activated (for those pre-provisioned in Access Gateway (AGW).
> INACTIVE (1) - This value is used to indicate that the PCC rule(s) are removed (for those provisioned from PCRF) or inactive (for those pre-provisioned in AGW).
> TEMPORARILY INACTIVE (2) - This value is used to indicate that, for some reason (for example, loss of IP flow), already installed or activated PCC rules are temporary disabled.
> Group Value
> N/A
> AVP Flag
> M
> PDFID
> This value matches all records from the same packet data flow.
> AVP Header
> 26 24757
> Vendor ID
> 24757
> VSA Type
> 26
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> PDG-Address
> This AVP contains the PDG IP address.
> AVP Header
> 895 10415
> Vendor ID
> 10415
> VSA Type
> 895
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> PDG-Charging-Id
> This AVP contains the charging identifier generated by the PDG for the tunnel. Charging identifier is generated at tunnel establishment and transferred to 3GPP AAA Server.
> AVP Header
> 896 10415
> Vendor ID
> 10415
> VSA Type
> 896
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> PDN-Connection-ID
> Contains the charging identifier to identify different records belonging to same PDN connection.
> AVP Header
> 2050 10415
> Vendor ID
> 10415
> VSA Type
> 2050
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> PDN-GW-Address
> IP address of the PDN GW and this IP address shall be used as the PDN GW IP address.
> AVP Header
> 6041 10415
> Vendor ID
> 10415
> VSA Type
> 6041
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> PDN-GW-Allocation-Type
> PDN-GW allocation type.
> AVP Header
> 1438 10415
> Vendor ID
> 10415
> VSA Type
> 1438
> AVP Type
> ENUM. Supported values are:
> STATIC (0)
> DYNAMIC (1)
> Group Value
> N/A
> AVP Flag
> M
> PDN-GW-Identity
> PDN-GW identity.
> AVP Header
> 6044 10415
> Vendor ID
> 10415
> VSA Type
> 6044
> AVP Type
> GROUPED
> Group Value
> [ PDN_GW_ADDRESS ]
> [ PDN_GW_NAME ]
> AVP Flag
> M
> PDN-GW-Name
> FQDN which is used to derive the PDN GW IP address using Domain Name Service function.
> AVP Header
> 6042 10415
> Vendor ID
> 10415
> VSA Type
> 6042
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> PDN-Type
> This attribute indicates the address type of PDN. It can be IPv4,IPV6 or both.
> AVP Header
> 1456 10415
> Vendor ID
> 10415
> VSA Type
> 1456
> AVP Type
> ENUM. Supported values are:
> IPv4 (0)
> IPv6 (1)
> IPv4v6 (2)
> Group Value
> N/A
> AVP Flag
> M
> PDP-Address
> This AVP contains the PDP context address.
> AVP Header
> 1227 10415
> Vendor ID
> 10415
> VSA Type
> 1227
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> PDP-Context
> This AVP contains the list of PDP contexts to which a user has subscribed.
> AVP Header
> 1469 10415
> Vendor ID
> 10415
> VSA Type
> 1469
> AVP Type
> GROUPED
> Group Value
> [ CONTEXT_IDENTIFIER ]
> [ PDP_TYPE ]
> [ QOS_SUBSCRIBED ]
> [ VPLMN_DYNAMIC_ADDRESS_ALLOWED ]
> [ SERVICE_SELECTION ]
> [ 3GPP_CHARGING_CHARACTERISTICS ]
> AVP Flag
> M
> PDP-Context-Type
> This AVP contains the type of PDP Context.
> AVP Header
> 1247 10415
> Vendor ID
> 10415
> VSA Type
> 1247
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> PDP-Session-Operation
> This value is used to report in an indication of bearer termination that this indication refers to the last PDP context within a PDP session. It is only applicable for GPRS.
> AVP Header
> 1015 10415
> Vendor ID
> 10415
> VSA Type
> 1015
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> PDP-Type
> This AVP indicates the type of protocol that is used by MS.
> AVP Header
> 1470 10415
> Vendor ID
> 10415
> VSA Type
> 1470
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> PGW-Address
> P-GW IP address. In 12.2 and later releases, this attribute is deprecated.
> AVP Header
> 1405 10415
> Vendor ID
> 10415
> VSA Type
> 1405
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> PGW-MCC-MNC
> MCC MNC of the network to which the P-GW belongs.
> AVP Header
> 1406 10415
> Vendor ID
> 10415
> VSA Type
> 1406
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> PGW-Type
> Type of P-GW of current flow.
> AVP Header
> 7002 10415
> Vendor ID
> 10415
> VSA Type
> 7002
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Physical-Access-Id
> This AVP contains the identity of the physical access where the user equipment is connected.
> AVP Header
> 313 0
> Vendor ID
> 0
> VSA Type
> 313
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> PLMN-Client
> PLMN client.
> AVP Header
> 1482 10415
> Vendor ID
> 10415
> VSA Type
> 1482
> AVP Type
> ENUM. Supported values are:
> BROADCAST_SERVICE (0)
> O_AND_M_HPLMN (1)
> O_AND_M_VPLMN (2)
> ANONYMOUS_LOCATION (3)
> TARGET_UE_SUBSCRIBED_SERVICE (4)
> Group Value
> N/A
> AVP Flag
> M
> PMIP6-MAG-Address
> This AVP contains IP address of MAG.
> AVP Header
> 6070 10415
> Vendor ID
> 10415
> VSA Type
> 6070
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Port-Limit
> Sets the maximum number of ports the NAS provides to the user.
> AVP Header
> 62 0
> Vendor ID
> 0
> VSA Type
> 62
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Pre-emption-Capability
> Indicates whether a service data flow can get resources that were already assigned to another service data flow with a lower priority level.
> AVP Header
> 1047 10415
> Vendor ID
> 10415
> VSA Type
> 1047
> AVP Type
> ENUM. Supported values are:
> PRE-EMPTION_CAPABILITY_ENABLED (0)
> PRE-EMPTION_CAPABILITY_DISABLED (1)
> Group Value
> N/A
> AVP Flag
> M
> Pre-emption-Vulnerability
> Indicates whether a service data flow can loose the resources assigned to it in order to admit a service data flow with higher priority level.
> AVP Header
> 1048 10415
> Vendor ID
> 10415
> VSA Type
> 1048
> AVP Type
> ENUM. Supported values are:
> PRE-EMPTION_VULNERABILITY_ENABLED (0)
> PRE-EMPTION_VULNERABILITY_DISABLED (1)
> Group Value
> N/A
> AVP Flag
> M
> Precedence
> Defines the precedence of a charging rule in case of overlapping charging rules.
> AVP Header
> 1010 10415
> Vendor ID
> 10415
> VSA Type
> 1010
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Primary-Charging-Collection-Function-Name
> Defines the address of the primary offline charging system for the bearer.
> AVP Header
> 621 10415
> Vendor ID
> 10415
> VSA Type
> 621
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Primary-Event-Charging-Function-Name
> This attribute specifies the address or name of the primary online charging system server for the bearer.
> AVP Header
> 619 10415
> Vendor ID
> 10415
> VSA Type
> 619
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Priority-Level
> This AVP is used to decide whether a bearer establishment or modification request can be accepted or needs to be rejected in case of resource limitations.
> AVP Header
> 1046 10415
> Vendor ID
> 10415
> VSA Type
> 1046
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Product-Name
> This AVP contains the vendor assigned name for the product.
> AVP Header
> 269 0
> Vendor ID
> 0
> VSA Type
> 269
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Proxy-Host
> This AVP contains the identity of the host that added the Proxy-Info AVP.
> AVP Header
> 280 0
> Vendor ID
> 0
> VSA Type
> 280
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Proxy-Info
> The Proxy-Info AVP allows stateless agents to add local state to a Diameter request.
> AVP Header
> 284 0
> Vendor ID
> 0
> VSA Type
> 284
> AVP Type
> GROUPED
> Group Value
> [ Proxy-Host ]
> [ Proxy-State ]
> AVP Flag
> M
> Proxy-State
> The Proxy-State AVP contains state local information, and MUST be treated as opaque data.
> AVP Header
> 33 0
> Vendor ID
> 0
> VSA Type
> 33
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> PS-Append-Free-Format-Data
> This AVP indicates if the information sent in the PS-Free-Format-Data AVP must be appended to the PS-free-format-data stored for the online-session.
> AVP Header
> 867 10415
> Vendor ID
> 10415
> VSA Type
> 867
> AVP Type
> ENUM. Supported values are:
> APPEND (0)
> OVERWRITE (1)
> Group Value
> N/A
> AVP Flag
> M
> PS-Free-Format-Data
> This AVP holds online charging session specific data.
> AVP Header
> 866 10415
> Vendor ID
> 10415
> VSA Type
> 866
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> PS-Furnish-Charging-Information
> This grouped AVP contains online charging session specific information.
> AVP Header
> 865 10415
> Vendor ID
> 10415
> VSA Type
> 865
> AVP Type
> GROUPED
> Group Value
> [ 3GPP_CHARGING_ID ]
> [ PS_FREE_FORMAT_DATA ]
> [ PS_APPEND_FREE_FORMAT ]
> AVP Flag
> M
> PS-Information
> Its purpose is to allow the transmission of additional PS service specific information elements.
> AVP Header
> 874 10415
> Vendor ID
> 10415
> VSA Type
> 874
> AVP Type
> GROUPED
> Group Value
> [ 3GPP_CHARGING_ID ]
> [ 3GPP_PDP_TYPE ]
> [ PDP_ADDRESS ]
> [ 3GPP_GPRS_QOS_NEGOTIATED_PROFILE ]
> [ 3GPP_SGSN_ADDRESS ]
> [ 3GPP_GGSN_ADDRESS ]
> [ 3GPP_CG_ADDRESS ]
> [ 3GPP_IMSI_MCC_MNC ]
> [ 3GPP_GGSN_MCC_MNC ]
> [ 3GPP_NSAPI ]
> [ CALLED_STATION_ID ]
> [ 3GPP_SESSION_STOP_INDICATOR ]
> [ 3GPP_SELECTION_MODE ]
> [ 3GPP_CHARGING_CHARACTERISTICS ]
> [ 3GPP_SGSN_MCC_MNC ]
> [ 3GPP_RAT_TYPE ]
> [ PDP_CONTEXT_TYPE ]
> AVP Flag
> M
> PSCID
> Contains the P-GW Session Correlation ID.
> AVP Header
> 1450 10415
> Vendor ID
> 10415
> VSA Type
> 1450
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> PUA-Flags
> The PUA-Flags AVP contains a bit mask.
> AVP Header
> 1442 10415
> Vendor ID
> 10415
> VSA Type
> 1442
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Public-Identity
> This AVP contains the public identity of a user in the IMS.
> AVP Header
> 601 10415
> Vendor ID
> 10415
> VSA Type
> 601
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> QoS-Capability
> QoS Capability
> AVP Header
> 6063 0
> Vendor ID
> 0
> VSA Type
> 6063
> AVP Type
> GROUPED
> Group Value
> [ QOS_PROFILE_TEMPLATE ]
> [ VENDOR_SPECIFIC_QOS_PROFILE_TEMPLATE ]
> AVP Flag
> M
> QoS-Class
> Defines the authorized traffic class for the PDP context.
> AVP Header
> 1017 10415
> Vendor ID
> 10415
> VSA Type
> 1017
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> QoS-Class-Identifier
> Identifies a set of IP-CAN specific QoS parameters that define the authorized QoS.
> AVP Header
> 1028 10415
> Vendor ID
> 10415
> VSA Type
> 1028
> AVP Type
> ENUM. Supported values are:
> TRAFFIC_CLASS_A (1)
> TRAFFIC_CLASS_B (2)
> TRAFFIC_CLASS_C (3)
> TRAFFIC_CLASS_D (4)
> TRAFFIC_CLASS_E (5)
> TRAFFIC_CLASS_F (6)
> TRAFFIC_CLASS_G (7)
> TRAFFIC_CLASS_H (8)
> TRAFFIC_CLASS_I (9)
> In 11.0 and later releases, for R8 Gx and R8 Gxx functionality, apart from the above, operator-specific values 128–254 are also considered as valid.
> Group Value
> N/A
> AVP Flag
> M
> QoS-Information
> Defines the QoS information for an IP-CAN bearer or PCC rule.
> AVP Header
> 1016 10415
> Vendor ID
> 10415
> VSA Type
> 1016
> AVP Type
> GROUPED
> Group Value
> [ QOS_CLASS_IDENTIFIER ]
> [ MAX_REQUESTED_BANDWIDTH_UL ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> [ GUARANTEED_BITRATE_UL ]
> [ GUARANTEED_BITRATE_DL ]
> [ BEARER_IDENTIFIER ]
> [ ALLOCATION_RETENTION_PRIORITY ]
> [ APN_AGGREGATE_MAX_BITRATE_UL ]
> [ APN_AGGREGATE_MAX_BITRATE_DL ]
> AVP Flag
> M
> QoS-Negotiation
> Indicates QoS negotiation capability. I.e., if the PCRF is allowed to negotiate the QoS.
> AVP Header
> 1029 10415
> Vendor ID
> 10415
> VSA Type
> 1029
> AVP Type
> ENUM. Supported values are:
> NO_QoS_NEGOTIATION (0)
> QoS_NEGOTIATION_SUPPORTED (1)
> Group Value
> N/A
> AVP Flag
> M
> QoS-Profile-Template
> This AVP contains the list of supported Quality of Service profile templates.
> AVP Header
> 6067 0
> Vendor ID
> 0
> VSA Type
> 6067
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> QoS-Resource-Request
> Resource requested by UE to PCRF.
> AVP Header
> 6106 10415
> Vendor ID
> 10415
> VSA Type
> 6106
> AVP Type
> GROUPED
> Group Value
> [ QOS_RESOURCE_IDENTIFIER ]
> [ QOS_RESOURCE_OPERATION ]
> [ TFT_PACKET_FILTER_INFORMATION ]
> [ QOS_INFORMATION ]
> AVP Flag
> M
> QoS-Resources
> This AVP provides the description of the Quality of Service resources for policing traffic flows.
> AVP Header
> 6065 0
> Vendor ID
> 0
> VSA Type
> 6065
> AVP Type
> GROUPED
> Group Value
> [ EXTENDED_QOS_FILTER_RULE ]
> AVP Flag
> M
> QoS-Rule-Base-Name
> Indicates the name of a predefined group of charging rules residing at the TPF.
> AVP Header
> 1074 10415
> Vendor ID
> 10415
> VSA Type
> 1074
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> QoS-Rule-Definition
> Defines the QoS rule for a service flow sent by PCRF to the BBERF.
> AVP Header
> 1053 10415
> Vendor ID
> 10415
> VSA Type
> 1053
> AVP Type
> GROUPED
> Group Value
> [ QOS_RULE_NAME ]
> [ FLOW_INFORMATION ]
> [ FLOW_DESCRIPTION ]
> [ QOS_INFORMATION ]
> [ PRECEDENCE ]
> AVP Flag
> M
> QoS-Rule-Install
> Contains the QoS rules that need to be installed.
> AVP Header
> 1051 10415
> Vendor ID
> 10415
> VSA Type
> 1051
> AVP Type
> GROUPED
> Group Value
> [ QOS_RULE_DEFINITION ]
> [ QOS_RULE_NAME ]
> [ QOS_RULE_BASE_NAME ]
> [ TUNNEL_INFORMATION ]
> [ ACCESS_NETWORK_CHARGING_IDENTIFIER_VALUE ]
> [ RESOURCE_ALLOCATION_NOTIFICATION ]
> [ RULE_ACTIVATION_TIME ]
> [ RULE_DEACTIVATION_TIME ]
> AVP Flag
> M
> QoS-Rule-Name
> For QoS rules provided by the CRF it uniquely identifies a charging rule for a bearer.
> AVP Header
> 1054 10415
> Vendor ID
> 10415
> VSA Type
> 1054
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> QoS-Rule-Remove
> Used to remove QoS rules from a Gateway Control Session.
> AVP Header
> 1052 10415
> Vendor ID
> 10415
> VSA Type
> 1052
> AVP Type
> GROUPED
> Group Value
> [ QOS_RULE_NAME ]
> [ QOS_RULE_BASE_NAME ]
> AVP Flag
> M
> QoS-Rule-Report
> Report the status of QoS rules.
> AVP Header
> 1055 10415
> Vendor ID
> 10415
> VSA Type
> 1055
> AVP Type
> GROUPED
> Group Value
> [ QOS_RULE_NAME ]
> [ QOS_RULE_BASE_NAME ]
> [ PCC_RULE_STATUS ]
> [ RULE_FAILURE_CODE ]
> AVP Flag
> M
> QoS-Subscribed
> This AVP indicates the quality of service subscribed for a certain service.
> AVP Header
> 1404 10415
> Vendor ID
> 10415
> VSA Type
> 1404
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> QoS-Upgrade
> Indicates whether SGSN supports upgrade of QoS by GGSN.
> AVP Header
> 1030 10415
> Vendor ID
> 10415
> VSA Type
> 1030
> AVP Type
> ENUM. Supported values are:
> QoS_UPGRADE_NOT_SUPPORTED (0)
> QoS_UPGRADE_SUPPORTED (1)
> Group Value
> N/A
> AVP Flag
> M
> RACS-Contact-Point
> Identifies the RACS element to which resource reservation requests should be sent.
> AVP Header
> 351 0
> Vendor ID
> 0
> VSA Type
> 351
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> RAI
> This AVP contains the Routing Area Identity of the SGSN where the UE is registered.
> AVP Header
> 909 10415
> Vendor ID
> 10415
> VSA Type
> 909
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> RAND
> This AVP contains the RAND (EAP Authentication Vector).
> AVP Header
> 1447 10415
> Vendor ID
> 10415
> VSA Type
> 1447
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> RAS-Id
> This AVP contains the RAS identifier.
> AVP Header
> 10000 0
> Vendor ID
> 0
> VSA Type
> 10000
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Rating-Group
> Identifier of a rating group for service. It contains the charging key (defined in 3GPP TS 23.125). Each quota allocated to a Diameter CC session has a unique Rating Group value as specified in RFC 4006.
> AVP Header
> 432 0
> Vendor ID
> 0
> VSA Type
> 432
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> RAT-Frequency-Selection-Priority
> Contains the RAT frequency selection priority.
> AVP Header
> 1440 10415
> Vendor ID
> 10415
> VSA Type
> 1440
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> RAT-Type
> This AVP contains value of the Radio Access Technology which is currently serving the UE.
> AVP Header
> 1032 10415
> Vendor ID
> 10415
> VSA Type
> 1032
> AVP Type
> ENUM. Supported values are:
> WLAN (0)
> UTRAN (1000)
> GERAN (1001)
> GAN (1002)
> HSPA_EVOLUTION (1003)
> EUTRAN (1004)
> CDMA2000_1X (2000)
> HRPD (2001)
> UMB (2002)
> Group Value
> N/A
> AVP Flag
> M
> Re-Synchronization-Info
> This AVP contains the concatenation of RAND and AUTS.
> AVP Header
> 6014 10415
> Vendor ID
> 10415
> VSA Type
> 6014
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Reason-Code
> This AVP contains the reason for the network initiated de-registration.
> AVP Header
> 616 10415
> Vendor ID
> 10415
> VSA Type
> 616
> AVP Type
> ENUM. Supported values are:
> PERMANENT_TERMINATION (0)
> NEW_SERVER_ASSIGNED (1)
> SERVER_CHANGE (2)
> REMOVE_S-CSCF (3)
> Group Value
> N/A
> AVP Flag
> M
> Reason-Info
> This AVP contains textual information to inform the user about the reason for a de-registration.
> AVP Header
> 617 10415
> Vendor ID
> 10415
> VSA Type
> 617
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Record-Route
> This AVP contains a comma separated list of Record Route header(s).
> AVP Header
> 646 10415
> Vendor ID
> 10415
> VSA Type
> 646
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> Reservation-Class
> Contains an integer used as an index pointing to the traffic characteristic of the flow.
> AVP Header
> 456 13019
> Vendor ID
> 13019
> VSA Type
> 456
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Resource-Allocation-Notification
> Defines whether the rules included within the Charging-Rule-Install/QoS-Rule-Install AVP need be notified.
> AVP Header
> 1063 10415
> Vendor ID
> 10415
> VSA Type
> 1063
> AVP Type
> ENUM. Supported values are:
> ENABLE_NOTIFICATION (0)
> Group Value
> N/A
> AVP Flag
> M
> Re-Auth-Request-Type
> Specifies the re-authorization request type and included in application-specific authorization answers to inform the client of the action expected upon expiration of the Authorization-Lifetime.
> AVP Header
> 285 0
> Vendor ID
> 0
> VSA Type
> 285
> AVP Type
> ENUM. Supported values are:
> AUTHORIZE_ONLY (0)
> AUTHORIZE_AUTHENTICATE (1)
> Group Value
> N/A
> AVP Flag
> M
> Redirect-Address-Type
> Defines the address type of the address given in the Redirect-Server-Address AVP.
> AVP Header
> 433 0
> Vendor ID
> 0
> VSA Type
> 433
> AVP Type
> ENUM. Supported values are:
> IPv4 Address (0)
> IPv6 Address (1)
> URL (2)
> SIP URL (2)
> Group Value
> N/A
> AVP Flag
> M
> Redirect-Host
> The alternate routing details to which the request need to be redirected to.
> AVP Header
> 292 0
> Vendor ID
> 0
> VSA Type
> 292
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Redirect-Host-Usage
> Dictates how the routing entry resulting from the Redirect-Host is to be used.
> AVP Header
> 261 0
> Vendor ID
> 0
> VSA Type
> 261
> AVP Type
> ENUM. Supported values are:
> DONT_CACHE (0)
> ALL_SESSION (1)
> ALL_REALM (2)
> REALM_AND_APPLICATION (3)
> ALL_APPLICATION (4)
> ALL_HOST (5)
> ALL_USER (6)
> Group Value
> N/A
> AVP Flag
> M
> Redirect-Max-Cache-Time
> Maximum duration in seconds the peer and route table entries, created as a result of the Redirect-Host, will be cached.
> AVP Header
> 262 0
> Vendor ID
> 0
> VSA Type
> 262
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Redirect-Server
> This AVP contains the address information of the redirect server (for example,, HTTP redirect server, SIP Server) with which the end user is to be connected when redirected as account cannot cover the service cost.
> AVP Header
> 434 0
> Vendor ID
> 0
> VSA Type
> 434
> AVP Type
> GROUPED
> Group Value
> [ Redirect-Address-Type ]
> [ Redirect-Server-Address ]
> AVP Flag
> M
> Redirect-Server-Address
> Defines the address of the redirect server.
> AVP Header
> 435 0
> Vendor ID
> 0
> VSA Type
> 435
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Regional-Subscription-Zone-Code
> Regional-Subscription-Zone-Code. Up to 10 zone codes are used to define the tracking areas into which the subscriber is allowed or not allowed to roam.
> AVP Header
> 1446 10415
> Vendor ID
> 10415
> VSA Type
> 1446
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Reply-Message
> This AVP contains text that may be displayed to the user.
> AVP Header
> 18 0
> Vendor ID
> 0
> VSA Type
> 18
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Reporting-Level
> Defines on what level the TPF reports the usage for the related charging rule.
> AVP Header
> 1011 10415
> Vendor ID
> 10415
> VSA Type
> 1011
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Requested-Action
> The action requested when the CC_Request_Type is EVENT_REQUEST.
> AVP Header
> 436 0
> Vendor ID
> 0
> VSA Type
> 436
> AVP Type
> ENUM. Supported values are:
> DIRECT_DEBITING (0)
> REFUND_ACCOUNT (1)
> CHECK_BALANCE (2)
> PRICE_ENQUIRY (3)
> Group Value
> N/A
> AVP Flag
> M
> Requested-Domain
> Indicates the access domain for which certain data are requested.
> AVP Header
> 706 0
> Vendor ID
> 0
> VSA Type
> 706
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Requested-EUTRAN-Authentication-Info
> This AVP contains the EU Tran authentication information.
> AVP Header
> 6010 10415
> Vendor ID
> 10415
> VSA Type
> 6010
> AVP Type
> GROUPED
> Group Value
> [ NUMBER_OF_REQUESTED_VECTORS ]
> [ IMMEDIATE_RESPONSE_PREFERRED ]
> [ RE_SYNCHRONIZATION_INFO ]
> AVP Flag
> M
> Requested-GERAN-Authentication-Info
> This AVP contains GE RAN authentication information.
> AVP Header
> 6012 10415
> Vendor ID
> 10415
> VSA Type
> 6012
> AVP Type
> GROUPED
> Group Value
> [ NUMBER_OF_REQUESTED_VECTORS ]
> [ IMMEDIATE_RESPONSE_PREFERRED ]
> [ RE_SYNCHRONIZATION_INFO ]
> AVP Flag
> M
> Requested-Information
> This AVP provides the list of items requested by the AF.
> AVP Header
> 353 13019
> Vendor ID
> 13019
> VSA Type
> 353
> AVP Type
> ENUM. Supported values are:
> NASS-USER-ID (0)
> LOCATION-INFORMATION (1)
> RACS-CONTACT-POINT (2)
> ACCESS-NETWORK-TYPE (3)
> TERMINAL-TYPE (4)
> LOGICAL-ACCESS-ID (5)
> PHYSICAL-ACCESS-ID (6)
> ACCESS-NETWORK-TYPE-RESERVED (7)
> INITIAL-GATE-SETTING-RESERVED (8)
> QOS-PROFILE-RESERVED (9)
> IP-CONNECTIVITY-STATUS-RESERVED (10)
> Group Value
> N/A
> AVP Flag
> M
> Requested-Party-Address
> In IMS it holds the address (SIP URI or TEL URI) of the party (Public User ID or Public Service ID) to whom the SIP transaction was originally posted.
> AVP Header
> 1251 10415
> Vendor ID
> 10415
> VSA Type
> 1251
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Requested-QoS
> It is used within the Flow-Info AVP to indicate the QoS requested by the UE for a particular IP flow in the high rate packet data radio access network.
> AVP Header
> 812 5535
> Vendor ID
> 5535
> VSA Type
> 812
> AVP Type
> GROUPED
> Group Value
> [ QoS-Class ]
> [ Min-Bandwidth-UL ]
> [ Min-Bandwidth-DL ]
> AVP Flag
> M
> Requested-Service-Unit
> Amount of requested units specified by the Diameter credit-control client.
> AVP Header
> 437 0
> Vendor ID
> 0
> VSA Type
> 437
> AVP Type
> GROUPED
> Group Value
> [ TARIFF_TIME_CHANGE ]
> [ TARIFF_CHANGE_USAGE ]
> [ CC_TIME ]
> [ CC_MONEY ]
> [ CC_TOTAL_OCTETS ]
> [ CC_INPUT_OCTETS ]
> [ CC_OUTPUT_OCTETS ]
> [ CC_SERVICE_SPECIFIC_UNITS ]
> AVP Flag
> M
> Requested-UTRAN-Authentication-Info
> This AVP contains the UTRAN authentication information.
> AVP Header
> 6011 10415
> Vendor ID
> 10415
> VSA Type
> 6011
> AVP Type
> GROUPED
> Group Value
> [ NUMBER_OF_REQUESTED_VECTORS ]
> [ IMMEDIATE_RESPONSE_PREFERRED ]
> [ RE_SYNCHRONIZATION_INFO ]
> AVP Flag
> M
> Requested-UTRAN-GERAN-Authentication-Info
> This AVP contains the information related to the authentication requests for UTRAN or GERAN.
> AVP Header
> 1409 10415
> Vendor ID
> 10415
> VSA Type
> 1409
> AVP Type
> GROUPED
> Group Value
> [ NUMBER_OF_REQUESTED_VECTORS ]
> [ IMMEDIATE_RESPONSE_PREFERRED ]
> [ RE_SYNCHRONIZATION_INFO ]
> AVP Flag
> M
> Requesting-Node-Type
> Requesting node type.
> AVP Header
> 1455 10415
> Vendor ID
> 10415
> VSA Type
> 1455
> AVP Type
> ENUM. Supported values are:
> MME (0)
> SGSN (1)
> MME-SGSN (2)
> Group Value
> N/A
> AVP Flag
> M
> Required-MBMS-Bearer-Capabilities
> Contains the minimum bearer capabilities the UE needs to support.
> AVP Header
> 901 10415
> Vendor ID
> 10415
> VSA Type
> 901
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Reservation-Priority
> Used by the PCRF to guarantee service for an application session of a higher relative priority.
> AVP Header
> 458 13019
> Vendor ID
> 13019
> VSA Type
> 458
> AVP Type
> ENUM. Supported values are:
> DEFAULT (0)
> PRIORITY-ONE (1)
> PRIORITY-TWO (2)
> PRIORITY-THREE (3)
> PRIORITY-FOUR (4)
> PRIORITY-FIVE (5)
> PRIORITY-SIX (6)
> PRIORITY-SEVEN (7)
> Group Value
> N/A
> AVP Flag
> N/A
> Restoration-Info
> Contains the information related to a specific registration.
> AVP Header
> 649 10415
> Vendor ID
> 10415
> VSA Type
> 649
> AVP Type
> GROUPED
> Group Value
> [ PATH ]
> [ CONTACT ]
> [ SUBSCRIPTION_INFO ]
> AVP Flag
> N/A
> Restriction-Filter-Rule
> Provides filter rules for a services that are to remain accessible even if there are no more service units granted.
> AVP Header
> 438 0
> Vendor ID
> 0
> VSA Type
> 438
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> Result-Code
> Indicates whether a particular request was completed successfully or whether an error occurred.
> AVP Header
> 268 0
> Vendor ID
> 0
> VSA Type
> 268
> AVP Type
> ENUM. Supported values are:
> DIAMETER_MULTI_ROUND_AUTH (1001)
> DIAMETER_SUCCESS (2001)
> DIAMETER_LIMITED_SUCCESS (2002)
> DIAMETER_COMMAND_UNSUPPORTED (3001)
> DIAMETER_UNABLE_TO_DELIVER (3002)
> DIAMETER_REALM_NOT_SERVED (3003)
> DIAMETER_TOO_BUSY (3004)
> DIAMETER_LOOP_DETECTED (3005)
> DIAMETER_REDIRECT_INDICATION (3006)
> DIAMETER_APPLICATION_UNSUPPORTED (3007)
> DIAMETER_INVALID_HDR_BITS (3008)
> DIAMETER_INVALID_AVP_BITS (3009)
> DIAMETER_UNKNOWN_PEER (3010)
> DIAMETER_AUTHENTICATION_REJECTED (4001)
> DIAMETER_OUT_OF_SPACE (4002)
> ELECTION_LOST (4003)
> DIAMETER_END_USER_SERVICE_DENIED (4010)
> DIAMETER_CREDIT_CONTROL_NOT_APPLICABLE (4011)
> DIAMETER_CREDIT_LIMIT_REACHED (4012)
> DIAMETER_BALANCE_IS_ZERO (4212)
> DIAMETER_AVP_UNSUPPORTED (5001)
> DIAMETER_UNKNOWN_SESSION_ID (5002)
> DIAMETER_AUTHORIZATION_REJECTED (5003)
> DIAMETER_INVALID_AVP_VALUE (5004)
> DIAMETER_MISSING_AVP (5005)
> DIAMETER_RESOURCES_EXCEEDED (5006)
> DIAMETER_CONTRADICTING_AVPS (5007)
> DIAMETER_AVP_NOT_ALLOWED (5008)
> DIAMETER_AVP_OCCURS_TOO_MANY_TIMES (5009)
> DIAMETER_NO_COMMON_APPLICATION (5010)
> DIAMETER_UNSUPPORTED_VERSION (5011)
> DIAMETER_UNABLE_TO_COMPLY (5012)
> DIAMETER_INVALID_BIT_IN_HEADER (5013)
> DIAMETER_INVALID_AVP_LENGTH (5014)
> DIAMETER_INVALID_MESSAGE_LENGTH (5015)
> DIAMETER_INVALID_AVP_BIT_COMBO (5016)
> DIAMETER_NO_COMMON_SECURITY (5017)
> DIAMETER_USER_UNKNOWN (5030)
> DIAMETER_RATING_FAILED (5031)
> Group Value
> N/A
> AVP Flag
> M
> Revalidation-Time
> This AVP contains the value indicating the NTP time before which the PCEF will have to re-request PCC rules.
> AVP Header
> 1042 10415
> Vendor ID
> 10415
> VSA Type
> 1042
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Roaming-Restricted-Due-To-Unsupported-Feature
> This AVP indicates that roaming is restricted due to unsupported feature.
> AVP Header
> 1457 10415
> Vendor ID
> 10415
> VSA Type
> 1457
> AVP Type
> ENUM. Supported values are:
> ROAMING_RESTRICTED_DUE_TO_UNSUPPORTED_FEATURE (0)
> Group Value
> N/A
> AVP Flag
> M
> Role-Of-Node
> This AVP specifies the role of the AS/CSCF.
> The identifier can be one of the following:

> • | ORIGINATING_ROLE (0): The AS/CSCF is applying a originating role, serving the calling subscriber.

> • | TERMINATING_ROLE (1): The AS/CSCF is applying a terminating role, serving the called subscriber.

> • | PROXY ROLE (2): The AS is applying a proxy role.

> • | B2BUA_ROLE (3): The AS is applying a B2BUA role.

> AVP Header
> 829 10415
> Vendor ID
> 10415
> VSA Type
> 829
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Route-Record
> The value added to this AVP same as the one received in the Origin-Host of the Capabilities Exchange message.
> AVP Header
> 282 0
> Vendor ID
> 0
> VSA Type
> 282
> AVP Type
> DIAMIDENT
> Group Value
> N/A
> AVP Flag
> M
> Routing-Area-Identity
> This attribute contains the routing area identifier of the user.
> AVP Header
> 1605 10415
> Vendor ID
> 10415
> VSA Type
> 1605
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Routing-Policy
> This attribute is used to describe a single IP flow.
> AVP Header
> 312 10415
> Vendor ID
> 10415
> VSA Type
> 312
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> RR-Bandwidth
> Indicates the maximum required bandwidth in bits per second for RTCP receiver reports within the session component.
> AVP Header
> 521 10415
> Vendor ID
> 10415
> VSA Type
> 521
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> RS-Bandwidth
> Indicates the maximum required bandwidth in bits per second for RTCP sender reports within the session component.
> AVP Header
> 522 10415
> Vendor ID
> 10415
> VSA Type
> 522
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Rule-Activation-Time
> Contains the value indicating the NTP time at which the PCC rule has to be enforced.
> AVP Header
> 1043 10415
> Vendor ID
> 10415
> VSA Type
> 1043
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Rule-Deactivation-Time
> Contains the value indicating the NTP time at which the PCEF has to stop enforcing the PCC rule.
> AVP Header
> 1044 10415
> Vendor ID
> 10415
> VSA Type
> 1044
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Rule-Failure-Code
> Contains the rule failure code.
> AVP Header
> 1031 10415
> Vendor ID
> 10415
> VSA Type
> 1031
> AVP Type
> ENUM. Supported values are:
> UNKNOWN_RULE_NAME (1)
> RATING_GROUP_ERROR (2)
> SERVICE_IDENTIFIER_ERROR (3)
> GW_PCEF_MALFUNCTION (4)
> RESOURCES_LIMITATION (5)
> MAX_NR_BEARERS_REACHED (6)
> UNKNOWN_BEARER_ID (7)
> MISSING_BEARER_ID (8)
> MISSING_FLOW_DESCRIPTION (9)
> RESOURCE_ALLOCATION_FAILURE (10)
> UNSUCCESSFUL_QOS_VALIDATION (11)
> Group Value
> N/A
> AVP Flag
> M
> Rule-Reason-Code
> Contains the rule reason code.
> AVP Header
> 814 10415
> Vendor ID
> 10415
> VSA Type
> 814
> AVP Type
> ENUM. Supported values are:
> UNKNOWN_FLOW_IDENTIFIER (0)
> UNKNOWN_RULE_NAME (1)
> RATING_GROUP_ERROR (2)
> SERVICE_IDENTIFIER_ERROR (3)
> AGW_MALFUNCTION (4)
> RESOURCES_LIMITATION (5)
> Group Value
> N/A
> AVP Flag
> M
> SCSCF-Restoration-Info
> Contains the information required for an S-CSCF to handle the requests for a user.
> AVP Header
> 639 10415
> Vendor ID
> 10415
> VSA Type
> 639
> AVP Type
> GROUPED
> Group Value
> [ USER_NAME ]
> [ RESTORATION_INFO ]
> [ SIP_AUTHENTICATION_SCHEME ]
> AVP Flag
> N/A
> SDP-Answer-Timestamp
> This AVP specifies the time in UTC format of the response to the SDP offer.
> AVP Header
> 1275 0
> Vendor ID
> 0
> VSA Type
> 1275
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> SDP-Media-Component
> Contains the interface representing the SDP-Media-Component grouped AVP type.
> AVP Header
> 843 10415
> Vendor ID
> 10415
> VSA Type
> 843
> AVP Type
> GROUPED
> Group Value
> [ SDP_MEDIA_NAME ]
> [ SDP_MEDIA_DESCRIPTION ]
> [ MEDIA_INITIATOR_FLAG ]
> [ AUTHORISED_QOS ]
> [ 3GPP_CHARGING_ID ]
> AVP Flag
> M
> SDP-Media-Description
> Contains the content of an attribute-line" (i=, c=, b=, k=, a=) related to a media component. The attributes are specifying the media described in the SDP-Media-Name AVP.
> AVP Header
> 845 10415
> Vendor ID
> 10415
> VSA Type
> 845
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> SDP-Media-Name
> This AVP holds the content of a "m=" line in the SDP data.
> AVP Header
> 844 10415
> Vendor ID
> 10415
> VSA Type
> 844
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> SDP-Offer-Timestamp
> This AVP specifies the time in UTC format of the SDP offer.
> AVP Header
> 1274 0
> Vendor ID
> 0
> VSA Type
> 1274
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> SDP-Session-Description
> This AVP holds the content of an "attribute-line" (i=, c=, b=, k=, a=) related to a session.
> AVP Header
> 842 10415
> Vendor ID
> 10415
> VSA Type
> 842
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> SDP-TimeStamps
> This AVP specifies the time of the SDP offer and the SDP answer.
> AVP Header
> 1273 0
> Vendor ID
> 0
> VSA Type
> 1273
> AVP Type
> GROUPED
> Group Value
> [ SDP_OFFER_TIMESTAMP ]
> [ SDP_ANSWER_TIMESTAMP ]
> AVP Flag
> M
> SDP-Type
> This AVP provides information on whether the SDP media component is of type SDP offer or SDP answer.
> AVP Header
> 2036 10415
> Vendor ID
> 10415
> VSA Type
> 2036
> AVP Type
> ENUM. Supported values are:
> SDP_OFFER (0)
> SDP_ANSWER (1)
> Group Value
> N/A
> AVP Flag
> M
> Secondary-Charging-Collection-Function-Name
> Defines the address of the secondary offline charging system for the bearer.
> AVP Header
> 622 10415
> Vendor ID
> 10415
> VSA Type
> 622
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Secondary-Event-Charging-Function-Name
> Defines the address of the secondary online charging system for the bearer.
> AVP Header
> 620 10415
> Vendor ID
> 10415
> VSA Type
> 620
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Sector-Id
> The identifier of sector that MS exists.
> AVP Header
> 10002 0
> Vendor ID
> 0
> VSA Type
> 10002
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Security-Parameter-Index
> This AVP contains the security parameter index of the IPSec packet.
> AVP Header
> 1056 10415
> Vendor ID
> 10415
> VSA Type
> 1056
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Send-Data-Indication
> This AVP indicates that sender requests user data in SNR.
> AVP Header
> 710 0
> Vendor ID
> 0
> VSA Type
> 710
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Served-Party-IP-Address
> This AVP holds the IP address of either the calling or called party, depending on whether the P-CSCF is in touch with the calling or the called party. This AVP is only provided by the P-CSCF and S-CSCF.
> AVP Header
> 848 10415
> Vendor ID
> 10415
> VSA Type
> 848
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Server-Assignment-Type
> This AVP contains the type of server update being performed in a Server-Assignment-Request operation.
> AVP Header
> 614 10415
> Vendor ID
> 10415
> VSA Type
> 614
> AVP Type
> ENUM. Supported values are:
> NO_ASSIGNMENT (0)
> REGISTRATION (1)
> RE_REGISTRATION (2)
> UNREGISTERED_USER (3)
> TIMEOUT_DEREGISTRATION (4)
> USER_DEREGISTRATION (5)
> TIMEOUT_DEREGISTRATION_STORE_SERVER_NAME (6)
> USER_DEREGISTRATION_STORE_SERVER_NAME (7)
> ADMINISTRATIVE_DEREGISTRATION (8)
> AUTHENTICATION_FAILURE (9)
> AUTHENTICATION_TIMEOUT (10)
> DEREGISTRATION_TOO_MUCH_DATA (11)
> Group Value
> N/A
> AVP Flag
> M
> Server-Capabilities
> This grouped AVP contains information/capabilities of an S-CSCF server.
> AVP Header
> 603 10415
> Vendor ID
> 10415
> VSA Type
> 603
> AVP Type
> GROUPED
> Group Value
> [ MANDATORY_CAPABILITY ]
> [ OPTIONAL_CAPABILITY ]
> [ SERVER_NAME ]
> AVP Flag
> M
> Server-Name
> This AVP contains a SIP-URL used to identify a SIP server.
> AVP Header
> 602 10415
> Vendor ID
> 10415
> VSA Type
> 602
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Area-Identity
> This attribute contains the service area identifier of the user.
> AVP Header
> 1607 10415
> Vendor ID
> 10415
> VSA Type
> 1607
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Class
> Contains the service class requested by the AF.
> AVP Header
> 459 13019
> Vendor ID
> 13019
> VSA Type
> 459
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> Service-Context-Id
> Unique identifier of credit-control service.
> AVP Header
> 461 0
> Vendor ID
> 0
> VSA Type
> 461
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Data-Container
> Service data container.
> AVP Header
> 2040 10415
> Vendor ID
> 10415
> VSA Type
> 2040
> AVP Type
> GROUPED
> Group Value
> [ AF_CORRELATION_INFORMATION ]
> [ CHARGING_RULE_BASE_NAME ]
> [ ACCOUNTING_INPUT_OCTETS ]
> [ ACCOUNTING_OUTPUT_OCTETS ]
> [ ACCOUNTING_INPUT_PACKETS ]
> [ ACCOUNTING_OUTPUT_PACKETS ]
> [ LOCAL_SEQUENCE_NUMBER ]
> [ QOS_INFORMATION ]
> [ RATING_GROUP ]
> [ CHANGE_TIME ]
> [ SERVICE_IDENTIFIER ]
> [ SERVICE_SPECIFIC_INFO ]
> [ SGSN_ADDRESS ]
> [ TIME_FIRST_USAGE ]
> [ TIME_LAST_USAGE ]
> [ TIME_USAGE ]
> [ CHANGE_CONDITION ]
> [ 3GPP_USER_LOCATION_INFO ]
> [ FLOW_DESCRIPTION ]
> [ CHARGING_RULE_NAME ]
> [ FIRST_PACKET_DIRECTION ]
> [ 3GPP2_BSID ]
> AVP Flag
> M
> Service-Identifier
> Specifies the identity of the service or service component the service data flow in a charging rule relates to.
> AVP Header
> 439 0
> Vendor ID
> 0
> VSA Type
> 439
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Service-Indication
> This AVP contains the Service Indication that identifies a service in AS.
> AVP Header
> 704 0
> Vendor ID
> 0
> VSA Type
> 704
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Information
> The purpose of this AVP is to allow the transmission of additional 3GPP service-specific information elements.
> AVP Header
> 873 10415
> Vendor ID
> 10415
> VSA Type
> 873
> AVP Type
> GROUPED
> Group Value
> [ IMS-Information ]
> AVP Flag
> M
> Service-Info-Status
> Indicates the status of the service information that the AF is providing to the PCRF.
> AVP Header
> 527 10415
> Vendor ID
> 10415
> VSA Type
> 527
> AVP Type
> ENUM. Supported values are:
> FINAL_SERVICE_INFORMATION (0)
> PRELIMINARY_SERVICE_INFORMATION (1)
> Group Value
> N/A
> AVP Flag
> M
> Service-Parameter-Info
> Service-specific information used for rating.
> AVP Header
> 440 0
> Vendor ID
> 0
> VSA Type
> 440
> AVP Type
> GROUPED
> Group Value
> [ Service-Parameter-Type ]
> [ Service-Parameter-Value ]
> AVP Flag
> M
> Service-Parameter-Type
> Service event specific parameter (for example, end-user location or service name.
> AVP Header
> 441 0
> Vendor ID
> 0
> VSA Type
> 441
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Service-Parameter-Value
> Value of the service parameter type.
> AVP Header
> 442 0
> Vendor ID
> 0
> VSA Type
> 442
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Selection
> Service-Selection.
> AVP Header
> 493 0
> Vendor ID
> 0
> VSA Type
> 493
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Specific-Data
> This AVP holds service specific data if and as provided by an Application Server.
> AVP Header
> 1249 0
> Vendor ID
> 0
> VSA Type
> 1249
> AVP Type
> GROUPED
> Group Value
> [ SERVICE_SPECIFIC_TYPE ]
> [ SERVICE_SPECIFIC_VALUE ]
> AVP Flag
> M
> Service-Specific-Info
> Service specific information.
> AVP Header
> 1249 10415
> Vendor ID
> 10415
> VSA Type
> 1249
> AVP Type
> GROUPED
> Group Value
> [ SERVICE_SPECIFIC_DATA ]
> [ SERVICE_SPECIFIC_TYPE ]
> AVP Flag
> M
> Service-Specific-Type
> This AVP holds the type of the Service-Specific-Data.
> AVP Header
> 1248 0
> Vendor ID
> 0
> VSA Type
> 1248
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Service-Specific-Value
> This AVP holds service specific value.
> AVP Header
> 863 0
> Vendor ID
> 0
> VSA Type
> 863
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Service-Type
> This AVP contains the type of service the user has requested or the type of service to be provided.
> AVP Header
> 6 0
> Vendor ID
> 0
> VSA Type
> 6
> AVP Type
> ENUM. Supported values are:
> Login (1)
> Framed (2)
> Callback-Login (3)
> Callback-Framed (4)
> Outbound (5)
> Administrative (6)
> NAS-Prompt (7)
> Authenticate-Only (8)
> Callback-NAS-Prompt (9)
> Call-Check (10)
> Callback-Administrative (11)
> Voice (12)
> Fax (13)
> Modem-Relay (14)
> IAPP-Register_IEEE-802_11f (15)
> IAPP-AP-Check_IEEE-802_11f (16)
> Authorize-Only-RADDynAuth (17)
> Group Value
> N/A
> AVP Flag
> M
> ServiceTypeIdentity
> This AVP contains the LCS service type identity.
> AVP Header
> 1484 10415
> Vendor ID
> 10415
> VSA Type
> 1484
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Service-URN
> This AVP indicates that an AF session is used for emergency traffic. It contains values of the service URN including sub-services, as registered at IANA.
> AVP Header
> 525 10415
> Vendor ID
> 10415
> VSA Type
> 525
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Serving-Node-Type
> This AVP identifies the Serving Node type.
> AVP Header
> 2047 10415
> Vendor ID
> 10415
> VSA Type
> 2047
> AVP Type
> ENUM. Supported values are:
> SGSN (0)
> PMIPSGW (1)
> GTPSGW (2)
> ePDG (3)
> hSGW (4)
> MME (5)
> Group Value
> N/A
> AVP Flag
> M
> Session-Bundle-Id
> Used to identify the group of sessions to which session of the AA-Answer belongs.
> AVP Header
> 400 13019
> Vendor ID
> 13019
> VSA Type
> 400
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Session-Id
> Specifies the specific session with an identifier.
> AVP Header
> 263 0
> Vendor ID
> 0
> VSA Type
> 263
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Session-Linking-Indicator
> Indicates whether the session linking between the Gateway Control Session and the Gx session must be deferred.
> AVP Header
> 1064 10415
> Vendor ID
> 10415
> VSA Type
> 1064
> AVP Type
> ENUM. Supported values are:
> SESSION_LINKING_IMMEDIATE (0)
> SESSION_LINKING_DEFERRED (1)
> Group Value
> N/A
> AVP Flag
> M
> Session-Priority
> Indicates to the HSS or accounting server the session's priority. PRIORITY-0 is the highest priority.
> AVP Header
> 650 10415
> Vendor ID
> 10415
> VSA Type
> 650
> AVP Type
> ENUM. Supported values are:
> PRIORITY-0 (0)
> PRIORITY-0 (1)
> PRIORITY-0 (2)
> PRIORITY-0 (3)
> PRIORITY-0 (4)
> Group Value
> N/A
> AVP Flag
> N/A
> Session-Release-Cause
> Determines the release cause of the IP-CAN session.
> AVP Header
> 1045 10415
> Vendor ID
> 10415
> VSA Type
> 1045
> AVP Type
> ENUM. Supported values are:
> UNSPECIFIED_REASON (0)
> UE_SUBSCRIPTION_REASON (1)
> INSUFFICIENT_SERVER_RESOURCES (2)
> Group Value
> N/A
> AVP Flag
> M
> Session-Request-Type
> This AVP indicates the action that the PDG is asking to the 3GPP AAA server to perform.
> AVP Header
> 311 10415
> Vendor ID
> 10415
> VSA Type
> 311
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Session-Start-Indicator
> This AVP contains the SFR Session Start Indication. Flags Primary PDP Context. Value is always 0xFF".
> AVP Header
> 522 8164
> Vendor ID
> 8164
> VSA Type
> 522
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Session-Timeout
> This AVP contains the maximum number of seconds of service to be provided to the user before termination of the session.
> AVP Header
> 27 0
> Vendor ID
> 0
> VSA Type
> 27
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SGSN-Address
> This AVP contains the IP address of the SGSN that was used during a report.
> AVP Header
> 1228 10415
> Vendor ID
> 10415
> VSA Type
> 1228
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> SGSN-Location-Information
> This AVP contains the location information of the SGSN user.
> AVP Header
> 1601 10415
> Vendor ID
> 10415
> VSA Type
> 1601
> AVP Type
> GROUPED
> Group Value
> [ CELL_GLOBAL_IDENTITY ]
> [ LOCATION_AREA_IDENTITY ]
> [ SERVICE_AREA_IDENTITY ]
> [ ROUTING_AREA_IDENTITY ]
> [ GEOGRAPHICAL_INFORMATION ]
> [ GEODETIC_INFORMATION ]
> [ CURRENT_LOCATION_RETRIEVED ]
> [ AGE_OF_LOCATION_INFORMATION ]
> AVP Flag
> M
> SGSN-Number
> This AVP contains the ISDN number of the SGSN.
> AVP Header
> 1489 10415
> Vendor ID
> 10415
> VSA Type
> 1489
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SGSN-User-State
> This AVP indicates the current state of the SGSN user.
> AVP Header
> 1498 10415
> Vendor ID
> 10415
> VSA Type
> 1498
> AVP Type
> GROUPED
> Group Value
> [ USER_STATE ]
> AVP Flag
> M
> SGW-Address
> This AVP contains the IP address of the Serving GW. In 12.2 and later releases, this attribute is deprecated.
> AVP Header
> 1403 10415
> Vendor ID
> 10415
> VSA Type
> 1403
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> SGW-Change
> This AVP indicates that this is the first Accounting Request (ACR) due to S-GW change.
> AVP Header
> 2065 10415
> Vendor ID
> 10415
> VSA Type
> 2065
> AVP Type
> ENUM. Supported values are:
> ACR_START_NOT_DUE_TO_SGW_CHANGE (0)
> ACR_START_DUE_TO_SGW_CHANGE (1)
> Group Value
> N/A
> AVP Flag
> M
> SGW-Type
> This AVP specifies the type of SGW of current flow.
> AVP Header
> 7001 10415
> Vendor ID
> 10415
> VSA Type
> 7001
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SIP-Auth-Data-Item
> This AVP contains the authentication and/or authorization information for the Diameter client.
> AVP Header
> 612 10415
> Vendor ID
> 10415
> VSA Type
> 612
> AVP Type
> GROUPED
> Group Value
> [ SIP_ITEM_NUMBER ]
> [ SIP_AUTHENTICATION_SCHEME ]
> [ SIP_AUTHENTICATE ]
> [ SIP_DIGEST_AUTHENTICATE ]
> [ SIP_AUTHORIZATION ]
> [ SIP_AUTHENTICATION_CONTEXT ]
> [ CONFIDENTIALITY_KEY ]
> [ INTEGRITY_KEY ]
> [ LINE_IDENTIFIER ]
> AVP Flag
> M
> SIP-Authenticate
> This AVP contains specific parts of the data portion of the WWW-Authenticate or Proxy-Authenticate SIP headers that are to be present in a SIP response.
> AVP Header
> 609 10415
> Vendor ID
> 10415
> VSA Type
> 609
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Authentication-Context
> This AVP contains authentication-related information relevant for performing the authentication but that is not part of the SIP authentication headers.
> AVP Header
> 611 10415
> Vendor ID
> 10415
> VSA Type
> 611
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Authentication-Scheme
> This AVP contains the authentication scheme used in the authentication of SIP messages.
> AVP Header
> 608 10415
> Vendor ID
> 10415
> VSA Type
> 608
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Authorization
> This AVP contains specific parts of the data portion of the Authorization or Proxy-Authorization SIP headers suitable for inclusion in a SIP request.
> AVP Header
> 610 10415
> Vendor ID
> 10415
> VSA Type
> 610
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Digest-Authenticate
> Contains a reconstruction of either the SIP WWW-Authenticate or Proxy-Authentication header fields specified in IETF RFC 2617.
> AVP Header
> 635 10415
> Vendor ID
> 10415
> VSA Type
> 635
> AVP Type
> GROUPED
> Group Value
> [ DIGEST_REALM ]
> [ DIGEST_DOMAIN ]
> [ DIGEST_ALGORITHM ]
> [ DIGEST_QOP ]
> [ DIGEST_HA1 ]
> [ DIGEST_AUTH_PARAM ]
> AVP Flag
> M
> SIP-Forking-Indication
> Describes if several SIP dialogues are related to one Diameter session.
> AVP Header
> 523 10415
> Vendor ID
> 10415
> VSA Type
> 523
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> SIP-Item-Number
> This AVP contains the order number of the SIP-Auth-Data-Item AVP.
> AVP Header
> 613 10415
> Vendor ID
> 10415
> VSA Type
> 613
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SIP-Message
> This AVP hold the entire SIP message or messages received by the IAP.
> AVP Header
> 229 4491
> Vendor ID
> 4491
> VSA Type
> 229
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Method
> This AVP holds the name of the SIP Method (INVITE, UPDATE, etc.) causing an accounting request to be sent to the AAA.
> AVP Header
> 824 10415
> Vendor ID
> 10415
> VSA Type
> 824
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> SIP-Number-Auth-Items
> This AVP contains the number of authentication vectors asked/provided.
> AVP Header
> 607 10415
> Vendor ID
> 10415
> VSA Type
> 607
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SIP-Request-Timestamp
> This AVP holds the time in UTC format of the initial SIP request (for example, Invite).
> AVP Header
> 834 10415
> Vendor ID
> 10415
> VSA Type
> 834
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> SIP-Response-Timestamp
> This AVP holds the time in UTC format of the response to the initial SIP request (for example, 200 OK).
> AVP Header
> 835 10415
> Vendor ID
> 10415
> VSA Type
> 835
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> SN-Absolute-Validity-Time
> This AVP contains the validity time of the granted service units.
> AVP Header
> 505 8164
> Vendor ID
> 8164
> VSA Type
> 505
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Bandwidth-Control
> Contains the value to control bandwidth usage.
> AVP Header
> 512 8164
> Vendor ID
> 8164
> VSA Type
> 512
> AVP Type
> ENUM. Supported values are:
> HIGH (0)
> LOW (1)
> Group Value
> N/A
> AVP Flag
> M
> SN-Charging-Id
> This AVP contains the charging identifier.
> AVP Header
> 525 8164
> Vendor ID
> 8164
> VSA Type
> 525
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Fast-Reauth-Username
> This AVP is used for fast reauthentication of subscriber.
> AVP Header
> 11010 8164
> Vendor ID
> 8164
> VSA Type
> 11010
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SN-Firewall-Policy
> This AVP contains the name of the Firewall policy to be enabled.
> AVP Header
> 515 8164
> Vendor ID
> 8164
> VSA Type
> 515
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Monitoring-Key
> It is an identifier to a usage monitoring control instance.
> AVP Header
> 518 8164
> Vendor ID
> 8164
> VSA Type
> 518
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Phase0-PSAPName
> This attribute contains name of the County to be used for a subscriber.
> AVP Header
> 523 8164
> Vendor ID
> 523
> VSA Type
> 8164
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Pseudonym-Username
> This AVP is used for reauthentication of subscriber.
> AVP Header
> 11011 8164
> Vendor ID
> 8164
> VSA Type
> 11011
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SN-Service-Flow-Detection
> This AVP defines whether the PCEF should notify the PCRF when it detects traffic matching rules included within Charging-Rule-Install AVP.
> AVP Header
> 520 8164
> Vendor ID
> 8164
> VSA Type
> 520
> AVP Type
> ENUM. Supported values are:
> ENABLE_DETECTION (0)
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Time-Quota-Threshold
> This AVP contains a quota threshold for time in percent value. This is vendor specific AVP.
> AVP Header
> 503 8164
> Vendor ID
> 8164
> VSA Type
> 503
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SN-Total-Used-Service-Unit
> This is a vendor-specific AVP. This AVP contains the total consumed service units.
> AVP Header
> 504 8164
> Vendor ID
> 8164
> VSA Type
> 504
> AVP Type
> GROUPED
> Group Value
> [ TARIFF_CHANGE_USAGE ]
> [ CC_TIME ]
> [ CC_TOTAL_OCTETS ]
> [ CC_INPUT_OCTETS ]
> [ CC_OUTPUT_OCTETS ]
> [ CC_SERVICE_SPECIFIC_UNITS ]
> [ 3GPP_REPORTING_REASON ]
> AVP Flag
> N/A
> SN-Traffic-Policy
> This AVP contains the Traffic Policing policy name.
> AVP Header
> 514 8164
> Vendor ID
> 8164
> VSA Type
> 514
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Transparent-Data
> This is a vendor-specific AVP. This AVP contains current PDP session information. This AVP provides information obtained from the RADIUS server during Access-Accept that can be put into vendor-specific extension towards the CGF and Prepaid server for billing purposes. This AVP is optional in the Access-Accept message.
> AVP Header
> 513 8164
> Vendor ID
> 8164
> VSA Type
> 513
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Unit-Quota-Threshold
> This is a vendor-specific AVP. Contains quota threshold for service specific units of quota in the CLCI-C in percent value.
> AVP Header
> 502 8164
> Vendor ID
> 8164
> VSA Type
> 502
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> SN-Usage-Monitoring
> This attribute is used by PCRF to indicate if usage-monitoring and reporting is enabled or disabled.
> AVP Header
> 521 8164
> Vendor ID
> 8164
> VSA Type
> 521
> AVP Type
> ENUM. Supported values are:
> USAGE_MONITORING_DISABLED (0)
> USAGE_MONITORING_ENABLED (1)
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Usage-Monitoring-Control
> This attribute is used for provisioning and reporting of usage information.
> AVP Header
> 517 8164
> Vendor ID
> 8164
> VSA Type
> 517
> AVP Type
> GROUPED
> Group Value
> [ SN_MONITORING_KEY ]
> [ SN_USAGE_MONITORING ]
> [ SN_USAGE_VOLUME ]
> AVP Flag
> N/A
> SN-Usage-Volume
> This AVP indicates total uplink and downlink usage volume in octets.
> AVP Header
> 519 8164
> Vendor ID
> 8164
> VSA Type
> 519
> AVP Type
> UINT64
> Group Value
> N/A
> AVP Flag
> N/A
> SN-Volume-Quota-Threshold
> This AVP contains a volume threshold value in percentage value.
> AVP Header
> 501 8164
> Vendor ID
> 8164
> VSA Type
> 501
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Software-Version
> This AVP contains the Software Version of the International Mobile Equipment Identity.
> AVP Header
> 6004 10415
> Vendor ID
> 10415
> VSA Type
> 6004
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Specific-Action
> Within an E-PDF initiated Re-Authorization Request; the Specific-Action AVP determines the type of the action.
> AVP Header
> 513 10415
> Vendor ID
> 10415
> VSA Type
> 513
> AVP Type
> ENUM. Supported values are:
> SERVICE_INFORMATION_REQUEST (0)
> CHARGING_CORRELATION_EXCHANGE (1)
> INDICATION_OF_LOSS_OF_BEARER (2)
> INDICATION_OF_RECOVERY_OF_BEARER (3)
> INDICATION_OF_RELEASE_OF_BEARER (4)
> INDICATION_OF_ESTABLISHMENT_OF_BEARER (5)
> IP_CAN_CHANGE (6)
> INDICATION_OF_SUBSCRIBER_DETACHMENT (6)
> INDICATION_OF_RESERVATION_EXPIRATION (7)
> Group Value
> N/A
> AVP Flag
> M
> Specific-APN-Info
> This AVP contains the APN which is not present in the subscription context but the UE is authorized to connect to and the identity of the registered PDN-GW.
> AVP Header
> 1472 10415
> Vendor ID
> 10415
> VSA Type
> 1472
> AVP Type
> GROUPED
> Group Value
> [ SERVICE_SELECTION ]
> [ MIP6_AGENT_INFO ]
> [ VISITED_NETWORK_IDENTIFIER ]
> AVP Flag
> M
> SRES
> This AVP contains the SRES.
> AVP Header
> 1454 10415
> Vendor ID
> 10415
> VSA Type
> 1454
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SS-Code
> This AVP contains the supplementary service codes that are to be deleted from the subscription.
> AVP Header
> 1476 10415
> Vendor ID
> 10415
> VSA Type
> 1476
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> SS-Status
> This AVP refers to the state information of individual supplementary services as defined in 3GPP TS 23.011.
> AVP Header
> 1477 10415
> Vendor ID
> 10415
> VSA Type
> 1477
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Starent-Subscriber-Permission
> This AVP is used to control the Network Mobility (NEMO) permission on a per Enterprise/PDN connection basis.
> AVP Header
> 20 8164
> Vendor ID
> 8164
> VSA Type
> 20
> AVP Type
> ENUM. Supported values are:
> None (0)
> Simple-IP (1)
> Mobile-IP (2)
> Simple-IP-Mobile-IP (3)
> HA-Mobile-IP (4)
> Simple-IP-HA-Mobile-IP (5)
> Mobile-IP-HA-Mobile-IP (6)
> SIP-MIP-HA-MIP (7)
> GGSN-PDP-TYPE-IP (8)
> GGSN-PDP-TYPE-PPP (16)
> Network-Mobility (32)
> FA-HA-NEMO (38)
> All (63)
> Group Value
> N/A
> AVP Flag
> M
> Start-Time
> Contains a time-stamp (in UTC format) which represents the start of a service flow at the BM.
> AVP Header
> 2041 10415
> Vendor ID
> 10415
> VSA Type
> 2041
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> State
> Sent by Diameter server to the NAS in an AA Response command that contains either a Result-Code of “DIAMETER_MULTI_ROUND_AUTH” or a “Termination-Action” AVP with the value of “AA-REQUEST”.
> AVP Header
> 24 0
> Vendor ID
> 0
> VSA Type
> 24
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> STN-SR
> This AVP contains the session transfer number for SRVCC.
> AVP Header
> 1433 10415
> Vendor ID
> 10415
> VSA Type
> 1433
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Stop-Time
> Contains a time-stamp (in UTC format) which represents the termination of a service flow at the BM. This AVP is only included in an accounting request with Accounting-Record-Type indicating STOP_RECORD.
> AVP Header
> 2042 10415
> Vendor ID
> 10415
> VSA Type
> 2042
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Subscriber-Priority
> Subscriber-Priority.
> AVP Header
> 6078 5535
> Vendor ID
> 5535
> VSA Type
> 6078
> AVP Type
> GROUPED
> Group Value
> [ 3GPP2_MAX_AUTH_AGGR_BW_BET ]
> [ 3GPP2_MAX_PER_FLOW_PRIORITY_USER ]
> [ 3GPP2_INTER_USER_PRIORITY ]
> [ 3GPP2_ALLOWED_PERSISTENT_TFTS ]
> [ 3GPP2_MAX_SVC_INST_LINK_FLOW_TOTAL ]
> [ 3GPP2_SERVICE_OPTION_PROFILE ]
> AVP Flag
> M
> Subscriber-Status
> Indicates if the service is barred or granted.
> AVP Header
> 1424 10415
> Vendor ID
> 10415
> VSA Type
> 1424
> AVP Type
> ENUM. Supported values are:
> SERVICEGRANTED (0)
> OPERATORDETERMINEDBARRING (1)
> Group Value
> N/A
> AVP Flag
> M
> Subscription-Data
> This AVP contains the information related to the user profile relevant for EPS and GERAN/UTRAN.
> AVP Header
> 6001 10415
> Vendor ID
> 10415
> VSA Type
> 6001
> AVP Type
> GROUPED
> Group Value
> [ SUBSCRIBER_STATUS ]
> [ MSISDN ]
> [ STN_SR ]
> [ ICS_INDICATOR ]
> [ NETWORK_ACCESS_MODE ]
> [ OPERATOR_DETERMINED_BARRING ]
> [ HPLMN_ODB ]
> [ REGIONAL_SUBSCRIPTION_ZONE_CODE ]
> [ ACCESS_RESTRICTION_DATA ]
> [ APN_OI_REPLACEMENT ]
> [ 3GPP_CHARGING_CHARACTERISTICS ]
> [ AMBR ]
> [ APN_CONFIGURATION_PROFILE ]
> [ RAT_FREQUENCY_SELECTION_PRIORITY ]
> AVP Flag
> M
> Subscription-Id
> Identifier for the end-users subscription (IMSI, MSISDN, etc.).
> AVP Header
> 443 0
> Vendor ID
> 0
> VSA Type
> 443
> AVP Type
> GROUPED
> Group Value
> [ Subscription-Id-Type ]
> [ Subscription-Id-Data ]
> AVP Flag
> M
> Subscription-Id-Data
> Used to identify the end user information.
> AVP Header
> 444 0
> Vendor ID
> 0
> VSA Type
> 444
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Subscription-Id-Type
> Determines the type of identifier carried by the Subscription-Id AVP.
> AVP Header
> 450 0
> Vendor ID
> 0
> VSA Type
> 450
> AVP Type
> ENUM. Supported values are:
> END_USER_E164 (0)
> END_USER_IMSI (1)
> END_USER_SIP_URI (2)
> END_USER_NAI (3)
> END_USER_PRIVATE (4)
> Group Value
> N/A
> AVP Flag
> M
> Subscription-Info
> Contains the UE's subscription information.
> AVP Header
> 642 10415
> Vendor ID
> 10415
> VSA Type
> 642
> AVP Type
> GROUPED
> Group Value
> [ CALL_ID_SIP_HEADER ]
> [ FROM_SIP_HEADER ]
> [ TO_SIP_HEADER ]
> [ RECORD_ROUTE ]
> [ CONTACT ]
> AVP Flag
> N/A
> Subs-Req-Type
> This AVP indicates the type of subscription to notifications request in SNR.Subs-Req-Type.
> AVP Header
> 705 0
> Vendor ID
> 0
> VSA Type
> 705
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Supported-Applications
> This AVP contains supported application identifiers of a Diameter node.
> AVP Header
> 631 10415
> Vendor ID
> 10415
> VSA Type
> 631
> AVP Type
> GROUPED
> Group Value
> [ AUTH_APPLICATION_ID ]
> [ ACCT_APPLICATION_ID ]
> [ VENDOR_SPECIFIC_APPLICATION_ID ]
> AVP Flag
> M
> Supported-Features
> May inform the destination host about the features supported by the origin host.
> AVP Header
> 628 10415
> Vendor ID
> 10415
> VSA Type
> 628
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID ]
> [ FEATURE_LIST_ID ]
> [ FEATURE_LIST ]
> AVP Flag
> M
> Supported-Features-Resp
> This AVP contains a list of supported features of the origin host (Answer message without M bit set).
> AVP Header
> 628 10415
> Vendor ID
> 10415
> VSA Type
> 628
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID_RESP ]
> [ FEATURE_LIST_ID_RESP ]
> [ FEATURE_LIST_RESP ]
> AVP Flag
> N/A
> Supported-RAT-Type
> This AVP contains one of E-UTRAN, UTRAN, GERAN, GAN, I-HSPA-EVOLUTION.
> AVP Header
> 6005 10415
> Vendor ID
> 10415
> VSA Type
> 6005
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Supported-Vendor-Id
> Specifies the vendor ID other than the device vendor.
> AVP Header
> 265 0
> Vendor ID
> 0
> VSA Type
> 265
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Tap-Id
> This AVP holds the Tap ID as provisioned by the DF.
> AVP Header
> 231 4491
> Vendor ID
> 4491
> VSA Type
> 231
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Tariff-Change-Usage
> Defines whether units are used before or after a tariff change.
> AVP Header
> 452 0
> Vendor ID
> 0
> VSA Type
> 452
> AVP Type
> ENUM. Supported values are:
> UNIT_BEFORE_TARIFF_CHANGE (0)
> UNIT_AFTER_TARIFF_CHANGE (1)
> UNIT_INDETERMINATE (2)
> Group Value
> N/A
> AVP Flag
> M
> Tariff-Time-Change
> It is sent from the server to the client and includes the time in seconds since January 1, 1900, 00:00 UTC, when the tariff of the service is changed.
> AVP Header
> 451 0
> Vendor ID
> 0
> VSA Type
> 451
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Teleservice-List
> This AVP contains the service codes for the short message related teleservice for a subscriber.
> AVP Header
> 1486 10415
> Vendor ID
> 10415
> VSA Type
> 1486
> AVP Type
> GROUPED
> Group Value
> [ TS_CODE ]
> AVP Flag
> M
> Terminal-Information
> This AVP contains the information about the user’s mobile equipment.
> AVP Header
> 6002 10415
> Vendor ID
> 10415
> VSA Type
> 6002
> AVP Type
> GROUPED
> Group Value
> [ ESN ]
> [ MEID ]
> [ IMEI ]
> [ SOFTWARE_VERSION ]
> AVP Flag
> M
> Terminal-Type
> This AVP contains a value of the User Class DHCP Option.
> AVP Header
> 352 13019
> Vendor ID
> 13019
> VSA Type
> 352
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Terminating-IOI
> This AVP holds the Inter Operator Identifier for the originating network as generated by the S-CSCF in the home network of the terminating end user.
> AVP Header
> 840 0
> Vendor ID
> 0
> VSA Type
> 840
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Termination-Cause
> Indicates the reason why a session was terminated on the access device.
> AVP Header
> 295 0
> Vendor ID
> 0
> VSA Type
> 295
> AVP Type
> ENUM. Supported values are:
> DIAMETER_LOGOUT (1)
> DIAMETER_SERVICE_NOT_PROVIDED (2)
> DIAMETER_BAD_ANSWER (3)
> DIAMETER_ADMINISTRATIVE (4)
> DIAMETER_LINK_BROKEN (5)
> DIAMETER_AUTH_EXPIRED (6)
> DIAMETER_USER_MOVED (7)
> DIAMETER_SESSION_TIMEOUT (8)
> Group Value
> N/A
> AVP Flag
> M
> TFT-Filter
> This AVP contains the flow filter for one Traffic Flow Template (TFT) packet filter.
> AVP Header
> 1012 10415
> Vendor ID
> 10415
> VSA Type
> 1012
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> TFT-Packet-Filter-Information
> This AVP contains the information from a single TFT packet filter including the evaluation precedence, the filter and the Type-of-Service/Traffic Class sent from the TPF to the CRF.
> AVP Header
> 1013 10415
> Vendor ID
> 10415
> VSA Type
> 1013
> AVP Type
> GROUPED
> Group Value
> [ Precedence ]
> [ TFT-Filter ]
> [ ToS-Traffic-Class ]
> AVP Flag
> M
> Time-First-Usage
> This AVP specifies the time in UTC format for the first IP packet to be transmitted and mapped to the current service data container.
> AVP Header
> 2043 10415
> Vendor ID
> 10415
> VSA Type
> 2043
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Time-Last-Usage
> This AVP specifies the time in UTC format for the last IP packet to be transmitted and mapped to the current service data container.
> AVP Header
> 2044 10415
> Vendor ID
> 10415
> VSA Type
> 2044
> AVP Type
> TIME
> Group Value
> N/A
> AVP Flag
> M
> Time-Quota-Mechanism
> Include this AVP in a Multiple-Services-Credit-Control AVP, when granting time quota.
> AVP Header
> 1270 10415
> Vendor ID
> 10415
> VSA Type
> 1270
> AVP Type
> GROUPED
> Group Value
> [ Base-Time-Interval ]
> [ Time-Quota-Type ]
> AVP Flag
> M
> Time-Quota-Type
> Indicate which time quota consumption mechanism shall be used for the associated category.
> AVP Header
> 1271 10415
> Vendor ID
> 10415
> VSA Type
> 1271
> AVP Type
> ENUM
> Group Value
> N/A
> AVP Flag
> M
> Time-Stamps
> This grouped AVP holds the time of the initial SIP request and the time of the response to the initial SIP Request.
> AVP Header
> 833 0
> Vendor ID
> 0
> VSA Type
> 833
> AVP Type
> GROUPED
> Group Value
> [ SIP_REQUEST_TIMESTAMP ]
> [ SIP_RESPONSE_TIMESTAMP ]
> AVP Flag
> M
> Time-Usage
> This AVP indicates the length of the current flow in seconds.
> AVP Header
> 2045 10415
> Vendor ID
> 10415
> VSA Type
> 2045
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> TMGI
> Contains the Temporary Mobile Group Identity allocated to a particular MBMS bearer service.
> AVP Header
> 900 10415
> Vendor ID
> 10415
> VSA Type
> 900
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> To-SIP-Header
> This AVP contains the information in the To header.
> AVP Header
> 645 10415
> Vendor ID
> 10415
> VSA Type
> 645
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> N/A
> ToS-Traffic-Class
> This AVP contains the Type-of-Service/Traffic-Class of a TFT packet filter.
> AVP Header
> 1014 10415
> Vendor ID
> 10415
> VSA Type
> 1014
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Trace-Collection-Entity
> This AVP contains the IPv4 or IPv6 address of the Trace Collection Entity.
> AVP Header
> 1452 10415
> Vendor ID
> 10415
> VSA Type
> 1452
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Trace-Data
> This AVP contains the information related to trace function.
> AVP Header
> 1458 10415
> Vendor ID
> 10415
> VSA Type
> 1458
> AVP Type
> GROUPED
> Group Value
> [ TRACE_REFERENCE ]
> [ TRACE_DEPTH_LIST ]
> [ TRACE_NE_TYPE_LIST ]
> [ TRACE_INTERFACE_LIST ]
> [ TRACE_EVENT_LIST ]
> [ OMC_ID ]
> [ TRACE_COLLECTION_ENTITY ]
> AVP Flag
> M
> Trace-Depth
> This AVP indicates whether entire signalling messages or just some IEs need to be recorded.
> AVP Header
> 1462 10415
> Vendor ID
> 10415
> VSA Type
> 1462
> AVP Type
> ENUM. Supported values are:
> Minimum (0)
> Medium (1)
> Maximum (2)
> MinimumWithoutVendorSpecificExtension (3)
> MediumWithoutVendorSpecificExtension (4)
> MaximumWithoutVendorSpecificExtension (5)
> Group Value
> N/A
> AVP Flag
> M
> Trace-Depth-List
> This AVP contains the list of Trade Depths per NE Type.
> AVP Header
> 1460 10415
> Vendor ID
> 10415
> VSA Type
> 1460
> AVP Type
> GROUPED
> Group Value
> [ TRACE_DEPTH_PER_NE_TYPE ]
> AVP Flag
> M
> Trace-Depth-Per-NE-Type
> This AVP contains the Network-Element-Type that is involved in a session trace, and the corresponding depth of trace for the specified Network-Element-Type.
> AVP Header
> 145110415
> Vendor ID
> 10415
> VSA Type
> 1451
> AVP Type
> GROUPED
> Group Value
> [ NETWORK_ELEMENT_TYPE ]
> [ TRACE_DEPTH ]
> AVP Flag
> M
> Trace-Event-List
> Trace-Event-List.
> AVP Header
> 1465 10415
> Vendor ID
> 10415
> VSA Type
> 1465
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Trace-Interface-List
> Trace-Interface-List.
> AVP Header
> 1464 10415
> Vendor ID
> 10415
> VSA Type
> 1464
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Trace-NE-Type-List
> This AVP contains the concatenation of MCC MNC.
> AVP Header
> 1463 10415
> Vendor ID
> 10415
> VSA Type
> 1463
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Trace-NE-TypeList
> Trace-NE-TypeList.
> AVP Header
> 1461 10415
> Vendor ID
> 10415
> VSA Type
> 1461
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Trace-Reference
> This AVP contains the concatenation of MCC MNC.
> AVP Header
> 1459 10415
> Vendor ID
> 10415
> VSA Type
> 1459
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Tracking-Area-Identity
> This attribute contains the tracking area identifier of the user.
> AVP Header
> 1603 10415
> Vendor ID
> 10415
> VSA Type
> 1603
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Traffic-Data-Volumes
> This AVP is used to allow the transmission of the IPCAN bearer container on encountering change on charging condition for this IP-CAN bearer.The Rf interface supports AMBR reporting for non-guaranteed bit rate (non-GBR) bearers in a TDV AVP group.
> AVP Header
> 2046 10415
> Vendor ID
> 10415
> VSA Type
> 2046
> AVP Type
> GROUPED
> Group Value
> [ QOS_INFORMATION ]
> [ ACCOUNTING_INPUT_OCTETS ]
> [ ACCOUNTING_INPUT_PACKETS ]
> [ ACCOUNTING_OUTPUT_OCTETS ]
> [ ACCOUNTING_OUTPUT_PACKETS ]
> [ CHANGE_CONDITION ]
> [ CHANGE_TIME ]
> [ 3GPP_USER_LOCATION_INFO ]
> AVP Flag
> M
> Transport-Class
> Contains an integer used as an index pointing to a class of transport services to be applied.
> AVP Header
> 311 13019
> Vendor ID
> 13019
> VSA Type
> 311
> AVP Type
> UNIT32
> Group Value
> N/A
> AVP Flag
> N/A
> Trigger
> Triggers in the client and to identify the triggers which caused re-authorization in usage.
> AVP Header
> 1264 10415
> Vendor ID
> 10415
> VSA Type
> 1264
> AVP Type
> GROUPED
> Group Value
> [ Trigger-Type ]
> AVP Flag
> M
> Trunk-Group-ID
> This grouped AVP identifies the incoming and outgoing PSTN legs.
> AVP Header
> 851 10415
> Vendor ID
> 10415
> VSA Type
> 851
> AVP Type
> GROUPED
> Group Value
> [ INCOMING_TRUNK_GROUP_ID ]
> [ OUTGOING_TRUNK_GROUP_ID ]
> AVP Flag
> M
> TS-Code
> This AVP contains the code identifying a single teleservice, a group of teleservices, or all teleservices.
> AVP Header
> 1487 10415
> Vendor ID
> 10415
> VSA Type
> 1487
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Assignment-Id
> Used to indicate to the tunnel initiator the particular tunnel to which a session is to be assigned.
> AVP Header
> 82 0
> Vendor ID
> 0
> VSA Type
> 82
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Client-Auth-Id
> Specifies the name used by the tunnel initiator during the authentication phase of tunnel establishment.
> AVP Header
> 90 0
> Vendor ID
> 0
> VSA Type
> 90
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Client-Endpoint
> This AVP contains the address of the initiator end of the tunnel.
> AVP Header
> 66 0
> Vendor ID
> 0
> VSA Type
> 66
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Header-Filter
> Tunnel Header Filter.
> AVP Header
> 1036 10415
> Vendor ID
> 10415
> VSA Type
> 1036
> AVP Type
> IPFILTERRULE
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Header-Length
> This AVP indicates the length of the tunnel header in octets.
> AVP Header
> 1037 10415
> Vendor ID
> 10415
> VSA Type
> 1037
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Information
> This AVP contains the tunnel (outer) header information from a single IP flow.
> AVP Header
> 1038 10415
> Vendor ID
> 10415
> VSA Type
> 1038
> AVP Type
> GROUPED
> Group Value
> [ TUNNEL_HEADER_LENGTH ]
> [ TUNNEL_HEADER_FILTER ]
> AVP Flag
> M
> Tunneling
> Used to describe a compulsory tunnel service.
> AVP Header
> 401 0
> Vendor ID
> 0
> VSA Type
> 401
> AVP Type
> GROUPED
> Group Value
> [ TUNNEL_TYPE ]
> [ TUNNEL_MEDIUM_TYPE ]
> [ TUNNEL_CLIENT_ENDPOINT ]
> [ TUNNEL_SERVER_ENDPOINT ]
> [ TUNNEL_PREFERENCE ]
> [ TUNNEL_CLIENT_AUTH_ID ]
> [ TUNNEL_SERVER_AUTH_ID ]
> [ TUNNEL_ASSIGNMENT_ID ]
> [ TUNNEL_PASSWORD ]
> [ TUNNEL_PRIVATE_GROUP_ID ]
> AVP Flag
> M
> Tunnel-Medium-Type
> This AVP contains the transport medium to use when creating a tunnel for protocols (such as L2TP) that can operate over multiple transports.
> AVP Header
> 65 0
> Vendor ID
> 0
> VSA Type
> 65
> AVP Type
> ENUM. Supported values are:
> IPv4_IPversion4 (1)
> IPv6_IPversion6 (2)
> NSAP (3)
> HDLC-8-bit_multidrop (4)
> BBN-1822 (5)
> 802-includes-all-802-media-plus-Ethernet-canonical_format (6)
> E163_POTS (7)
> E164_SMDS_Frame-Relay_ATM (8)
> F69_Telex (9)
> X121_X25_Frame-Relay (10)
> IPX (11)
> Appletalk (12)
> Decnet_IV (13)
> Banyan_Vines (14)
> E164-with-NSAP-format-subaddress (15)
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Password
> This AVP contains a password to be used to authenticate to a remote server.
> AVP Header
> 69 0
> Vendor ID
> 0
> VSA Type
> 69
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Preference
> Used to identify the relative preference assigned to each tunnel when more than one set of tunneling AVPs is returned within separate Grouped-AVPs.
> AVP Header
> 83 0
> Vendor ID
> 0
> VSA Type
> 83
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Private-Group-Id
> This AVP contains the group ID for a particular tunneled session.
> AVP Header
> 81 0
> Vendor ID
> 0
> VSA Type
> 81
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Server-Auth-Id
> Contains the name used by the tunnel terminator during the authentication phase of tunnel establishment.
> AVP Header
> 91 0
> Vendor ID
> 0
> VSA Type
> 91
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Server-Endpoint
> This AVP contains the address of the server end of the tunnel.
> AVP Header
> 67 0
> Vendor ID
> 0
> VSA Type
> 67
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Tunnel-Type
> This AVP contains the tunneling protocol(s) to be used (in the case of a tunnel initiator) or in use (in the case of a tunnel terminator).
> AVP Header
> 64 0
> Vendor ID
> 0
> VSA Type
> 64
> AVP Type
> ENUM. Supported values are:
> Point-to-Point_Tunneling_Protocol-PPTP (1)
> Layer-Two-Forwarding_L2F (2)
> Layer-Two-Tunneling_Protocol-L2TP (3)
> Ascend-Tunnel-Management-Protocol-ATMP (4)
> Virtual-Tunneling-Protocol-VTP (5)
> IP-Authentication-Header-in-the-Tunnel-mode_AH (6)
> IP-in-IP_Encapsulation_IP-IP (7)
> Minimal_IP-in-IP_Encapsulation_MIN-IP-IP (8)
> IP_Encapsulating_Security_Payload_in_the_Tunnel-mode_ESP (9)
> Generic_Route_Encapsulation_GRE (10)
> Bay_Dial_Virtual_Services-DVS (11)
> IP-in-IP-Tunneling (12)
> Virtual-LANs-VLAN (13)
> Group Value
> N/A
> AVP Flag
> M
> UAR-Flags
> Contains a bit mask, if the bit 0 is set, it indicates that the request corresponds to an IMS Emergency Registration.
> AVP Header
> 637 0
> Vendor ID
> 0
> VSA Type
> 637
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> ULA-Flags
> The ULR-Flags AVP is of type Unsigned32 and it contains a bit mask.
> AVP Header
> 6007 10415
> Vendor ID
> 10415
> VSA Type
> 6007
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> ULR-Flags
> The ULR-Flags AVP is of type Unsigned32 and it contains a bit mask.
> AVP Header
> 6006 10415
> Vendor ID
> 10415
> VSA Type
> 6006
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> UMTS-Vector
> This AVP contains Authentication Information for UMTS.
> AVP Header
> 6018 10415
> Vendor ID
> 10415
> VSA Type
> 6018
> AVP Type
> GROUPED
> Group Value
> [ ITEM_NUMBER ]
> [ RAND ]
> [ XRES ]
> [ AUTN ]
> [ CONFIDENTIALITY_KEY ]
> [ INTEGRITY_KEY ]
> AVP Flag
> M
> Unit-Value
> Cost estimate (type of money) of the service.
> AVP Header
> 445 0
> Vendor ID
> 0
> VSA Type
> 445
> AVP Type
> GROUPED
> Group Value
> [ VALUE_DIGITS ]
> [ EXPONENT ]
> AVP Flag
> M
> Usage-Monitoring-Information
> This AVP contains the usage monitoring control information.
> AVP Header
> 1067 10415
> Vendor ID
> 10415
> VSA Type
> 1067
> AVP Type
> GROUPED
> Group Value
> [ MONITORING_KEY ]
> [ GRANTED_SERVICE_UNIT ]
> [ USED_SERVICE_UNIT ]
> [ USAGE_MONITORING_LEVEL ]
> [ USAGE_MONITORING_REPORT ]
> [ USAGE_MONITORING_SUPPORT ]
> AVP Flag
> N/A
> Usage-Monitoring-Level
> This AVP is used by the PCRF to indicate whether the usage monitoring instance applies to the IP-CAN session or to one or more PCC rules.
> AVP Header
> 1068 10415
> Vendor ID
> 10415
> VSA Type
> 1068
> AVP Type
> ENUM. Supported values are:
> SESSION_LEVEL (0)
> PCC_RULE_LEVEL (1)
> Group Value
> N/A
> AVP Flag
> N/A
> Usage-Monitoring-Report
> This AVP is used by the PCRF to indicate that accumulated usage is to be reported by the PCEF regardless of whether a usage threshold is reached for certain usage monitoring key.
> AVP Header
> 1069 10415
> Vendor ID
> 10415
> VSA Type
> 1069
> AVP Type
> ENUM. Supported values are:
> USAGE_MONITORING_REPORT_REQUIRED (0)
> Group Value
> N/A
> AVP Flag
> N/A
> Usage-Monitoring-Support
> This AVP is used by the PCRF to indicate whether usage monitoring should be disabled for certain Monitoring Key.
> AVP Header
> 1070 10415
> Vendor ID
> 10415
> VSA Type
> 1070
> AVP Type
> ENUM. Supported values are:
> USAGE_MONITORING_DISABLED (0)
> Group Value
> N/A
> AVP Flag
> N/A
> Used-Service-Unit
> The used service unit measured from the point when service is active.
> AVP Header
> 446 0
> Vendor ID
> 0
> VSA Type
> 446
> AVP Type
> GROUPED
> Group Value
> [ TARIFF_TIME_CHANGE ]
> [ TARIFF_CHANGE_USAGE ]
> [ CC_TIME ]
> [ CC_MONEY ]
> [ CC_TOTAL_OCTETS ]
> [ CC_INPUT_OCTETS ]
> [ CC_OUTPUT_OCTETS ]
> [ CC_SERVICE_SPECIFIC_UNITS ]
> AVP Flag
> M
> User-Authorization-Type
> This AVP contains the type of user authorization being performed in a User Authorization operation.
> AVP Header
> 623 10415
> Vendor ID
> 10415
> VSA Type
> 623
> AVP Type
> ENUM. Supported values are:
> REGISTRATION (0)
> DE_REGISTRATION (1)
> REGISTRATION_AND_CAPABILITIES (2)
> Group Value
> N/A
> AVP Flag
> M
> User-Data
> This AVP contains the user data requested in the PUR and SNR operations and the data to be modified in the UPR operations.
> AVP Header
> 702 0
> Vendor ID
> 0
> VSA Type
> 702
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> User-Data-Already-Available
> Indicates whether S-CSCF is already storing the user data or not.
> AVP Header
> 624 10415
> Vendor ID
> 10415
> VSA Type
> 624
> AVP Type
> ENUM. Supported values are:
> USER_DATA_NOT_AVAILABLE (0)
> USER_DATA_ALREADY_AVAILABLE (1)
> Group Value
> N/A
> AVP Flag
> M
> User-Equipment-Info
> Indicates the identification and capabilities of the terminal.
> AVP Header
> 458 0
> Vendor ID
> 0
> VSA Type
> 458
> AVP Type
> GROUPED
> Group Value
> [ USER_EQUIPMENT_INFO_TYPE ]
> [ USER_EQUIPMENT_INFO_VALUE ]
> AVP Flag
> M
> User-Equipment-Info-Type
> Defines the type of information present in User-Equipment-Info-Value AVP.
> AVP Header
> 459 0
> Vendor ID
> 0
> VSA Type
> 459
> AVP Type
> ENUM. Supported values are:
> IMEISV (0)
> MAC (1)
> EUI64 (2)
> MODIFIED_EUI64 (3)
> ESN (4)
> MEID (5)
> Group Value
> N/A
> AVP Flag
> M
> User-Equipment-Info-Value
> Defines the type of identifier used.
> AVP Header
> 460 0
> Vendor ID
> 0
> VSA Type
> 460
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> User-Id
> User ID.
> AVP Header
> 1444 10415
> Vendor ID
> 10415
> VSA Type
> 1444
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> User-Identity
> This grouped AVP contains either a Public-Identity AVP or an MSISDN AVP.
> AVP Header
> 700 10415
> Vendor ID
> 10415
> VSA Type
> 700
> AVP Type
> GROUPED
> Group Value
> [ PUBLIC_IDENTITY ]
> [ MSISDN ]
> AVP Flag
> M
> User-Name
> Identification of the service user in a format consistent with the NAI specification.
> AVP Header
> 1 0
> Vendor ID
> 0
> VSA Type
> 1
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> User-Password
> This attribute indicates PAP for multiauth in PDG.
> AVP Header
> 2 0
> Vendor ID
> 0
> VSA Type
> 2
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> User-Session-Id
> This AVP holds the session identifier.
> AVP Header
> 830 10415
> Vendor ID
> 10415
> VSA Type
> 830
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> User-State
> User-State
> AVP Header
> 1499 10415
> Vendor ID
> 10415
> VSA Type
> 1499
> AVP Type
> ENUM. Supported values are:

> • | DETACHED (0)

> • | ATTACHED_NOT_REACHABLE_FOR_PAGING (1)

> • | ATTACHED_REACHABLE_FOR_PAGING (2)

> • | CONNECTED_NOT_REACHABLE_FOR_PAGING (3)

> • | CONNECTED_REACHABLE_FOR_PAGING (4)

> • | NETWORK_DETERMINED_NOT_REACHABLE (5)

> Group Value
> N/A
> AVP Flag
> M
> UTRAN-Vector
> This AVP contains Authentication Information for UTRAN.
> AVP Header
> 1415 10415
> Vendor ID
> 10415
> VSA Type
> 1415
> AVP Type
> GROUPED
> Group Value
> [ ITEM_NUMBER ]
> [ RAND ]
> [ XRES ]
> [ AUTN ]
> [ CONFIDENTIALITY_KEY ]
> [ INTEGRITY_KEY ]
> AVP Flag
> M
> V4-Transport-Address
> Contains a single IPv4 address and a single port number.
> AVP Header
> 454 13019
> Vendor ID
> 13019
> VSA Type
> 454
> AVP Type
> GROUPED
> Group Value
> [ FRAMED_IP_ADDRESS ]
> [ PORT_NUMBER ]
> AVP Flag
> N/A
> V6-Transport-Address
> Contains a single IPv6 address and a single port number.
> AVP Header
> 453 13019
> Vendor ID
> 13019
> VSA Type
> 453
> AVP Type
> GROUPED
> Group Value
> [ FRAMED_IPV6_PREFIX ]
> [ PORT_NUMBER ]
> AVP Flag
> N/A
> Validity-Time
> Validity time of the granted service units. Measurement starts upon receipt of the Credit-Control-Answer Message containing this AVP.
> AVP Header
> 448 0
> Vendor ID
> 0
> VSA Type
> 448
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Value-Digits
> This AVP contains the significant digits of the number. If decimal values are needed to present the units, the scaling MUST be indicated with the related Exponent AVP.
> AVP Header
> 447 0
> Vendor ID
> 0
> VSA Type
> 447
> AVP Type
> INT64
> Group Value
> N/A
> AVP Flag
> M
> VBM-Address
> VBM Address.
> AVP Header
> 1460 10415
> Vendor ID
> 10415
> VSA Type
> 1460
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> Vendor-Id
> Unique Identifier of the Vendor and contains the IANA "SMI Network Management Private Enterprise Codes" value assigned to the vendor of the Diameter application.
> AVP Header
> 266 0
> Vendor ID
> 0
> VSA Type
> 266
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> Vendor-Id-Resp
> Unique identifier of the vendor.
> AVP Header
> 266 10415
> Vendor ID
> 10415
> VSA Type
> 266
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> N/A
> Vendor-Specific-Application-Id
> Specifies the Vendor Specific Application ID and is used to advertise support of a vendor-specific Diameter Application.
> AVP Header
> 260 0
> Vendor ID
> 0
> VSA Type
> 260
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID ]
> [ AUTH_APPLICATION_ID ]
> [ ACCT_APPLICATION_ID ]
> AVP Flag
> M
> Vendor-Specific-QoS-Profile-Template
> This AVP defines the namespace of the QoS profile (indicated in the Vendor-ID AVP) followed by the specific value for the profile.
> AVP Header
> 6064 0
> Vendor ID
> 0
> VSA Type
> 6064
> AVP Type
> GROUPED
> Group Value
> [ VENDOR_ID ]
> [ QOS_PROFILE_TEMPLATE ]
> AVP Flag
> M
> Visited-Network-Identifier
> This AVP contains an identifier that helps the home network to identify the visited network (for example, the visited network domain name).
> AVP Header
> 600 10415
> Vendor ID
> 10415
> VSA Type
> 600
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> Visited-PLMN-Id
> Contains the concatenation of MCC and MNC.
> AVP Header
> 6008 10415
> Vendor ID
> 10415
> VSA Type
> 6008
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> VOA-Session-ID
> VOA-Session-ID.
> AVP Header
> 1464 10415
> Vendor ID
> 10415
> VSA Type
> 1464
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> VPLMN-Dynamic-Address-Allowed
> This AVP indicates whether for this APN, the UE is allowed to use the PDN GW in the domain of the HPLMN only, or additionally, the PDN GW in the domain of the VPLMN.
> AVP Header
> 1432 10415
> Vendor ID
> 10415
> VSA Type
> 1432
> AVP Type
> ENUM. Supported values are:
> NOTALLOWED (0)
> ALLOWED (1)
> Group Value
> N/A
> AVP Flag
> M
> Wildcarded-IMPU
> This AVP contains a wild-carded Public User Identity stored in the HSS.
> AVP Header
> 636 10415
> Vendor ID
> 10415
> VSA Type
> 636
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> Wildcarded-PSI
> This AVP contains a wild-carded PSI stored in the HSS.
> AVP Header
> 634 10415
> Vendor ID
> 10415
> VSA Type
> 634
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> M
> Wildcarded-Public-Identity
> This AVP contains a Wildcarded PSI or Wildcarded Public User Identity stored in the HSS.
> AVP Header
> 634 10415
> Vendor ID
> 10415
> VSA Type
> 634
> AVP Type
> UTF8STRING
> Group Value
> N/A
> AVP Flag
> N/A
> WiMAX-A-PCEF-Address
> This AVP indicates the IP address of the A-PCEF to the PDF.
> AVP Header
> 411 24757
> Vendor ID
> 24757
> VSA Type
> 411
> AVP Type
> ADDRESS
> Group Value
> N/A
> AVP Flag
> M
> WiMAX-PCC-R3-P-Capability
> This AVP identifies in a CCR message the WiMAX capabilities supported by the ASN. In a CCA it identifies the options selected by the PCRF.
> AVP Header
> 404 24757
> Vendor ID
> 24757
> VSA Type
> 404
> AVP Type
> GROUPED
> Group Value
> [ WIMAX_RELEASE ]
> [ ACCOUNTING_PCC_R3_P_CAPABILITY ]
> AVP Flag
> M
> WiMAX-QoS-Information
> This AVP contains the WiMAX QoS information for ASN GW.
> AVP Header
> 407 24757
> Vendor ID
> 24757
> VSA Type
> 407
> AVP Type
> GROUPED
> Group Value
> [ QOS_CLASS_IDENTIFIER ]
> [ MAX_REQUESTED_BANDWIDTH_UL ]
> [ MAX_REQUESTED_BANDWIDTH_DL ]
> [ GUARANTEED_BITRATE_UL ]
> [ GUARANTEED_BITRATE_DL ]
> [ PACKET_INTERVAL ]
> [ PACKET_SIZE ]
> AVP Flag
> M
> WiMAX-Release
> This AVP indicates a WiMAX release formatted as major/minor.
> AVP Header
> 301 24757
> Vendor ID
> 24757
> VSA Type
> 301
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M
> WLAN-Session-Id
> This AVP contains the WLAN Session ID that is used to correlate PDG and WLAN AN charging data.
> AVP Header
> 11009 0
> Vendor ID
> 0
> VSA Type
> 11009
> AVP Type
> UINT32
> Group Value
> N/A
> AVP Flag
> M
> XRES
> This AVP contains the XRES.
> AVP Header
> 1448 10415
> Vendor ID
> 10415
> VSA Type
> 1448
> AVP Type
> OCTETSTRING
> Group Value
> N/A
> AVP Flag
> M

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883