> MSEG Peer Profile Configuration Mode Commands
> This configuration mode enables to configure the non-local MSEG instances in the network. Though this is intended to contain peer-MSEG information, there is no restriction on configuring local MSEG instances. Local MSEG service instances will look up both this list as well as the list of local MSEG services whenever necessary.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> mseg-gtpc
> This command adds/removes MSEG service control addresses in an MSEG peer profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> mseg-gtpc ipv4/ipv6_address [ udp-port port_number ]
> no mseg-gtpc
> no
> Deletes the previously configured MSEG GTP-C address from the current MSEG peer profile.
> ipv4/ipv6_address
> Specifies the MSEG GTP-C address.
> ipv4/ipv6_address must be an IPv4 address in dotted decimal notation, or an IPv6 address in colon notation. IPv6 address in :: notation is also supported.
> udp-port port_number
> Specifies the UDP port number.
> port_number must be an integer from 1 through 65535.
> Usage
> Use this command to add/remove MSEG service control addresses in an MSEG peer profile.
> Example
> The following command configures the MSEG GTP-C address 1.1.1.1 and the UDP port 111 in the current MSEG peer profile:
> mseg-gtpc 1.1.1.1 udp-port 111
> mseg-gtpu
> This command adds/removes MSEG service data addresses in an MSEG peer profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] mseg-gtpu ipv4/ipv6_address
> no
> Deletes the specified MSEG GTP-U address from the current MSEG peer profile.
> ipv4/ipv6_address
> Specifies the MSEG GTP-U address.
> ipv4/ipv6_address must be an IPv4 address in dotted decimal notation, or an IPv6 address in colon notation. IPv6 address in :: notation is also supported.
> Usage
> Use this command to add/remove MSEG service data addresses in an MSEG peer profile. Multiple GTP-U addresses can be associated with an MSEG instance.
> Example
> The following command configures the MSEG GTP-U address 1.1.1.1 for the current MSEG peer profile:
> mseg-gtpu 1.1.1.1
> mseg-id
> This command configures the MSEG instance ID in an MSEG peer profile. Note that the MSEG profile is not activated until this ID is configured.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] mseg-id mseg_id
> no
> Deactivates the specified MSEG peer profile.
> mseg_id
> Specifies the MSEG instance ID.
> mseg_id must be an integer from 1 through 65535.
> Usage
> Use this command to configure the MSEG instance ID in an MSEG peer profile.
> This ID must be unique across all MSEG installations in an operator’s domain. The MSEG profile is not activated until this ID is configured.
> Example
> The following command configures the MSEG instance ID in the current MSEG peer profile to 111:
> mseg-id 111

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883