> MSEG Associated Services Profile Configuration Mode Commands
> The MSEG Associated Services Profile Configuration Mode enables to configure the associated services, such as NAT, accounting context, and destination context, that must be applied to an off-loaded session once it is set up.
> active-charging-rulebase
> This command configures an ACS rulebase in the MSEG associated services profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> active-charging-rulebase acs_rulebase_name
> no active-charging-rulebase
> no
> Deletes the ACS rulebase, if previously configured, from the current MSEG associated services profile.
> acs_rulebase_name
> Specifies name of the ACS rulebase.
> acs_rulebase_name must be an alpha and/or numeric string of 1 through 63 characters in length.
> Usage
> Use this command to configure an ACS rulebase in the MSEG associated services profile. By default, there is no ACS rulebase configured in a profile.
> Rulebase configuration is used in the ACS context for configuring collection of rule definitions and their associated billing policy. Different rulebases can be configured for different set of subscribers by defining appropriate MSEG filters.
> Example
> The following command configures an ACS rulebase named test in the current MSEG associated services profile:
> active-charging-rulebase test
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> fw-nat-policy
> This command configures a Firewall-and-NAT policy in the MSEG associated services profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> fw-nat-policy fw_nat_policy_name
> no fw-nat-policy
> no
> Deletes the Firewall-and-NAT policy, if previously configured, from the current MSEG associated services profile.
> fw_nat_policy_name
> Specifies name of the Firewall-and-NAT policy.
> fw_nat_policy_name must be an alpha and/or numeric string of 1 through 63 characters in length.
> Usage
> Use this command to configure a Firewall-and-NAT policy in the MSEG associated services profile. By default, there is no Firewall-and-NAT policy configured in a profile.
> If, in the profile, an ACS rulebase is configured and there is a Firewall-and-NAT policy configured in that rulebase, the Firewall-and-NAT policy configured using this command will take precedence for sessions that are offloaded. If not configured, the MSEG will act as an anchor-proxy for the offloaded calls.
> Example
> The following command configures a Firewall-and-NAT policy named test in the current MSEG associated services profile:
> fw-nat-policy test
> ip
> This command configures IP parameters in the MSEG associated services profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> ip { access-group access_group_name { in | out } | context-name context_name }
> no ip { access-group { in | out } | context-name }
> no
> Deletes the specified IP configuration, if previously configured, from the current MSEG associated services profile.
> access-group access_group_name { in | out }
> Specifies name of the IPv4/IPv6 access group to use for redirecting traffic to the ACS subsystem.
> access_group_name must be an alpha and/or numeric string of 1 through 63 characters in length.
> in specifies that the ACL group be applied to inbound traffic.
> out specifies the ACL group be applied to outbound traffic.
> context-name context_name
> Specifies name of the destination context to use.
> context_name must be an alpha and/or numeric string of 1 through 63 characters in length.
> Important: If the context name is not configured, MSEG service context will be used.
> Usage
> Use this command to configure IP parameters in an MSEG associated services profile. The IPv4/IPv6 access group is used for redirecting the traffic to ACS Subsystem.
> Example
> The following command configures the IP access group named test to be applied on outbound traffic in the current MSEG associated services profile:
> ip access-group test out

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883