> SCCP Schema Statistics
> The SCCP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SGSN
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the SCCP Service Schema

> Variables | Description | Data Type
> ssa-txed | Total number of subsystem available messages sent by Signalling Connection Control Part (SCCP) function. | Int32
> ss-oos-grant-txed | Total number of subsystem out of service grant messages sent by SCCP function. | Int32
> ss-oos-req-txed | Total number of subsystem out of service request messages sent by SCCP function. | Int32
> ssp-txed | Total number of subsystem prohibited messages sent by SCCP function. | Int32
> ss-status-test-txed | Total number of subsystem status test messages sent by SCCP function. | Int32
> ssa-rcvd | Total number of subsystem available messages received by Signalling Connection Control Part (SCCP) function. | Int32
> ss-oos-grant-rcvd | Total number of subsystem out of service grant messages received by SCCP function. | Int32
> ss-oos-req-rcvd | Total number of subsystem out of service request messages received by SCCP function. | Int32
> ss-prohibit-rcvd | Total number of subsystem prohibited messages received by SCCP function. | Int32
> ss-status-test-rcvd | Total number of subsystem status test messages received by SCCP function. | Int32
> ss-congested-txed | Total number of subsystem congested messages sent by SCCP function. | Int32
> ss-congested-rcvd | Total number of subsystem congested messages received by SCCP function. | Int32
> sccp-rtf-notrans-addr-nature | Total number of SCCP function routing failed due to no translation for address of specific such type. | Int32
> sccp-rtf-notrans-addr-specific | Total number of SCCP function routing failed due to no translation of specific address. | Int32
> sccp-rtf-netwfail-pc-unavail | Total number of SCCP function routing failed due to network failure or point code unavailable. | Int32
> sccp-rtf-netw-conges | Total number of SCCP function routing failed due to network failure congestion. | Int32
> sccp-rtf-ssn-fail | Total number of SCCP function routing failed due to failure of subsystem of specific SS number. | Int32
> sccp-rtf-ssn-conges | Total number of SCCP function routing failed due to congestion of subsystem of specific SS number. | Int32
> sccp-syntax-error | Total number of SCCP function failed due to syntax error in message. | Int32
> sccp-reassem-err-timer | Total number of SCCP function failed as reassembly timer expired for message. This is a counter type of statistic. | Int32
> sccp-reassem-err-sequence | Total number of SCCP function failed as segment out of sequence during reassembly. This is a counter type of statistic. | Int32
> sccp-reassem-err-space | Total number of SCCP function failed as out of memory/space error occurred during reassembly. This is a counter type of statistic. | Int32
> sccp-hop-counter-violation | Total number of SCCP function failed due to hop counter violation in message. | Int32
> sccp-provider-ini-reset | Total number of SCCP function failed due service provider initiated reset occurred. | Int32
> sccp-provider-ini-rel | Total number of SCCP function failed due service provider initiated release occurred. | Int32
> sccp-msg-toolarge-segment | Total number of SCCP function failed as message is too large for segmentation. | Int32
> sccp-segmentation-fail | Total number of SCCP function failed due to segmentation procedure failure. | Int32
> sccp-total-msgs-handled | Total number of SCCP messages handled by subsystem. | Int32
> sccp-total-msgs-handl-local-ss | Total number of SCCP messages handled by subsystem which were intended for local subsystems. | Int32
> sccp-total-msgs-req-gtt | Total number of SCCP messages requiring global address translation. | Int32
> sccp-udt-sent | Total unit data messages sent by SCCP function. | Int32
> sccp-udt-rcvd | Total unit data messages received by SCCP function. | Int32
> sccp-udts-sent | Total unit data service messages sent by SCCP function. | Int32
> sccp-udts-rcvd | Total unit data service messages received by SCCP function. | Int32
> sccp-xudt-sent | Total extended unit data messages sent by SCCP function. | Int32
> sccp-xudt-rcvd | Total extended unit data messages received by SCCP function. | Int32
> sccp-xudts-sent | Total extended unit data service messages sent by SCCP function. | Int32
> sccp-xudts-rcvd | Total extended unit data service messages received by SCCP function. | Int32
> sccp-ludt-sent | Total long unit data messages sent by SCCP function. | Int32
> sccp-ludt-rcvd | Total long unit data messages received by SCCP function. | Int32
> sccp-ludts-sent | Total long unit data service messages sent by SCCP function. | Int32
> sccp-ludts-rcvd | Total long unit data service messages received by SCCP function. | Int32
> sccp-cr-sent | Total connection refuse messages for message transfer part (MTP) and ISDN user part (ISUP) sent by SCCP function. | Int32
> sccp-cr-rcvd | Total connection refuse messages for message transfer part (MTP) and ISDN user part (ISUP) received by SCCP function. | Int32
> sccp-cc-sent | Total connection confirm messages for message transfer part (MTP) and ISDN user part (ISUP) sent by SCCP function. | Int32
> sccp-cc-rcvd | Total connection confirm messages for message transfer part (MTP) and ISDN user part (ISUP) received by SCCP function. | Int32
> sccp-cref-sent | Total connection refusal messages for message transfer part (MTP) and ISDN user part (ISUP) sent by SCCP function. | Int32
> sccp-cref-rcvd | Total connection refusal messages for message transfer part (MTP) and ISDN user part (ISUP) received by SCCP. | Int32
> sccp-rsr-msg-sent | Total reset request messages sent by SCCP function. | Int32
> sccp-rsr-msg-rcvd | Total reset request messages received by SCCP function. | Int32
> sccp-err-msg-sent | Total error messages sent by SCCP function. | Int32
> sccp-err-msg-rcvd | Total error messages received by SCCP function. This is a counter type of statistic. | Int32
> sccp-unequipped-user | Total number of unequipped users on SCCP function. This is a counter type of statistic. | Int32
> sccp-reason-unknown | Total number of failure at SCCP function due to unknown reasons or reasons not specified in this table. This is a counter type of statistic. | Int32
> sccp-congested-msg-rcvd | Total number of messages received for congested SCCP function. This is a counter type of statistic. | Int32
> sccp-prohibit-msg-rcvd | Total number of SCCP-Prohibit messages received for SCCP function. This is a counter type of statistic. | Int32
> sccp-class-0-sent | Total number of SCCP class -0 (basic connectionless) messages sent by SCCP function. | Int32
> sccp-class-0-rcvd | Total number of SCCP class -0 (basic connectionless) messages received by SCCP function. | Int32
> sccp-class-1-sent | Total number of SCCP class -1 (sequenced connectionless) messages sent by SCCP function. | Int32
> sccp-class-1-rcvd | Total number of SCCP class -1 (sequenced connection) messages received by SCCP function. | Int32
> sccp-DT1-sent | Total number of SCCP DT -1 (data format - 1) messages sent by SCCP function. | Int32
> sccp-DT1-rcvd | Total number of SCCP DT -1 (data format - 1) messages received by SCCP function. | Int32
> sccp-rel-compl-supv-fail | Total number of SCCP function released due to failure in SCCP supervisor endpoint. | Int32
> sccp-rel-disconn-req-rx | Total number of SCCP function released due to disconnect request messages received by SCCP function. | Int32
> sccp-routing-fail-invalid-ins-routing-req | Total number of routing failed due to invalid instance information in routing request by SCCP function. | Int32
> sccp-routing-fail-invalid-isni-routing-req | Total number of routing failed due to invalid intermediate signaling network identification (ISNI) information in routing request by SCCP function. | Int32
> sccp-routing-fail-isni-constrained-routing | Total number of routing failed due to constraints by ISNI information in routing request by SCCP function. | Int32
> sccp-routing-fail-redundant-isni-routing-req | Total number of routing failed due to redundant ISNI information in routing request by SCCP function. | Int32
> sccp-routing-fail-isni-identify-network | Total number of times theSCCP routing failed due to missing ISNI network identification information. | Int32
> sccp-inactivity-rcv-tmr-expired | Total number of expired SCCP inactivity timer received. | Int32
> sccp-inactivity-test-sent | Total number of SCCP inactivity test messages sent. | Int32
> sccp-inactivity-test-received | Total number of SCCP inactivity test messages received. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883