> MSEG IMSI Profile Configuration Mode Commands
> The MSEG IMSI Profile Configuration Mode enables to configure International Mobile Subscriber Identifier (IMSI) ranges, which are level-1 filters, in MSEG IMSI profiles.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> imsi-range
> This command adds/removes IMSI ranges in an MSEG IMSI profile.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imsi-range mcc mobile_country_code mnc mobile_network_code msin start msin_start end msin_end
> no
> Deletes the specified IMSI range.
> mcc mobile_country_code
> Specifies the Mobile Country Code (MCC) of IMSI.
> mobile_country_code must be an integer from 100 through 999.
> Note that MCC values 000 through 099 are reserved codes.
> mnc mobile_network_code
> Specifies the Mobile Network Code (MNC) of IMSI.
> mobile_network_code must be an integer from 00 through 999.
> msin start msin_start end msin_end
> Specifies the Mobile Subscriber International Number (MSIN) range.
> msin start msin_start: Specifies start of the MSIN prefix range. msin_start must be an integer.
> end msin_end: Specifies end of the MSIN prefix range. msin_end must be an integer.
> Usage
> Use this command to add/remove IMSI ranges in an MSEG IMSI profile.
> Multiple, non-overlapping, IMSI ranges can be specified in each IMSI profile.
> Example
> The following command adds an IMSI range to the current IMSI profile with the MCC and MNC set to 111:
> imsi-range mcc 111 mnc 111 msin start 123 end 456

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883