> Exec Mode Show Commands (A-C)
> This section includes the commands show aaa through show css service.
> show aaa
> Use this command to view AAA (Authentication Authorization and Accounting) statistics for the current context.
> Product
> PDSN, GGSN, SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show aaa { group { all | name aaa_group_name } | local counters } [ | { grep grep_options | more } ]
> group { all | name aaa_group_name }
> Displays AAA information.

> • | all: If the exec context is local, information for all the default AAA groups, and the AAA groups configured in all the contexts are displayed. If the exec context is not local, information for only the context-specific AAA groups are displayed.

> • | name aaa_group_name: Displays information of the specified AAA group.

> aaa_group_name must be the name of an AAA group, and must be an alphanumeric string of 0 through 64 characters.
> local counters
> Displays information for current context.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command is used to view accounting and authentication statistics for the current context.
> Example
> The following command displays AAA statistics for the current context:
> show aaa local counters
> The following command displays AAA statistics for the AAA group aaa_group1:
> show aaa group name aaa_group1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging analyzer statistics
> This command displays statistic information for protocol analyzers.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging analyzer statistics [ name protocol [ verbose ] ] [ | { grep grep_options | more } ]
> name protocol
> Displays detailed information for the specified protocol analyzer.
> protocol must be an available analyzer name, and must be one of the following:

> • | dns

> • | file-transfer

> • | ftp

> • | http

> • | icmp

> • | icmpv6

> • | imap

> • | ip

> • | ipv6

> • | mms

> • | p2p

> • | pop3

> • | pptp

> • | rtcp

> • | rtp

> • | rtsp

> • | sdp

> • | secure-http

> • | sip

> • | smtp

> • | tcp

> • | tftp

> • | udp

> • | wsp

> • | wtp

> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output is the standard level which is the concise mode.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display statistic information for active charging protocol analyzers.
> Example
> The following command displays detailed statistic information for all P2P protocol analyzers:
> show active-charging analyzer statistics name p2p verbose
> The following command displays detailed statistic information for all TCP protocol analyzers:
> show active-charging analyzer statistics name tcp verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging bandwidth-policy
> This command displays information on bandwidth policies configured in a service.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging bandwidth-policy { all | name bandwidth_policy_name } [ | { grep grep_options | more } ]
> all
> Displays information for all bandwidth policies configured in the service.
> name bandwidth_policy_name
> Displays detailed information for the specified bandwidth policy.
> bandwidth_policy_name must be the name of a bandwidth policy, and must be an alphanumeric string of 1 through 63 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information on bandwidth policies configured in a service.
> Example
> The following command displays detailed information for the bandwidth policy named standard:
> show active-charging bandwidth-policy name standard
> show active-charging charging-action
> This command displays information for charging actions configured in the Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging charging-action { { { all | name charging_action_name } [ service name acs_service_name ] } | statistics [ name charging_action_name ] } [ | { grep grep_options | more } ]
> all
> Displays information for each configured charging action.
> name charging_action_name
> Displays detailed information for the specified charging action.
> charging_action_name must be the name of a charging action, and must be an alphanumeric string of 1 through 63 characters.
> statistics
> Displays statistical information for all configured charging actions.
> service name acs_service_name
> Displays information for all or a specific charging action in the specified ACS.
> acs_service_name must be the name of an ACS, and must be an alphanumeric string of 1 through 15 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for charging actions configured in a service.
> Example
> The following command displays a detailed information for all charging actions:
> show active-charging charging-action all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging content-filtering category policy-id
> This command displays Content Filtering category policy definitions. This command is not available on StarOS 8.0 and earlier.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging content-filtering category policy-id { all | id policy_id } [ | { grep grep_options | more } ]
> all
> Displays definitions of all Content Filtering category policies.
> id policy_id
> Displays definitions of a specific Content Filtering category policy.
> policy_id must be a CF policy ID, and must be an integer from 1 through 4294967295.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view Content Filtering category definitions for a specific/all Policy IDs.
> Example
> The following command displays Content Filtering category definitions for policy ID 3:
> show active-charging content-filtering category policy-id id 3
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging content-filtering category statistics
> This command displays category-based content filtering statistics.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging content-filtering category statistics [ rulebase { name rulebase_name | all } ] [ verbose ] [ | { grep grep_options | more } ]
> rulebase { name rulebase_name | all }
> Displays category-based content filtering statistics, either for all or for a specific rulebase.

> • | name rulebase_name: Specifies the rulebase.

> rulebase_name must be the name of an existing rulebase, and must be an alphanumeric string of 1 through 63 characters.

> • | all: Displays category-based content filtering statistics for each rulebase in the ACS.

> verbose
> Specifies that the output should provide as much information as possible. If this option is not specified then the output is the standard level, which is the concise mode.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view category-based content filtering statistics for a specific rulebase, or cumulative statistics for all rulebases in the ACS.
> Example
> The following command displays category-based content filtering statistics for the rulebase named consumer:
> show active-charging content-filtering category statistics rulebase name consumer
> The following command displays cumulative category-based content filtering statistics for all rulebases in verbose mode:
> show active-charging content-filtering category statistics verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging content-filtering server-group
> This command displays information for Content Filtering Server Group (CFSG) configured in the service.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging content-filtering server-group [ name cfsg_name | statistics [ name cfsg_name [ acsmgr instance instance [ priority priority ] ] | verbose ] [ | { grep grep_options | more } ]
> name cfsg_name
> Specifies name of the CFSG.
> cfsg_name must be the name of a CFSG, and must be an alphanumeric string of 1 through 63 characters.
> acsmgr instance instance
> Specifies the manager instance.
> instance must be an integer from 1 through 65535.
> priority priority
> Specifies priority of the server for which statistics has to be displayed.
> priority must be an integer from 1 through 65535.
> verbose
> Specifies that the output display all available statistics of each Internet Content Adaptation Protocol (ICAP) server connection at each instance. If this option is not specified then the output is at the standard level, which is the concise mode.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view CFSG information/statistics.
> show active-charging content-filtering server-group name cfsg_name: The output of this command displays detailed information for the specified CFSG.
> show active-charging content-filtering server-group statistics name cfsg_name: The output of this command displays cumulative statistics for the specified CFSG. This will include all the instances and all the servers configured in the CFSG.
> show active-charging content-filtering server-group statistics name cfsg_name acsmgr instance instance: The output of this command displays the cumulative statistics of all the ICAP server connections on the specified manager instance.
> show active-charging content-filtering server-group statistics name cfsg_name acsmgr instance instance priority priority: The output of this command displays the statistics for the specified ICAP server connection on the specified manager instance.
> show active-charging content-filtering server-group statistics verbose: The output of this command displays statistics of each ICAP server connection at each instance.
> Example
> The following command displays information for the CFSG named test12:
> show active-charging content-filtering server-group name test12
> The following command displays detailed information for all CFSGs:
> show active-charging content-filtering server-group statistics verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging credit-control
> This command displays statistics for Diameter/RADIUS Prepaid Credit Control Service in the Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging credit-control { statistics [ all | group group_name ] | session-states [ rulebase rulebase_name ] [ content-id content_id ] } [ | { grep grep_options | more } ]
> statistics [ all | group group_name ]
> Displays prepaid credit control statistics.

> • | all: Displays all available statistics.

> • | group group_name: Displays statistics for the specified credit control group.

> group_name must be the name of a credit control group, and must be an alphanumeric string of 1 through 63 characters.
> session-states [ rulebase rulebase_name ] [ content-id content_id ]
> Displays prepaid CCA session status based on rulebase and/or content ID.

> • | rulebase rulebase_name: Displays the Credit Control Application (CCA) session state counts for the specified rulebase.

> rulebase_name must be the name of a rulebase configured for credit control service, and must be an alphanumeric string of 1 through 63 characters.

> • | content-id content_id: Displays CCA session state counts for the specified content ID.

> content_id must be the content ID of a credit control service, and must be an integer from 1 through 65535.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view statistics for Diameter/RADIUS prepaid credit control service in the ACS.
> Example
> The following command shows ACS statistics of configured Diameter or RADIUS Credit Control Application:
> show active-charging credit-control statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging edr-format
> This command displays information about EDR formats configured in the Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging edr-format [ statistics ] [ all | name edr_format_name ] [ | { grep grep_options | more } ]
> all
> Displays information for all EDR formats.
> statistics
> Displays statistics for all or the specified EDR format.
> If neither all nor name is specified, summarized statistics over all EDR formats is displayed.
> name edr_format_name
> Displays information for the specified EDR format.
> edr_format_name must be the name of an existing EDR format, and must be an alphanumeric string of 1 through 63 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for EDR format(s) in the ACS.
> Example
> The following command displays all configured EDR formats in the ACS.
> show active-charging edr-format all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging edr-udr-file
> This command displays CDR flow control information. This command also displays the EDR and UDR file related information.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging edr-udr-file { flow-control-counters [ verbose ] | statistics } [ | { grep grep_options | more } ]
> flow-control-counters [ verbose ]
> Displays the counters for dropped EDR/UDR records. These counters are for when CDRMOD uses flow control to stop ACS/Session Managers from sending the records.
> verbose displays detailed information.
> statistics
> Displays EDR and UDR file statistics.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view CDR flow control information.
> Example
> The following command displays EDR and UDR files statistics:
> show active-charging edr-udr-file statistics
> The following command displays CDR flow control information:
> show active-charging edr-udr-file flow-control-counters
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging file-space-usage
> This command displays the file space used by CDR/EDR files.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging file-space-usage [ | { grep grep_options | more } ]
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view CDR/EDR file space usage information. The context in which this command is used is not relevant.
> show active-charging firewall statistics
> This command displays Active Charging Stateful Firewall statistics.
> Product
> FW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> acsmgr instance instance_id
> Specifies the ACS/Session Manager instance ID.
> instance_id must be an integer from 1 through 65535.
> callid call_id
> Specifies the call identification number.
> call_id must be an 8-digit hexadecimal number.
> domain-name domain_name
> Specifies the domain name.
> domain_name must be a string of 1 through 127 characters.
> nat-realm nat_realm
> Specifies the NAT realm name.
> nat_realm must be an alphanumeric string of 1 through 31 characters.
> protocol { icmp | ip | other | tcp | udp }
> Specifies the protocol:

> • | icmp: ICMPv4

> • | icmpv6

> • | ip: IPv4

> • | ipv6

> • | other: Protocols other than TCP, UDP, and ICMPv4/ICMPv6.

> • | tcp

> • | udp

> username user_name
> Specifies the user name.
> user_name must be a string of 1 through 127 characters.
> verbose
> Specifies that the output displays all available information. If this option is not specified then the output is the standard level, which is the concise mode.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view Stateful Firewall statistics. If you are in the local context, statistics for all contexts are displayed. Otherwise, only statistics of your current context are displayed.
> Example
> The following command displays Stateful Firewall statistics:
> show active-charging firewall statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging firewall track-list
> This command displays the list of servers being tracked for involvement in any Denial-of-Service (DOS) attacks.
> Product
> FW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging firewall track-list attacking-servers [ | { grep grep_options | more } ]
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view details of servers being tracked for involvement in any DOS attack.
> Example
> The following command displays the list of servers being tracked for involvement in any DOS attacks:
> show active-charging firewall track-list attacking-servers
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging flows
> This command displays information for active charging flows.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ pacing-bitrate [ < | > | = | greater-than | less-than | equal-to ] number [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> all
> Displays information for all active charging flows.
> connected-time [ < | > | greater-than | less-than ] seconds
> Displays information for flows filtered by connected time period.

> • | < seconds: Displays flows that have been connected less than the specified number of seconds.

> • | > seconds: Displays flows that have been connected more than the specified number of seconds.

> • | greater-than seconds: Displays flows that have been connected more than the specified number of seconds.

> • | less-than seconds: Displays flows that have been connected less than the specified number of seconds.

> seconds must be an integer from 0 through 4294967295.
> flow-id flow_id
> Displays information for specified active charging flow ID.
> full
> Displays all available information for the specified flows.
> idle-time [ < | > | greater-than | less-than ] seconds
> Displays information for flows filtered by idle time period.

> • | < seconds: Displays flows that have been idle less than the specified number of seconds.

> • | > seconds: Displays flows that have been idle more than the specified number of seconds.

> • | greater-than seconds: Displays flows that have been idle more than the specified number of seconds.

> • | less-than seconds: Displays flows that have been idle less than the specified number of seconds.

> seconds must be an integer from 0 through 4294967295.
> ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address
> Displays information for flows filtered by IPv4 IP address.

> • | server: Specifies the IP address for a specific server.

> • | subscriber: Specifies subscriber details for this ip-address. address is an IPv4 IP address in the x.x.x.x dotted-decimal format.

> • | < address: Specifies an IPv4 IP address that is lesser than address.

> • | > address: Specifies an IPv4 IP address that is greater than address.

> • | greater-than address: Specifies an IPv4 IP address that is greater than address.

> • | less-than address: Specifies an IPv4 IP address that is lesser than address.

> address must be an IPv4 address in decimal notation.
> nat { not-required | required [ nat-ip nat_ip_address [ nat-port nat_port ] ] }
> Important: The nat keyword and options are only available in StarOS 8.3 and later releases.
> Displays information for flows filtered by Network Address Translation (NAT) required or not required setting.

> • | not-required: Sessions with NAT processing not required.

> • | required: Sessions with NAT processing required.

> • | nat-ip nat_ip_address: Sessions using specified NAT IP address. nat_ip_address must be an IPv4 address in dotted-decimal format.

> • | nat-port nat_port: Sessions using specified NAT IP address and NAT port number. nat_port must be an integer from 0 through 65535.

> pacing-bitrate [ < | > | = | greater-than | less-than | equal-to ] number
> Displays information on video flows filtered by a specific video pacing bit rate. number can be an integer from 1 to 256000000.

> • | < number: Specifies a number that is less than the specified video pacing bit rate.

> • | > number: Specifies a number that is greater than the specified video pacing bit rate.

> • | = number: Specifies a number that is equal to the specified video pacing bit rate.

> • | greater-than number: Specifies a number that is greater than the specified video pacing bit rate.

> • | less-than number: Specifies a number that is less than the specified video pacing bit rate

> • | equal-to number: Specifies a number that is equal to the specified video pacing bit rate.

> port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number
> Displays information on flows filtered by port number.

> • | server: Specifies the port-number for a specific server.

> • | subscriber: Specifies subscriber details for this port-number. number must be an integer from 0 through 65535.

> • | < number: Specifies a port number that is less than the specified port-number.

> • | > number: Specifies a port number that is greater than the specified port-number.

> • | greater-than number: Specifies a port number that is greater than the specified port-number.

> • | less-than number: Specifies a port number that is less than the specified port-number.

> rx-bytes [ < | > | greater-than | less-than ] number
> Displays information on flows filtered by the number of bytes received in the flow.

> • | < number: Specifies the number of bytes that is less than the specified rx-bytes.

> • | > number: Specifies number of bytes that is greater than the specified rx-bytes.

> • | greater-than number: Specifies number of bytes that is greater than the specified rx-bytes.

> • | less-than number: Specifies number of bytes that is less than the specified rx-bytes.

> number must be an integer from 0 through 18446744073709551615.
> rx-packets [ < | > | greater-than | less-than ] number
> Displays information on flows filtered by the number of packets received in the flow.

> • | greater-than number: Specifies the number of packets that is greater than the specified rx-packets.

> • | less-than number: Specifies the number of packets that is less than the specified rx-packets.

> number must be an integer from 0 through 18446744073709551615.
> session-id session_id
> Displays detailed information for specific active charging session ID.
> summary
> Displays summary information for defined sessions, based on defined parameters.
> trans-proto { icmp | tcp | udp }
> Displays information on flows filtered by the transport protocol.

> • | icmp: ICMP protocol type flow

> • | tcp: TCP protocol type flow

> • | udp: User Datagram Protocol (UDP) flows

> tx-bytes [ < | > | greater-than | less-than ] number
> Displays information on flows filtered by the number of bytes received in the flow.

> • | < number: Specifies the number of bytes that is less than the specified tx-bytes.

> • | > number: Specifies number of bytes that is greater than the specified tx-bytes.

> • | greater-than number: Specifies number of bytes that is greater than the specified tx-bytes.

> • | less-than number: Specifies number of bytes that is less than the specified tx-bytes.

> number must be an integer from 0 through 18446744073709551615.
> tx-packets [ < | > | greater-than | less-than ] number
> Displays information on flows filtered by the number of packets received in the flow.

> • | greater-than number: Specifies the number of packets that is greater than the specified tx-packets.

> • | less-than number: Specifies the number of packets that is less than the specified tx-packets.

> number must be an integer from 0 through 18446744073709551615.
> type flow_type
> Displays information on flows filtered by flow type of application protocol.
> flow_type must be one of the following:

> • | dns

> • | ftp

> • | http

> • | icmp

> • | icmpv6

> • | imap

> • | ip

> • | ipv6

> • | mms

> • | p2p: P2P protocol type flows including one or more of the following applications:

> • | actsync

> • | aimini

> • | antsp2p

> • | applejuice

> • | ares

> • | armagettron

> • | battlefd

> • | bittorrent

> • | blackberry

> • | citrix

> • | clubpenguin

> • | crossfire

> • | ddlink

> • | directconnect

> • | dofus

> • | edonkey

> • | facebook

> • | facetime

> Important: The facetime protocol is available only in releases 9.0 and 11.0. This protocol is not available in release 10.0.

> • | fasttrack

> • | feidian

> • | fiesta

> • | filetopia

> • | florensia

> • | freenet

> • | fring

> • | funshion

> • | gadu_gadu

> • | gamekit

> Important: The gamekit protocol is available only in releases 9.0 and 11.0. This protocol is not available in release 10.0.

> • | gmail

> • | gnutella

> • | gtalk

> • | guildwars

> • | halflife2

> • | hamachivpn

> • | iax

> • | icecast

> • | imesh

> • | imo

> • | iptv

> • | irc

> • | isakmp

> • | iskoot

> • | itunes

> • | jabber

> • | kontiki

> • | manolito

> • | maplestory

> • | meebo

> • | mgcp

> • | msn

> • | mute

> • | myspace

> • | netmotion

> • | nimbuzz

> • | octoshape

> • | off

> • | ogg

> • | oovoo

> • | openft

> • | openvpn

> • | orb

> • | oscar

> • | paltalk

> • | pando

> • | pandora

> • | popo

> • | pplive

> • | ppstream

> • | ps3

> • | qq

> • | qqgame

> • | qqlive

> • | quake

> • | quicktime

> • | rdp

> • | rfactor

> • | rmstream

> • | scydo

> • | secondlife

> • | shoutcast

> • | skinny

> • | skype

> • | slingbox

> • | sopcast

> • | soulseek

> • | splashfighter

> • | spotify

> • | ssdp

> • | stealthnet

> • | steam

> • | stun

> • | tango

> • | teamspeak

> • | teamviewer

> • | thunder

> • | tor

> • | truphone

> • | tunnelvoice

> • | tvants

> • | tvuplayer

> • | twitter

> • | ultrabac

> • | usenet

> • | uusee

> • | veohtv

> • | viber

> • | vpnx

> • | vtun

> • | warcft3

> • | whatsapp

> • | wii

> • | winmx

> • | winny

> • | wmstream

> • | wofkungfu

> • | wofwarcraft

> • | xbox

> • | xdcc

> • | yahoo

> • | yourfreetunnel

> • | zattoo

> • | pop3

> • | pptp

> • | rtcp

> • | rtp

> • | rtsp

> • | secure-http

> • | sip

> • | smtp

> • | tcp

> • | tftp

> • | udp

> • | unknown: Unknown type of protocol type flow not listed here.

> • | wsp-connection-less

> • | wsp-connection-oriented

> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display charging flow type information.
> Example
> The following command displays a detailed flow information for a session ID of test:
> show active-charging flows session-id test
> The following command displays a detailed flow information for a P2P type session:
> show active-charging flows full type p2p
> The following command displays a detailed information for a P2P type flow:
> show active-charging flows type p2p
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging flow-mappings
> This command displays information about all the active flow mappings based on the applied filters.
> Product
> FW, NAT
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging flow-mappings [ all | call-id callid | [ nat { not-required | required [ nat-realm realm_name ] } | trans-proto { tcp | udp } ] + [ | { grep grep_options | more } ]
> all
> Displays the all the available active charging flow-mapping information.
> call-id callid
> Displays detailed information for specific calls.
> callid must be an 8 digit Hex number.
> nat { required [ nat-realm string ] not-required }
> Displays the active charging flow mappings for which NAT is enabled or disabled.
> trans-proto { tcp | udp }
> Displays the transport layer.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the Active Charging flow-mapping details.
> Example
> The following command displays the total number of Active Charging flow-mappings:
> show active-charging flow-mappings all
> The following command displays the the flow-mappings for which NAT is enabled and the NAT-realm used is natpool3:
> show active-charging flow-mappings nat required nat-realm natpool3
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging fw-and-nat policy
> This command displays Firewall-and-NAT Policy information.
> Important: This command is only available in StarOS 8.1, and in StarOS 9.0 and later. For more information on this command please contact your local service representative.
> Product
> ACS, FW, NAT
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy_name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> all
> Displays information for all Firewall-and-NAT policies configured, optionally all in a specified service.
> name fw_nat_policy_name
> Displays detailed information for the specified Firewall-and-NAT policy.
> fw_nat_policy_name must be the name of the Firewall-and-NAT policy, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays information for all or the specified Firewall-and-NAT policy in the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alphanumeric string of 1 through 15 characters.
> statistics
> Displays statistics for the all/specified Firewall-and-NAT policy.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view Firewall-and-NAT Policy information.
> Example
> The following command displays detailed information for the Firewall-and-NAT policy named standard:
> show active-charging fw-and-nat policy name standard
> show active-charging group-of-prefixed-urls
> This command displays information on group of prefixed URLs configured in an Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging group-of-prefixed-urls { all | name prefixed_url_group } [ service name acs_service_name ] [ | { grep grep_options | more } ]
> all
> Displays information for all group of prefixed URLs configured in an ACS.
> name prefixed_url_group
> Displays detailed information for the specified group of prefixed URLs.
> prefixed_url_group must be the name of a group of prefixed URLs, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays information for all or the specified group of prefixed URLs in the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alphanumeric string of 1 through 15 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter
> Usage
> Use this command to view information on group of prefixed URLs configured in the ACS.
> Example
> The following command displays for the group of prefixed URLs named test123:
> show active-charging group-of-prefixed-urls name test123
> show active-charging group-of-ruledefs
> This command displays information on group of ruledefs configured in an Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging group-of-ruledefs { { all | name group_of_ruledefs } [ service name acs_service_name ] | statistics name group_of_ruledefs } [ | { grep grep_options | more } ]
> all
> Displays information for all groups of ruledefs configured, optionally all in a specified ACS.
> name group_of_ruledefs
> Displays detailed information for the specified group of ruledefs.
> group_of_ruledefs must be the name of a group of ruledefs, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays information for all or the specified group of ruledefs within the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alphanumeric string of 1 through 15 characters.
> statistics name group_of_ruledefs
> Displays statistics for the specified group of ruledefs.
> group_of_ruledefs must be the name of a group of ruledefs, and must be an alphanumeric string of 1 through 63 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information on group of ruledefs configured in a ACS.
> Example
> The following command displays information on all groups of ruledefs configured:
> show active-charging group-of-ruledefs all
> show active-charging nat statistics
> This command displays Network Address Translation (NAT) realm statistics.
> Product
> NAT
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging nat statistics [ nat-realm nat_realm [ summary ] ] [ | { grep grep_options | more } ]
> show active-charging nat statistics
> This command when issued in the local context displays statistics for all NAT realms in all contexts. When issued in a specific context, this command displays statistics for all NAT realms in that context.
> show active-charging nat statistics nat-realm nat_realm
> This command when issued in the local context displays statistics for the specified NAT realm in all contexts. When issued in a specific context, this command displays statistics for the specified NAT realm in that context.
> nat-realm nat_realm
> Specifies the NAT realm’s / NAT realm group’s name.
> nat_realm must be an alphanumeric string of 1 through 31 characters.
> summary
> When the nat_realm specified is a “pool group” and the summary option is used, summary statistics of all pools in the pool group is displayed.
> When the nat_realm specified is a pool and the summary option is not used, all available statistics for the specified pool is displayed.
> When the nat_realm specified is a “pool group” and the summary option is not used, all available statistics of each pool in the specified “pool group” is displayed.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view NAT realm statistics.
> Example
> The following command when issued in the local context, displays NAT realm statistics for NAT realms named test135 in all contexts:
> show active-charging nat statistics nat-realm test135
> show active-charging packet-filter
> This command displays information on packet filters configured in an Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging packet-filter { all | name packet_filter_name } [ service name acs_service_name ] [ | { grep grep_options | more } ]
> all
> Displays information for all packet filters configured, optionally all configured in an ACS.
> name packet_filter_name
> Displays detailed information for the specified packet filter.
> packet_filter_name must be the name of a packet filter, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays information for all or the specified packet filter in the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alphanumeric string of 1 through 15 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information on packet filters configured in an ACS.
> Example
> The following command displays information for the packet filter filter12:
> show active-charging packet-filter name filter12
> show active-charging rulebase
> This command shows information for rulebases.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging rulebase { { { all | name rulebase_name } [ service name acs_service_name ] } | statistics [ name rulebase_name ] } | [ | { grep grep_options | more } ]
> all
> Displays details of all rulebases configured in the system.
> name rulebase_name
> Displays details of the specified rulebase.
> rulebase_name must be the name of a rulebase, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays details of all or the specified rulebase configured in the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alpha an/or numeric string of 1 through 15 characters.
> statistics
> Displays statistical information for all or the specified rulebase.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view various statistics for a specific charging rulebase.
> Example
> The following command displays active charging rulebase statistics.
> show active-charging rulebase statistics
> The following command displays configurations and statistics for a rulebase named rulebase_1.
> show active-charging rulebase name rulebase_1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging ruledef
> This command displays information for rule definitions (ruledefs) configured in the Active Charging Service (ACS).
> Product
> ACS, FW, TPO
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging ruledef { all | charging | firewall | name ruledef_name | post-processing | routing | statistics [ all { charging | firewall [ wide ] | post-processing | tpo } | name ruledef_name [ wide ] ] | tpo } [ | { grep grep_options | more } ]
> all
> Displays information for all ruledefs configured in the ACS.
> charging
> Displays information for all Charging ruledefs configured in the ACS.
> firewall
> Displays information for all Stateful Firewall ruledefs configured in the ACS.
> name ruledef_name
> Displays detailed information for the specified ruledef.
> ruledef_name must be the name of an existing ruledef, and must be an alphanumeric string of 1 through 63 characters.
> post-processing
> Important: This keyword is only available in StarOS 8.3 and later.
> Displays information for all post-processing ruledefs configured in the ACS.
> routing
> Displays information for all Routing ruledefs configured in the ACS.
> service service_name
> This keyword is obsolete.
> statistics [ all { charging | firewall [ wide ] | post-processing | tpo } | name ruledef_name [ wide ] ]
> Displays statistical information for all/specified ruledefs configured in the ACS. If none of the optional arguments are supplied, statistics totaled for all ruledefs will be displayed.

> • | all: Displays statistics for all ruledefs of the specified type configured in the ACS.

> • | charging: Displays statistics for all Charging ruledefs configured in the ACS.

> • | firewall: Displays statistics for all Firewall ruledefs configured in the service.

> • | post-processing: Displays statistics for all Post-processing ruledefs configured in the ACS.

> Important: The post-processing keyword is available only in StarOS 8.3 and later releases.

> • | tpo: Displays statistics for all Traffic Performance Optimization (TPO) ruledefs configured in the ACS.

> Important: The tpo keyword is available only in 12.2 and later releases.

> • | name ruledef_name: Displays statistics for the specified ruledef.

> ruledef_name must be the name of a ruledef, and must be an alphanumeric string of 1 through 63 characters.

> • | wide: Displays all available information in a single wide line.

> tpo
> Important: The tpo keyword is available only in 12.2 and later releases.
> Displays information for all Traffic Performance Optimization (TPO) ruledefs configured in the ACS.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information for ruledefs configured in the ACS.
> Example
> The following command displays ACS ruledef statistics.
> show active-charging ruledef statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging service
> This command displays detailed information about an Active Charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging service { all | name acs_service_name } [ | { grep grep_options | more } ]
> all
> Displays information for all configured ACSs.
> name acs_service_name
> Displays detailed information for the specified ACS.
> acs_service_name must be the name of an ACS, and must be an alphanumeric string of 1 through 15 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view ACS details.
> Example
> The following command displays details for the ACS named test1.
> show active-charging service name test1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging sessions
> This command displays statistics for Active Charging Service (ACS) sessions.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> full [ wide ]
> Displays all available information for the specified session.
> Optionally all available information can be displayed in a single wide line.
> summary
> Displays summary information for defined sessions based on defined parameters.
> display-dynamic-charging-rules
> Displays information for the dynamic charging rules configured per session under Gx interface support.
> dynamic-charging
> Displays information for dynamic charging sessions.
> filter_keyword
> The following keywords are filters that modify or filter the output of the Command Keywords. Not all filters are available for all command keywords. Multiple filter keywords can be entered on a command line.
> When multiple filter keywords are specified, the output conforms to all of the filter keywords specifications.
> For example, if you enter the following command:
> show active-charging sessions full active-charging-service acs_1
> Counters for active charging sessions active in ACS acs_1 with full details is displayed. Information for all other services is not displayed.
> acsmgr instance instance
> Displays session information for a specific ACS/Session Manager instance.
> active-charging-service acs_service_name
> Displays session information for the specified ACS.
> acs_service_name must be the name of an ACS, and must be an alphanumeric string of 1 through 15 characters.
> all
> Displays session information for all active charging sessions.
> callid
> Specifies the call identification number.
> display-dynamic-charging-rules
> Displays dynamic charging rules configured.
> dynamic-charging
> Displays session information for all dynamic charging sessions.
> firewall { not-required | required }
> Displays session information for sessions with Firewall Processing required or not required, as specified.
> fw-and-nat policy fw_nat_policy_name
> Displays information for the specified Firewall-and-NAT Policy.
> fw_nat_policy_name specifies name of the Firewall-and-NAT policy, and must be an alphanumeric string of 1 through 63 characters.
> imsi
> Specifies the International Mobile Subscriber Identity (IMSI) of the subscriber session.
> ip-address
> Specifies the IP address for the specific charging service.
> msid
> Displays active charging session information for a specific subscriber’s Mobile Station Identification (MSID) number.
> ipv4
> Displays active charging session information with IPv4 Firewall enabled/disabled.
> ipv6
> Displays active charging session information with IPv6 Firewall enabled/disabled.
> nat { not-required | required [ nat-realm nat_realm ] } [ ipv4 | ipv6 ]
> Displays session information for sessions with NAT required or not required, as specified.
> nat-realm nat_realm specifies the name of a NAT realm. nat_realm must be an alphanumeric string of 1 through 63 characters.
> ipv4: Displays active-charging sessions for which NAT44 processing is required.
> ipv6: Displays active-charging sessions for which NAT64 processing is required.
> rulebase
> Displays information for a rulebase that is configured in an active charging session.
> rx-data
> Displays the bytes received in the session.
> session-id
> Displays detailed session information for a specific session identification.
> tx-data
> Displays the bytes sent in the session.
> type
> Displays session information for specified DNS application type(s).

> • | dns

> • | ftp

> • | http

> • | icmp

> • | icmpv6

> • | imap

> • | ip

> • | ipv6

> • | mms

> • | p2p: Displays session information for a P2P application type:

> • | actsync

> • | aimini

> • | antsp2p

> • | applejuice

> • | ares

> • | armagettron

> • | battlefd

> • | bittorrent

> • | blackberry

> • | citrix

> • | clubpenguin

> • | crossfire

> • | ddlink

> • | directconnect

> • | dofus

> • | edonkey

> • | facebook

> • | facetime

> Important: The facetime protocol is available only in releases 9.0 and 11.0. This protocol is not available in release 10.0.

> • | fasttrack

> • | feidian

> • | fiesta

> • | filetopia

> • | florensia

> • | freenet

> • | fring

> • | funshion

> • | gadu_gadu

> • | gamekit

> Important: The gamekit protocol is available only in releases 9.0 and 11.0. This protocol is not available in release 10.0.

> • | gmail

> • | gnutella

> • | gtalk

> • | guildwars

> • | halflife2

> • | hamachivpn

> • | iax

> • | icecast

> • | imesh

> • | imo

> • | iptv

> • | irc

> • | isakmp

> • | iskoot

> • | itunes

> • | jabber

> • | kontiki

> • | manolito

> • | maplestory

> • | meebo

> • | mgcp

> • | msn

> • | mute

> • | myspace

> • | netmotion

> • | nimbuzz

> • | octoshape

> • | off

> • | ogg

> • | oovoo

> • | openft

> • | openvpn

> • | orb

> • | oscar

> • | paltalk

> • | pando

> • | pandora

> • | popo

> • | pplive

> • | ppstream

> • | ps3

> • | qq

> • | qqgame

> • | qqlive

> • | quake

> • | quicktime

> • | rdp

> • | rfactor

> • | rmstream

> • | scydo

> • | secondlife

> • | shoutcast

> • | skinny

> • | skype

> • | slingbox

> • | sopcast

> • | soulseek

> • | splashfighter

> • | spotify

> • | ssdp

> • | stealthnet

> • | steam

> • | stun

> • | tango

> • | teamspeak

> • | teamviewer

> • | thunder

> • | tor

> • | truphone

> • | tunnelvoice

> • | tvants

> • | tvuplayer

> • | twitter

> • | ultrabac

> • | usenet

> • | uusee

> • | veohtv

> • | viber

> • | vpnx

> • | vtun

> • | warcft3

> • | whatsapp

> • | wii

> • | winmx

> • | winny

> • | wmstream

> • | wofkungfu

> • | wofwarcraft

> • | xbox

> • | xdcc

> • | yahoo

> • | yourfreetunnel

> • | zattoo

> • | pop3

> • | pptp

> • | rtcp

> • | rtp

> • | rtsp

> • | secure-http

> • | sip

> • | smtp

> • | tcp

> • | tftp

> • | udp

> • | unknown

> • | wsp-connection-less

> • | wsp-connection-oriented

> username
> Displays session information for a specific user name.
> dynamic-charging
> Displays the all sessions having received at least one Gx message from Session Manager/IMS Authorization.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display the configuration information for an active charging session.
> Example
> The following command displays full information of an active charging session.
> show active-charging sessions full all
> The following command displays an active charging session summary.
> show active-charging sessions summary
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging subsystem
> This command shows service and configuration counters for the ACS.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> all
> Displays ACS subsystem information.
> facility acsmgr [ all | instance instance_value ]
> Displays logged events for all ACS/Session Managers or for a specific instance.
> instance_value must be an integer from 1 through 65535.
> rulebase name rulebase_name
> Displays rulebase statistics for the specified rulebase.
> rulebase_name must be the name of a rulebase, and must be an alphanumeric string of 1 through 63 characters.
> sip
> Displays SIP related statistics.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view ACS/Session Manager information.
> Example
> The following command displays ACS subsystem information:
> show active-charging subsystem all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging tcp-proxy statistics
> This command displays TCP Proxy statistics.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging tcp-proxy statistics [ all | ip-layer | proxy-fac | rulebase rulebase_name | socket-migration | tcp-layer ] [ verbose ] [ | { grep grep_options | more } ]
> all
> Displays all TCP Proxy statistics aggregated over all rulebases, including for both IP and TCP layers.
> ip-layer
> Displays TCP Proxy statistics for IP layer.
> proxy-fac
> Displays TCP Proxy Flow Admission Control statistics.
> rulebase rulebase_name
> Displays TCP Proxy statistics for the specified rulebase.
> rulebase_name must be the name of a rulebase, and must be an alphanumeric string of 1 through 63 characters.
> socket-migration
> Displays TCP Proxy statistics for socket migration.
> tcp-layer
> Displays TCP Proxy statistics for TCP layer.
> verbose
> Displays detailed TCP Proxy statistics.
> grep grep_options | more
> Specifies that the output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view TCP Proxy statistics.
> Example
> The following command displays detailed TCP proxy statistics for the rulebase named test14:
> show active-charging tcp-proxy statistics rulebase test14 verbose
> show active-charging timedef
> This command displays the details of timeslots configured in specified time definition(s).
> Important: This command is only available in StarOS 8.1 and in StarOS 9.0 and later.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging timedef { all | name timedef_name } [ service name acs_service_name ] [ | { grep grep_options | more } ]
> all
> Displays information for all timedefs configured in the service.
> name timedef_name
> Displays detailed information for the specified timedef.
> timedef_name must be the name of a timedef, and must be an alphanumeric string of 1 through 63 characters.
> service name acs_service_name
> Displays information for all or a specific timedef configured in the specified ACS.
> acs_service_name must be the name of the ACS, and must be an alphanumeric string of 1 through 15 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view details of timeslots configured in specified timedef(s) that have been configured for the Time-of-Day Activation/Deactivation of Rules feature.
> Example
> The following command displays timeslot details of all timedefs configured in the ACS:
> show active-charging timedef all
> show active-charging tpo policy statistics
> This command displays Traffic Performance Optimization (TPO) policy statistics.
> Product
> TPO
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging tpo policy statistics [ all | name tpo_policy_name ] [ | { grep grep_options | more } ]
> name tpo_policy_name
> Displays detailed statistics for the specified TPO policy.
> tpo_policy_name must be the name of an existing TPO policy, and must be an alphanumeric string of 1 through 63 characters.
> all
> Displays statistics for all TPO policies configured in the active charging service.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view TPO policy statistics.

> • | “show active-charging tpo policy statistics all” command displays statistics for each TPO policy configured in the active charging service.

> • | “show active-charging tpo policy statistics name tpo_policy_name” command displays statistics for the specified TPO policy.

> • | “show active-charging tpo policy statistics” command displays aggregated statistics for all TPO policies configured in the active charging service.

> Example
> The following command displays statistics for the TPO policy named policy12:
> show active-charging tpo policy statistics name policy12
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging tpo profile statistics
> This command displays Traffic Performance Optimization (TPO) profile statistics.
> Product
> TPO
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging tpo profile statistics [ name tpo_profile_name | all ] [ | { grep grep_options | more } ]
> name tpo_profile_name
> Displays detailed statistics for the specified TPO profile.
> tpo_profile_name must be the name of an existing TPO profile, and must be an alphanumeric string of 1 through 63 characters.
> all
> Displays statistics for all TPO profiles configured in the active charging service.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view TPO profile statistics.

> • | “show active-charging tpo profile statistics all” command displays statistics for each TPO profile configured in the active charging service.

> • | “show active-charging tpo profile statistics name tpo_profile_name” command displays statistics for the specified TPO profile.

> • | “show active-charging tpo profile statistics” command displays aggregated statistics for all TPO profiles configured in the active charging service.

> Example
> The following command displays statistics for the TPO profile named profile12:
> show active-charging tpo profile statistics name profile12
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging udr-format
> This command displays information about UDR formats configured in an Active charging Service (ACS).
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging udr-format { all | name udr_fromat_name } [ | { grep grep_options | more } ]
> all
> Displays information for all UDR formats.
> name udr_fromat_name
> Displays information for the specified UDR format.
> udr_format_name must be the name of an existing UDR format, and must be an alphanumeric string of 1 through 63 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for UDR format(s) in an ACS.
> Example
> The following command displays all configured UDR formats in an ACS.
> show active-charging udr-format all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging url-blacklisting statistics
> This command displays URL Blacklisting statistics.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging url-blacklisting statistics [ rulebase { all | name rulebase_name } ] [ verbose ] [ | { grep grep_options | more } ]
> rulebase { all | name rulebase_name }
> Displays URL Blacklisting statistics for all or a specific rulebase.

> • | all: Displays URL Blacklisting statistics for all configured rulebases.

> • | name rulebase_name: Displays URL Blacklisting statistics for the specified rulebase.

> rulebase_name must be the name of a rulebase, and must be an alphanumeric string of 1 through 63 characters.
> verbose
> Displays detailed URL Blacklisting statistics.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view URL Blacklisting hits and misses statistics.
> Example
> The following command displays cumulative URL Blacklisting statistics:
> show active-charging url-blacklisting statistics
> The following command displays URL Blacklisting statistics for the rulebase rulebase_1:
> show active-charging url-blacklisting statistics rulebase name rulebase_1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show active-charging video detailed-statistics
> This command displays detailed statistics for TCP video flows. The command options enable you to collect statistical data for video per UE device type, per radio access type, and per video container type.
> Product
> MVG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging video detailed-statistics [ container { flv | mp4 | others } | rat { cdma | gprs | hspa | lte | others | umts | wlan } | ue { android | ios | laptop | others } ]
> container { flv | mp4 | others }
> Displays detailed statistics for TCP video flows based on the specified container file format.
> rat { cdma | gprs | hspa | lte | others | umts | wlan }
> Displays detailed statistics for TCP video flows based on the specified radio access type.
> ue { android | ios | laptop | others }
> Displays detailed statistics for TCP video flows based on the specified UE device type.
> Usage
> Use this command to display detailed statistics about video usage. Use the command options to display detailed statistics based on the UE device type, radio access type, or container file format.
> Example
> The following command displays detailed statistics about video usage based on the UE device type ios:
> show active-charging video detailed-statistics ue ios
> show active-charging xheader-format
> This command displays x-header format configurations for an Active Charging Service (ACS).
> Important: This is a customer-specific command. Please contact your local sales representative for more information.
> Product
> ACS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show active-charging xheader-format { all | name xheader_format } [ | { grep grep_options | more } ]
> all
> Displays information for all x-header formats configured.
> name xheader_format
> Displays information for the specified x-header format.
> xheader_format must be the name of an x-header format, and must be an alphanumeric string of 1 through 63 characters.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view details of x-header formats configured in an ACS.
> Example
> The following command displays information for the x-header format named test12:
> show active-charging xheader-format test12
> show administrators
> Displays information regarding all CLI users currently connected to the system.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show administrators [ session id ] [ | { grep grep_options | more } ]
> session id
> Indicates the output is to contain additional information about the CLI user session including the assigned session ID.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command displays a list of administrative users that have command line interface sessions active.
> Example
> show administratorsshow administrators session id
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show alarm
> Displays alarm information.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show alarm { all | audible | central-office | facility | outstanding [ all | chassis | port slot/port | slot slot ] [ verbose ] | statistics } [ | { grep grep_options | more } ]
> all
> Displays the state of all alarms in one screen.
> audible
> Displays the state of the internal audible alarm buzzer on the SMC.
> central-office
> Displays the state of the CO Alarm relays on the SPIO.
> facility
> Displays the state of the facility (audible and CO) alarms.
> outstanding [ all | chassis | port slot/port | slot slot ] [ verbose ]
> Displays information on currently outstanding alarms.

> • | all: Displays all alarm information.

> • | chassis: Displays chassis/power/fan alarms.

> • | port slot/port: Shows the alarm information for the specified port.

> • | slot slot: Shows the alarm information for the card in the specified slot.

> • | verbose: Displays more verbose output, including the internal alarm ID

> statistics
> Displays basic statistics on the alarming subsystem, including the current number of outstanding alarms of different severities and a cumulative total of alarms generated.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command Output section of the Command Line Interface Overview chapter.
> Usage
> View alarms to verify system status or to periodically check the general health of the system.
> Important: This command is not supported on all platforms.
> Example
> The following command displays all alarms that are currently outstanding:
> show alarm outstanding all
> The following command displays more detailed information on all alarms that are currently outstanding:
> show alarm outstanding all verbose
> The following command displays alarm statistics:
> show alarm statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show alcap counters
> This command displays the Access Link Control Application Part (ALCAP) protocol message counters related to ALCAP protocol sessions associated with a Home-NodeB Gateway (HNB-GW) service instance configured and running on a system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show alcap counters [ alcap-service alcap_svc_name [ aal2-node aal2_node_name [ aal2-path aal2_path_id ] ] ] [ | { grep grep_options | more } ]
> name alcap_svc_name
> Sepecifies the name of the ALCAP service for which ALCAP protocol session counters are to be displayed.
> alcap_svc_name identifies the name of the ALCAP service.
> aal2-node aal2-node
> Specifies the name of the ATM Adaptation Layer 2 (AAL2) node for whichprotocol session counters will be filtered.
> aal2_node_name is name of the AAL2 node.
> aal2-path aal2_path_id
> Specifies the identity number of the AAL2 path on a specific ATM Adaptation Layer 2 (AAL2) node for which ALCAP protocol counters will be filtered.
> aal2_path_id is the identifier of the AAL2 path on AAL2 node.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> This command is used to display the sessions statistics and counters for ALCAP service.
> Example
> The following command displays the ALCAP protocol session counters for ALCAP service named as alcap_hnb_svc1:
> show alcap counters alcap-service alcap_hnb_svc1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show alcap-service
> This command displays the Access Link Control Application Part (ALCAP) session statistics of an ALCAP service associated with a Home-NodeB Gateway (HNB-GW) service instance configured and running on a system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show alcap-service { all | name alcap_svc_name [ aal2-node aal2_node_name [ aal2-path aal2_path_id [ aal2-channel aal2_channel_num] ] | endpoint aal2_endpoint_name ] } [ | { grep grep_options | more } ]
> name alcap_svc_name
> Specifies the name of the ALCAP service oor which service statistics are to be displayed.
> alcap_svc_name identifies the name of the ALCAP service.
> aal2-node aal2-node
> Specifies the name of the ATM Adaptation Layer 2 (AAL2) node that will be used to filter the display of the ALCAP service statistics.
> aal2_node_name is name of the AAL2 node configured in the ALCAP service.
> aal2-path aal2_path_id
> Specifies the identity number of the AAL2 path on a specific ATM Adaptation Layer 2 (AAL2) node that will be used to filter the display of the ALCAP service statistics.
> aal2_path_id is the identifier of the AAL2 path on the AAL2 node.
> aal2-channel aal2_channel_num
> Specifies the AAL2 channel number of the AAL2 path on a specific ATM Adaptation Layer 2 (AAL2) node that will be used to filter the display of the ALCAP service statistics.
> aal2_channel_num is the identifier of the AAL2 channel on the AAL2 path of the AAL2 node.
> endpoint atm_endpoint_name
> Specifies the ATM endpoint name that will be used to filter the display of the ALCAP service statistics for a specific ATM endpoint.
> aal2_endpoint_name is the name of the ATM endpoint.
> Usage
> This command is used to clear the sessions statistics and counters for ALCAP service.
> Example
> The following command displays the service statistics of ALCAP service named as alcap_hnb_svc1:
> show alcap-service name alcap_hnb_svc1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show alcap statistics
> This command displays the session statistics related to Access Link Control Application Part (ALCAP) protocol sessions associated with a Home-NodeB Gateway (HNB-GW) service instance configured and running on a system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show alcap statistics [ alcap-service alcap_svc_name [ aal2-node aal2_node_name [ aal2-path aal2_path_id ] ] ] [ verbose ] [ | { grep grep_options | more } ]
> name alcap_svc_name
> Specifies the name of the ALCAP service for which statistics are to be displayed.
> alcap_svc_name identifies the name of the ALCAP service.
> aal2-node aal2-node
> Seecifies the name of the ATM Adaptation Layer 2 (AAL2) node for which ALCAP service related statistics will be displayed.
> aal2_node_name is name of the AAL2 node.
> aal2-path aal2_path_id
> Specifies the identity number of the AAL2 path on a specific ATM Adaptation Layer 2 (AAL2) node for which ALCAP service statistics counters will be displayed.
> aal2_path_id is the identifier of the AAL2 path on AAL2 node.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> This command is used to display the sessions statistics and counters for ALCAP service.
> Example
> The following command displays the service session statistics counters for ALCAP service named as alcap_hnb_svc1:
> show alcap counters alcap-service alcap_hnb_svc1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show apn
> Displays configuration information for either a specific or all configured Access Point Names (APNs).
> Product
> GGSN, P-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show apn { all | name apn_name } [ | { grep grep_options | more } ]
> all
> Displays information on all APNs configured on the system.
> name apn_name
> Displays information for a specific APN.
> apn_name is the name of the APN and can be from 1 to 62 alphanumeric characters and is case sensitive.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more options, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command is used to verify the configuration of one or all APNs for monitoring or troubleshooting purposes. The output is a concise listing of APN parameter settings.
> If this command is executed from within the local context with the all keyword, information for all APNs configured on the system will be displayed.
> Example
> The following command displays configuration information for all APNs:
> show apn all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show apn counters ip-allocation
> This command displays the IP allocation method information/statistics counters on per Access Point name (APN) basis for all currently active calls.
> Product
> GGSN, P-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show apn counters ip-allocation [ all | name apn_name ] [ | { grep grep_options | more } ]
> all
> Displays statistics for all APNs.
> name apn_name
> Displays statistics for a specific APN.
> apn_name is the name of the preconfigured APN and can be from 1 to 63 alphanumeric characters and is case sensitive.
> { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command is used to display the IP allocation counters on per APN basis for all currently active calls. Output of this command gives the user clear idea of how many sessions in each APN are using a particular type of ip-allocation method.
> If this command is issued from within the local context, the statistics displayed will be cumulative for all APNs configured on the system regardless of context. If no APN name is specified and the command is executed from a context with multiple APNs configured, the output will be cumulative for all APNs in the context.
> Example
> The following command displays statistics for all APN on a system:
> show apn counter ip-allocation all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show apn statistics
> Displays statistics for either a specific Access Point Name (APN) or all configured APNs.
> Product
> GGSN, P-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show apn statistics [ all | name apn_name ] [ | { grep grep_options | more } ]
> all
> Displays statistics for all APNs.
> name apn_name
> Displays statistics for a specific APN.
> apn_name is the name of the APN and can be from 1 to 63 alphanumeric characters and is case sensitive.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command is used to view statistics for one or all APNs within a context for monitoring or troubleshooting purposes.
> If this command is issued from within the local context, the statistics displayed will be cumulative for all APNs configured on the system regardless of context. If no APN name is specified and the command is executed from a context with multiple APNs configured, the output will be cumulative for all APNs in the context.
> Example
> The following command displays statistics for an APN named isp2:
> show apn statistics name isp2
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show apn-profile
> Displays information for configured Access Point Name (APN) profiles.
> Product
> MME, SGSN
> Privilege
> Inspector
> Syntax
> show apn-profile { all | full { all | name apn_name } | name apn_name } [ | { grep grep_options | more } ]
> all
> Lists all APN profiles configured on the system.
> full { all | name apn_name }
> full: Instructs the system to display all information in the APN profile(s).
> all: Displays full set of information for all APN profiles configured on the system.
> name apn_name: Displays full set of information for a specific APN profile.
> apn_name: Must be an existing APN profile and be from 1 to 64 alphanumeric characters.
> name apn_name
> Displays information for a specific APN profile. apn_name must be an existing APN profile and be from 1 to 64 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for APN profiles configured on the system. APN profiles are configured through the global configuration mode and in the APN profile configuration mode. For more information regarding APN profile commands, refer to the APN Profile Configuration Mode Commands chapter.
> Example
> The following command displays all available information for an APN profile named apn-prof3:
> show apn-profile full name apn-prof3
> show aps
> Displays information for configured Automatic Protection Switching (APS) parameters.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show aps { all | card-stats slot_number [ clear ] | info slot_number/port_number | port-stats slot_number/port_number [ clear ] | port-status } [ | { grep grep_options | more } ]
> all
> Lists APS information for all cards configured with APS.
> card-stats slot_number [ clear ]
> Displays the APS statistics for the identified card. If the clear keyword is included with the command then the APS statistics for the specified card are cleared (reset to zero).
> slot_number: Must be an integer from 1 to 48 to identify the chassis slot holding the specified card.
> info slot_number/port_number
> Displays APS information for a specific port.
> slot_number/port_number: The first number must be an integer from 1 to 48 to identify the chassis slot holding the specified card. The slot number must be followed by a slash ‘/’, which must be followed immediately by the port number - an integer from 1 to 4 depending upon the type of card.
> port-stats slot_number/port_number [ clear ]
> Displays APS statistics for a specific port. If the clear keyword is included with the command then the APS statistics for the specified port are cleared (reset to zero).
> slot_number/port_number: The first number must be an integer from 1 to 48 to identify the chassis slot holding the specified card. The slot number must be followed by a slash ‘/’, which must be followed immediately by the port number - an integer from 1 to 4 depending upon the type of card.
> port-status slot_number/port_number
> Displays APS status information for a specific port.
> slot_number/port_number: The first number must be an integer from 1 to 48 to identify the chassis slot holding the specified card. The slot number must be followed by a slash ‘/’, which must be followed immediately by the port number - an integer from 1 to 4 depending upon the type of card.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display APS redundancy configuration, APS card and port status, and APS card and port statistics. APS is configured at the card level. For details on configuring APS, refer to the Card Configuration Mode Commands chapter in this reference.
> Important: APS is only relevant for the CLC2 and OLC2 line cards supporting SONET/SDH.
> Example
> The following command displays all available APS configuration information for a specific port 1 on the line card in slot 27:
> show aps info 27/1
> show apn-remap-table
> Displays information for Access point name (APN) remap tables configured on the system.
> Product
> MME, SGSN
> Privilege
> Inspector
> Syntax
> show apn-remap-table { all | full { all | name remap_table_name } | name remap_table_name } [ | { grep grep_options | more } ]
> all
> Lists all APN remap tables configured on the system.
> full { all | name remap_table_name }
> full: Displays a full set (all) of available information for the configured APN remap table(s).
> all: Displays the full set of available information for all APN remap tables configured on the system.
> name remap_table_name: Displays the full set of available information for a specific APN remap table configured on the system. remap_table_name: Must be an existing APN remap table and the name is comprised of 1 to 64 alphanumeric characters.
> name remap_table_name
> Displays information for a specific APN remap table. remap_table_name: Must be an existing APN remap table and the name must consist of 1 to 64 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for APN remap tables configured on the system. APN remap tables are configured through the global donfiguration mode and in the APN remap table configuration mode. For more information regarding APN remap table commands, refer to the APN Remap Table Configuration Mode Commands chapter.
> Example
> The following command displays all available information for an APN remap table named remap-table12:
> show apn-remap-table full name remap-table12
> show asngw-service
> This command displays information about selected Access Service Network Gateway (ASN-GW) calls/services.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service { all | name service_name | session | statistics } [ bs-status [ address ip_address | filter { all | icmp-monitored | no-calls | summary | up ] ] [ | { grep grep_options | more } ]
> all
> Displays information for all configured ASN-GW services.
> name service_name
> Displays information only for the specified ASN-GW service.
> service_name must be the name of an existing ASN-GW service in the current context. The service name must be an alphanumeric string of 1 through 63 characters.
> session
> Displays information about configured ASNGW sessions. See the show asngw-service session command
> statistics
> Total of collected information for specific protocol since the last restart or clear command.
> bs-status { address ip_address | filter { all | icmp-monitored | no-calls | summary | up } }
> Displays the ASN base station (BS) status based on IP address and various filters.
> address ip_address specifies the IP address of ASN base station whose status is requested. ip_address must be entered in IPv4 dotted-decimal or IPv6 colon-separated notation.
> filter { all | icmp-monitored | no-calls | summary | up }: Filters the requested BS’s status on the basis of following criteria:

> • | all: Displays the status of all ASN base stations.

> • | icmp-monitored: Displays the status of ASN base stations that are monitored through ICMP ping messages.

> • | no-calls: Displays the status of an ASN base station that has no active calls.

> • | summary: Displays a summary of the status of requested ASN base stations.

> • | up: Displays the of status of ASN base stations that are in active state.

> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information for selected configured ASN-GW services.
> Example
> The following command displays available information for all active ASN-GW services.
> show asngw-service all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asngw-service session
> This command displays statistics for specific Access Service Network Gateway (ASN-GW) sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service session [ all | anchor-only [ full ] | callid call_id | counters | full | ip-address ipv4_address | msid msid_number | non-anchor-only [ full ] | peer-address ipv4_address | summary | username user_name ] [ | { grep grep_options | more } ]
> all
> Displays all related information for all active ASN-GW service sessions.
> anchor-only
> Displays all available information for all active ASN-GW service sessions on an anchor ASN-GW only.
> callid call_id
> Displays available information for the specific call identification number.
> call_id must be an 8-digit hexadecimal number.
> full
> Displays all available information for the associated display or filter keyword.
> ip-address ipv4_address
> IP address of the subscriber.
> ipv4_address must be an IPv4 address, in dotted decimal notation.
> msid msid_number
> Displays available information for the specific mobile station identification number.
> msid_number must be an MSID number.
> non-anchor-only
> Displays all available information for all active ASN-GW service sessions on a non-anchor ASN-GW only.
> peer-address ipv4_address
> Address of specific IP peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> summary
> Displays summary of available information for associated display or filter keyword (previous keyword).
> username user_name
> Name of specific user within current context. Displays available information for the specific user name.
> user_name must be followed by an user name.
> The user name can an alphanumeric string of 1 through 127 characters.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view configuration information for an ASN-GW session.
> Example
> The following command displays all available ASN-GW sessions.
> show asngw-service session all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asngw-service session counters
> This command displays statistics for specific Access Service Network Gateway (ASN-GW) sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service session counters [ [ function-type { auth-relay | context-transfer | data-path | handoff | im-operation | ms-state-change | paging | qos } ] | [ anchor-only | callid call_id | ip-address ipv4_address | msid msid_number | non-anchor-only | peer-address ipv4_address | username user_name ] [ r4-only | r6-only | verbose ] ] [ | { grep grep_options | more } ]
> anchor-only
> Displays all available information for all active anchor sessions in an ASN-GW service.
> callid call_id
> Displays available information for the specific call identification number.
> call_id must be an 8-digit hexadecimal number.
> function-type { auth-relay | context-transfer | data-path | handoff | im-operation | ms-state-change | paging | qos }
> Displays the counters for specific type of functions in an ASN-GW session.
> auth-relay: Displays information about authentication relay messages.
> context-transfer: Displays information about context-transfer messages.
> data-path: Displays information about data-path registration messages.
> handoff: Displays information about hand-off messages.
> im-operations: Displays information about idle mode state operation messages.
> ms-state-change: Displays information about MS state change messages.
> paging: Displays information about paging messages.
> qos: Displays information about RR messages.
> ip-address ipv4_address
> IP address of the subscriber.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> msid msid_number
> Displays available information for the specific mobile station identification number.
> msid_number must be an MSID number.
> non-anchor-only
> Displays all available information for all active non-anchor sessions in an ASN-GW service.
> peer-address ipv4_address
> Address of specific IP peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> r6-only
> Displays all available counters for R6 interface in an ASN-GW session.
> r4-only
> Displays all available counters for R4 interface in an ASN-GW session.
> username user_name
> Displays available session information for the specific WiMAX user in ASN-GW service session.
> user_name must be followed by an user name.
> The user name can an alphanumeric string of 1 through 127 characters.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the counters of an ASN-GW session.
> Example
> The following command displays the counters for data path type function.
> show asngw-service session counters function-type data-path
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asngw-service statistics
> Displays statistics for all Access Service Network Gateway (ASN-GW) sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service statistics [ function-type { auth-relay | context-transfer | data-path | handoff | im-operations | ms-state-change | paging | qos | capability }] [ name < service_name > | r4-only | r6-only | verbose | peer-address < ipv4_address > ] [ peer-id < id > ][ verbose ] [ { grep < grep_options | more } ]
> function-type
> Displays information about selected function type on R4 or R6 interface.
> function-type { auth-relay | context-transfer | data-path | handoff | im-operations | ms-state-change | paging | qos | capability} [ r4-only | r6-only ]
> Displays the counters for specific type of functions in an ASN-GW session.
> auth-relay: Displays information about authentication relay messages.
> context-transfer: Displays information about context-transfer messages.
> data-path: Displays information about data-path registration messages.
> handoff: Displays information about hand-off messages.
> im-operations: Displays information about idle mode state operation messages.
> ms-state-change: Displays information about MS state change messages.
> paging: Displays information about paging messages.
> qos: Displays information about RR messages.
> capability: Displays the capability negotiation between the ASNGW and the base station.
> r4-only: Displays information about selected function on R4 interface.
> r6-only: Displays information about selected function on R6 interface.
> name service_name
> Displays specific service.
> service_name must be a service name.
> The service name can be one to 63 alphanumeric characters long.
> r4-only
> Displays statistics of R4 interface in ASN-GW services.
> r6-only
> Displays statistics of R6 interface in ASN-GW services.
> peer-address ipv4_address
> Address of specific IP Peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> peer-id < id >
> Display the statistics based on the 6-byte BSID or ASNGW ID in addition to the IPv4 address.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display ASN-GW statistics.
> Example
> The following command displays information about selected MS-State-Change function.
> show asngw-service statistics function-type ms-state-change
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service
> This command displays information about selected Access Service Network Paging Controller and Location Registry (ASN PC/LR) services.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asnpc-service { all | id | name service_name | session | statistics } [ | { grep grep_options | more } ]
> all
> Displays information for all configured ASN PC services.
> paging-group
> Displays all the configured paging-groups and associated paging nodes, and the offset count. For a specific paging group, enter the paging group id number.
> name service_name
> Displays information only for the specified ASN PC service.
> service_name must be the name of an existing ASN PC service in the current context. The service name must be an alphanumeric string of 1 through 63 characters.
> session
> Displays information about configured ASN PC sessions.
> statistics
> Total of collected information for specific protocol since last restart or clear command.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view information for selected configured ASN PC services.
> Example
> The following command displays available information for all active ASN PC services.
> show asnpc-service all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service session
> This command displays statistics for specific Access Service Network Paging Controller (ASN PC) service sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asnpc-service session [ all | callid call_id | counters | full | msid msid_number | peer-address ipv4_address | summary ] [ | { grep grep_options | more } ]
> all
> Displays all related information for all active ASN PC service sessions.
> callid call_id
> Displays available information for the specific call identification number.
> call_id must be an 8-digit hexadecimal number.
> full
> Displays all available information for the associated display or filter keyword.
> msid msid_number
> Displays available information for the specific mobile station identification number.
> msid_number must be an MSID number.
> peer-address ipv4_address
> Address of specific peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> summary
> Displays summary of available information for associated display or filter keyword (previous keyword).
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view configuration information for an ASN PC session.
> Example
> The following command displays all available ASN PC session counters in verbose mode.
> show asnpc-service session all
> The following command displays full ASN PC session counters in verbose mode.
> show asnpc-service session full
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service session counters
> This command displays session counters for Access Service Network Paging Controller (ASN PC) service sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service session counters [ all | callid call_id | msid msid_number | peer-address ipv4_address | verbose ] ] [ | { grep grep_options | more } ]
> all
> Displays all available counters for all ASN PC service sessions.
> callid call_id
> Displays available information for the specific call identification number.
> call_id must be an 8-digit hexadecimal number.
> msid msid_number
> Displays available information for the specific mobile station identification number.
> msid_number must be an MSID number.
> peer-address ipv4_address
> Address of specific IP peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the counters of an ASN PC session.
> Example
> The following command displays the counters for ASN PC service sessions in verbose mode.
> show asnpc-service session counters verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service session counters verbose
> This command displays session counters for Access Service Network Paging Controller (ASN PC) service sessions in complete detail.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asngw-service session counters verbose [ function-type { context-transfer | im-operations | ms-state-change | paging } ] [ all | callid call_id | msid msid_number | peer-address ipv4_address ] ] [ | { grep grep_options | more } ]
> all
> Displays all available counters for all ASN PC service sessions in verbose mode.
> callid call_id
> Displays available information for the specific call identification number in verbose mode.
> call_id must be an 8-digit hexadecimal number.
> function-type { context-transfer | im-operations | ms-state-change | paging }
> Displays the counters for specific type of functions in an ASN-GW session.
> context-transfer: Displays information about context-transfer messages.
> im-operations: Displays information about idle mode state operation messages.
> ms-state-change: Displays information about MS state change messages.
> paging: Displays information about paging messages.
> msid msid_number
> Displays available information for the specific mobile station identification number in verbose mode.
> msid_number must be an MSID number.
> peer-address ipv4_address
> Address of specific IP peer.
> ipv4_address must be an IPv4 address, in dotted decimal notation.
> r4-only
> Displays statistics of R4 interface in ASN PC services in verbose mode.
> r6-only
> Displays statistics of R6 interface in ASN PC services in verbose mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the counters of an ASN PC session in verbose mode.
> Example
> The following command displays the counters for data path type function.
> show asnpc-service session counters verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service statistics
> Displays statistics for all ASN PC service sessions.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asnpc-service statistics [ name service_name | peer-address ipv4_address | verbose ] [ r4-only | r6-only[ | { grep grep_options | more } ]
> name service_name
> Displays specific service.
> service_name must be a service name.
> The service name can be one to 63 alphanumeric characters long.
> peer-address ipv4_address
> Address of specific IP Peer.
> ipv4_address must be an IPv4 address in dotted-decimal notation.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display ASN PC statistics.
> Example
> The following command displays information about ASN PC service in verbose mode.
> show asnpc-service statistics verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show asnpc-service statistics verbose
> Displays statistics for all Access Service Network Paging Controller (ASN PC) service in verbose mode.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show asnpc-service statistics verbose [ function-type { context-transfer | im-operations | ms-state-change | paging } ] | all | r4-only | r6-only ] [ | { grep grep_options | more } ]
> function-type { context-transfer | ms-state-change | paging }
> Displays the statistics for specific type of functions in an ASN PC service in verbose mode.
> context-transfer: Displays information about context-transfer messages.
> im-operations: Displays information about idle mode state operation messages.
> ms-state-change: Displays information about MS state change messages.
> paging: Displays information about paging messages.
> all
> Displays statistics of all ASN PC services in verbose mode.
> r4-only
> Displays statistics of R4 interface in ASN PC services.
> r6-only
> Displays statistics of R6 interface in ASN PC services.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display ASN PC service statistics in verbose mode.
> Example
> The following command displays information about selected MS-State-Change function.
> show asnpc-service statistics verbose function-type ms-state-change
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show banner
> Displays the configured banner message for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show banner { all | charging-service | motd | lawful-intercept | pre-login } [ | { grep grep_options | more } ]
> all
> Displays all banners configured for a service in a system including enhanced charging service.
> charging-service
> Displays banner message configured for a enhanced charging service in current context.
> motd
> Display the banner message that is configured for the current context.
> lawful-intercept
> Refer to the Lawful Intercept Configuration Guide for a description of this command.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Show the configured banner to verify the message of the day contents for possible change
> Example
> show banner
> show bcmcs counters
> Displays Broadcast and Multicast Service (BCMCS)-specific counters and statistics.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show bcmcs counters { all | callid call_id | flow-id flow_id }
> all
> Displays BCMCS-specific counters and statistics for all multicast sessions.
> callid call_id
> Displays BCMCS-specific counters and statistics for a specific call ID.
> flow_id flow_id
> Displays BCMCS-specific counters and statistics for a specific BCMCS flow, defined by a flow ID.
> Usage
> Use this command to view BCMCS-specific statistics. You may narrow the results of the command output by specifying a specific call ID or flow ID.
> Example
> show bcmcs counters all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show bcmcs statistics
> Displays Broadcast and Multicast Service (BCMCS)-specific statistics for the current PDSN-service.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show bcmcs statistics [ pdsn-service service_name ]
> pdsn-service service_name
> Defines a specific PDSN service from which to gather BCMCS-specific statistics.
> Usage
> Shows several sets of BCMCS-specific statistics, and may be configured to show statistics only for a certain PDSN service.
> Example
> show bcmcs statistics pdsn-service service_name
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show boot
> Displays information on the current boot image in use.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show boot [ initial-config | { grep grep_options | more } ]
> initial-config
> Identifies the OS image, configuration file, and boot priority used during the initial start up of the system.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Show the boot information in preparing for maintenance activities by verifying current boot data. The boot image in use may not be the same as the boot image stored on the SMC due to upgrades and pending reboots. show boot initial-config displays the actual boot image and configuration file loaded during boot. This may or may not be the highest priority image and makes this command useful when comparing the loaded image to the priority list.
> Important: This command is not supported on all platforms.
> Example
> The following command displays the boot system configuration priority list:
> show boot
> The following command displays the initial configuration after a system boot:
> show boot initial-config
> show bssap+ statistics
> Displays Base Station system Application Part (BSSAP+) protocol statistics for the Gs interface between the SGSN and the Mobile services Switching Centre, Visitor Location Register (MSC/VLR).
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show bssap+ statistics [ gs-service gs_svc_name ] [ vlr { isdn-number ISDN_Num| name vlr_name } ] [ verbose ] [ | { grep grep_options | more } ]
> gs-service gs_svc_name
> Specifies the name of a specific Gs service to filter the BSSAP+ information.
> gs_svc_name is the name of a configured Gs service for which BSSAP+ is applied. The name can be from 1 to 63 alphanumeric characters and is case sensitive.
> vlr { isdn-number ISDN_Num| name vlr_name
> Identifies a specific VLR (by name or ISDN number) to filter BSSAP+ information.
> vlr_name is the configured name of the VLR. Enter a string of 1 to 63 alphanumeric characters to identify the VLR.
> VLR_num is the configured E.164-type ISDN number for the VLR. Enter a numerical string of 1 to 15 digits.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be limited to a concise summary.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display the BSSAP+ statistics for the SGSN’s Gs interface(s). Based on how the command is entered, this command displays collected BSSAP+ protocol statistics for the entire SGSN or for a specified Gs interface. Using the keywords of this command, the interface can be identified by defining a specific VLR connected to the SGSN or by identifying the Gs service to which the interface has been configured.
> Example
> The following command displays all BSSAP+ information for the Gs interface configured for the Gs service named gssvc1.
> show bssap+ statistics gs-service gssvc1 verbose
> Important: Descriptions for show command outputs are available in the Statistics and Counters Reference.
> show bssgp statistics
> Displays base station subsystem GPRS protocol statistics for traffic between the base station subsystem (BSS) and the SGSN over the Gb interface.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show bssgp statistics [ gprs-service gprs_svc_name | nse nse_id [ bvc bvc_id [ sessmgr | verbose ] ] ] [ verbose ] [ | { grep grep_options | more } ]
> gprs-service gprs_svc_name
> Specifies the name of a specific GPRS service for which the BSSGP information will be filtered.
> gprs_svc_name - Enter from 1 to 63 alphanumeric case-sensitive characters to identify the name of an already defined GPRS service.
> nse nse_ID
> Enter this keyword to display the BSSGP statistics for the identified network service entity (NSE).
> nse_ID - Enter an integer from 0 to 65535.
> bvc bvc_ID
> Enter this keyword to display the BSSGP statistics for the identified BSSGP virtual connection (BVC).
> bvc_ID - Enter an integer from 0 to 65000.
> sessmgr instance sessmgr_instance
> Enter this keyword to display the BSSGP statistics for a specific session manager.
> sessmgr_instance - Enter an integer from 1 to 4294967295.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display the BBSGP statistics for a particular GPRS service or NSEI.
> Example
> The following command displays BSSGP statistics for the GPRS service named gprs1.
> show bssgp statistics gprs-service gprs1
> Important: Descriptions for show command outputs are available in the Statistics and Counters Reference.
> show bssgp status
> Displays the traffic status through the BSSGP (base station subsystem GPRS protocol) layer between the base station subsystem (BSS) and the SGSN over the Gb interface.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show bssgp status { bvc-bucket nsei nse_id bvci bvc_id | bvc-stat nsei nse_id bvci bvc_id } [ | { grep grep_options | more } ]
> bvc-bucket nsei nse_id bvci bvc_id
> Displays traffic status for a specific BVC bucket identified by the NSEI (network service entity ID) and BVCI (BSSGP virtual connection ID).
> nse_ID - Enter an integer from 0 to 65535.
> bvc_ID - Enter an integer from 0 to 65000.
> bvc-stat nsei nse_id bvci bvc_id
> Displays traffic status for a specific BVC identified by the NSEI (network service entity ID) and BVCI (BSSGP virtual connection ID).
> nse_ID - Enter an integer from 0 to 65535.
> bvc_ID - Enter an integer from 0 to 65000.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display BVC status of the BBSGP layer for specified NSEI and BVCI.
> Example
> The following command displays BSSGP traffic status for the BVC bucket for NSEI 2556 BVCI 241 .
> show bssgp status bvc-bucket nsei 2556 bvci 35523
> Important: Descriptions for show command outputs are available in the Statistics and Counters Reference.
> show bulkstats
> Displays the information on bulk statistics.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show bulkstats [ [ data ] | [ schemas ] | [ variables [ schema_name ] [ obsolete ] ] [ | { grep grep_options | more } ] ]
> data
> Displays collected bulk statistical data.
> schema
> Displays the configuration of the statistics to be collected on a per-schema basis.
> Important: For information on available schemas, refer to the Bulk Statistics Configuration Mode Commands chapter.
> variables schema_name
> Displays all valid bulkstat schema statistics, or only the statistics for the specified schema.
> schema_name specifies the name of the schemas available on system. Following is the list of available schems in this release.

> • | aal2

> • | alcap

> • | apn

> • | asngw

> • | asnpc

> • | bcmcs

> • | card

> • | closedrp

> • | common

> • | context

> • | cs-network-ranap

> • | cs-network-rtp

> • | cscf

> • | cscfintf

> • | dcca

> • | diameter-acct

> • | diameter-auth

> • | diameter-acct

> • | dpca

> • | ecs

> • | egtpc

> • | epdg

> • | fa

> • | fng

> • | gprs

> • | gtpc

> • | gtpp

> • | gtpu

> • | ha

> • | hnbgw-hnbap

> • | hnbgw-ranap

> • | hnbgw-rtp

> • | hnbgw-rua

> • | hnbgw-sctp

> • | hsgw

> • | imsa

> • | ippool

> • | ipsg

> • | lac

> • | lma

> • | lns

> • | mag

> • | map

> • | mipv6ha

> • | mme

> • | mvs

> • | nat-realm

> • | pcc-af

> • | pcc-policy

> • | pcc-service

> • | pcc-sp-endpt

> • | pdg

> • | pdif

> • | pgw

> • | phsgw

> • | phspc

> • | port

> • | ppp

> • | ps-network-ranap

> • | radius

> • | rp

> • | sccp

> • | sgs

> • | sgsn

> • | sgtp

> • | sgw

> • | ss7link

> • | ss7rd

> • | system

> • | vpn

> obsolete
> This keyword shows the obsolete (but still available) schema variables. An asterisk (*) is displayed next to schema variables that have been obsoleted.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For information on usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command is used to display information on bulk statistics supported by the system.
> The variable keyword can be used to list statistics supported by the system either for all schemas, or for an individual schema.
> The schema keyword can be used to display the configuration of bulkstatistic settings including the schema.
> The data keyword can be used to display bulkstatistic data collected up to that point.
> Example
> The following command displays the bulk statistics data:
> show bulkstats data
> The following command displays the bulk statistics schema configuration:
> show bulkstats data schemas
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ca-certificate
> Displays information for Certificate Authority (CA) certificates on this system.
> Product
> All
> Privilege
> Inspector
> Syntax
> show ca-certificate { all | name name }
> all
> Displays CA certificate information for all CA certificates known to this system.
> name name
> Displays CA certificate information for a specific CA certificate name. name must be an existing CA certificate name and be from 1 to 128 alphanumeric characters.
> Usage
> View information for CA certificates on this system.
> Example
> The following command displays information for a CA certificate named cert-1:
> show ca-certificate name cert-1
> Important: Output descriptions for some commands are available in the Statistics and Counters Reference.
> show ca-crl
> Displays information for Certificate Authority (CA) Certificate Revocation List (CRL) on this system.
> Product
> All
> Privilege
> Inspector
> Syntax
> show ca-crl { all | name name }
> all
> Displays CA-CRL information for all CA-CRLs known to this system.
> name name
> Displays CA-CRL information for a specific CA-CRL name. name must be an existing CA-CRL name and be from 1 to 128 alphanumeric characters.
> Usage
> View information for CA-CRLs on this system.
> Example
> The following command displays information for a CA-CRL named crl-5:
> show ca-crl name crl-5
> Important: Output descriptions for some commands are available in the Statistics and Counters Reference.
> show cae-group server
> This command shows configuration information, including the name of the associated CAE group, for all CAEs or for a specific CAE. The CAE (Content Adaptation Engine) is an optional component of the Mobile Videoscape.
> Product
> MVG
> Privilege
> Security Administrator, Administrator
> Syntax
> show cae-group server { all | name cae_name }
> all
> Shows the configuration information, including the associated CAE group, for all CAEs.
> name cae_name
> Shows the configuration information for a specific CAE.
> Usage
> Use this command to display configuration information for all CAEs or for a specific CAE. This command can be issued from either the local context or the context in which the associated CAE group is defined.
> Example
> The following command displays configuration information for the CAE named server_1:
> show cae-group server name server_1
> show call-control-profile
> Displays information for call control profiles configured on the system.
> Product
> MME, SGSN
> Privilege
> Inspector
> Syntax
> show call-control-profile { all | full { all | name profile_name } | name profile_name } [ | { grep grep_options | more } ]
> all
> Lists all calll-control profiles configured on the system.
> full { all | name profile_name }
> full: Displays a full set (all) of available information in the call-control profile.
> all: Displays a full set of available information for all call-control profiles configured on the system.
> name profile_name: Displays a full set of available information for a specific call-control profile configured on the system. profile_name: Must be an existing call-control profile and the name must consist of 1 to 64 alphanumeric characters.
> name profile_name
> Displays information for a specific call-control profile. profile_name: Must be an existing call-control profile and the name must consist of 1 to 64 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for call-control profiles configured on the system. Call-control profiles are configured through the global configuration mode and in the call-control profile configuration mode. For more information regarding call-control profile commands, refer to the Call-Control Profile Configuration Mode Commands chapter in this reference.
> Example
> The following command displays all available information for a call-control profile named call-prof2:
> show call-control-profile full name call-prof2
> show call-home
> Displays information for call-home settings configured on the system.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> show call-home [ alert-group | detail | mail-server status | profile [ all | name profile_name ] | statistics [ | { grep grep_options | more } ] ]
> alert-group
> Displays information for the available alert group configured on the system. This also indicates if an alert-group is disabled by the user.
> detail
> Displays general information and alert-group settings for all configured call-home profiles.
> mail-server status
> Displays status information for call-home mail servers that are configured on the system.
> profile { all | name profile_name }
> Displays all available information for all call-home profiles on the system or a specified call-home profile.
> all: Displays all available information for all call-home profiles configured on the system.
> name profile_name: Displays all available information for a specific call-home profile configured on the system. profile_name must be an existing call-home profile and be from 1 to 31 alphanumeric characters.
> name profile_name
> Displays information for a specific call-home profile. profile_name must be an existing call-home profile and be from 1 to 31 alphanumeric characters.
> statistics
> Displays information for call-home statistics configured on the system.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display profile and notification policy information associated with the call-home profiles configured on the system. Call-home profiles are configured through the Context Configuration Mode and in the Call-home Configuration Mode. For more information regarding call-home commands, refer to the Call Control Profile Configuration Mode Commands chapter.
> Example
> The following command displays all available information for a call-home profile named call-home-prof1:
> show call-home profile name call-home-prof1
> show call-control-profile
> Displays information for call control profiles configured on the system.
> Product
> MME, SGSN
> Privilege
> Inspector
> Syntax
> show call-control-profile { all | full { all | name profile_name } | name profile_name } [ | { grep grep_options | more } ]
> all
> Lists all calll-control profiles configured on the system.
> full { all | name profile_name }
> full: Displays a full set (all) of available information in the call-control profile.
> all: Displays a full set of available information for all call-control profiles configured on the system.
> name profile_name: Displays a full set of available information for a specific call-control profile configured on the system. profile_name: Must be an existing call-control profile and the name must consist of 1 to 64 alphanumeric characters.
> name profile_name
> Displays information for a specific call-control profile. profile_name: Must be an existing call-control profile and the name must consist of 1 to 64 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for call-control profiles configured on the system. Call-control profiles are configured through the global configuration mode and in the call-control profile configuration mode. For more information regarding call-control profile commands, refer to the Call-Control Profile Configuration Mode Commands chapter in this reference.
> Example
> The following command displays all available information for a call-control profile named call-prof2:
> show call-control-profile full name call-prof2
> show camel-service
> Displays configuration details for Customised Applications for Mobile networks Enhanced Logic (CAMEL) services configured for this SGSN.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show camel-service { all | name service_name } [ | grep grep_options | more ]
> all
> Displays the configuration details for all configured CAMEL services.
> name
> Displays the configuration details for the identified CAMEL service.
> service_name: Enter a string of 1 to 63 alphanumeric characters to identify the CAMEL service.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View configuration information for CAMEL services.
> Example
> The following command displays the configuration information for a CAMEL service identified as camel4sgsnTO:
> show camel-service name camel4sgsnTO
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show certificate
> Displays information for local node certificates configured on this system.
> Product
> All
> Privilege
> Inspector
> Syntax
> show certificate { all | name name }
> all
> Displays certificate information for all node certificates configured on this system.
> name name
> Displays information for a specific certificate name. name must be an existing certificate name and be from 1 to 128 alphanumeric characters.
> Usage
> View information for local node certificates on this system.
> Example
> The following command displays information for a node certificate named certificate-3:
> show certificate name certificate-3
> Important: Output descriptions for some commands are available in the Statistics and Counters Reference.
> show cli
> Displays current command line interface (CLI) users and associated session information.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show cli { session | history } [ | { grep grep_options | more } ]
> session
> Displays information about the current CLI session.
> history
> Displays CLI command history for this CLI session.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Show current command line interface sessions when there is some unexpected output from a chassis and a check of current CLI users may reveal other activities in progress.
> Example
> show cli
> show clock
> Displays the current system data and time.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show clock [ universal ] [ | { grep grep_options | more } ]
> universal
> Displays the date and time in universal coordinated time (UTC/GMT).
> grep grep_options more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command Output section of the Command Line Interface Overview chapter.
> Usage
> Check the current time of a chassis to compare with network wide time or for logging purposes if network accounting and/or event records appear to have inconsistent timestamps.
> Important: This command is not supported on all platforms.
> Example
> The following displays the system time in local time and UTC, respectively.
> show clock
> show clock universal
> show configuration
> Displays current configuration information for the card, context, port, or target configuration file as specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show configuration [ card card_num | context name [ radius group [ all | name group ] ] | port slot/port | srp ] [ showsecrets ] [ url url ] [ verbose ] [ | { grep grep_options | more } ]
> card card_num | context name [ radius group [ all | name group ] ] | port slot/port
> Specifies the type of configuration information to be displayed.
> card card_num: specifies a specific card for which configuration information is to be displayed. card_num must be a value in the range 1 through 48.
> context name: specifies a specific context for which configuration information is to be displayed.
> radius group [ all | name group: specifies a specific or all RADIUS server group/s configured in a specific context for which configuration information is to be displayed.
> port slot/port: specifies a specific port for which configuration information is to be displayed.
> srp
> Shows the Service Redundancy Protocol configuration.
> showsecrets
> Show encrypted/unencrytpted secret keys saved in the configuration. If this keyword is not specified, secret keys are not displayed.
> url url
> Default: configuration which is currently in use.
> This keyword is not available to users with Operator level permissions. Specifies the location of the configuration data to use for information display. The url may refer to a local or a remote file. url must be entered using one of the following formats:
> Specifies the source of the copy. url may refer to a local or a remote file. url must be entered using one of the following formats:

> • | ASR 5000:

> • | [file: ]{ /flash | /pcmcia1 | /hd }[ /directory ]/file_name

> • | tftp://{ host[ :port# ] }[ /directory ]/file_name

> • | [ http: | ftp: | sftp: ]//[ username[ :password ]@ ] { host }[ :port# ][ /directory ]/file_name

> directory is the directory name.
> filename is the actual file of interest.
> Important: Configuration files should be named with a .cfg extension.
> username is the user to be authenticated.
> password is the password to use for authentication.
> host is the IP address or host name of the server.
> port# is the logical port number that the communication protocol is to use.
> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View the current configuration to review recent changes.
> Important: This command is not supported on all platforms.
> Example
> The following command displays the local in use port configuration information for port 24/1 in verbose mode.
> show configuration port 24/1 verbose
> The following command displays the card configuration for card 17 on host remoteABC stored in the configuration file in /pub/config.cfg.
> show configuration card 17
> The following command displays the configuration of all RADIUS server groups configured in context local
> show configuration context local radius group all
> The following command shows the configuration for a context named PDIF.
> show configuration context pdif
> show configuration errors
> Displays current configuration errors and warning information for the target configuration file as specified for a service.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show configuration errors [section {section_name} } [verbose] [ | {grep grep_options | more} ]
> section {section_name}
> Specifies the services and section to display and validate configuration.
> Following section_name services and sections are supproted:

> • | aaa-config: Displays configuration errors/warnings for the AAA service(s) configured on the system.

> • | active-charging: Displays configuration errors/warnings for the Enhanced Charging Service(s) and the Personal Stateful Firewall service(s) configured on the system.

> • | apn: Displays configuration errors/warnings for the APN configuration(s) on the system.

> • | apn-profile: Displays configuration errors/warnings for the APN Profile configuration(s) on the system.

> • | apn: Displays configuration errors/warnings for the APN Remap Table configuration(s) on the system.

> • | asngw-service: Displays configuration errors/warnings for the Access Service Network Gateway (ASN-GW) Service configured in a specific context for which configuration errors/warnings is to be displayed.

> • | asnpc-service: Displays configuration errors/warnings for the ASN Paging Controller and Location Registry (ASN PC-LR) Service(s) configured on the system.

> • | call-control-profile: Displays configuration errors/warnings for the Call Control Profile configuration(s) on the system.

> • | camel-service: Displays configuration errors/warnings for the CAMEL Service configuration(s) on the system.

> • | closed-rp-service: Displays configuration errors/warnings for the closed RP service(s) configured on the system.

> • | cs-network: Displays configuration errors/warnings for the CS Network configuration(s) on the system.

> • | cscf-service: Displays configuration errors/warnings for the Call Session Control Function (CSCF) service(s) configured on the system.

> • | diameter: Displays configuration errors/warnings for the Diameter configuration(s) on the system.

> • | dns-client: Displays configuration errors/warnings for the DNS Client configuration(s) on the system.

> • | egtp-service: Displays configuration errors/warnings for the eGTP Service configuration(s) on the system.

> • | fa-service: Displays configuration errors/warnings for the Foreign Agent (FA) service(s) configured on the system.

> • | fng-service: Displays configuration errors/warnings for the Femto Network Gateway (FNG) configuration(s) on the system.

> • | ggsn-service: Displays configuration errors/warnings for the GGSN service(s) configured on the system.

> • | gprs-service: Displays configuration errors/warnings for the GPRS service(s) configured on the system.

> • | gs-service: Displays configuration errors/warnings for the GS service(s) configured on the system.

> • | ha-service: Displays configuration errors/warnings for the Home Agent (HA) service(s) configured on the system.

> • | hnbgw-service: Displays configuration errors/warnings for the Home Evolved Node B Gateway (HNB-GW) Service configuration(s) on the system.

> • | hsgw-service: Displays configuration errors/warnings for the HRPD Serving Gateway (HSGW) service(s) configured on the system.

> • | imei-profile: Displays configuration errors/warnings for the International Mobile Equipment Identity (IMEI) Profile configuration(s) on the system.

> • | imsa-config: Displays configuration errors/warnings for the IMS Authorization (IMSA) configuration(s) on the system.

> • | imssh-service: Displays configuration errors/warnings for the IMS Sh (IMSSh) service(s) configured on the system.

> • | imsue-service: Displays configuration errors/warnings for the IMS UE service(s) configured on the system.

> • | ipms: Displays configuration errors/warnings for the Intelligent Packet Monitoring System (IPMS) service(s) configured on the system.

> • | ipsg-service: Displays configuration errors/warnings for the IP Security Gateway (IPSG) service(s) configured on the system.

> • | iups-service: Displays configuration errors/warnings for the IuPS service(s) configured on the system.

> • | lac-service: Displays configuration errors/warnings for the Layer 2 Tunneling Protocol (L2TP) Access Concentrator (LAC) service(s) configured on the system.

> • | lns-service: Displays configuration errors/warnings for the L2TP Network Server (LNS) service(s) configured on the system.

> • | local-policy: Displays configuration errors/warnings for the Local Policy configuration(s) on the system.

> • | map-service: Displays configuration errors/warnings for the SS7 Mobile Application Part (MAP) service(s) configured on the system.

> • | mme-service: Specifies the configuration errors for a Mobility Management Entity (MME) service configured in a specific context for which configuration errors/warnings are to be displayed.

> • | operator-policy: Displays configuration errors/warnings for the Operator Policy configuration(s) on the system.

> • | pcc-policy-service: Displays configuration errors/warnings for the Policy and Charging Control (PCC) Policy Service configuration(s) on the system.

> • | pcc-service: Displays configuration errors/warnings for the PCC Service configuration(s) on the system.

> • | pdg-service: Displays configuration errors/warnings for the Packet Data Gateway (PDG) Service configuration(s) on the system.

> • | pdif-service: Displays configuration errors/warnings for the Packet Data Interworking Function (PDIF) service(s) configured on the system.

> • | pdsn-service: Displays configuration errors/warnings for the PDSN service(s) configured on the system.

> • | pgw-service: Displays configuration errors/warnings for the P-GW Service configuration(s) on the system.

> • | phsgw-service: Displays configuration errors/warnings for the PHS Gateway service(s) configured on the system.

> • | policy-grp-config: Displays configuration errors/warnings for the Policy Group configuration(s) on the system.

> • | ps-network: Displays configuration errors/warnings for the PS Network configuration(s) on the system.

> • | sccp-network: Displays configuration errors/warnings for the SCCP network configuration(s) on the system.

> • | sgs-service: Displays configuration errors/warnings for the SGs Service configuration(s) on the system.

> • | sgsn-mode: Displays configuration errors/warnings for the SGSN Mode configuration(s) on the system.

> • | sgsn-service: Displays configuration errors/warnings for the SGSN service(s) configured on the system.

> • | sgtp-service: Displays configuration errors/warnings for the SGSN GPRS Tunneling Protocol (SGTP) service(s) configured on the system.

> • | sgw-service: Displays configuration errors/warnings for the S-GW Service configuration(s) on the system.

> • | subscriber-config: Displays configuration errors/warnings for the Subscriber configuration(s) on the system.

> • | subscriber-map: Displays configuration errors/warnings for the Subscriber Map configuration(s) on the system.

> verbose
> Indicates the output should provide as much information as possible. If this option is not specified then the output will be the standard level which is the concise mode.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For more information on the usage of grep and more, refer Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the current configuration errors and warning to review recent changes.
> Example
> The following command displays configuration errors and warnings for all services configured in a context/system:
> show configuration errors verbose | more
> The following command displays configuration errors and warnings for Enhanced Charging service and Personal Stateful Firewall service configured in a context:
> show configuration errors section active-charging verbose
> show congestion-control
> Displays information pertaining to congestion control functionality on the system
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show congestion-control {configuration | statistics {demux_mgr } [all | instance task_instance ] } [ | { grep grep_options | more } ]
> configuration
> Displays congestion control configuration information including threshold parameters and policy settings for the configured services.
> statistics
> Displays congestion control statistics for Demux managers demux_mgr.
> all: Select this keyword to display statistics based on the current state of all instances of the specified task.
> instance task_instance: Specifies that statistics are to be displayed for a specific software task instance. task_instance can be configured to any integer value from 1 to 128.
> Important: The inst column of the show task table command output can be used to determine the instance of a particular task.
> demux_mgr
> Specifies the name of the service/session Demux manager for which statistics are displayed. Following of the demux_mgr are supported:

> • | a11mgr: Specifies that statistics are displayed for PDSN services.

> • | asngwmgr: Specifies that statistics are displayed for ASN-GW services.

> • | asnpcmgr: Specifies that statistics are displayed for ASN PC-LR services.

> • | bindmux: Specifies that statistics are displayed for Bindmux Manager used by PCC service.

> • | egtpinmgr: Specifies that statistics are displayed for EGTP ingress demuxmgr.

> • | gtpcmgr: Specifies that statistics are displayed for GGSN services.

> • | hamgr: Specifies that statistics are displayed for HA services.

> • | hnbmgr: Specifies that statistics are displayed for HNB Manager used by HNB-GW service.

> • | imsimgr: Specifies that statistics are displayed for IMSI managers.

> • | ipsecmgr: Specifies that statistics are displayed for IPSec managers.

> • | l2tpmgr: Specifies that statistics are displayed for L2TP managers.

> all
> Displays the statistics based on the current state of all instances of the specified task.
> instance task_instance
> Specifies that statistics are to be displayed for a specific software task instance. task_instance can be configured to any integer value from 1 to 128.
> Important: The inst column of the show task table command output can be used to determine the instance of a particular task.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command displays congestion control configuration information or statistics for a particular service type.
> When the all keyword is used, the system compares the current state of all instances of the specified task. The state is based on whether or not any congestion control thresholds have been exceeded. If one or more instances are experiencing congestion, the state is displayed as “Applied”, and the various thresholds that have been crossed are indicated.
> Example
> The following command displays congestion control statistics for a PDSN service using an a11mgr task with an instance of 2:
> show congestion-control statistics a11mgr instance 2
> The following command displays congestion control statistics for an ASN-GW service using an asngwmgr task with an instance of 2:
> show congestion-control statistics asngwmgr instance 2
> The following command displays congestion control statistics for an ASN PC-LR service using an asnpcmgr task with an instance of 2:
> show congestion-control statistics asnpcmgr instance 2
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show content-filtering category database
> This command displays details of the specified category based content filtering database for content filtering application configured in a system/service.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show content-filtering category database [ active | all | facility srdbmgr { all | instance instance_value } | url url_string ] [ verbose ] [ | { grep grep_options | more } ]
> active
> Displays the information about all active databases, for example databases in memory.
> This is the default setting for category database information.
> all
> Displays the information about all active databases, for example, databases in memory and all saved databases on a system.
> facility
> Displays logged events for a specific facility.
> srdbmgr { all | instance instance_value }
> Displays logged events for all static rating database managers or for all or for a specific instance.

> • | all: Displays the logged events for all Static Rating Database (SRDB) Manager instances.

> • | instance instance_value: Displays events logged for a specific SRDB Manager instance. instance_value must be an integer from 1 through 8.

> url url_string
> Displays the information of the specific database located at the given URL.
> url_string specifies the name/location of category database to retrieve information, and must be an alphanumeric string of 1 through 512 characters.
> verbose
> This option enables the detailed mode for additional information display for specific database.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information of database for category based content filtering application in a service.
> Example
> The following command displays a detailed information for all active databases in memory.
> show content-filtering category database active all
> The following command displays the CF database status of all running SRDB managers.
> show content-filtering category database facility srdbmgr all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show content-filtering category policy-id
> This command displays Content Filtering category policy definitions.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show content-filtering category policy-id { all | id cf_policy_id } [ | { grep grep_options | more } ]
> all
> Displays definitions of all Content Filtering category policies.
> id cf_policy_id
> Displays definitions of a specific Content Filtering category policy.
> cf_policy_id must be a preconfigured category policy ID, and must be an integer from 1 through 4294967295.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view Content-Filtering Category definitions for a specific/all Policy IDs.
> Example
> The following command displays Content Filtering category definitions for policy ID 3:
> show content-filtering category policy-id id 3
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show content-filtering category statistics
> This command displays statistics for the category-based Content Filtering application configured in a system/service.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show content-filtering category statistics [ facility srdbmgr { all | instance instance_value } ] [ | { grep grep_options | more } ]
> facility
> Displays logged events for a specific facility.
> srdbmgr { all | instance instance_value }
> Displays logged events for all Static Rating Database (SRDB) Manager instances or for the specified instance.

> • | all: Displays events logged for all SRDB Manager instances.

> • | instance instance_value: Displays events logged for a specific SRDB Manager instance.

> instance_value must be an integer from 1 through 8.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to view the statistics of Category Based Content Filtering application in a service. This command’s output also indicates capability of the system to perform Content Filtering and Dynamic Content Filtering if configured.
> Important: Content filtering cannot be performed if less than two PSCs are activated. Dynamic Content Filtering cannot be performed if less than three PSCs are activated.
> Example
> The following command displays the detailed statistics of configured category based content filtering application:
> show content-filtering category statistics
> The following command displays the detailed statistics of configured category based content filtering application based on running SRDB Manager instance1.
> show content-filtering category statistics facility srdbmgr instance instance1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show content-filtering category url
> This command displays the information about the categories of the database at the specific URL configured for the category-based content filtering application in a system/service.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show content-filtering category url url_string [ policy-id cf_policy_id | rulebase rulebase_name ] [ verbose ] [ | { grep grep_options | more } ]
> url url_string
> Displays the category information of the specific URL.
> url_string specifies the URL, and must be an alphanumeric string of 1 through 512 characters.
> policy-id cf_policy_id
> Displays the category information of specific URL configured with specified content filtering category policy ID.
> cf_policy_id must be a category policy ID configured in the ACS Configuration Mode, and must be an integer from 0 through 65535.
> rulebase rulebase_name
> This option displays the category information of specific URL configured in ACS Configuration Mode for category-based content filtering in specific rulebase.
> rulebase_name must be the name of an existing rulebase and an alphanumeric string of 1 through 15 characters.
> verbose
> This option enables the detailed mode for additional information display for specific database.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information of a database URL for category based content filtering application in a service.
> Example
> The following command displays a detailed information for all active databases in memory.
> show content-filtering category url verbose /cf_server/cf/optcmd.bin verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show content-filtering server-group
> This command displays information for Content Filtering Server Group (CFSG) configured in the service.
> Product
> CF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show content-filtering server-group [ name cfsg_name | statistics ] | [ | { grep grep_options | more } ]
> name cfsg_name
> Displays information for the specified CFSG.
> cfsg_name must be the name of a CFSG and an alphanumeric string of 1 through 63 characters.
> statistics
> Displays statistical information for all configured CFSGs.
> grep grep_options | more
> Specifies that output of this command is to be piped (sent) to the command specified. A command to send the output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for Content Filtering Server Group configured in a service.
> Example
> The following command displays a detailed information for all charging actions:
> show content-filtering server-group statistics
> The following command displays a details of a specific charging action:
> show content-filtering server-group name test123
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show context
> Displays information for currently configured contexts.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show context [ all | name context_name ] [ | { grep grep_options | more } ]
> all | name context_name
> all: Display information for all currently configured contexts.
> name context_name: Display information for the context specified as context_name only.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View configured contexts. This may be useful in verifying configuration or troubleshooting the system.
> Example
> The following command displays information for the configured context named sampleContext:
> show context name sampleContext
> The following command displays information for all contexts:
> show context all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cpu
> Displays information on system CPUs.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show cpu { info [ card card_num [ cpu cpu_num ] ] [ graphs ] [ verbose ] | table } [ | { grep grep_options | more } ]
> info [ card card_num [ cpu cpu_num ] ] [ graphs ] [ verbose ]
> Specifies information for an entire card or a specific CPU is to be displayed.
> card card_num: Specifies the card to display associated information. card_num must be a value in the range 1 through 48 and must refer to an installed card.
> cpu cpu_num: Optionally selects a specific CPU on the card of interest to display specific information. cpu_num must be a value in the range 0 through 3 and must refer to an installed CPU.
> graphs: In addition to textual CPU information display CPU utilization information in graphs.
> verbose: Output is to display all information available.
> table
> Display, in tabular format, all cards and CPUs.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View CPU statistics to aid in diagnosing service problems for the case of overload conditions.
> Important: This command is not supported on all platforms.
> Example
> The following command displays the CPU information in tabular format for all CPUs on all installed cards:
> show cpu table
> The following command displays CPU information for card 8 in verbose mode:
> show cpu info card 8 verbose
> The following command displays information for CPU 0 on card 1:
> show cpu info card 1 cpu 0
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crash
> Displays summary of system/task crashes or information on a specific crash.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crash { list | number crash_num } [ | { grep grep_options | more } ]
> list | number crash_num
> list: Indicates a list of recent crash data is to be displayed.
> number crash_num: Indicates the information for the crash specified by crash_num is to be displayed. The crash number must be an existing crash which would be displayed using the list keyword.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> VIew the crash list to determine frequency of crashes or if crashes occur at some specific time of day. This may also be used to view information on a specific crash to aid in troubleshooting.
> Example
> The following displays the list of recent crashes.
> show crash list
> The following command will display the crash information for crash number 11.
> show crash number 11
> show credit-control sessions
> This command displays credit control sessions information.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show credit-control session [ all | callid | full | mdn | nai | summary ] [ | { grep grep_options | more } ]
> session [ all | callid | full | mdn | nai | summary ]
> Displays the credit control session status based on the following keywords:
> all: Displays all available information for Credit Control sessions
> callid: Displays the Credit Control Session Call ID
> full: Displays All available information for the associated display or the filter keyword
> mdn: Displays the Credit Control MDN
> nai: Displays the Credit Control NI
> summary: Displays the summary of Credit Control session information
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to show active credit control application for service sessions.
> Example
> The following command shows the configured Credit Control application sessions:
> show credit-control sessions
> show credit-control statistics
> This command displays credit control statistics.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show credit-control statistics cc-service name
> cc-service
> Specifies the Credit Control Service name.
> name must be an existing Credit Control Service and an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to show active credit control statistics.
> Example
> The following command shows the configured credit control statistics for a service named service1:
> show credit-control statistics cc-service service1
> show crypto group
> Displays information pertaining to configured crypto groups.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto group [ name group_name | summary ]
> name group_name
> Displays information for a specific crypto group.
> group_name is the name of the group for which to display information.
> summary
> Displays state and statistical information for configured crypto groups in this context.
> Usage
> Use this command to display information and statistics pertaining to one or all configured crypto groups within the current context.
> If the summary keyword is not used, detailed information is displayed.
> The following command displays detailed information for a crypto group called group1:
> show crypto group name group1
> show crypto ikev1
> Displays pre-shared key information for peer security gateways configured within the context.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto ikev1 { keys | policy [ preference ] | security-associations [ summary ] }
> keys
> Specifies the IKE pre-shared key information based on the peer security gateway.
> policy [ preference ]
> Specifies the Internet Exchange Key (IKE) policy priority for which configuration information will be displayed.
> The priority can be configured to any integer value from 1 to 100.
> If no preference is specified, information will be displayed for all configured policies.
> security-associations [ summary ]
> Specifies that established IPSec SA information should be displayed.
> Usage
> Use this command to:

> • | Display pre-shared key information. This information can be used to verify configuration and/or for troubleshooting.

> • | Verify the configuration of IKE policies within the context.

> • | Display established IPSec SA information. This information can be used for troubleshooting.

> Example
> The following command lists the pre-shared keys received from peer security gateways as part of the Diffie-Hellman exchange:
> show crypto ikev1 keys
> The following command displays information for an IKE policy with a preference of 1:
> show crypto ikev1 policy 1
> The following command displays the currently established SAs:
> show crypto ikev1 security-associations summary
> show crypto ikev2-ikesa security-associations summary
> Summary view of Internet Key Exchange v2 (IKEv2) IKE Security Associations (IKE SAs).
> Product
> PDIF
> Privilege
> Administrator, Security Administrator
> Syntax
> show crypto ikev2-ikesa security-associations summary
> Usage
> Shows a summary of the of the SAs configured for a crypto template. It shows the total configured SA lifetime in seconds and the number of seconds left on the timer.
> Example
> Use this command to create the SA summary:
> show crypto ikev2-ikesa security-associations summary
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto ikev2-ikesa transform-set
> Displays IKEv2/IKESA (Internet Key Exchange v2/IKE Security Association) transform set configuration information.
> Product
> All using IKEv2/IPSec
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto ikev2-ikesa transform-set transform_set_name
> show crypto ikev2-ikesa transform-set
> Specifies the name of a particular IKEv2/IKSA transform set for which to display information.
> transform_set_name is the name of the IKEv2/IKESA transform set, which can be 1 to 127 alpha-numeric characters and is case sensitive.
> Usage
> Use this command to verify the configuration of IKEv2/IKESA transform sets within the context.
> If no keyword is specified, information will be displayed for all IKEv2/IKESA transform sets configured within the context.
> Example
> The following command displays information for an IKEv2/IKESA transform set named test1:
> show crypto ikev2-ikesa transform-set test1
> show crypto ipsec
> Displays IPSec security associations (SAs) configured within or facilitated by the context and can optionally display statistics for them.
> Product
> PDSN, GGSN, PDIF, SCM
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto ipsec security-associations map-type { ipsec-3gpp-cscf-subscriber | ipsec-dynamic | ipsec-ikev1 | ipsec-l2tp | ipsec-manual | ipsec-mobile-ip } | summary [ distribution | ipsecmgr ipsec_mgr_id | map-type map_type ] | tag map_name
> map-type { ipsec-dynamic | ipsec-ikev1 | ipsec-l2tp | ipsec-manual | ipsec-mobile-ip }
> Specifies that information for all crypto maps of a specific type configured within the context will be displayed. The following types can be specified:

> • | ipsec-3gpp-cscf-subscriber: P-CSCF Subscriber IPSec Tunnel

> • | ipsec-dynamic: Dynamic IPSec Tunnel

> • | ipsec-ikev1: IKEv1 IPSec Tunnel

> • | ipsec-ikev2-subscriber: IKEv2 Subscriber Tunnel

> • | ipsec-l2tp: L2TP IPSec Tunnel

> • | ipsec-manual: Manual (Static) IPSec Tunnel

> • | ipsec-mobile-ip: Mobile IP IPSec Tunnel

> summary [ distribution | ipsecmgr ipsec_mgr_id | map-type map_type | template-map map_name ]
> Specifies that only security association summary information should be displayed.
> distribution: Show IPSec Manager SA distribution information.
> ipsecmgr ipsec_mgr_id: Show summary SA information for the specified IPSec manager instance ID. Must be an integer from 1 through 200.
> map-type map_type: Show summary SA information for the specified type of crypto map.The following types can be specified:

> • | ipsec-3gpp-cscf-subscriber: P-CSCF Subscriber IPSec Tunnel

> • | ipsec-dynamic: Dynamic IPSec Tunnel

> • | ipsec-ikev1: IKEv1 IPSec Tunnel

> • | ipsec-l2tp: L2TP IPSec Tunnel

> • | ipsec-manual: Manual (Static) IPSec Tunnel

> • | ipsec-mobile-ip: Mobile IP IPSec Tunnel

> tag map_name
> Specifies that SAs should be displayed for the specified crypto map.
> map_name is the name of the crypto map configured in the context and can be from 1 to 127 alphanumeric characters and is case sensitive.
> Usage
> Use this command to display IPSec SA information and statistics. This information can be used for performance monitoring and/or troubleshooting.
> The displayed information categorizes control signal and data statistics. Data statistics are further categorized according to the encapsulation method, either GRE or IP-in-IP.
> Example
> The following command displays summary SA statistics for all IPSec managers.
> show crypto ipsec security-associations summary
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto ipsec transform-set
> Displays IPSec transform set configuration information.
> Product
> PDG/TTG, PDIF
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto ipsec transform-set [ transform_name ]
> transform_name
> Specifies the name of a particular IPsec transform set for which to display information.
> transform_name is the name of the IPsec transform set and can be from 1 to 127 alphanumeric characters and is case sensitive.
> Usage
> Use this command to verify the configuration of IPsec transform sets within the context.
> If no keyword is specified, information will be displayed for all IPsec transform sets configured within the context.
> Important: This command is used in PDIF Release 8.3 only.
> Example
> The following command displays information for an IPsec transform set named test1:
> show crypto ipsec transform-set test1
> show crypto isakmp keys
> Displays pre-shared key information (Internet Security Association and Key Management Protocol, ISAKMP) for peer security gateways configured within the context.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto isakmp keys
> Usage
> Use this command to display pre-shared key information based on the peer security gateway. This information can be used to verify configuration and/or for troubleshooting.
> Example
> The following command lists the pre-shared keys received from peer security gateways as part of the Diffie-Hellman exchange:
> show crypto isakmp keys
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto isakmp policy
> Displays Internet Security Association and Key Management Protocol (ISAKMP) policy configuration information.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto isakmp policy [ preference ]
> preference
> Specifies the ISAKMP policy priority for which configuration information will be displayed.
> The priority can be configured to any integer value from 1 to 100.
> Usage
> Use this command to verify the configuration of ISAKMP policies within the context.
> If no preference is specified, information will be displayed for all configured policies.
> Example
> The following command displays information for an ISAKMP policy with a preference of 1:
> show crypto isakmp policy 1
> show crypto isakmp security-associations
> Displays currently established Internet key Exchange (IKE) security associations (SAs) facilitated by the context.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto isakmp security-associations [ cookies ]
> cookies
> Specifies that cookies should be displayed.
> Usage
> Use this command to display established IPSec SA information. This information can be used for troubleshooting.
> Example
> The following command displays the currently established SAs:
> show crypto isakmp security-associations
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto managers
> Shows statistics per IPSec Manager.
> Product
> PDSN, GGSN, PDIF, SCM
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto managers [ context context_id | crypto-map map_name | instance instance_num | summary [ distribution | ike-stats | ipsec-3gpp-cscf-stats | ikev2-stats [ demux-stats ] | ipsec-sa-stats | npu-stats ] ]
> context context_id
> Show IPSec manager statistics for the context with the specified context identifier number.
> must be an integer from 1 through 64.
> crypto-map map_name
> Show IPSec Managers for a specific crypto map.
> map_name must be the name of an existing crypto map.
> instance instance_num
> Show statistics for the specified IPSec manager instance.
> instance_num must be an integer from 1 through 284.
> summary [ distribution | ike-stats | ipsec-3gpp-cscf-stats | ikev2-stats [ demux-stats ] | ipsec-sa-stats | npu-stats ]
> Shows stats per service IP address for each manager.
> distribution: Shows a summary list of IPsec manager distribution.
> ike-stats: Shows a summary list of IPSec IKE statistics. for each IPsec manager.
> ipsec-3gpp-cscf-stats - Displays CSCF IPSec Statistics on each IPsec Manager.
> ikev2-stats: Displays IKEv2 Statistics on each IPsec Manager.

> • | demux-stats: Displays session demux statistics on each IPsec Manager.

> ipsec-sa-stats: Shows a summary list of IPsec Security Association statistics for each IPsec Manager.
> npu-stats: Displays NPU statistics on each IPsec Manager.
> Usage
> Use this command to view statistics relating to IPSec managers.
> Example
> The following command displays summary information for all IPSec managers:
> show crypto managers summary
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto map
> Displays crypto map configuration information.
> Product
> PDIF, PDSN, GGSN, SCM
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto map [ map-type [ ipsec-3gpp-cscf-subscriber | ipsec-dynamic | ipsec-ikev1 | ipsec-ikev2-subscriber | ipsec-l2tp | ipsec-manual | ipsec-mobile-ip ] | tag map_name | summary ]
> map-type [ ipsec-3gpp-cscf-subscriber | ipsec-dynamic | ipsec-ikev1 | ipsec-ikev2-subscriber | ipsec-l2tp | ipsec-manual | ipsec-mobile-ip ]
> Specifies that information for all crypto maps of a specific type configured within the context will be displayed. The following types can be specified:

> • | ipsec-3gpp-cscf-subscriber: P-CSCF subscriber IPSec Tunnel

> • | ipsec-dynamic: Dynamic IPSec Tunnel

> • | ipsec-ikev1: IKEv1 IPSec Tunnel

> • | ipsec-ikev2-subscriber: IKEv2 Subscriber Tunnel

> • | ipsec-l2tp: L2TP IPSec Tunnel

> • | ipsec-manual: Manual (Static) IPSec Tunnel

> • | ipsec-mobile-ip: Mobile IP IPSec Tunnel

> tag map_name
> Specifies the name of a crypto map for which to display configuration information.
> map_name is the name of the crypto map configured in the context and can be from 1 to 127 alphanumeric characters and is case sensitive.
> summary
> Displays summary information for all crypto maps configured in the context.
> Usage
> Use this command to verify the configuration of crypto maps within the context.
> If no keyword is specified, information will be displayed for all maps configured within the context regardless of type.
> Example
> The following command displays configuration information for a dynamic crypto map named test_map3:
> show crypto map tag test_map3
> show crypto statistics
> Displays Internet Protocol Security (IPSec) statistics.
> Product
> PDSN, GGSN, PDG/TTG, PDIF, SCM
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto statistics ikev1 | ikev2 [ service-ip-address ip-address ] [ service-name name ] | ipsec-3gpp-cscf [ service-ip-address ip-address ] [ service-name name ]| srtp [ service-ip-address ip-address ] [ service-name name ]
> ikev1
> Displays global ikev1 statistics for this context.
> ikev2 [ service-ip-address ip-address ] [ service-name name ]
> Displays global ikev2 statistics for this context.
> service-ip-address ip-address: Packet Data Interworking Function (PDIF) service IP address entered in IPv4 dotted-decimal or IPv6 colon-separated notation.
> service-name name: Specified PDIF service name.
> ipsec-3gpp-cscf [ service-ip-address ip-address ] [ service-name name ]
> Displays global CSCF IPSec SA statistics for this context.
> service-ip-address ip-address: CSCF service IP address entered in IPv4 dotted-decimal or IPv6 colon-separated notation.
> service-name name: Specified CSCF service name.
> srtp [ service-ip-address ip-address ] [ service-name name ]
> Displays global SRTP (Secure Real-time Transport Protocol) statistics for this context.
> service-ip-address ip-address: CSCF service IP address entered in IPv4 dotted-decimal or IPv6 colon-separated notation.
> service-name name: Specified CSCF service name.
> Usage
> Use this command to display statistics for IPSec tunnels facilitated by the context. This information can be used for performance monitoring and/or troubleshooting
> Example
> The following command displays cumulative IPSec statistics for the current context:
> show crypto statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show crypto transform-set
> Displays transform set configuration information.
> Product
> PDIF, PDSN, GGSN, SCM
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show crypto transform-set [ transform_name ]
> transform_name
> Specifies the name of a particular transform set for which to display information.
> transform_name is the name of the transform set and can be from 1 to 127 alphanumeric characters and is case sensitive.
> Usage
> Use this command to verify the configuration of transform sets within the context.
> If no keyword is specified, information will be displayed for all transform sets configured within the context.
> Important: This command is used in PDIF Release 8.1. In PDIF Release 8.3, the syntax of this command is changed to show crypto ipsec transform-set.
> Example
> The following command displays information for a transform set named test1:
> show crypto transform-set test1
> show cs-network
> Displays statistics for Circuit Switched (CS)-network(s) instance configured on a chassis for HNB-GW service sessions.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cs-network { all | name cs_name } [ status ] [ | { grep grep_options | more }]
> all
> Displays status counters for all CS networks configured for HNB-GW service sessions on a chassis.
> name cs_name
> Displays status counters for a specific CS network configured for HNB-GW service sessions on a chassis.
> cs_name specificies the name of a configured CS network instance on a chassis for HNB-GW service sessions and can be from 1 to 127 alphanumeric characters and is case sensitive.
> grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display the status of any or all CS-network(s) instance configured on a chassis for HNB-GW service sessions..
> Example
> The following command displays the output for CS network instance status named cs_1_hnb:
> show cs-network name cs_1_hnb status
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cs-network counters
> This command displays the session counter information for an HNB-CS Network associated with Home-NodeB Gateway (HNB-GW) services configured and running on a system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show cs-network counters [ name cs_svc_name [ msc msc_point_code ] ] [ | { grep grep_options | more } ]
> name cs_svc_name
> This keyword is used to filter the counter display based on the HNB-CS Network service name cs_svc_name configured and associated with HNB-GW service running on system.
> cs_svc_name must be an existing HNB-CS Network service, and be from 1 to 63 alphanumeric characters.
> msc msc_point_code
> This keyword is used to filter the counter display filtered on the basis of MSC address provided in SS7 point code msc_point_code which is connected to particular HNB-CS Network service.
> msc_point_code must be the address of an MSC in SS7 point code notation.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view the session counter information for HNB-CS Network services configured and MSCs connected on a system.
> Example
> The following command displays the counters for the HNB-CS Network service named hnb_cs_svc1:
> show cs-network counters name hnb_cs_svc1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cs-network statistics
> This command displays the Circuit Switched session statistics for Home-NodeB Gateway (HNB-GW) services configured and running on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show cs-network statistics [ name cs_svc_name | ranap-only | rtp-only | sccp-only ] [ | { grep grep_options | more } ]
> name cs_svc_name
> This keyword is used to filter the session statistics display based on the HNB-CS Network service name cs_svc_name configured and associated with an HNB-GW service running on this system.
> cs_svc_name must be an existing HNB-CS Network service, and be from 1 to 63 alphanumeric characters.
> ranap-only
> This keyword is used to filter the session statistics display limited to Radio Access Network Application Protocol (RANAP) traffic only for selected HNB-CS Network service which is configured and associated with an HNB-GW service running on this system.
> rtp-only
> This keyword is used to filter the session statistics display limited to Realtime Streaming Protocol (RTP) and Realtime Streaming Control Protocol (RTCP) traffic only for selected HNB-CS Network service which is configured and associated with an HNB-GW service running on this system.
> sccp-only
> This keyword is used to filter the session statistics display limited to Signaling Connection Control Part (SCCP) traffic only for selected HNB-CS Network service which is configured and associated with an HNB-GW service running on this system.
> | { grep grep_options | more }
> Indicates the output of the command is to be piped (sent) to the command specified.
> A command to send output to must be specified.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to view the session statistics for overall session or in selected part of user session for HNB-GW services configured and running on this system.
> Example
> The following command displays the session statistics for RTP and RTCP part of session for the HNB-CS Network service named hnb_cs1:
> show cs-network statistics name hnbcs1 rtp-only
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf ifc
> Displays the Initial Filter Criteria (iFC) for shared iFC functionality.
> Product
> SCM (S-CSCF, SIP Proxy)
> Privilege
> Security Administrator, Administrator
> Syntax
> show cscf ifc { all | id fc_id } [ | { grep grep_options | more } ]
> all | id fc_id
> all: Displays all iFC.
> id fc_id: Displays information for a specific iFC.
> fc_id must be an existing iFC and be from 1 to 200 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display configuration information for any or all iFC on this system.
> Example
> The following command displays the configuration information for all iFC on this system:
> show cscf ifc all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf nat
> Displays the Call Session Control Function (CSCF) mapping created for each of the media streams present in an established dialog.
> Product
> SCM (P-CSCF, A-BG)
> Privilege
> Security Administrator, Administrator
> Syntax
> show cscf nat media mapping { all | aor aor } [ | { grep grep_options | more } ]
> media mapping { all | aor aor }
> all: Displays the UE/Network origins and destinations, including their IP addresses/port numbers and associated contexts.
> aor aor: Displays information for a specific Address of Record (AoR).
> aor must be an existing AoR and be from 1 to 79 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display the status of configured Network Address Translation (NAT) support.
> Example
> The following command displays the status of the mapping created for each of the media streams present on this system:
> show cscf nat media mapping all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf peer-servers
> Displays name, IP address, and status of configured Call Session Control Function (CSCF) peer servers visible to the system.
> Product
> SCM
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cscf peer-servers { all | full | name service_name [ server-name server_name ] } [ | { grep grep_options | more } ]
> all | full | name service_name [ server-name server_name ]
> all: Displays the peer server list names and the servers within those lists including their IP addresses/port numbers and domain names.
> full: Displays additional details regarding the peer servers within the configured lists on the system.
> name service_name [ server-name server_name ]: Displays the same information as the full keyword output, but for a specific peer server list or specific server.
> service_name/server_name must be an existing peer server list or server and be from 1 through 80 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display the status of configured peer servers.
> Example
> The following command displays the status of a peer server named icscf3 that is a member of peer server list cscf-main:
> show cscf peer-servers name cscf-main server-name icscf3
> The following command displays the status of all peer servers in configured peer server groups in this context:
> show cscf peer-servers full
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf service
> Displays configuration and/or statistic information for Call Session Control Function (CSCF) services on this system.
> Product
> SCM
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cscf service { all [ counters ] | diameter { location-info statistics service-name service_name [ vpn-name name ] | policy-control statistics service-name service_name [ vpn-name name ] } | grey-list name name | li-packet-cable statistics service-name service_name | performance-counters name service_name | statistics name service_name [ all | calls | ip-security | message | package-name { message-summary | presence | reg | winfo } | registrations | sigcomp | tcp { msrp | sip }] | subscription name service_name } [ | { grep grep_options | more } ]
> all [ counters ]
> Displays configuration information for all CSCF services configured on this system.
> counters: Displays statistics with the configuration information for all CSCF services configured on the system.
> diameter { location-info statistics service-name service_name [ vpn-name name ] | policy-control statistics service-name service_name [ vpn-name name ] }
> location-info statistics: Displays Diameter statistics on the E2 interface with the location information.
> policy-control statistics: Displays Diameter (DPECA) statistics on the CSCF Rx interface with the configuration information.
> service-name service_name: Specifies the name of a CSCF service for which the statistics will be displayed. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> vpn-name name: Specifies the name of a context in which all statistics for all services will be displayed. name must be an existing context and be from 1 to 79 alphanumeric characters.
> grey-list name name
> Displays the list of run-time grey-listed users and their remaining barred period for the specified CSCF service.
> name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> li-packet-cable statistics service-name service_name
> Refer to the Lawful Intercept Configuration Guide for a description of this command.
> name service_name [ counters ]
> Displays configuration information for a specific CSCF service configured on this system.
> service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> counters: Displays statistics with the configuration information for the specific CSCF service.
> performance-counters name service_name
> Displays performance counters specified in 3GPP TS 32.409 for a specific CSCF service configured on this system. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> statistics name service_name [ all | calls | ip-security | message | package-name { message-summary | presence | reg | winfo } | registrations | sigcomp | tcp { msrp | sip } ]
> Displays service statistics for a specific CSCF service configured on this system. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> all: Displays all CSCF service statistics.
> calls: Displays session statistics related to CSCF calls.
> ip-security: Displays session statistics related to CSCF IPSec.
> message: Displays session statistics for the SIP method MESSAGE.
> package-name: Displays session statistics for the associated event package.

> • | message-summary: Displays session statistics for the “message-summary” event package.

> • | presence: Displays session statistics for the “presence” event package.

> • | reg: Displays session statistics for the “reg” event package.

> • | winfo: Displays session statistics for the “watcher-info” event package.

> registrations: Displays session statistics related to CSCF registrations, re-registrations, and de-registrations.
> sigcomp: Displays session statistics related to CSCF sigcomp.
> tcp: Displays session statistics related to CSCF TCP.

> • | msrp: Displays statistics related to CSCF TCP MSRP statistics.

> • | sip: Displays statistics related to CSCF TCP SIP statistics.

> Important: This keyword must be followed by another statistics-related keyword.
> subscription name service_name
> Displays service level subscription information for a specific service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display configuration information and/or statistics for any or all CSCF services on this system.
> Example
> The following command displays service statistics for the CSCF service named cscf1:
> show cscf service statistics name cscf1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf sessions
> Displays statistics for Call Session Control Function (CSCF) sessions on this system.
> Product
> SCM
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cscf sessions { counters { calls { duration | first-response-time | invite-processing-time | post-answer-delay | post-dial-delay | service service_name | session-release-delay | session-setup-delay } service service_name | subscription { duration | service service_name | setup-time } service service_name } | duration | full [ callleg-id id | from-aor aor | service service_name | session-id id | to-aor aor ] [ media-type type ] | summary [ from-aor aor | service service_name | session-id id | to-aor aor ] } [ | { grep grep_options | more } ]
> counters { calls { duration | first-response-time | invite-processing-time | post-answer-delay | post-dial-delay | service service_name | session-release-delay | session-setup-delay } service service_name | subscription { duration | service service_name | setup-time } service service_name }
> Displays counters for all CSCF sessions matching the filter criteria.
> calls: Counters associated with calls in CSCF service.

> • | duration: Displays the call duration time.

> • | first-response-time: Displays the time interval for the first response received for INVITE.

> • | invite-processing-time: Displays the INVITE message processing time in CSCF.

> • | post-answer-delay: Displays the time interval for post answer delay.

> • | post-dial-delay: Displays the time interval for the ringing or success response for INVITE.

> • | service service_name: Displays specific service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.

> Important: This keyword may be used alone with the counters keyword or following any other counters-specific keyword.

> • | session-release-delay: Displays the time interval for releasing the call.

> • | session-setup-delay: Displays the time interval for session setup.

> • | subscription: Counters associated with subscriptions in CSCF service.

> • | duration: Displays the SIP Subscription duration time.

> • | service service_name: Displays specific service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.

> Important: This keyword may be used alone with the subscription keyword or following any other subscription-specific keyword.

> • | setup-time: Displays the SIP Subscription setup time.

> duration
> Displays the call duration for all CSCF sessions.
> full [ callleg-id id | from-aor aor | service service_name | session-id id | to-aor aor ] [ media-type type ]
> Displays all the session information for the active CSCF sessions matching the filter criteria.
> callleg-id id: Specifies a call leg from which session statistics are to be displayed. id must be an existing call-leg ID and be from 1 to 63 alphanumeric characters.
> from-aor aor: Specifies that session statistics are to be displayed for sessions originating from this specific Address of Record (AoR). aor must be an existing AoR and be from 1 to 79 alphanumeric characters.
> service service_name: Specifies that session statistics are to be displayed for sessions using this CSCF service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> session-id id: Specifies that session statistics are to be displayed for sessions with this ID. id must be an existing session ID and be from 1 to 63 alphanumeric characters.
> to-aor aor: Specifies that session statistics are to be displayed for sessions sent to this specific AoR. aor must be an existing AoR and be from 1 to 79 alphanumeric characters.
> media-type type: Displays information about specific media type, if any. type must be an existing media type and be from 1 to 9 alphanumeric characters.
> summary [ from-aor aor | service service_name | session-id id | to-aor aor ]
> Displays session summary information for sessions matching the filter criteria.
> from-aor aor: Specifies that session statistics are to be displayed for sessions originating from this specific Address of Record (AoR). aor must be an existing AoR and be from 1 to 79 alphanumeric characters.
> service service_name: Specifies that session statistics are to be displayed for sessions using this CSCF service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> session-id id: Specifies that session statistics are to be displayed for sessions with this ID. id must be an existing session ID and be from 1 to 63 alphanumeric characters.
> to-aor aor: Specifies that session statistics are to be displayed for sessions sent to this specific AoR. aor must be an existing AoR and be from 1 to 79 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display session information for any or all CSCF sessions.
> Example
> The following command displays the output for CSCF session duration:
> show cscf sessions duration
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf sip
> Displays Session Initiation Protocol (SIP) statistics for a specific Call Session Control Function (CSCF) service configured on this system.
> Product
> SCM
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cscf sip statistics name service_name [ interface { domain { list | name domain_name } | ip { address ip_address | list } } | vpn-name name ] [ | { grep grep_options | more } ]
> statistics name service_name
> Specifies the name of the CSCF service. service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> [ interface { domain { list | name domain_name } | ip { address ip_address | list } }
> SIP statistics will be displayed for this interface.
> domain list: Displays list of interfaces associated with the CSCF service.
> domain name domain_name: Specifies the domain associated with the CSCF service. domain_name must be an existing domain and be from 1 to 80 alphanumeric characters.
> ip address ip_address: Specifies the destination or source ip address associated with the CSCF service. ip_address is expressed in IPv4 dotted-decimal or IPv6 colon-separated notation.
> ip list: Displays list of interfaces associated with the CSCF service.
> vpn-name name
> Specifies the name of the context in which the service is configured. name must be an existing context and be from 1 to 79 alphanumeric characters.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display SIP statistics for a specific CSCF service.
> Important: This command displays counters for SIP statistics for a specified CSCF service. Counters are incriminated when SIP messages are sent (Tx) or received (Rx). SIP Request, Response, and Error counters are maintained at various levels in the SIP stack. These values are dependent on the packet flow. For example, if packets are dropped at an initial stage of parsing and error detection, the counters may not increment. All 2xx Response counters for individual requests are maintain outside the SIP layer and will not track re-transmissions and erroneous packets that are dropped. All other counters do keep track of re-transmissions.
> Example
> The following command displays SIP statistics for the CSCF service named cscf1:
> show cscf sip statistics name cscf1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show cscf tcp
> Displays TCP connection information for a specific Call Session Control Function (CSCF) service configured on this system.
> Product
> SCM
> Privilege
> Security Administrator, Administrator, Operator
> Syntax
> show cscf tcp connections service service_name [ facility { cscfmgr | sessmgr } ] [ full ] [ msrp ] [ remote-ip ip_address ] [ remote-port port_number ] [ sip ] [ | { grep grep_options | more } ]
> connections service service_name
> service service_name: Specifies the name of the CSCF service.
> service_name must be an existing CSCF service and be from 1 to 63 alphanumeric characters.
> facility { cscfmgr | sessmgr }
> Facility type for which connection details have to be retrieved.
> cscfmgr: Facility type cscfmgr.
> sessmgr: Facility type sessmgr.
> full
> Displays detailed information related to each connection.
> msrp
> Displays statistics related to CSCF TCP Message Session Relay Protocol (MSRP) statistics.
> remote-ip ip_address
> Remote IP address to match the connection. ip_address is expressed in IPv4 dotted-decimal or IPv6 colon-separated notation.
> remote-port port_number
> Remote port to match the connection. port_number is an integer from 1 to 65534.
> sip
> Displays statistics related to CSCF TCP SIP statistics.
> | grep grep_options | more
> Indicates the output of the command is to be piped (sent) to the command specified. A command to send output to must be specified.
> Refer to Regulating a Command’s Output section of the Command Line Interface Overview chapter for details on the usage of grep and more.
> Usage
> Use this command to display TCP connection information for a specific CSCF service.
> Important: More than one optional keyword may be used per command.
> Example
> The following command displays TCP connections for the CSCF service named cscf1:
> show cscf tcp connections service cscf1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show css delivery-sequence
> In StarOS 9.0 and later releases, this command is obsolete.
> show css server
> In StarOS 9.0 and later releases, this command is obsolete.
> show css service
> In StarOS 9.0 and later releases, this command is obsolete.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883