> TFTP Configuration Mode Commands
> The TFTP configuration mode is used to manage the TFTP servers for the current context.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> max servers
> Configures the maximum number of TFTP servers that can be started within any 60 second interval. If this limit is reached, the system waits two minutes before trying to start any more servers.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> max servers count
> count
> Default: 40
> Specifies the maximum number of servers that can be spawned in any 60 second interval. count must be a value in the range from 1 to 100.
> Usage
> Set the number of servers to tune the system response as a heavily loaded system may need more servers to support the incoming requests.
> The converse would be true as well in that a system can benefit by reducing the number of servers such that TFTP services do not cause excessive system impact to other services.
> Example
> max servers 50

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883