> PS-Network-RANAP Schema Statistics
> The PS-Network schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HNB-GW.
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the PS-Network-RANAP Schema

> Variables | Description | Data Type
> nwname | Indicates the name of the Packet Switch (PS) Network connected with specific HNB-GW on which statistics are collected or displayed. This is a key variable. | String
> initial-ue-tx | Indicates the total number of Initial UE message transmitted. Trigger: When Initial UE message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> dir-transfer-rx | Indicates the total number of Direct Transfer message received. Trigger: When Direct Transfer message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> dir-transfer-tx | Indicates the total number of Direct Transfer message transmitted. Trigger: When Direct Transfer message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-rx | Indicates the total number of Reset message received. Trigger: When Reset message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-tx | Indicates the total number of Reset message transmitted. Trigger: When Reset message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-ack-rx | Indicates the total number of Reset Ack message received. Trigger: When Reset Ack message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-ack-tx | Indicates the total number of Reset Ack message transmitted. Trigger: When Reset Ack message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-res-rx | Indicates the total number of Reset Resource message received. Trigger: When Reset Resource message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-res-tx | Indicates the total number of Reset Resource message transmitted. Trigger: When Reset Resource message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-res-ack-rx | Indicates the total number of Reset Resource Ack message received. Trigger: When Reset Resource Ack message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reset-res-ack-tx | Indicates the total number of Reset Resource Ack message transmitted. Trigger: When Reset Resource Ack message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> iu-rel-req-tx | Indicates the total number of Iu Release Request message transmitted. Trigger: When Iu Release Request message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> iu-rel-cmd-rx | Indicates the total number of Iu Release Command message received. Trigger: When Iu Release Command message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> iu-rel-comp-tx | Indicates the total number of Iu Release Complete message transmitted. Trigger: When Iu Release Complete message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> paging-req-rx | Indicates the total number of Paging Request message received. Trigger: When Paging Request message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx | Indicates the total number of RAB Assignment Response message transmitted. Trigger: When RAB Assignment Response message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-total-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-rab-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-total-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rsp-tx-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-req-rx | Indicates the total number of RAB Assignment Request message received by PS Network. Trigger: When RAB Assignment Request message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-req-rx-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-req-rx-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rab-setup-mod-timer-exp | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify Timer Expire. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify Timer Expire. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rab-rel-timer-exp | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Release Timer Expire. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Release Timer Expire. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rab-setup-mod-rel-local-failure | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-invalid-rab-id | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Radio Network Layer Cause - Invalid RAB Id. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Radio Network Layer Cause - Invalid Rab Id. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-interact-with-othr-proc | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Radio Network Layer Cause - Interaction With Other Proc. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Radio Network Layer Cause - Interaction With Other Proc. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-sig-trans-res-fail | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Transport Layer Cause - Signal Transport Resource Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Transport Layer Cause - Signal Transport Resource Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-iu-conn-fail-to-estab | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-trans-syn-err | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Transfer syntax error. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Transfer syntax error. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-abs-syn-err-ign | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error (Ignore). Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error(Ignore). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-semantic-err | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Semantic error. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Semantic error. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-abs-syn-err-rej | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error (Reject). Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error (Reject). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-msg-not-comp | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Message not compatible with receiver state. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Message not compatible with receiver state. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-falsely-construct-msg | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed message). Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed msg). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-local-fail-no-res-avalable | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Miscellaneous Cause - No Resource Available. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Miscellaneous Cause - No Resource Available. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-rep-rx-local-fail-unspecified | Indicates the total number of RAB Assignment Response message transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Miscellaneous Cause - Unspecified. Trigger: When RAB Assignment Response message is transmitted by PS Network for RAB Setup/Modify/Release Local Failure with Miscellaneous Cause - Unspecified. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Conversational Class for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network with Conversational Class for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Conversational Class for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network with Conversational Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-tot-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-setup-mod-fail-lcl-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-tot-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-conv-class-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Conversational Class for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network with Conversational Class for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Streaming Class for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network with Streaming Class for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Streaming Class for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network with Streaming Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-tot-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-setup-mod-fail-lcl-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-tot-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-stream-class-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Streaming Class for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network with Streaming Class for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Interactive Class for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network with Interactive Class for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Interactive Class for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network with Interactive Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-tot-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-setup-mod-fail-lcl-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-tot-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-inter-class-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Interactive Class for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network with Interactive Class for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Background Class for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network with Background Class for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Background Class for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network with Background Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-tot-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-setup-mod-fail-lcl-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-tot-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-back-class-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Background Class for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network with Background Class for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-setup-mod-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Unknown Class for RAB Setup/Modify. Trigger: When RAB Assignment Request message is received by PS Network with Unknown Class for RAB Setup/Modify. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-rel-rx | Indicates the total number of RAB Assignment Request message received by PS Network with Unknown Class for RAB Release. Trigger: When RAB Assignment Request message is received by PS Network with Unknown Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-setup-mod-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Setup/Modify Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Setup/Modify Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-tot-rab-setup-mod-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Setup/Modify Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Setup/Modify Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-setup-mod-fail-lcl-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Setup/Modify Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Setup/Modify Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-rel-succ-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Release Success. Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Release Success. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-tot-rab-rel-fail-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Release Fail. Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Release Fail. Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-rel-fail-local-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Release Fail (Local). Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Release Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> rab-ass-unkwn-class-rab-que-tx | Indicates the total number of RAB Assignment Response message transmitted by PS Network with Unknown Class for RAB Queued. Trigger: When RAB Assignment Response message is transmitted by PS Network with Unknown Class for RAB Queued. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-rx | Indicates the total number of Relocation Request message received by PS Network. Trigger: When Relocation Request message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-rx-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network for RAB Setup. Trigger: When Relocation Request message is received by PS Network for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network. Trigger: When Relocation Request Ack message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-tx-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-tx-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-tx-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network for RAB Setup Fail for RAB Setup Fail(Local). Trigger: When Relocation Request Ack message is transmitted by PS Network for RAB Setup Fail for RAB Setup Fail(Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-invalid-rab-id | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Radio Network Layer Cause - Invalid Rab Id. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Radio Network Layer Cause - Invalid Rab Id. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-interact-othr-proc | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Radio Network Layer Cause - Interaction With Other Proc. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Radio Network Layer Cause - Interaction With Other Proc. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-sig-trans-res-fail | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Transport Layer Cause - Signal Transport Resource Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Transport Layer Cause - Signal Transport Resource Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-iu-conn-fail-to-estab | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-trans-syn-err | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Transfer syntax error. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Transfer syntax error. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-abs-syn-err-ign | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error(Ignore). Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error(Ignore). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-semantic-err | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Semantic error. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Semantic error. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-abs-syn-err-rej | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error (Reject). Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error (Reject). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-msg-not-comp | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Message not compatible with receiver state. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Message not compatible with receiver state. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-falsely-construct-msg | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed msg). Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed msg). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-no-res-avalable | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Miscellaneous Cause - No Resource Available. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Miscellaneous Cause - No Resource Available. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-ack-local-fail-unspecified | Indicates the total number of Relocation Request Ack message transmitted by PS Network for Local RAB Setup Failure with Miscellaneous Cause - Unspecified. Trigger: When Relocation Request Ack message is transmitted by PS Network for Local RAB Setup Failure with Miscellaneous Cause - Unspecified. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-conv-class-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network with Conversational Class for RAB Setup. Trigger: When Relocation Request message is received by PS Network with Conversational Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-conv-class-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Conversational Class for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network with Conversational Class for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-conv-class-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Conversational Class for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network with Conversational Class for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-conv-class-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Conversational Class for RAB Setup Fail (Local). Trigger: When Relocation Request Ack message is transmitted by PS Network with Conversational Class for RAB Setup Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-stream-class-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network with Streaming Class for RAB Setup. Trigger: When Relocation Request message is received by PS Network with Streaming Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-stream-class-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Streaming Class for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network with Streaming Class for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-stream-class-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Streaming Class for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network with Streaming Class for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-stream-class-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Streaming Class for RAB Setup Fail (Local). Trigger: When Relocation Request Ack message is transmitted by PS Network with Streaming Class for RAB Setup Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-inter-class-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network with Interactive Class for RAB Setup. Trigger: When Relocation Request message is received by PS Network with Interactive Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-inter-class-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Interactive Class for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network with Interactive Class for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-inter-class-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Interactive Class for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network with Interactive Class for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-inter-class-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Interactive Class for RAB Setup Fail (Local). Trigger: When Relocation Request Ack message is transmitted by PS Network with Interactive Class for RAB Setup Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-back-class-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network with Background Class for RAB Setup. Trigger: When Relocation Request message is received by PS Network with Background Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-back-class-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Background Class for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network with Background Class for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-back-class-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Background Class for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network with Background Class for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-back-class-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Background Class for RAB Setup Fail (Local). Trigger: When Relocation Request Ack message is transmitted by PS Network with Background Class for RAB Setup Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-req-unkwn-class-rab-setup-rx | Indicates the total number of Relocation Request message received by PS Network with Unknown Class for RAB Setup. Trigger: When Relocation Request message is received by PS Network with Unknown Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-unkwn-class-rab-setup-succ-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Unknown Class for RAB Setup Success. Trigger: When Relocation Request Ack message is transmitted by PS Network with Unknown Class for RAB Setup Success. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-unkwn-class-tot-rab-setup-fail-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Unknown Class for RAB Setup Fail. Trigger: When Relocation Request Ack message is transmitted by PS Network with Unknown Class for RAB Setup Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-req-unkwn-class-rab-setup-fail-local-tx | Indicates the total number of Relocation Request Ack message transmitted by PS Network with Unknown Class for RAB Setup Fail (Local). Trigger: When Relocation Request Ack message is transmitted by PS Network with Unknown Class for RAB Setup Fail (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-detect-tx | Indicates the total number of Relocation Detect message transmitted by PS Network. Trigger: When Relocation Detect message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-comp-tx | Indicates the total number of Relocation Complete message transmitted by PS Network. Trigger: When Relocation Complete message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> total-reloc-fail-tx | Indicates the total number of Relocation Failure message transmitted by PS Network. Trigger: When Relocation Failure message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-local-tx | Indicates the total number of Relocation Failure message transmitted by PS Network for Relocation Failure (Local). Trigger: When Relocation Failure message is transmitted by PS Network for Relocation Failure (Local). Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-invalid-rab-id | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Radio Network Layer Cause - Invalid RAB Id. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Radio Network Layer Cause - Invalid RAB Id. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-interact-othr-proc | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Radio Network Layer Cause - Interaction with other procedure.. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Radio Network Layer Cause - Interaction with other procedure.. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-sig-trans-res-fail | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Transport Layer Cause - Signal Transport Resource Fail. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Transport Layer Cause - Signal Transport Resource Fail. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-iu-conn-fail-to-estab | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Transport Layer Cause - Iu Transport Conn failed to Establish. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-trans-syn-err | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause Transfer syntax error. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause Transfer syntax error. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-abs-syn-err-ign | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error(Ignore). Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error(Ignore). Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-semantic-err | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause - Semantic error. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause - Semantic error. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-abs-syn-err-rej | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error (Reject). Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error (Reject). Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-msg-not-comp | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause - Message not compatible with receiver state. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause - Message not compatible with receiver state. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-falsely-construct-msg | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed msg). Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Protocol Layer Cause - Abstract syntax error (Falsely constructed msg). Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-no-res-avalable | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Miscellaneous Cause - No Resource Available. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Miscellaneous Cause - No Resource Available. Availability: Across all PS Networks | Unsigned Int32
> reloc-fail-tx-local-fail-unspecified | Indicates the total number of Relocation Failure message received by PS Network for Local Relocation Failure with Miscellaneous Cause - Unspecified. Trigger: When Relocation Failure message is received by PS Network for Local Relocation Failure with Miscellaneous Cause - Unspecified. Availability: Across all PS Networks | Unsigned Int32
> reloc-reqd-tx | Indicates the total number of Relocation Required message transmitted by PS Network. Trigger: When Relocation Required message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-prep-failure-rx | Indicates the total number of Relocation Prep Failure message received by PS Network. Trigger: When Relocation Prep Failure message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> fwd-srns-ctx-req-tx | Indicates the total number of Fwd SRNS Context Request message transmitted by PS Network. Trigger: When Fwd SRNS Context Request message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-rx | Indicates the total number of Relocation Command message received by PS Network. Trigger: When Relocation Command message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-rx-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network for RAB Setup. Trigger: When Relocation Command message is received by PS Network for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-rx-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network for RAB Release. Trigger: When Relocation Command message is received by PS Network for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-conv-class-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network with Conversational Class for RAB Setup. Trigger: When Relocation Command message is received by PS Network with Conversational Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-conv-class-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network with Conversational Class for RAB Release. Trigger: When Relocation Command message is received by PS Network with Conversational Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-stream-class-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network with Streaming Class for RAB Setup. Trigger: When Relocation Command message is received by PS Network with Streaming Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-stream-class-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network with Streaming Class for RAB Release. Trigger: When Relocation Command message is received by PS Network with Streaming Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-inter-class-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network with Interactive Class for RAB Setup. Trigger: When Relocation Command message is received by PS Network with Interactive Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-inter-class-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network with Interactive Class for RAB Release. Trigger: When Relocation Command message is received by PS Network with Interactive Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-back-class-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network with Background Class for RAB Setup. Trigger: When Relocation Command message is received by PS Network with Background Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-back-class-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network with Background Class for RAB Release. Trigger: When Relocation Command message is received by PS Network with Background Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-unkwn-class-rab-setup-rx | Indicates the total number of Relocation Command message received by PS Network with Unknown Class for RAB Setup. Trigger: When Relocation Command message is received by PS Network with Unknown Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> reloc-cmd-unkwn-class-rab-rel-rx | Indicates the total number of Relocation Command message received by PS Network with Unknown Class for RAB Release. Trigger: When Relocation Command message is received by PS Network with Unknown Class for RAB Release. Availability: Across all PS Networks | Unsigned Int32
> srns-ctx-req-rx | Indicates the total number of SRNS Context Request message received by PS Network. Trigger: When SRNS Context Request message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> srns-ctx-rsp-tx | Indicates the total number of SRNS Context Response message transmitted by PS Network. Trigger: When SRNS Context Response message is transmitted by PS Network. Availability: Across all PS Networks | Unsigned Int32
> srns-data-fwd-cmd-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network. Trigger: When SRNS Data Fwd Command message is received by PS Network. Availability: Across all PS Networks | Unsigned Int32
> srns-data-fwd-cmd-rx-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> srns-conv-class-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network with Conversational Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network with Conversational Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> srns-stream-class-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network with Streaming Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network with Streaming Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> srns-inter-class-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network with Interactive Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network with Interactive Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> srns-back-class-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network with Background Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network with Background Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> srns-unkwn-class-rab-setup-rx | Indicates the total number of SRNS Data Fwd Command message received by PS Network with Unknown Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is received by PS Network with Unknown Class for RAB Setup. Availability: Across all PS Networks | Unsigned Int32
> Important: See Bulk Statistics Overview chapter for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883