> P-CDR Field Reference Tables
> This chapter provides reference tables for the CDR fields reported as part of P-GW CDRs (P-CDRs) generated by the system.
> A complete list of supported CDR fields is provided in the P-CDR Field Descriptions chapter of this reference guide.
> The specific CDRs reported in P-CDRs and their encoding are user-selectable via GTPP dictionaries. The use of GTPP dictionaries is configurable using the gtpp dictionary command in the Context Configuration Mode of the system’s Command Line Interface (CLI).
> This section provides information on the fields reported in P-CDRs for the GTPP dictionaries.
> Important: For more information on custom dictionaries, contact your local service representative.
> The category column in all tables use keys described in the following table.
> Dictionary Table Key

> Abbreviation | Meaning | Description
> M | Mandatory | A field that must be present in the CDR.
> C | Conditional | A field that must be present in a CDR if certain conditions are met.
> O M | Operator Provisionable: Mandatory | A field that an operator has provisioned and must be included in the CDR for all conditions.
> O C | Operator Provisionable: Conditional | A field that an operator has provisioned that must included in the CDR if certain conditions are met.

> ‌
> CDR Fields Supported in P-CDRs
> The table in this section lists the P-CDR fields present in the available GTPP dictionaries.
> Custom Dictionaries
> The following custom dictonaries are supported:

> • | custom1

> • | custom2

> • | custom3

> • | custom4

> • | custom5

> • | custom7

> • | custom8

> • | custom40

> • |

> Field | Category | Description
> Record Type | M | P-GW IP CAN bearer record
> Served IMSI | M | IMSI of the served party (if Anonymous Access Indicator is FALSE or not supplied)
> P-GW Address | M | The control plane IP address of the P-GW used.
> Charging ID | M | IP CAN bearer identifier used to identify this IP CAN bearer in different records created by PCNs
> Serving Node Address | M | List of serving node control plane IP addresses (e.g. SGSN, MME, etc.) used during this record.
> Access Point Name Network Identifier | O M | The logical name of the connected access point to the external packet data network (network identifier part of APN).
> PDP/PDN Type | O M | Indicates PDP type (IP, PPP, or IHOSS:OSP) or PDN type (IPv4, IPv6, or IPv4v6).
> Served PDP/PDN Address | O C | IP address allocated for the PDP context / PDN connection (IPv4 or IPv6), if available.
> Dynamic Address Flag | O C | Indicates whether served PDP/PDN address is dynamic, which is allocated during IP CAN bearer activation, initial attach (E-UTRAN or over S2x) and UE requested PDN connectivity. This field is missing if address is static.
> Record Opening Time | M | Time stamp when IP CAN bearer is activated in this S-GW or record opening time on subsequent partial records.
> Duration | M | Duration of this record in the S-GW.
> Cause for Record Closing | M | The reason for the release of record from this P-GW.
> Diagnostics | O C | A more detailed reason for the release of the connection.
> Record Sequence Number | C | Partial record sequence number, only present in case of partial records.
> Node ID | O M | Name of the recording entity.
> Local Record Sequence Number | O M | Consecutive record number created by this node. The number is allocated sequentially including all CDR types.
> APN Selection Mode | O M | An index indicating how the APN was selected.
> Served MSISDN | O M | The primary MSISDN of the subscriber.
> Charging Characteristics | M | The Charging Characteristics applied to the IP CAN bearer.
> Charging Characteristics Selection Mode | O M | Information about how Charging Characteristics were selected.
> Serving Node PLMN Identifier | O M | Serving node PLMN Identifier (MCC and MNC) used during this record, if available.
> Served IMEISV | O C | IMEISV of the ME, if available.
> RAT Type | O C | Indicates the Radio Access Technology (RAT) type currently used by the Mobile Station, when available.
> MS Time Zone | O C | Indicates the offset between universal time and local time in steps of 15 minutes where the MS currently resides.
> User Location Information | O C | Contains the User Location Information of the MS as defined in TS 29.060 [203] for GPRS case, and in TS 29.274 [210] for EPC case, if available.
> List of Service Data | O M | List of changes in charging conditions for all service data flows within this IP CAN bearer categorized per rating group or per combination of the rating group and service id.
> Data Service Volume Block | O M | Service data container associated with a service condition change on a service data flow (categorized per rating group or per combination of the rating group and service id) within this IP CAN bearer.
> Rating Group | O M | Service flow identity, also known as content-id.
> Charging Rulebase Name | O C | Name of the Rulebase used for charging.
> Local Sequence Number (LOSD) | O C | Service data container sequence number.
> Time of First Usage | O C | Timestamp for the first IP packet to be transmitted for the service data flow.
> Time of Last Usage | O C | Timestamp for the last IP packet to be transmitted for the service data flow.
> Time Usage | O C | Difference in seconds, within range of 0 to 4294967295, between “time of first usage” and “time of last usage”.
> Service Condition Change | O C | Reason for closing the service data container.
> QoS Information Negotiated | O C | Authorized QoS for the IP-CAN bearer.
> Serving Node Address (LOSD) | O C | IP address of the serving node (SGSN/S-GW) control plane.
> Data Volume FBC Uplink | O C | Number of octets received in the uplink direction for this container.
> Data Volume FBC Downlink | O C | Number of octets transmitted in the downlink direction for this container.
> Time of Report | O M | Timestamp defining the moment when the service data container is closed.
> Service Identifier | O C | Identifier for a service.
> User Location Information (LOSD) | O C | Location of the user known at the time when container is created.
> Serving node Type | M | List of serving node types in control plane. The serving node types listed here map to the serving node addresses listed in the field “Serving node Address” in sequence.
> Served MNNAI | O C | Mobile Node Identifier in NAI format (based on IMSI), if available.
> P-GW PLMN Identifier | O C | PLMN identifier (MCC MNC) of the P-GW.
> Start Time | O C | The time when User IP-CAN session starts, available in the CDR for the first bearer in an IP-CAN session.
> Stop Time | O C | The time when User IP-CAN session is terminated, available in the CDR for the last bearer in an IP-CAN session .
> PDN Connection Id | O M | PDN connection (IP-CAN session) identifier to identify different records belonging to same PDN connection.

> Notes:

> • | custom7: This customer-specific file format contains CDRs converted from ASN.1 format to ASCII format according to the following conventions. Each line in the file consists of one CDR which contains 33 parameters occupying 491 bytes.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883