> TFTP Configuration Mode Commands
> The TFTP configuration mode is used to manage the TFTP (Trivial File Transfer Protocol) servers for the current context.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> max servers
> Configures the maximum number of TFTP servers that can be started within any 60-second interval. If this limit is reached, the system waits two minutes before trying to start any more servers.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> max servers count
> count
> Default: 40
> Specifies the maximum number of servers that can be spawned in any 60-second interval. count must be an integer from 1 through 100.
> Usage
> Set the number of servers to tune the system response as a heavily loaded system may need more servers to support the incoming requests.
> The converse would be true as well in that a system can benefit by reducing the number of servers such that TFTP services do not cause excessive system impact to other services.
> Example
> max servers 50

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883