> LTE Network Global MME ID Management Database Configuration Mode Commands
> The LTE Network Global MME ID Management Database Configuration Mode is used to create associations between PLMN IDs and MME group ID ranges.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> plmn
> Configures associations between PLMN IDs and ranges of MME group IDs.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] plmn mcc mcc_value mnc mnc_value mme-group-id-range first id last id
> no
> Removes the selected PLMN ID to MME group ID range from the MME ID management database.
> mcc mcc_value mnc mnc_value
> mcc mcc_value: Specifies the mobile country code (MCC) part of PLMN identifier. mcc_value must be an integer value from 100 through 999.
> mnc mnc_value: Specifies the mobile network code (MNC) part of PLMN identifier. mnc_value must be an integer value from 00 through 999.
> mme-group-id-range first id last id
> Specifies the range of MME group IDs to apply to the PLMN ID. id must be an integer value from 0 to 65535.
> Usage
> Use this command to create associations between PLMN IDs and a range of MME group IDs.
> Example
> The following command creates an associuation between a PLMN ID of 12323 and a set of MME group IDs with a range of 500 through 575:
> plmn mcc 123 mnc 23 mme-group-id-range first 500 last 575

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883