> VLAN Configuration Mode Commands
> The VLAN Configuration Mode is used to create and manage Virtual LANs and their bindings between contexts.
> bind interface
> Configures a virtual interface to context association for the current VLAN.
> Product
> HA, HSGW, PDSN, P-GW, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] bind interface interface_name context_name
> no
> Indicates the binding between the virtual interface specified and the context specified is to be unbound for the current VLAN.
> interface_name context_name
> Specifies the name and context of the virtual interface to be bound to the context. interface_name must be an alphanumeric string of 1 through 79 characters.
> context_name must refer to a previously configured context expressed as an alphanumeric string of 1 through 79 characters.
> Usage
> Bind a virtual interface and context to allow the VLAN to provide service.
> Example
> bind interface sampleVirtual sampleContext
> no bind interface sampleVirtual sampleContext
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> ingress-mode
> Toggles between enabling and disabling the port ingress (incoming) mode.
> Product
> HA, HSGW, PDSN, P-GW, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] ingress-mode
> no
> Disables the port ingress mode.
> Usage
> Use this command to enable or disable the ingress mode for the port.
> Example
> ingress-mode
> priority
> Configures 802.1p VLAN priority bit for ASN-GW only.
> Product
> ASN-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> priority value
> no priority
> no
> Disables the setting of the 802.1p priority bit.
> value
> Sets the value of the 802.1p priority bit as an integer from 0 through 7, with 7 being the highest priority.
> Usage
> Set a value for the VLAN priority bit as used in the ANS-GW.
> Refer to the ASN-GW Administration Guide for additional information on support for 802.1p.
> Example
> To set a VLAN priority bit value, use the following command:
> priority 3
> To disable the use of a VLAN priority bit, use the following command:
> no priority
> shutdown
> Disables or enables traffic over the current VLAN.
> Product
> HA, HSGW, PDSN, P-GW, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] shutdown
> no
> Enables the VLAN. When omitted the VLAN is shutdown.
> Usage
> Shut down a VLAN.
> To bring a VLAN into service, execute this command using the no keyword.
> Example
> To disable a VLAN from sending or receiving network traffic use the following command:
> shutdown
> To enable a VLAN use the following command:
> no shutdown
> vlan-map
> Sets a single next-hop IP address so that multiple VLANs can use a single next-hop gateway. vlan-map is associated with a specific interface.
> Product
> HA, HSGW, PDSN, P-GW, SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> vlan-map next-hop ip_address
> next-hop ip_address
> Defines an IP address for the next-hop gateway.
> ip_address: can be entered using IPv4 dotted-decimal or IPv6 colon-separated notation.
> Usage
> Use vlan-map to combine multiple VLAN links to go through a single IP address. This feature is used in conjunction with nexthop forwarding and overlapping IP pools.
> After configuring the vlan-map, go to the Port Ethernet Configuration mode to attach the vlan-map to a specific VLAN.
> Example
> The following command sets an IPv4 for a next-hop gateway.
> vlan-map next-hop 123.123.123.1

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883