> OSPFv3 Configuration Mode Commands
> The OSPFv3 Configuration sub-mode is used to configure the OSPFv3 routing protocol. This mode includes commands that configure OSPFv3 routing parameters.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> area
> Configures an Open Shortest Path First Version 3 (OSPFv3) area and enables authentication for that area.
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] area { decimal_value | ipv4address } default-cost default_integer_value | stub [ no-summary ] | virtual-link virtuallink_neighbour_Ipv4_address [ dead-interval virtuallink_dead_interval ] [ hello-interval virtuallink_hello_interval ] [ retransmit-interval virtuallink_retransmit_interval ] [ transmit-delay virtuallink_transmit_delay ]
> no
> Disables authentication for the specified area.
> decimal_value | ipv4address
> decimal_value: Specifies the identification number of the area where authentication will be enabled as an integer from 0 through 4294967295.
> ipv4address: Specifies the IP address of the area where authentication will be enabled in IPv4 dotted-decimal notation.
> default-cost default_integer_value
> Sets the OSPFV3 authentication area’s default cost as an integer from 1 through 16777215.
> stub [ no-summary ]
> Sets the OSPFV3 stub area. Only Router-LSAs, Network-LSAs, Inter-area Prefix-LSAs, Intra-area Prefix-LSAs and Link-LSAs are allowed in a Stub area.
> no-summary Does not inject inter-area routes into stub area.
> virtual-link virtuallink_neighbour_Ipv4_address
> Configures a virtual link to the authentication area.
> virtuallink_neighbour_Ipv4_address is the IPv4 address for the virtual link of the authenticated area in dotted-decimal notation.
> The following interval timers can be set for the virtual link:

> • | dead-interval virtuallink_dead_interval: Sets the virtual link dead-interval (in seconds) as an integer from 1 through 65535.

> • | hello-interval virtuallink_hello_interval: Sets the virtual link hello interval (in seconds) as an integer from 1 through 65535.

> • | retransmit-interval virtuallink_retransmit_interval: Sets the virtual link retransmit interval (in seconds) as an integer from 1 through 3600.

> • | transmit-delay virtuallink_transmit_delay: Sets the virtual link transmit delay (in seconds) as n integer from 1 through 3600.

> Usage
> Use this command to establish OPSFv3 areas and enable authentication.
> Example
> The following command enables authentication for an OSPFv3 area defined by the IP address 192.168.100.10 with default cost of 256
> area 192.168.100.10 default-cost 256
> default-metric
> Configures the default metric value for routes redistributed from another protocol into Open Shortest Path First Version 3 (OSPFv3).
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] default-metric default_metric_integer_value
> no
> Disables the default metric.
> default_metric_integer_value
> Specifies the default metric as an integer from 1 through 16777214.
> Usage
> Use this command to configure OPSFv3 default metric.
> Example
> The following command configures OSPFv3 default metric to 256
> default-metric 256
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> passive Interface
> Configures an OSPFv3 passive interface as passive. If a network interface is configured as passive, it will not receive or send any OSPFv3 packets.
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] passive-interface passive_interface_name
> no
> Disables the passive interface.
> passive-interface passive_interface_name
> Sets the named interface to be a passive interface as an alphanumeric string of 1 through 79 characters.
> Usage
> Use this command to configure an OPSFv3 passive interface in this context.
> Example
> The following command configures an OSPFv3 passive interface.
> passive-interface OSPF-if1
> redistribute
> Redistributes routes from other protocols to OSPFv3 neighbors using the OSPFv3 protocol.
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] redistribute { connected | static } redistribute connected [ metric metric_value [ metric-type external_metric_type ] [ route-map route_map_name ] ] [ metric-type external_metric_type [ route-map route_map_name ] ] [ route-map route_map_name ] static [ metric metric_value [ metric-type external_metric_type ] [ route-map route_map_name ] ] [ metric-type external_metric_type [ route-map route_map_name ] ] [ route-map route_map_name ]
> no
> Disables the route redistribution.
> connected
> Redistributes connected routes.
> static
> Redistributes static routes.
> metric metric_value
> Specifies the OSPFv3 default metric value as an integer from 0 through 16777214.
> metric-type external_metric_type
> Specifies the OSPFv3 external metric type as the integer 1 or 2
> route-map route_map_name
> Specifies a route map as an alphanumeric string of 1 through 79 characters.
> Usage
> Use this command to configure OPSFv3 redistribution of connected or static routes.
> Example
> The following command configures OSPFv3 redistribution of connected routes.
> redistribute connected metric 45 metric-type 1 route-map rt
> router-id
> Sets the OSPFv3 router ID for the Open Shortest Path First Version 3 (OSPFv3) routing process.
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] router-id router_id_ipaddress
> no
> Disables the router-id.
> router_id_ipaddress
> Specifies the router-id an IPv4 address in dotted-decimal notation.
> Usage
> Use this command to configure OPSF v3 router id to the given IPv4 address.
> Example
> The following command configures OSPFv3 router id to the given IPv4 address.
> router-id 11.22.22.21
> timers spf
> Sets OSPFv3 the delay in the time between the detection of a topology change and when the SPF algorithm actually runs.
> Product
> PDSN, HA GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] timers spf spf_delay_timer_value
> no
> Disables the SPF delay timer.
> spf spf_delay_timer_value
> Sets the Shortest Path First (SPF) delay timer (in milliseconds) as an integer from 0 through 4294967295.
> Usage
> Use this command to configure the OPSFv3 SPF delay timer.
> Example
> The following command sets OSPFv3 SPF timer.
> timers spf 256

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883