> ACS Group-of-Objects Configuration Mode Commands
> The ACS Group-of-Objects Configuration Mode is used to configure groups of Active Charging Service (ACS) objects.
> Important: This configuration mode is available only in 10.2 and later releases.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> member-object
> This command allows you to add or remove objects from the current group-of-objects.
> Important: A maximum of 128 objects can be added to a group-of-objects.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] member-object object
> no
> If previously added, removes the specified member object from the current group-of-objects.
> object
> Specifies the member object to add to or remove from the current group-of-objects.
> object must be an alpha and/or numeric string of 1 through 63 characters.
> Usage
> Use this command to add or remove member objects from a group-of-objects.
> Example
> The following command adds the object test to the current group-of-objects:
> member-object test

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883