> show pcc-sp-endpoint
> This chapter describes the output of the show pcc-sp-endpoint command.
> show pcc-sp-endpoint all
> show pcc-sp-endpoint all Command Output Description

> Variables | Description
> SP Endpoint Name | The name of the PCC-Sp-Endpoint instance for which statistics are displayed.
> Context | The name of the context in which PCC-Sp-Endpoint instnace is configured.
> Address | Indicates the local IP address of PCC-Sp-Endpoint instance.
> Access Type | Indicates the type of access, Diameter or Lightweight Directory Access Protocol (LDAP) used by a PCC-Sp-Endpoint instance for Sp interface procedures. By default it is Diameter.
> SPR Subscriber Identifier | Indicates the subscriber identifier (imsi / msisdn / nai) used by PCC-Sp-Endpoint instance in SSC database while requesting subscriber data from SSC.
> User-Name | Indicates the subscriber user name used by PCC-Sp-Endpoint instance in SSC database while requesting subscriber data from SSC.
> Password | Indicates the password used by PCC-Sp-Endpoint instance in SSC database while requesting subscriber data from SSC.
> LDAP Dn | Indicates the name of the LDAP Dn used by PCC-Sp-Endpoint instance.
> Diameter Endpoint | Indicates the name of the Diameter origin endpoint configured for PCC-Sp-Endpoint instance.
> Profile update notification | Indicates whether profile update notifications is allowed or not for a PCC-Sp-Endpoint instance.
> Profile-data key data-reference | Indicates the data-reference values used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter.
> Profile-data key service-indication | Indicates the service indication values used in UDR/SNR message for profile data sent over Sp endpoint when access type is set to Diameter.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883