> CSCF Peer Servers Group Configuration Mode Commands
> The CSCF Peer Servers Group Configuration Mode is used to configure peer servers lists within a peer servers group.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> peer-servers
> Configures peer servers lists in the peer servers group.
> Product
> SCM
> Privilege
> Administrator
> Syntax
> peer-servers list_name { default | mode { active | standby } }
> no peer-servers list_name
> list_name
> Specifies a name for the peer servers list. list_name must be from 1 to 79 alpha and/or numeric characters in length.
> default
> Specifies that the peer servers list is default.
> mode { active | standby }
> Specifies whether the peer servers list is active or standby.
> no peer-servers list_name
> Removes the specified peer servers list from the group.
> Usage
> Use this command to manage peer servers lists in a peer servers group.
> Important: There can be one active, one standby, and one default peer servers list in a peer servers group.
> Example
> The following command configures an active peer servers list named active_as_list:
> peer-servers active_as_list mode active

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883