> CSCF URI Readdress Configuration Mode Commands
> The URI Readdress Configuration Mode is used to set URI translations.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> action
> Adjusts a target address to route sessions to appropriate locations.
> Product
> SCM
> Privilege
> Administrator, Config-administrator
> Syntax
> action { add string | delete num_chars | modify string } position num length length target { destination | source } { aor | domain | user }
> no action
> add string | delete num_chars | modify string
> add string: Adds a specified string to a location indicated by the position keyword for the targeted source or destination address component (aor, domain, or user). string must be from 1 to 79 alpha and/or numeric characters.
> delete num_chars: Deletes a number of characters starting from a location specified by the position keyword for the targeted source or destination address component (aor, domain, or user). num_chars must be an integer from 1 to 79.
> modify string: Modifies a specified string in a location starting with the position keyword for the targeted source or destination address component (aor, domain, or user). The number of characters in the string variable will replace the same number in the address. string must be from 1 to 79 alpha and/or numeric characters.
> position num
> Specifies the position in the target string where the action is to occur. num must be an integer from 1 to 79.
> length length
> Specifies the length of the target string where the action is to occur. length must be an integer from 1 to 79.
> Important: The length keyword is only supported in modify actions.
> target { destination | source }
> Species that the action is to occur within the source or destination address.
> aor | domain | user
> aor: Specifies that the action is applied to AoRs in the targeted source or destination address.
> domain: Specifies that the action is applied to domains in the targeted source or destination address.
> user: Specifies that the action is applied to users in the targeted source or destination address.
> no
> Disables target address to route sessions.
> Usage
> Use this command to manipulate SIP packets matching the criteria in the uri-readdress command.
> Example
> The following command prepends a “+1” to a destination AoR:
> action add +1 position 1 target destination aor
> The following command removes the first two characters from the destination AoR:
> action delete 2 position 1 target destination aor
> The following command replaces characters 2 through 4 with the characters “abc” in the destination AoR:
> action modify abc position 2 target destination aor
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883