> MPLS-IP Configuration Mode Commands
> The MPLS-IP Configuration Mode is used for configuration of Multiprotocol Label Switching (MPLS) IP forwarding specific parameters. This mode is entered from the Context Configuration Mode.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> protocol
> This command creates or removes the MPLS protocol family configuration modes, or configures an existing protocol and enters the MPLS-LDP Configuration Mode in the current context. This command configures the protocol parameters for the MPLS protocol family.
> Product
> GGSN, P-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] protocol ldp
> no
> Removes the configured MPLS-LDP mode from MPLS-IP Configuration mode.
> ldp
> Specifies the type of MPLS protocol to LDP and creates/enters the MPLS-LDP Configuration Mode for Label Distribution Protocol (LDP) specific configuration in an MPLS-IP configuration instance.
> Usage
> Use this command to create/ or remove the MPLS protocol family configuration mode, or configure an existing protocol. If required mode already exists it enters the MPLS-LDP Configuration Mode in the current context.
> Entering this command results in the following prompt:
> [context_name]hostname(config-ldp)#
> The commands configured in this mode are defined in the MPLS-LDP Configuration Mode Commands chapter.
> Example
> The following command creates and enters the MPLS-LDP Protocol mode for Label Distribution Protocol parameters in MPLS-IP Configuration instance:
> protocol ldp

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883