> MSEG RNC Profile Configuration Mode Commands
> The MSEG RNC Profile Configuration Mode enables to configure Mobile Service Edge Gateway (MSEG) Radio Network Controller (RNC) profiles.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> associate
> This command allows you to configure the MSEG to associate with/serve the RNC.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] associate mseg-profile mseg_profile_name
> no
> Disassociates the specified MSEG filter from the RNC.
> mseg_profile_name
> Specifies the name of an MSEG profile as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to configure the MSEG to associate with/serve the RNC.
> Only one MSEG can be associated with an RNC.
> Example
> The following command associates the MSEG named test with the RNC:
> associate mseg-profile test
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> location
> This command allows you to add/remove locations that the RNC serves in an MSEG RNC profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> location mcc mobile_country_code mnc mobile_network_code lac location_area_code sac service_area_code
> no location
> no
> Deletes the previously configured location address in the current MSEG RNC profile.
> mcc mobile_country_code
> Specifies the Mobile Country Code (MCC) as an integer from 100 through 999.
> Note that MCC values from 000 through 099 are reserved codes.
> mnc mobile_network_code
> Specifies the Mobile Network Code (MNC) as a 2- or 3-digit integer fromv00 through 999.
> lac location_area_code
> Specifies the Location Area Code (LAC) as an integer from 1 through 65535.
> sac service_area_code
> Specifies the Service Area Code (SAC) as an integer from 1 through 65535.
> Usage
> Use this command to add/remove locations that the RNC serves in an MSEG RNC profile.
> Multiple locations can be configured in an MSEG RNC profile.
> Example
> The following command adds a location address to the current RNC profile with the MCC, MNC, LAC, and SAC set to 111:
> location mcc 111 mnc 111 lac 111 sac 111
> rnc-gtpu
> This command allows you to add/remove data addresses associated with the RNC.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] rnc-gtpu ipv4/ipv6_address [ udp-port port_number ]
> no
> Deletes the specified RNC GTP-U address from the current RNC profile.
> ipv4/ipv6_address
> Specifies the GTP-U address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> udp-port port_number
> Specifies the UDP port number as an integer from 1 through 65535.
> Usage
> Use this command to add/remove RNC data addresses associated with the RNC in an MSEG RNC profile. Multiple GTP-U addresses can be associated with the RNC.
> Example
> The following command configures the RNC GTP-U address 1.1.1.1 and the UDP port 111 in the current MSEG RNC profile:
> rnc-gtpu 1.1.1.1 udp-port 111
> rnc-id
> This command allows you to configure the RNC ID in an MSEG RNC profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] rnc-id rnc_id
> no
> Deletes the specified RNC ID from the current MSEG RNC profile.
> rnc_id
> Specifies the RNC ID as an integer from 1 through 65535.
> Usage
> Use this command to configure the RNC ID in an MSEG RNC profile.
> Only one RNC ID can be configured in an MSEG RNC profile.
> Example
> The following command configures the RNC ID 111 in the current MSEG RNC profile:
> rnc-id 111

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883