> Performance Management
> This chapter identifies new, modified, and obsoleted performance commands available in Release 12.x.
> Topics covered in this chapter are:

> l | New Commands

> l | Modified Commands

> l | Obsolete Commands

> l | GTPP Storage Server Changes

> l | Web Element Manager Changes

> New Commands
> This section identifies performance management commands that are new in Release 12.x.

> l | Common Commands - New in Release 12.0

> l | Common Commands - New in Release 12.2

> l | Application Detection and Control - New in Release 12.0

> l | Content Filtering Commands - New in Release 12.0

> l | ECS Commands - New in Release 12.0

> l | Firewall Commands - New in Release 12.0

> l | GGSN Commands - New in Release 12.0

> l | HA Commands - New in Release 12.0

> l | IPCF Commands - New in Release 12.1

> l | Mobility Management Entity Commands - New in Release 12.0

> l | Mobility Management Entity Commands - New in Release 12.0

> l | NAT Commands - New in Release 12.0

> l | Packet Data Network Gateway Commands - New in Release 12.0

> l | PDIF Commands - New in Release 12.0

> l | PDSN Commands - New in Release 12.0

> l | Session Control Manager Commands - New in Release 12.2

> l | SGSN Commands - New in Release 12.0

> l | XT2 Commands - New in Release 12.0

> Common Commands - New in Release 12.0
> The following common commands are new in Release 12.0.
> monitor diameter
> This command enables SRP monitoring of the connection between the specified Diameter server and the primary chassis.
> CLI (Service Redundancy Protocol Configuration Mode)
> [ no ] monitor diameter context context_name endpoint endpoint_name [ fqdn fqdn | peer { IPv4_address | IPv6_address } ] [ port port_number ]
> show tacacs
> Provides TACACS+ configuration and session state information for each active TACACS+ session.
> CLI (Exec Mode)
> show tacacs
> show tacacs client statistics
> Provides system-wide client statistics for all TACACS+ sessions.
> CLI (Exec Mode)
> show tacacs client statistics
> show tacacs session statistics
> Provides system-wide session statistics, including protocol statistics, for active TACACS+ sessions.
> CLI (Exec Mode)
> show tacacs session statistics
> Common Commands - New in Release 12.2
> The following common commands are new in Release 12.2.
> clear srp
> This command clears system Service Redundancy Protocol (SRP) statistics.
> CLI (Exec Mode)
> clear srp { audit-statistics | call-loss statistics | checkpoint statistics | statistics }
> threshold aaa-acct-archive-queue
> This command configures accounting message archive queue size threshold for generating alerts or alarms based on the archive queue percentage of AAA accounting messages in the buffer during the polling interval.
> CLI (Global Configuration Mode)
> threshold aaa-acct-archive-queue-size1 high_thresh [ clear low_thresh ]
> threshold aaa-acct-archive-queue-size2 high_thresh [ clear low_thresh ]
> threshold aaa-acct-archive-queue-size3 high_thresh [ clear low_thresh ]
> default threshold aaa-acct-archive-queue-size1
> default threshold aaa-acct-archive-queue-size2
> default threshold aaa-acct-archive-queue-size3
> threshold monitoring aaa-acct-archive-queue
> This command enables/disables threshold monitoring for accounting message archive queue size thresholds.
> CLI (Global Configuration Mode)
> threshold monitoring aaa-acct-archive-queue
> default threshold monitoring aaa-acct-archive-queue
> threshold poll aaa-acct-archive-queue
> This command configures the polling interval for accounting message archive queue size thresholds.
> CLI (Global Configuration Mode)
> threshold poll aaa-acct-archive-queue-size1 interval time
> threshold poll aaa-acct-archive-queue-size2 interval time
> threshold poll aaa-acct-archive-queue-size3 interval time
> default threshold poll aaa-acct-archive-queue-size1 interval
> default threshold poll aaa-acct-archive-queue-size2 interval
> default threshold poll aaa-acct-archive-queue-size3 interval
> Application Detection and Control - New in Release 12.0
> The following Application Detection and Control commands are new in Release 12.0.
> None for this release.
> Content Filtering Commands - New in Release 12.0
> The following Content Filtering commands are new in Release 12.0.
> None for this release.
> ECS Commands - New in Release 12.0
> The following ECS commands are new in Release 12.0.
> None for this release.
> ECS Commands - New in Release 12.2
> The following ECS commands are new in Release 12.2.
> clear active-charging dns-learnt-ip-addresses
> This command clears DNS learnt IP address statistics for the DNS Snooping feature.
> CLI (Exec Mode)
> clear active-charging dns-learnt-ip-addresses statistics sessmgr { all | instance sessmgr_instance } [ | { grep grep_options | more } ]
> clear active-charging tethering-detection statistics
> This command clears statistics pertaining to the Tethering Detection feature.
> CLI (Exec Mode)
> clear active-charging tethering-detection statistics
> show active-charging dns-learnt-ip-addresses
> This command displays DNS learnt IP address statistics for the DNS Snooping feature.
> CLI (Exec Mode)
> show active-charging dns-learnt-ip-addresses statistics { sessmgr { all | instance sessmgr_instance } [ verbose ] | summary } [ | { grep grep_options | more } ]
> show active-charging tethering-detection
> This command displays information/statistics pertaining to Tethering Detection databases.
> CLI (Exec Mode)
> show active-charging tethering-detection { database [ os-signature | tac | ua-signature ]+ [ sessmgr { all | instance instance } ] [ | { grep grep_options | more } ] | statistics }
> Firewall Commands - New in Release 12.0
> The following Stateful Firewall commands are new in Release 12.0.
> None for this release.
> GGSN Commands - New in Release 12.0
> The following GGSN commands are new in Release 12.0.
> None for this release.
> HA Commands - New in Release 12.0
> The following HA commands are new in Release 12.0.
> None for this release.
> IPCF Commands - New in Release 12.1
> This section provides information on new IPCF commands available in Release 12.1.
> IPCF is new product for this release.
> Command Line Interface
> Exec Mode Commands

> l | clear event-notif server

> l | clear event-notif statistics

> l | clear pcc-af service

> l | clear pcc-af session

> l | clear pcc-policy service statistics

> l | clear pcc-policy session

> l | clear pcc-service

> l | clear pcc-sp-endpoint statistics

> l | show event-notif server

> l | show event-notif statistics

> l | show pcc-af service

> l | show pcc-af session

> l | show pcc-policy service

> l | show pcc-policy session

> l | show pcc-service

> l | show pcc-service session

> l | show pcc-service statistics

> l | show pcc-sp-endpoint

> l | show pcc-sp-endpoint connection

> Mobility Management Entity Commands - New in Release 12.0
> The following Mobility Management Entity (MME) commands are new in Release 12.0.
> show lte-policy
> The show lte-policy command is new in release 12.0 and is a direct replacement for the obsolete command show mme-policy.
> CLI (Exec Mode)
> show lte-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary }} [ | { grep grep_options | more } ]
> show sctp-param-template
> The show sctp-param-template command is new in release 12.0. The output of this command displays configuration information for SCTP parameter templates configured on the system.
> CLI (Exec Mode)
> show sctp-param-template { all | name temlate_name } { | grep grep_options | more } ]
> Mobility Management Entity Commands - New in Release 12.2
> The following Mobility Management Entity (MME) commands are new in Release 12.2.
> show ip traffic sctp card
> The show iptraffic sctp command displays kernel traffic information for Stream Control Traffic Protocol. The card slot number and CPU number must be specified.
> CLI (Exec Mode)
> show ip traffic sctp card card_number cpu cpu_number
> show sgs-service offload-status service-name
> This command displays VLR offload information and statistics for the specified SGs service.
> CLI (Exec Mode)
> show sgs-service offload-status service-name sgs_svc_name
> NAT Commands - New in Release 12.0
> The following NAT commands are new in Release 12.0.
> show active-charging analyzer statistics name h323 verbose
> This command displays active charging protocol analyzer statistics for H323 analyzer. The output of this command includes the following new fields:

> l | H323 Session Stats

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Packets

> l | Total Downlink Packets

> l | Total H323 calls

> l | Total RAS messages

> l | Total Q931 messages

> l | Total H245 messages

> l | RAS messages

> l | GatekeeperRequest

> l | GatekeeperConfirm

> l | GatekeeperReject

> l | RegistrationRequest

> l | RegistrationConfirm

> l | RegistrationReject

> l | UnregistrationRequest

> l | UnregistrationConfirm

> l | AdmissionRequest

> l | UnregistrationReject

> l | AdmissionRequest

> l | AdmissionConfirm

> l | AdmissionReject

> l | LocationRequest

> l | LocationConfirm

> l | LocationReject

> l | DisengageRequest

> l | DisengageConfirm

> l | DisengageReject

> l | InfoRequest

> l | InfoRequestResponse

> l | RequestInProgress

> l | Unclassified

> l | Q931 messages

> l | Alerting

> l | CallProceeding

> l | Setup

> l | Connect

> l | ReleaseComplete

> l | Facility

> l | Progress

> l | Information

> l | Unclassified

> l | H245 messages

> l | OpenLogicalChannel

> l | OpenLogicalChannelAck

> l | OpenLogicalChannelReject

> l | OpenLogicalChannelConfirm

> l | RequestChannelClose

> l | CloseLogicalChannel

> l | CloseLogicalChannelAck

> l | EndSessionCommand

> l | Unclassified

> CLI (Exec Mode)
> show active-charging analyzer statistics name h323 [ verbose ] ] [ | { grep grep_options | more } ]
> Packet Data Network Gateway Commands - New in Release 12.0
> This section provides information on new P-GW commands available in Release 12.0.
> clear local-policy
> Clears local QoS policy service statistics and counters found in show command outputs and bulk statistics associated with all local QoS policy services or a specific service defined by the parameter in this command.
> CLI (Exec Mode)
> clear local-policy statistics [ service service_name ]
> PDIF Commands - New in Release 12.0
> The following PDIF commands are new in Release 12.0.
> None for this release.
> PDSN Commands - New in Release 12.0
> The following PDSN commands are new in Release 12.0.
> None for this release.
> Serving Gateway Commands - New in Release 12.0
> The following commands are new in Release 12.0.
> show lte-policy
> The show lte-policy command is new in release 12.0 and is a direct replacement for the obsolete command show mme-policy. The S-GW now supports commands in the LTE Policy Configuration Mode.
> CLI (Exec Mode)
> show lte-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary } } [ | { grep grep_options | more } ]
> Serving Gateway Commands - New in Release 12.2
> The following command is new in Release 12.2.
> accounting mode
> The accounting mode command is new in release 12.2 The S-GW now supports accounting via GTPP (default), RADIUS/Diameter or None.
> CLI (S-GW Service Configuration Mode)
> [ default ] accounting mode { gtpp | none| radius-diameter }
> Session Control Manager Commands - New in Release 12.2
> The following SCM commands are new in Release 12.2.
> show cscf ifc
> Displays configured iFC in XML format, as per 3GPP TS 29.228 Annex E, for CSCF services on this system.
> CLI (Exec Mode)
> show cscf ifc { all | id id } [ | { grep grep_options | more } ]
> show cscf npdb-servers
> Displays connection status of NPDB (Number Portability Data Base) server in S-CSCF service.
> CLI (Exec Mode)
> show cscf npdb-servers service service_name
> [local]asr5000# show cscf npdb-servers service <service_name>
> -----------------------------------------------------------------------
> Context : v4scscf Service : v4scscf
> Client : npdb-client Address : 192.168.1.1
> Req ID : lgt
> -----------------------------------------------------------------------
> Smgr-ID Client-ID Type State Peer Address
> ====== ======= ==== =========== ==============
> 1 10021 PRI OPEN [TCP] 192.168.50.1:3868
> 1 10021 SEC OPEN [NPDB] 192.168.70.1:3878
> 200 10230 PRI IDLE 192.168.50.1:3868
> 150 10170 PRI PROGRESS 192.168.50.1:3868
> 100 10120 PRI IDLE 192.168.50.1:3868
> Peers Summary:
> Peers in IDLE state: 2
> Peers in OPEN state: 2
> Peers in PROGRESS: 1
> Total peers matching specified criteria: 5
> SGSN Commands - New in Release 12.0
> The following SGSN commands are new in Release 12.0.
> clear sgsn-pool statistics
> The following command clears statistics collected for monitoring the number of subscribers offloaded to a target NRI.
> CLI (Exec Mode)
> clear sgsn-pool statistics { gprs-service <service_name> | sgsn-service <service_name> } { nri-value <a - 63> | peer-non-broadcast-lac <1 - 65535> rac <0 - 255> | target-offloaded-to-peer [ target-nri <0 - 63> ] }
> show linecard dlci-utilization
> The following command is new in this release to track DLCI utilization per CLC-type line card:
> CLI (Exec Mode)
> show linecard dlci-utilization card# [ | { grep grep_options | more } ]
> The output for this command includes the fields listed below:

> l | Port

> l | Path

> l | E1T1

> l | TS

> l | DLCI

> l | NSE

> l | NSVC

> l | Average DLCI Utilization (in kbps)

> l | Current Rx

> l | Current Tx

> l | 5min Rx

> l | 5min Tx

> l | 15min Rx

> l | 15min Tx

> show sgsn-pool statistics
> The following command displays statistics collected for monitoring the number of subscribers offloaded to a target NRI.
> CLI (Exec Mode)
> show sgsn-pool statistics { gprs-service <service_name> | sgsn-service <service_name> } { nri-value <0 - 63> | peer-non-broadcast-lac <1 - 65535> rac <0 - 255> | target-load-in-progress [ smgr-instance <1 - 230> | target-nri <0 - 63> ] | target-offloaded-to-peer [ target-nri <0 - 63> ] }
> XT2 Commands - New in Release 12.0
> The following XT2 commands are new in Release 12.0.
> None for this release.
> Modified Commands
> This section identifies performance management commands modified in Release 12.x.

> l | Common Commands - Modified in Release 12.0

> l | Common Commands - Modified in Release 12.2

> l | Application Detection and Control Commands - Modified in Release 12.0

> l | Application Detection and Control Commands - Modified in Release 12.2

> l | Content Filtering Commands - Modified in Release 12.0

> l | ECS Commands - Modified in Release 12.0

> l | Firewall Commands - Modified in Release 12.0

> l | GGSN Commands - Modified in Release 12.0

> l | GGSN Commands - Modified in Release 12.2

> l | HA Commands - Modified in Release 12.0

> l | HA Commands - Modified in Release 12.2

> l | HSGW Commands - Modified in Release 12.0

> l | HSGW Commands - Modified in Release 12.2

> l | IPCF Commands - Modified in Release 12.1

> l | Mobility Management Entity Commands - Modified in Release 12.0

> l | Mobility Management Entity Commands - Modified in Release 12.2

> l | NAT Commands - Modified in Release 12.0

> l | NAT Commands - Modified in Release 12.2

> l | Packet Data Network Gateway Commands - Modified in Release 12.0

> l | Packet Data Network Gateway Commands - Modified in Release 12.0

> l | PDIF Commands - Modified in Release 12.0

> l | PDSN Commands - Modified in Release 12.0

> l | PDSN Commands - Modified in Release 12.2

> l | Serving Gateway Commands - Modified in Release 12.2

> l | Session Control Manager Commands - Modified in Release 12.0

> l | Session Control Manager Commands - Modified in Release 12.0

> l | SGSN Commands - Modified in Release 12.0

> l | SGSN Commands - Modified in Release 12.2

> l | TPO Commands - Modified in Release 12.0

> l | XT2 Commands - Modified in Release 12.0

> Common Commands - Modified in Release 12.0
> The following common commands have been modified in Release 12.0.
> clear dns-client
> The clear dns-client command has two new query-type keywords in release 12.0: AAAA and NAPTR. These keywords clear filtered DNS results based on 128-bit domain IPv6 addresses (AAAA resource records) or on Naming Authority Pointer records (NAPTR).
> CLI (Exec Mode)
> clear dns-client name { cache client name [ query-name name | query-type { A | AAAA | NAPTR | SRV } ] | statistics }
> logging filter active facility
> The logging filter active facility command adds the ability to generate logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the logging filter active facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> logging filter active facility facility
> logging filter runtime facility
> The logging filter runtime facility command adds the ability to generate logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the logging filter runtime facility command in release 12.0: event-notif.
> CLI (Global Configuration Mode)
> logging filter runtime facility facility
> monitor protocol
> The monitor protocol command adds the ability to monitor four new protocols in release 12.0: SSCOP, SSCFNNI, PHS (Payload Header Suppression), and PPPOE.
> CLI (Exec Mode)
> monitor protocol
> save logs facility
> The save logs facility command adds the ability to save logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the save logs facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> save logs facility facility
> show aaa group name
> This command is used to view AAA statistics for the current context. The output of this command includes a new field “Fire-and-Forget” to display whether or not the Fire-And-Forget feature is enabled in the AAA Group configuration.
> CLI (Exec Mode)
> show aaa { group { all | name aaa_group_name } | local counters } [ | { grep grep_options | more } ]
> show active-charging analyzer statistics name pptp
> This command displays active charging protocol analyzer statistics for the PPTP analyzer. The output of this command includes the following new fields to display PPTP-GRE traffic statistics:

> l | ACS PPTP-GRE Session Stats

> l | Total Uplink Bytes

> l | Total Downlink Bytes

> l | Total Uplink Pkts

> l | Total Downlink Pkts

> CLI (Exec Mode)
> show active-charging analyzer statistics name sip [ verbose ] ] [ | { grep grep_options | more } ]
> show active-charging flows type p2p
> This command displays active charging protocol analyzer statistics for the PPTP analyzer. The following data transport protocols are added:

> l | (I) - ICMP and ICMPv6

> l | (G) - GREv1

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> show active-charging service all
> This command displays ACS service details. The output of this command includes the following new fields:

> l | Server Unreachable Failure-Handling

> l | Initial-Request

> l | Update-Request

> CLI (Exec Mode)
> show active-charging service { all | name service_name } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays active charging statistics for ACS sessions. The output of the following commands includes the new field “Current PPTP-GRE Sessions”.

> l | show active-charging sessions summary

> l | show active-charging sessions summary type p2p

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full
> This command displays active charging statistics for ACS sessions. The output of this command includes the following new field:

> l | Current PPTP-GRE Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full all
> This command displays ACS session statistics. The output of this command includes the following new fields:

> l | CCR-I Server Unreachable Handling

> l | CCR-U Server Unreachable Handling

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays active statistics for ACS sessions. The output of this command includes the following new fields:

> l | Total PPTP-GRE flows

> l | Current PPTP-GRE flows

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> show apn name
> This command is used to display configuration information for either a specific or all configured APNs. The output of this command includes the following new fields:

> l | Radius Secondary Group — to indicate the secondary Accounting group configured in the APN configuration.

> l | Accounting Policy Name — to indicate the name of accounting policy associated with the APN.

> CLI (Exec Mode)
> show apn { all | name apn_name } [ | { grep grep_options | more } ]
> show diameter route table
> This command displays the Diameter routing table. The output of this command has been modified to display the dynamic routes with a flag ‘D’.
> CLI (Exec Mode)
> show diameter route table [ wide ] [ endpoint endpoint_name ] [ | { grep grep_options | more } ]
> show diameter statistics
> This command displays the Diameter peer statistics. The output of this command includes the following new fields.

> l | Dynamic Route statistics

> l | Adds

> l | Add Failures

> l | Removes

> l | Hits

> l | Expires

> CLI (Exec Mode)
> show diameter statistics [ [ proxy ] | endpoint endpoint_name [ peer-host peer_id [ peer-realm realm_id ] ] ] [ | { grep grep_options | more } ]
> show dns-client
> The show dns-client command has two new query-type keywords in release 12.0: AAAA and NAPTR. These keywords filter DNS results based on 128-bit domain IPv6 addresses (AAAA resource records) or on Naming Authority Pointer records (NAPTR).
> CLI (Exec Mode)
> show dns-client { cache client name [ query-name name | query-type { A | AAAA | NAPTR | SRV } ] | statistics client name } [ | { grep grep_options | more } ]
> show gtpc statistics
> This command displays the GTPC statistics. The output of this command includes the following new fields:

> l | current-ipv4v6

> l | setup-ipv4v6

> l | dyn-ipv4v6

> CLI (Exec Mode)
> show gtpc statistics [ verbose ]
> show ims-authorization policy-control statistics server
> Displays information and statistics specific to the policy control in IP Multimedia Subsystem (IMS) authorization service. This command has been enhanced to display IPv6 address in addition to IPv4 address in Release 12.0.
> CLI (Exec Mode)
> show ims-authorization policy-control statistics [ service ims_auth_svc_name | server { ip-address ip_address [ port port_value ] | name server_name } ] [ | { grep grep_options | more } ]
> show logs facility
> The show logs facility command adds the ability to display logging outputs for the following seven facilities in release 12.0: callhome, epdg, lagmgr, phs, pppoe, testctrl, and testmgr.
> The following facility is no longer in the show logs facility command in release 12.0: event-notif.
> CLI (Exec Mode)
> show logs facility facility
> show session subsystem facility aaamgr
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes the following new fields to track the number of secondary accounting requests in the AAAMgr instance.

> l | Total radius sec acct requests

> l | Current radius sec acct requests

> l | Total radius sec acct cancelled

> l | Total radius sec acct purged

> l | Total radius sec acct requests retried

> CLI (Exec Mode)
> show session subsystem facility aaamgr { all | instance | verbose } [ | { grep grep_options | more } ]
> show srp
> This command displays the Service Redundancy Protocol information. The following keywords have been added to this command:

> l | active

> l | standby

> l | diameter

> CLI (Exec Mode)
> show srp { call-loss statistics | checkpoint statistics [ active | standby ] [ verbose ] | info | monitor [ all | authentication-probe | bgp | diameter ] | statistics } | [ grep grep_options | more ]
> show subscribers configuration username
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes a new field “Radius Secondary Group” to indicate the secondary Accounting group configured in the Subscriber configuration.
> CLI (Exec Mode)
> show subscribers configuration { all | username user_name } [ | { grep grep_options | more } ]
> show subscribers full all
> Shows information for subscriber sessions defined by the specified keywords. The output of this command includes a new field “AAA Radius Secondary group” to indicate the secondary Accounting group configured in the Subscriber configuration.
> CLI (Exec Mode)
> show subscribers full all [ | { grep grep_options | more } ]
> Common Commands - Modified in Release 12.2
> The following common commands have been modified in Release 12.2.
> clear active-charging ruledef statistics
> This command clears statistics for rule definitions configured in the Active Charging Service (ACS). The tpo option was added to this command, which enables to clear statistics for Traffic Performance Optimization (TPO) ruledefs configured in the ACS.
> CLI (Exec Mode)
> clear active-charging ruledef statistics [ charging | firewall | name ruledef_name | tpo ] [ | { grep grep_options | more } ]
> monitor protocol
> This command enters the system‘s protocol monitoring utility. The following protocols have been added to this utility:

> l | RTP (IMS)

> l | RTCP (IMS)

> CLI (Exec Mode)
> monitor protocol
> show active-charging ruledef
> This command displays information/statistics for rule definitions (ruledefs) configured in the Active Charging Service (ACS). The tpo option was added to this command, which enables to view information/statistics for all TPO ruledefs configured in the ACS.
> CLI (Exec Mode)
> show active-charging ruledef { all | charging | firewall | name ruledef_name | post-processing | routing | statistics [ all { charging | firewall [ wide ] | post-processing | tpo } | name ruledef_name [ wide ] ] | tpo } [ | { grep grep_options | more } ]
> show active-charging service all
> This command displays active charging protocol analyzer statistics for the PPTP analyzer. The output of this command includes the following new fields to display PPTP-GRE traffic statistics:

> l | MSISDN-Range-Mode

> l | MSISDN-Based End-Value

> l | MSISDN-Based Start-Value

> CLI (Exec Mode)
> show active-charging service { all | name acs_service_name } [ | { grep grep_options | more } ]
> show active-charging sessions full
> This command displays statistics for Active Charging Service (ACS) sessions. A new field "Backpressured" has been added to the output of this command to display backpressure condition in credit-control sessions.
> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging credit-control session-states
> This command displays statistics for Diameter/RADIUS Prepaid Credit Control Service in the Active Charging Service (ACS). A new field "Backpressured" has been added to the output of this command to display backpressure condition in credit-control sessions.
> CLI (Exec Mode)
> show active-charging credit-control { statistics [ all | group group_name ] | session-states [ rulebase rulebase_name ] [ content-id content_id ] } [ | { grep grep_options | more } ]
> show ims-authorization service statistics
> This command displays information, configuration, and statistics of all/specific IP Multimedia Subsystem (IMS) authorization service. A new counter "Resource Modification Req" has been added to the output of this command.
> CLI (Exec Mode)
> show ims-authorization service { { all [ verbose ] | name ims_auth_svc_name | summary ] } | { statistics [ all | name ims_auth_svc_name ] [ verbose ] } [ | { grep grep_options | more } ]
> show srp
> This command displays Service Redundancy Protocol (SRP) related information.
> The ability to display statistics of external audit has been added to this command.
> For Traffic Performance Optimization (TPO) ICSR support, the output of the following commands include the new field “tpo-policy-mapping-id failures”, which indicates the number of TPO policy ID mapping failures in the standby Session Manager.

> l | show srp checkpoint statistics

> l | show srp checkpoint statistics sessmgr [ all | instance ] — this is a hidden CLI command

> l | show srp checkpoint statistics standby verbose

> l | show srp checkpoint statistics standby debug-info verbose — this is a hidden CLI command

> CLI (Exec Mode)
> show srp { audit-statistics [ all | instance number ] [ message-level | session-level ] | call-loss statistics | checkpoint statistics [ active | standby ] [ verbose ] | info | monitor [ all | authentication-probe | bgp | diameter ] | statistics } | [ grep grep_options | more ]
> show task
> New memory keword. displays detailed task memory use information.
> CLI (Exec Mode)
> show task { info | memory | resources | table } [ card card_num ] [ facility
> facility { all | instance id } ] [ process process_name all ] [ max ] [ | { grep grep_options | more } ]
> Application Detection and Control Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging analyzer statistics
> This command supports the clearing of protocol analyzer statistics for the following P2P applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> clear active-charging charging-action statistics [ name string ] [ | { grep grep_options | more } ]
> show active-charging analyzer statistics name p2p verbose
> This command displays Active Charging protocol analyzer statistics for the P2P protocol analyzer. The output of this command includes the following new fields to display the uplink/downlink bytes and uplink/downlink packets for the following protocols:

> l | Blackberry

> l | Gmail

> l | iTunes

> l | MySpace

> l | TeamViewer

> l | Twitter

> l | Viber

> l | Yahoo-video

> l | Oscar-video

> l | Gtalk-video

> CLI (Exec Mode)
> show active-charging analyzer statistics name p2p [ verbose ] [ | { grep grep_options | more } ]
> show active-charging flows
> This command displays the information for the active charging flows. The P2P protocol type flows now support the following applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays statistics for ACS sessions. The P2P protocol type flows now support the following applications:

> l | blackberry

> l | gmail

> l | itunes

> l | myspace

> l | teamviewer

> l | twitter

> l | viber

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary
> This command displays statistics for specific active charging service sessions. The output of this command includes the following new fields:

> l | Current BLACKBERRY Sessions

> l | Current GMAIL Sessions

> l | Current ITUNES Sessions

> l | Current MYSPACE Sessions

> l | Current TEAMVIEWER Sessions

> l | Current TWITTER Sessions

> l | Current VIBER Sessions

> l | Current YAHOO Video Sessions

> l | Current OSCAR Video Sessions

> l | Current GTALK Video Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary type p2p
> This command displays summary information for P2P active charging service sessions. The output of this command includes the following new fields:

> l | Current BLACKBERRY Sessions

> l | Current GMAIL Sessions

> l | Current ITUNES Sessions

> l | Current MYSPACE Sessions

> l | Current TEAMVIEWER Sessions

> l | Current TWITTER Sessions

> l | Current VIBER Sessions

> l | Current YAHOO Video Sessions

> l | Current OSCAR Video Sessions

> l | Current GTALK Video Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Application Detection and Control Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2.
> clear active-charging analyzer statistics
> This command supports the clearing of protocol analyzer statistics for the following P2P applications:

> l | antsp2p

> l | imo

> l | mypeople

> l | netmotion

> l | ogg

> l | openvpn

> l | quicktime

> l | rdt

> l | scydo

> l | spotify

> l | tango

> l | tunnelvoice

> l | ultrabac

> l | usenet

> l | whatsapp

> CLI (Exec Mode)
> clear active-charging charging-action statistics [ name string ] [ | { grep grep_options | more } ]
> show active-charging analyzer statistics name p2p verbose
> This command displays Active Charging protocol analyzer statistics for the P2P protocol analyzer. The output of this command includes the following new fields to display the uplink/downlink bytes and uplink/downlink packets for the following protocols:

> l | AntsP2P

> l | IMO

> l | MyPeople

> l | Netmotion

> l | OGG

> l | OpenVPN

> l | Quicktime

> l | RDT

> l | Scydo

> l | Spotify

> l | Tango

> l | TunnelVoice

> l | Ultrabac

> l | Usenet

> l | WhatsApp

> CLI (Exec Mode)
> show active-charging analyzer statistics name p2p [ verbose ] [ | { grep grep_options | more } ]
> show active-charging flows
> This command displays the information for the active charging flows. The P2P protocol type flows now support the following applications:

> l | antsp2p

> l | imo

> l | mypeople

> l | netmotion

> l | ogg

> l | openvpn

> l | quicktime

> l | rdt

> l | scydo

> l | spotify

> l | tango

> l | tunnelvoice

> l | ultrabac

> l | usenet

> l | whatsapp

> CLI (Exec Mode)
> show active-charging flows { all | [ connected-time [ < | > | greater-than | less-than ] seconds ] [ flow-id flow_id ] [ full ] [ idle-time [ < | > | greater-than | less-than ] seconds ] [ ip-address [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] address ] [ nat { not-required | required [ nat-ip nat_ip_address ] } ] [ port-number [ server | subscriber ] [ < | > | IPv4 | greater-than | less-than ] number ] [ rx-bytes [ < | > | greater-than | less-than ] number ] [ rx-packets [ < | > | greater-than | less-than ] number ] [ session-id session_id ] [ summary ] [ trans-proto { icmp | tcp | udp } ] [ tx-bytes [ < | > | greater-than | less-than ] number ] [ tx-packets [ < | > | greater-than | less-than ] number ] [ type flow_type ] } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays statistics for ACS sessions. The P2P protocol type flows now support the following applications:

> l | antsp2p

> l | imo

> l | mypeople

> l | netmotion

> l | ogg

> l | openvpn

> l | quicktime

> l | rdt

> l | scydo

> l | spotify

> l | tango

> l | tunnelvoice

> l | ultrabac

> l | usenet

> l | whatsapp

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary
> This command displays statistics for specific active charging service sessions. The output of this command includes the following new fields:

> l | Current ANTSP2P Sessions

> l | Current IMO Sessions

> l | Current MYPEOPLE Sessions

> l | Current NETMOTION Sessions

> l | Current OGG Sessions

> l | Current OPENVPN Sessions

> l | Current QUICKTIME Sessions

> l | Current RDT Sessions

> l | Current SCYDO Sessions

> l | Current SPOTIFY Sessions

> l | Current TANGO Sessions

> l | Current TUNNELVOICE Sessions

> l | Current ULTRABAC Sessions

> l | Current USENET Sessions

> l | Current WHATSAPP Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions summary type p2p
> This command displays summary information for P2P active charging service sessions. The output of this command includes the following new fields:

> l | Current ANTSP2P Sessions

> l | Current IMO Sessions

> l | Current MYPEOPLE Sessions

> l | Current NETMOTION Sessions

> l | Current OGG Sessions

> l | Current OPENVPN Sessions

> l | Current QUICKTIME Sessions

> l | Current RDT Sessions

> l | Current SCYDO Sessions

> l | Current SPOTIFY Sessions

> l | Current TANGO Sessions

> l | Current TUNNELVOICE Sessions

> l | Current ULTRABAC Sessions

> l | Current USENET Sessions

> l | Current WHATSAPP Sessions

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> Content Filtering Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> ECS Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging tcp-proxy statistics
> This command clears TCP Proxy related statistics. The socket-migration keyword was added to this command. This enables to clear TCP Proxy Socket Migration related statistics.
> CLI (Exec Mode)
> clear active-charging tcp-proxy statistics [ all | ip-layer | rulebase rulebase_name | socket-migration | tcp-layer ]
> show active-charging flows full
> This command displays active-charging flow information. The output of this command now includes the following TCP Proxy Socket Migration related fields:

> l | Socket Migration Details:

> l | State

> l | Highest ACK Frm Server

> l | Highest Seq Frm Server

> l | Highest ACK Frm MS

> l | Highest Seq Frm MS

> l | Seq Frm MS at Mig

> l | ACK Frm MS at Mig

> l | Seq Frm Server at Mig

> l | ACK Frm Server at Mig

> l | Data To Be Delivered To MS

> l | Data To Be Delivered To Server

> l | Highest Seq Frm MS

> l | Timestamps Enabled

> l | SACK Enabled

> l | Wscale From MS

> l | Wscale From Server

> CLI (Exec Mode)
> show active-charging flows full
> show active-charging tcp-proxy statistics
> This command displays TCP Proxy related statistics. The socket-migration keyword was added to this command. This enables to view TCP Proxy statistics for socket migration.
> CLI (Exec Mode)
> show active-charging tcp-proxy statistics [ all | ip-layer | rulebase rulebase_name | socket-migration | tcp-layer ] [ verbose ] [ | { grep grep_options | more } ]
> ECS Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2.
> show active-charging service all
> This command displays detailed ACS service configuration information. The output of this command includes the following new counter:
> Selection of Charging-rule-base: If multiple Charging-Rule-Base-Name AVP are received from the PCRF, indicates which rulebase is selected and applied to the call, the first or the last rulebase.
> For more information, in the Configuration Management chapter see the policy-control charging-rule-base-name CLI command.
> CLI (Exec Mode)
> show active-charging service { all | name acs_service_name } [ | { grep grep_options | more } ]
> Firewall Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> clear active-charging firewall statistics
> This command clears Active Charging Firewall statistics. The following keywords were added to this command:

> l | icmpv6

> l | ipv6

> CLI (Exec Mode)
> clear active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ | { grep grep_options | more } ]
> clear subscribers
> This command disconnects subscribers based on specified criteria.The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> clear subscribers [ keywords ] [ verbose ] [ -noconfirm ]
> show active-charging firewall statistics
> This command displays Active Charging Firewall statistics. The following keywords were added to this command:

> l | icmpv6

> l | ipv6

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics verbose
> This command displays Active Charging Stateful Firewall statistics. The output of this command includes the following new ICMPv6 and IPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> l | IPv6 Stats:

> l | Land Attacks

> l | Jolt Attacks

> l | Teardrop Attacks

> l | Invalid IP Option Length

> l | IPv6 Source-router Attacks

> l | Packets with Short IPv6 Header Length

> l | Packets with Nested Fragmentation Header

> l | Packets with Unspecified IPv6 Address

> l | Packets with invalid Payload Length

> l | Packets with more than threshold Extension Headers

> l | Packets with invalid Hop By Hop Extension Header

> l | Packets with ICMPv4 in IPv6 Header

> l | Packets with invalid Destination Extension Header

> l | Downlink Dropped Bytes on IPv6 Reassembly Failure

> l | Uplink Dropped Bytes on IPv6 Reassembly Failure

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics callid <call_id> verbose
> This command displays Active Charging Stateful Firewall statistics with Call ID. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics domainname <domain_name> verbose
> This command displays Active Charging Stateful Firewall statistics with Domain name. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics username <user_name> verbose
> This command displays Active Charging Stateful Firewall statistics with Username. The output of this command includes the following new ICMPv6 statistics:

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics protocol icmpv6 verbose
> This command displays Active Charging Stateful Firewall statistics for ICMPv6 protocol. The output of this command includes the following new ICMPv6 statistics:

> l | Firewall Statistics for Protocol: ICMPv6

> l | ICMPv6 Stats:

> l | Invalid ICMPv6 Response

> l | ICMPv6 Reply Error

> l | Invalid ICMPv6 Type Packet

> l | ICMPv6 Error Message Replay Attacks

> l | ICMPv6 Packets with Duplicate Sequence Number

> l | Packets with Short ICMPv6 Header Length

> l | Invalid ICMPv6 Packet Length

> l | Packets Dropped on ICMPv6 Flood Attack

> l | Ping Of Death Attacks

> l | Packets Dropped due to ICMPv6 Checksum Errors

> l | ICMPv6 Packets With Destination Unreachable Message

> l | ICMPv6 Echo Packets Dropped due to ID Zero

> l | Data Stats:

> l | Total Packets Received

> l | Total Bytes Received

> l | Total Packets Sent

> l | Total Bytes Sent

> l | Total Packets Injected

> l | Total Bytes Injected

> l | Uplink Packets Dropped

> l | Uplink Bytes Dropped

> l | Downlink Packets Dropped

> l | Downlink Bytes Dropped

> l | Total Malformed Packets

> l | Total DOS Attacks

> l | Total Flows Processed by Firewall

> l | Total NAT Flows Processed by Firewall

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging firewall statistics protocol ipv6 verbose
> This command displays Active Charging Stateful Firewall statistics for IPv6 protocol. The output of this command includes the following new IPv6 statistics:

> l | Firewall Statistics for Protocol: IPv6

> l | IPv6 Stats:

> l | Land Attacks

> l | Jolt Attacks

> l | Teardrop Attacks

> l | Invalid IP Option Length

> l | IPv6 Source-router Attacks

> l | Packets with Short IPv6 Header Length

> l | Packets with Nested Fragmentation Header

> l | Packets with Unspecified IPv6 Address

> l | Packets with invalid Payload Length

> l | Packets with more than threshold Extension Headers

> l | Packets with invalid Hop By Hop Extension Header

> l | Packets with ICMPv4 in IPv6 Header

> l | Packets with invalid Destination Extension Header

> l | Downlink Dropped Bytes on IPv6 Reassembly Failure

> l | Uplink Dropped Bytes on IPv6 Reassembly Failure

> l | Data Stats:

> l | Total Packets Received

> l | Total Bytes Received

> l | Total Packets Sent

> l | Total Bytes Sent

> l | Total Packets Injected

> l | Total Bytes Injected

> l | Uplink Packets Dropped

> l | Uplink Bytes Dropped

> l | Downlink Packets Dropped

> l | Downlink Bytes Dropped

> l | Total Malformed Packets

> l | Total DOS Attacks

> l | Total Flows Processed by Firewall

> l | Total NAT Flows Processed by Firewall

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging fw-and-nat policy name
> This command displays Firewall-and-NAT Policy information. The output of this command includes the following new fields:

> l | IPv6 Extension Headers Limit

> l | IPv6 Hop By Hop Options

> l | Hop By Hop Router Alert Option

> l | Hop By Hop Jumbo Payload Option

> l | Invalid Hop By Hop Options

> l | Unknown Hop By Hop Options

> l | IPv6 Destination Options

> l | Invalid Destination Options

> l | Unknown Destination Options

> l | IPv6 Nested Fragmentation

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy_name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> show active-charging fw-and-nat policy name
> This command displays Firewall-and-NAT Policy information. The output of this command includes the following new fields:

> l | Firewall Status IPv4

> l | Firewall Status IPv6

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy_name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> show active-charging sessions
> This command displays statistics for ACS sessions. The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays service and configuration counters for the active charging service. The output of this command includes the following new fields:

> l | Firewall IPv4

> l | Firewall IPv6

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> show subscribers
> This command displays all available subscriber information. The following keywords were added to this command:

> l | ipv4

> l | ipv6

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> show subscribers full
> This command displays all available subscriber information. The output of this command includes the following new fields:

> l | Firewall-and-Nat Policy

> l | Firewall Policy IPv4

> l | Firewall Policy IPv6

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> GGSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> show dhcp-service
> This command displays the service and configuration counters for a DHCP service. The output of this command includes following new field:

> l | DHCP chaddr validation

> CLI (Exec Mode)
> show dhcp-service name [ service_name ]
> GGSN Commands - Modified in Release 12.2
> show apn name
> This command displays the service and configuration statistics for an APN. The output of this command now includes following new field:

> l | radius returned-username

> Under the APN configuration, this option is to either use the username sent by RADIUS in Access-Accept or send the constructed username itself in the RADIUS Acct messages.
> CLI (Exec Mode)
> show apn name [ apn_name ]
> show gtpu-service
> This command displays configuration information for GPRS Tunneling Protocol user plane (GTP-U) services. The output of this command now includes following new field:

> l | Sequence Number

> HA Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release
> HA Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.0.
> None for this release.
> HSGW Commands - Modified in Release 12.0
> The following HSGW commands have been modified in Release 12.0.
> show apn name
> This command displays the service and configuration statistics for an APN. The output of this command now includes the following new field:

> l | Accounting Policy Name

> Under the APN configuration, this option is used to associate an accounting policy.
> CLI (Exec Mode)
> show apn name [ apn_name ]
> clear hsgw-service
> The keyword all has been removed from this command.
> CLI (Exec Mode)
> clear hsgw-service statistics [ name service_name ] [ | { grep grep_options | more } ]
> show hsgw-service
> The keywords statistics and pcf-status have been added to this command.
> CLI (Exec Mode)
> show hsgw-service { all | name service_name | statistics { all | name service _name } } [ pcf-status [ address IPv4_address | filter { all | icmp-monitored | no-calls | summary | up } ] [ | { grep grep_options | more } ]
> show mag-service
> The keyword ip-address has been added to this command.
> CLI (Exec Mode)
> show mag-service { all | name service_name | session [ all | callid id | counters | full | ip-address home_ip_address | msid id | summary | username name ] | statistics [ name service_name ] } [ | { grep grep_options | more } ]
> HSGW Commands - Modified in Release 12.2
> The following HSGW commands have been modified in Release 12.2.
> show gtpu-service
> This command displays configuration information for GPRS Tunneling Protocol user plane (GTP-U) services. The output of this command now includes following new field:

> l | Sequence Number

> show mag-service
> This command displays statistic and counter information for Mobile Access Gateway (MAG) services. The output of this command now includes the following new field:

> l | IPv6 Traffic

> This field displays if IPv6 Traffic is Disabled.
> CLI (Exec Mode)
> show mag-service session full
> show subscribers
> This command displays information for subscriber sessions. The output of this command now includes the following new field:

> l | IPv6 Traffic

> This field displays if IPv6 Traffic is Disabled.
> CLI (Exec Mode)
> show subscribers full (HSGW call)
> IPCF Commands - Modified in Release 12.1
> This section provides information on modified IPCF commands in Release 12.1.
> IPCF is new product for this release.
> Mobility Management Entity Commands - Modified in Release 12.0
> The following Mobility Management Entity (MME) commands are modified in Release 12.0.
> show mme-service
> The following commands have been enhanced to include the ipsec keyword option.
> CLI (Exec Mode)
> show mme-service enodeb-association [ summary | full ] [ all | ipsec | mme-service-name mme_svc_name | peer-address peer_ip_address | peer-id peer_identifier ] [ | { grep grep_options | more } ]
> show mme-service session [ summary | full | counters ] [ all | call-id call_identifier | imei imei_id | imsi imsi_id | ipsec | mme-service service_name | msisdn number | pdn-address pdn_ip_address | s1-peer s1_peer_ip_address | s11- peer s11_peer_ip_address | ue-ecm-state { connected | idle } ] [ | { grep grep_options | more } ]
> show mme-service session full
> This command no longer includes the following fields showing authentication information about the session.

> l | Authentication Information

> l | RAND: Random Number

> l | XRES: Expected Response

> l | K-ASM: Key-Authentication Security Model

> l | AUTN: Authentication Token

> CLI (Exec Mode)
> show mme-service session full
> show mme-service db record imsi
> This command no longer displays the following fields showing authentication information.

> l | Security Context

> l | Auth Status

> l | Security Context Type

> l | Ciphering Algo

> l | Integrity Algo

> l | NAS Count

> l | NAS Overflow

> l | NAS Integrity Key

> l | NAS Ciphering Key

> CLI (Exec Mode)
> show mme-service db record imsi <imsi>
> Mobility Management Entity Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2.
> show mme-service session
> This command now includes an option to filter the results based on Visitor Location Register (VLR) name.
> CLI (Exec Mode)
> show mme-service session full vlr-name <vlr_name>
> show mme-service session vlr-name <imsi>
> show egtpc sessions
> The output of this command is now fully documented.
> CLI (Exec Mode)
> show egtpc sessions
> show egtpc statistics verbose
> This command has been enhanced to include 3GPP 29.274 and SRVCC statistics.
> CLI (Exec Mode)
> show egtpc statistics verbose
> show mme-service statistics verbose
> This command has been enhanced as follows:

> l | Add “Identity Response” under Total EMM Control Messages -Received

> l | Add “Deactivate Bearer Accepts” under Total ESM Control Messages - Sent

> l | Remove invalid EMM counters: Detach Request 0 IMSI Detach and TAU Reject - ESM Failure

> l | Remove invalid ESM counter: PDN Disconnect reject - Rejected By PGW/SGW.

> CLI (Exec Mode)
> show mme-service statistics verbose
> NAT Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> show active-charging sessions full
> This command displays statistics for ACS sessions. The output of this command includes the following new field:

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full all
> This command displays statistics for ACS sessions. The output of this command includes the following new field:

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging subsystem all
> This command displays service and configuration counters for the active charging service. The output of this command includes the following new fields:

> l | Total H323 Flows

> l | Current H323 Flows

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> NAT Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2.
> show active-charging firewall statistics verbose
> This command displays Active Charging Stateful Firewall statistics. The output of this command includes the following new fields:

> l | Packets dropped due to NAT Translation failed on unsupported ICMP code

> l | Packets dropped due to NAT Translation failed on invalid Param Problem

> l | Packets dropped due to IPv6 routing header with non-zero segments left

> l | Packets dropped due to Unsupported Embedded IPv4 Address

> l | Packets dropped due to Destination IPv6 Prefix Mismatch

> l | Total Packets (NAT64 Translation)

> l | Total Bytes Reduced (NAT64 Translation)

> l | Total NAT44 Flows Processed by Firewall

> l | Total NAT64 Flows Processed by Firewall

> l | Total Bypass-NAT Flows Processed by Firewall

> l | Total Bypass-NAT IPv4 Flows Processed by Firewall

> l | Total Bypass-NAT IPv6 Flows Processed by Firewall

> CLI (Exec Mode)
> show active-charging firewall statistics [ callid call_id | domain-name domain_name | nat-realm nat_realm | protocol { icmp | icmpv6 | ip | ipv6 | other | tcp | udp } | username user_name ] [ acsmgr instance instance_id ] [ verbose ] [ | { grep grep_options | more } ]
> show active-charging fw-and-nat policy name
> This command displays Firewall-and-NAT Policy information. The output of this command includes the following new fields:

> l | NAT Status NAT44

> l | NAT Status NAT64

> l | ICSR Flow-recovery Status

> l | Non-ALG

> l | SIP-ALG

> l | H323-ALG

> CLI (Exec Mode)
> show active-charging fw-and-nat policy { { { all | name fw_nat_policy name } [ service name acs_service_name ] } | { statistics { all | name fw_nat_policy_name } } } [ | { grep grep_options | more } ]
> show active-charging nat statistics
> This command displays NAT realm statistics. The output of this command includes the following new fields:

> l | NAT44 flows denied IP

> l | NAT44 flows denied port

> l | NAT64 flows denied IP

> l | NAT64 flows denied port

> l | NAT44 bytes Transferred

> l | NAT44 flows processed

> l | NAT64 bytes Transferred

> l | NAT64 flows processed

> CLI (Exec Mode)
> show active-charging nat statistics [ nat-realm nat_realm [ summary ] ] [ | { grep grep_options | more } ]
> show active-charging sessions full
> This command displays statistics for ACS sessions. The output of this command includes the following new fields:

> l | NAT Policy NAT44

> l | NAT Policy NAT64

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions full all
> This command displays statistics for ACS sessions. The output of this command includes the following new fields:

> l | NAT Policy NAT44

> l | NAT Policy NAT64

> CLI (Exec Mode)
> show active-charging sessions [ full [ wide ] | summary | display-dynamic-charging-rules | dynamic-charging ] { [ all ] | [ filter_keyword ] + } [ | { grep grep_options | more } ]
> show active-charging sessions nat
> This command displays statistics for ACS sessions. The following keywords are added to this command to display active-charging sessions for which NAT44/NAT64 processing is required:

> l | ipv6

> l | ipv6

> CLI (Exec Mode)
> show active-charging sessions nat { not-required | required [ nat-realm nat_realm ] } [ ipv4 | ipv6 ]
> show active-charging subsystem all
> This command displays service and configuration counters for the active charging service. The output of this command includes the following new fields:

> l | NAT44 Enabled

> l | NAT64 Enabled

> CLI (Exec Mode)
> show active-charging subsystem { all | facility acsmgr { all | instance instance_value } [ rulebase name rulebase_name ] | sip } [ | { grep grep_options | more } ]
> show configuration
> Displays current configuration information for the card, context, port, or target configuration file as specified. The output of this command includes the following new field for non default configuration:

> l | nat icsr-flow-recovery

> CLI (Exec Mode)
> show configuration [ card card_name | context context_name [ radius group [ all | name group ] ] | port slot/port | srp ] [ showsecrets ] [ url url ] [ verbose ] [ | { grep grep_options | more } ]
> show configuration verbose
> Displays current configuration information for the card, context, port, or target configuration file as specified. The output of this command includes the following new field for default configuration:

> l | no nat icsr-flow-recovery

> CLI (Exec Mode)
> show configuration [ card card_name | context context_name [ radius group [ all | name group ] ] | port slot/port | srp ] [ showsecrets ] [ url url ] [ verbose ] [ | { grep grep_options | more } ]
> show subscribers nat
> This command displays all available subscriber information. The following keywords are added to this command to display subscribers for whom NAT44/NAT64 processing is required:

> l | ipv6

> l | ipv6

> CLI (Exec Mode)
> show subscribers nat { not-required | required [ nat-ip nat_ip_address | nat-realm nat_realm ] } [ ipv4 | ipv6 ]
> show subscribers full
> This command displays all available subscriber information. The output of this command includes the following new fields:

> l | NAT Policy NAT44

> l | NAT Policy NAT64

> CLI (Exec Mode)
> show subscribers [ command_keyword ] [ filter_keywords ] [ | { grep grep_options | more } ]
> Packet Data Network Gateway Commands - Modified in Release 12.0
> The following P-GW commands have been modified in Release 12.0.
> clear apn statistics
> The keyword smgr-instance has been added to this command.
> CLI (Exec Mode)
> clear apn statistics [ name apn_name | smgr-instance instance ] [ | { grep grep_options | more } ]
> clear pgw-service
> The keyword all has been removed from this command.
> CLI (Exec Mode)
> clear pgw-service statistics [ name service_name ] [ | { grep grep_options | more } ]
> show apn name
> This command displays the service and configuration statistics for an APN. The output of this command now includes the following new field:

> l | Accounting Policy Name

> Under the APN configuration, this option is used to associate an accounting policy.
> CLI (Exec Mode)
> show apn name [ apn_name ]
> show crypto ipsec security-associations
> The output of this command now includes the Diffie-Hellman group for each IPSec security association.
> CLI (Exec Mode)
> show crypto ipsec security-associations
> show pgw-service
> The keyword verbose has been added to this command.
> CLI (Exec Mode)
> show pgw-service { all | name service_name | statistics { all | name service_name } [ verbose ] } [ | { grep grep_options | more } ]
> Packet Data Network Gateway Commands - Modified in Release 12.2
> The following P-GW commands have been modified in Release 12.2.
> show active-charging credit-control
> This command displays statistics for Diameter/RADIUS Prepaid Credit Control Service in the Active Charging Service (ACS). The output of this command now includes the following new row:

> l | Backpressured

> This row specifies the number of sessions in backpressured state and the number of categories that are blacklisted.
> CLI (Exec Mode)
> show active-charging credit-control sessions-states
> show active-charging sessions
> This command displays statistics for Active Charging Service (ACS) sessions. The output of this command now includes the following new field:

> l | Backpressured

> This value shows how many times the category was subsequently moving into backpressured state (unable to send message due to message queue being full) while sending a CCR-U out. Maximum value is 15.
> If this field is not displayed, the category is currently not in backpressured state.
> CLI (Exec Mode)
> show active-charging sessions full
> show apn name
> This command displays the service and configuration statistics for an APN. The output of this command now includes the following new field:

> l | radius returned-username

> Under the APN configuration, this option is to either use the username sent by RADIUS in Access-Accept or send the constructed username itself in the RADIUS Acct messages.
> CLI (Exec Mode)
> show apn name [ apn_name ]
> show gtpu-service
> This command displays configuration information for GPRS Tunneling Protocol user plane (GTP-U) services. The output of this command now includes following new field:

> l | Sequence Number

> show lma-service
> This command displays statistic and counter information for Local Mobility Anchor (LMA) services. The output of this command now includes the following new field:

> l | IPv6 Traffic

> This field displays if IPv6 Traffic is Disabled.
> CLI (Exec Mode)
> show lma-service session full
> show subscribers
> This command displays information for subscriber sessions. The output of this command now includes the following new field:

> l | IPv6 Traffic

> This field displays if IPv6 Traffic is Disabled.
> CLI (Exec Mode)
> show subscribers full (P-GW call)
> PDIF Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> PDSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> show active-charging sessions full all
> The following keyword has been added to the command.

> l | full all

> CLI (Config Mode)
> show active charging sessions full all.
> PDSN Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.0.
> None for this release.
> Serving Gateway Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2.
> show egtp statistics verbose
> The output of the show egtpc statistics verbose command now includes detailed rejection statistics for the following call request/response/notification denials [3GPP Release 9, 29.274]:

> l | Reject Statistics

> l | Modify Bearer Request Denied

> l | Delete Bearer Request Denied

> l | Delete Session Request Denied

> l | Downlink Data Notification Denied

> l | Release Access Bearers Denied

> l | Create Bearer Denied

> l | Update Bearer Denied

> l | Delete Bearer Command Denied

> l | Modify Bearer Command Denied

> l | Bearer Resource Command Denied

> l | Create Indirect Data Forwarding Tunnel Request Denied

> l | Delete Indirect Data Forwarding Tunnel Request Denied

> l | Change Notification Request Denied

> l | Context Request Denied

> l | Context Response Denied

> l | Identification Request Denied

> l | Forward Relocation Request Denied

> l | Forward Access Context Notification Denied

> l | Forward Relocation Complete Notification Denied

> l | Relocation Cancel Request Denied

> l | Suspend Notification Denied

> l | Resume Notification Denied

> CLI (Exec Mode)
> show egtp statististics verbose
> show gtpu-service
> This command displays configuration information for GPRS Tunneling Protocol user plane (GTP-U) services. The output of this command now includes following new field:

> l | Sequence Number

> show sgw-service
> The output of the show sgw-service command now displays the currently configured Accounting Mode.
> CLI (Exec Mode)
> show sgw-service [ all | name sgw_srv_name ]
> Session Control Manager Commands - Modified in Release 12.0
> The following SCM commands have been modified in Release 12.0.
> show cscf tcp
> The keywords msrp and sip have been added to this command.
> CLI (Exec Mode)
> show cscf tcp connections service service_name [ facility { cscfmgr | sessmgr } ] [ full ] [ msrp ] [ remote-ip ip_address ] [ remote-port port_number ] [ sip ] [ | { grep grep_options | more } ]
> Session Control Manager Commands - Modified in Release 12.2
> The following SCM commands have been modified in Release 12.2.
> clear crypto statistics
> This command can now clear statistics for SRTP (Secure Real-time Transport Protocol).
> CLI (Exec Mode)
> clear crypto { isakmp [ tag map_name | peer peer_ip ] | security-association { counters tag map_name [ tx | rx ] | tag map_name | peer peer_ip } | statistics { ikev2 | ipsec-3gpp-cscf | srtp } [ service-ip-address ip_address | service-name service_name ] }
> show crypto statistics
> This command can now display SRTP (Secure Real-time Transport Protocol) statistics.
> CLI (Exec Mode)
> show crypto statistics ikev1 | ikev2 [ service-ip-address ip_address ] [ service-name service_name ] | ipsec-3gpp-cscf [ service-ip-address ip_address ] [ service-name service_name ] | srtp [ service-ip-address ip_address ] [ service-name service_name ]
> show cscf service
> This command displays configuration and/or statistic information for Call Session Control Function (CSCF) services on this system. The output of this command includes the following new fields to to show additional statistics pertaining to AAR sent for INV, 18X and 2XX separately:

> l | DPECA Message Stats:

> l | Messages Sent

> l | AAR-Invite

> l | AAR-18X

> l | AAR-2XX

> l | DPECA Message Stats:

> l | Messages Received

> l | AAA-INVITE

> l | AAR-18X

> l | AAR-2XX

> CLI (Exec Mode)
> show cscf service diameter policy-control statistics service-name <service_name>
> show subscribers cscf-only
> This command displays information for Call Session Control Function (CSCF) subscribers only. The output of this command now includes the field Private User ID.
> CLI (Exec Mode)
> show subscribers cscf-only full
> [local]asr5000# show subscribers cscf-only full
> AoR: userA@192.208.2.11:5060 callid: 00004e21
> User-Agent: LGT-client/VT1.5 + MIM 1.0 SPH-W8350
> Private User ID: userAP@192.208.2.11
> I-Path: n/a
> show subscribers summary
> This command displays information for subscriber sessions. The output of this command now includes the following new fields:

> l | cscf-sip-v4

> l | cscf-sip-v6

> l | cscf-access-wifi

> l | cscf-access-evdo

> l | cscf-access-wcdma

> l | cscf-access-ehrpd

> l | cscf-ue-ims

> l | cscf-ue-nonims

> l | cscf-sip-pcscf

> l | cscf-sip-scscf

> l | cscf-sip-rfc3261

> l | cscf-access-wired

> l | cscf-access-1xcdma

> l | cscf-access-lte

> l | cscf-access-undetermined

> l | cscf-security-ipsec

> l | cscf-security-tls

> These fields provide the IPv4/v6 subscriber count per PSC
> CLI (Exec Mode)
> show subscribers summary
> show subscribers summary cscf-service
> This command displays information for cscf subscriber sessions. The output of this command now includes the following new fields:

> l | No of IPv4 subscribers : 1

> l | No of IPv6 subscribers : 0

> l | No of PCSCF subscribers : 1

> l | No of SCSCF subscribers : 0

> l | No of RFC3261 subscribers :0

> l | No of WiFi subscribers : 0

> l | No of Wired subscribers : 1

> l | No of EvDO subscribers : 0

> l | No of WCDMA subscribers : 0

> l | No of 1xCDMA subscribers : 0

> l | No of LTE subscribers : 0

> l | No of EHRPD subscribers : 0

> l | No of undetermined access subscribers : 0

> l | No of IMS subscribers : 1

> l | No of non-IMS subscribers: 0

> l | No of IPSec subscribers : 0

> l | No of TLS subscribers : 0

> l | No of Domain cisco1.com subscribers : 1

> These fields provide the IPv4/v6 subscriber count per PSC
> CLI (Exec Mode)
> show subscribers summary cscf-service cscf_service
> SGSN Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0 - unless otherwise indicated, the listed fields have been added to the output displays:
> show apn-profile full name <profile_name>

> l | APN Name

> l | Quality of Service Capping

> l | Prefer Type

> l | Traffic Class

> l | SDU delivery order

> l | Delivery Of Erroneous Sdus

> l | Convert Max Bit Rate Uplink From

> l | Convert Max Bit Rate Downlink From

> l | SDU Max Size

> l | DNS Extension with LAC-RAC

> show apn-remap-table full name

> l | Fallback APN to use when Default APN not present in subscription

> show bssgp statistics

> l | packets dropped due to clearing subscriber

> show bulkstats
> A keyword has been added to the command to display the DLCI utilization variables.
> CLI (Exec Mode)
> show bulkstat variables dlci-util
> show call-control-profile full all

> l | PTMSI-Signature-Realloc Attach Access-Type

> l | PTMSI-Signature-Realloc Attach Frequency value UMTS

> l | PTMSI-Signature-Realloc Attach Frequency value GPRS

> l | PTMSI-Signature-Realloc Interval Access-Type

> l | PTMSI-Signature-Realloc Interval value UMTS

> l | PTMSI-Signature-Realloc Interval value GPRS

> l | PTMSI-Signature-Realloc Frequency Access-Type

> l | PTMSI-Signature-Realloc Frequency value UMTS

> l | PTMSI-Signature-Realloc Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU(Generic)Access-Type

> l | PTMSI-Signature-Realloc RAU(Generic) Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU(Generic) Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Periodic Access-Type

> l | PTMSI-Signature-Realloc RAU Periodic Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Periodic Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU RA Update Access-Type

> l | PTMSI-Signature-Realloc RAU RA Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU RA Update Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Combined Update Access-Type

> l | PTMSI-Signature-Realloc RAU Combined Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Combined Update Frequency value GPRS

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Access-Type

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value UMTS

> l | PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value GPRS

> l | Authentication SMS

> l | Authentication SMS Access-Type

> l | Authentication SMS Frequency

> l | Authentication SMS (MO-SMS)

> l | Authentication SMS (MO-SMS) Access-Type

> l | Authentication SMS (MO-SMS) Frequency

> l | Authentication SMS (MT-SMS)

> l | Authentication SMS (MT-SMS) Access-Type

> l | Authentication SMS (MT-SMS) Frequency

> show configuration

> l | gmm-message attach-with-tlli-in-use discard-message

> l | old-tlli invalidate tlli <hex>

> l | old-tlli invalidate tlli <hex>

> l | old-tlli hold-time <seconds>

> show gmm-sm statistics verbose

> l | 2G-Failure due to Internal Error:

> l | IMEI black listed:

> l | APP Init Abort:

> l | Identity Send Failed:

> l | Page-Requests-Per-LA:

> l | Ret-Page-Requests-Per-LA:

> l | Page-Requests-Per-RA:

> l | Ret-Page-Requests-Per-RA:

> l | CAMEL Subscription Ignored:

> l | Modify-Request Abort:

> l | 3G-Modify-Request Abort:

> l | 2G-Modify-Request Abort:

> l | irat-att-dsd-rcvd-in-2g

> l | irat-att-cl-sub-in-2g

> l | pac-drop-att-rau-ongoing

> l | ActivateContextRequest

> l | Total-Actv-Request

> l | 3G-Actv-Request

> l | 2G-ActvRequest

> l | Primary-Actv-Request

> l | 3G-Primary-Actv-Request

> l | 2G-Primary-Actv-Request

> l | Secondary-Actv-Request

> l | 3G-Secondary-Actv-Request

> l | 2G-Secondary-Actv-Request

> l | Actv-Request-Nrpca

> l | Actv-Request-Mbms

> l | ActivateContextAccept

> l | Total-Actv-Accept

> l | 3G-Actv-Accept

> l | 2G-ActvAccept

> l | Primary-Actv-Accept

> l | 3G-Primary-Actv-Accept

> l | 2G-Primary-Actv-Accept

> l | Secondary-Actv-Accept

> l | 3G-Secondary-Actv-Accept

> l | 2G-Secondary-Actv-Accept

> l | Actv-Mbms-Accept

> l | 3G-Actv-Mbms-Accept

> l | ActivateContextReject

> l | Total-Actv-Reject

> l | 3G-Actv-Reject

> l | 2G-Actv-Reject

> l | Primary-Actv-Reject

> l | 3G-Primary-Actv-Reject

> l | 2G-Primary-Actv-Reject

> l | Secondary-Actv-Reject

> l | 3G-Secondary-Actv-Reject

> l | 2G-Secondary-Actv-Reject

> l | RequestPdpContextActivationReject

> l | Total-Request-Pdp-Ctxt-Reject

> l | 3G-Request-Pdp-Ctxt-Reject

> l | 2G-Request-Pdp-Ctxt-Reject

> The following counters have been obsoleted and removed from the output display:

> l | Local Tlli

> l | IMSI Attach For SMID

> l | SMID SLIST Insert Failed

> l | CLP or SMID not found

> l | Incorrect State(Intra RAU)

> l | Incorrect State(Detached)

> The following counters are new network-sharing counters for attach reject cause:

> l | Redirection Indication:

> l | PLMN not allowed:

> l | Location area not allowed

> l | Tot-Attach-Rej:

> l | Tot-Attach-Rej:

> l | Attach-Gprs:

> l | Attach-Gprs:

> l | Attach-Comb:

> l | Attach-Comb:

> l | Tot-Rau-Rej:

> l | Tot-Rau-Rej:

> l | Rau-Periodic:

> l | Rau-Periodic:

> l | Rau-Intra-SGSN:

> l | Rau-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Inter-Rat:

> l | Rau-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Inter-Serv:

> l | Rau-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Tot-Serv-Rej:

> l | Tot-Serv-Rej:

> l | Roaming not allowed in LA:

> l | No GPRS services in PLMN:

> l | Tot-Attach-Rej:

> l | Tot-Attach-Rej:

> l | Attach-Gprs:

> l | Attach-Gprs:

> l | Attach-Comb:

> l | Attach-Comb:

> l | Tot-Rau-Rej:

> l | Tot-Rau-Rej:

> l | Rau-Periodic:

> l | Rau-Periodic:

> l | Rau-Intra-SGSN:

> l | Rau-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Inter-Rat:

> l | Rau-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Inter-Serv:

> l | Rau-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Tot-Serv-Rej:

> l | Tot-Serv-Rej:

> l | CS/PS co-ord required:

> l | Unknown Reasons:

> l | Tot-Attach-Rej:

> l | Tot-Attach-Rej:

> l | Attach-Gprs:

> l | Attach-Gprs:

> l | Attach-Comb:

> l | Attach-Comb:

> l | Tot-Rau-Rej:

> l | Tot-Rau-Rej:

> l | Rau-Periodic:

> l | Rau-Periodic:

> l | Rau-Intra-SGSN:

> l | Rau-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Comb-Intra-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Comb-Inter-SGSN:

> l | Rau-Inter-Rat:

> l | Rau-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Comb-Inter-Rat:

> l | Rau-Inter-Serv:

> l | Rau-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Rau-Comb-Inter-Serv:

> l | Tot-Serv-Rej:

> l | Tot-Serv-Rej:

> show gprsns statistics

> l | Number of ns-block dropped due to invalid nsvc

> l | Number of ns-block-ack dropped due to invalid nsvc

> l | Number of ns-status dropped due to invalid nsvc

> show gprs-service
> The following field has been removed as it is not configurable:

> l | GMM LLC MAX Retries

> show gprs-service all
> The following fields have been added in a GMM Message Handler display:

> l | Procedure

> l | Condition

> l | Action

> show linecard
> A keyword has been added to the command to display the DLCI utilization counters for a specific card.
> CLI (Exec Mode)
> show linecard dlci-utilization <card#>
> show linecard dlci-utilizaton
> The following utilization counters have been added to this new display output:

> l | Port

> l | Path

> l | E1T1

> l | TS

> l | DLCI

> l | NSE

> l | NSVC

> l | Average DLCI Utilization

> l | Current Rx

> l | Current Tx

> l | 5 min Rx

> l | 5 min Tx

> l | 15 min Rx

> l | 15 min Tx

> show linkmgr all parser statistics
> New keyword, sgsn-empty-cr, has been added to display statistics supporting the handling of empty SCCP CRs.
> CLI (Exec Mode)
> show linkmgr { all | instance <> } parser statistics sgsn-empty-cr
> The following new counters have been added for this new display output:

> l | SGSN Empty-Cr Statistics

> l | Empty-Cr sent to Imsimgr : 4

> l | Msg from Peer

> l | Released Rcvd :

> l | Rel Complete Rcvd :

> l | Inactivity Rcvd :

> l | Error Rcvd :

> l | DT1 Rcvd :

> l | DT1 DLR Modify :

> l | DT1 Decode attempt :

> l | Ranap Decode

> l | Init-UE Rcvd :

> l | Other Rcvd :

> l | Gmm Decode

> l | Gmm Rcvd :

> l | Attach Rcvd :

> l | Rau Rcvd :

> l | Detach Rcvd :

> l | Service Req Rcvd :

> l | Decoded DT1 msg

> l | Rau (Non-Local Old RAI):

> l | Rau (Local Old RAI) :

> l | Rau(LOR) diff Inst :

> l | Rau (LOR) Same Inst :

> l | Service/Detach Req :

> l | Serv/Detach diff Inst :

> l | Serv/Detach Same Inst :

> l | DT1 to be Fwd on Host cc :

> l | Msg to Donor Smgr

> l | Freezed Sent :

> l | Msg to Host Smgr

> l | CR Sent :

> l | Msg from Donor Smgr

> l | CC Rcvd :

> l | CREF Rcvd :

> l | Released Rcvd :

> l | Rel Complete Rcvd :

> l | Inactivity Rcvd :

> l | Error Rcvd :

> l | DT1 Rcvd :

> l | Others :

> l | Msg from Host Smgr

> l | CC Rcvd :

> l | CREF Rcvd :

> l | Released Rcvd :

> l | Rel Complete Rcvd :

> l | Inactivity Rcvd :

> l | Error Rcvd :

> l | DT1 Rcvd :

> l | Others :

> l | Local Purge :

> l | Failures

> l | CR Excess Len (>24) :

> l | Mem alloc fail Cb :

> l | Cb List insert fail :

> l | Duplicate Connection :

> l | DLR mdfy Buff Rem Fail :

> l | DLR mdfy Buff Add Fail:

> l | Lmgr UDatInd Fail :

> l | Lmgr Empty-cr Cb release reason

> l | Attach Request :

> l | Rau(Non local Old RAI):

> l | Rau (LOR)Same Inst :

> l | Serv/Detach Same Inst :

> l | Rel Complete from Peer :

> l | Rel Complete Local :

> l | Local Purge :

> l | CRef from Donor smgr :

> l | CRef from Host smgr :

> l | Guard timer Exp :

> l | Recovery :

> l | Others :

> show linkmgr { all | instance <>} parser statistics memory

> l | SGSN-EMPCR entry

> Enter the following modified CLI to dump empty-cr detail for a particular Session Manager associated with a specified LinkMgr:
> show sgsn linkmgr instance <1-4> sgsn-empty-cr [ donor smgr-instance <1-384> | host smgr-instance <1-384> ]
> show session disconnect-reasons
> The following SGSN-supported session disconnect reasons are new in this release:

> l | sgsn-ard-failure(436)

> l | sgsn-camel-release(437)

> l | sgsn-zone-code-failure(455)

> The following session disconnect reasons are visible in this release but are in development for a future release:

> l | sgsn-egtpc-connection-failed(438)

> l | sgsn-egtpc-create-session-failed(439)

> l | sgsn-hss-detach(440)

> l | sgsn-hss-connection-failure(441)

> l | sgsn-pgw-detach(442)

> l | sgsn-s5-not-supported-for-apn(443)

> l | sgsn-no-rab-for-gbr-bearer(444)

> l | sgsn-sgw-selection-failure(445)

> l | sgsn-pgw-selection-failure(446)

> show sgsn-fast-path statistics

> l | Total number of Bad Stats rcvd from NPU 1:

> show sgsn-mode

> l | PDP Deactivation Rate per Session Manager

> l | Connected/Ready Mode Subscribers:

> l | Idle/Stand-By Mode Subscribers :

> show sgtpc statistics verbose

> l | Note Ms Gprs Present Req Denied:

> l | Mandatory IE Incorrect

> l | Mandatory IE Missing

> l | Optional IE Incorrect

> l | Invalid Message Format

> show sgtp-service all

> l | GTP-C IP QOS DSCP value

> l | Gn Delay Monitoring

> l | Response wait time

> l | Delay responses to flag delay

> l | Normal responses to clear delay

> show snmp trap statistics verbose

> l | SGSNGnMsgDelay

> l | SGSNGnMsgDelayClear

> show ss7rd all sctp asp all status peer-server all peer-server-process all verbose

> l | Peer RWND

> l | Self RWND

> l | SSThresh

> l | Partial Bytes Acked

> l | Current RTO for this Path(in ms)

> l | Advertised RWND in received SACK

> show ss7-routing-domain <ss7rd_id> mtp2 statistics linkset all link all

> l | Number of SIN packets transmitted

> l | Number of SIE packets transmitted

> l | Number of SIOS packets transmitted

> l | Number of SIPO packets transmitted

> l | Number of SIB packets transmitted

> l | Number of SIN packets received

> l | Number of SIE packets received

> l | Number of SIOS packets received

> l | Number of SIPO packets received

> l | Number of SIB packets received

> show subs [ grps-only | sgsn-only ] full

> l | Number of Free Vectors:

> l | Number of Used Vectors:

> l | Number of In-Use Vectors:

> SGSN Commands - Modified in Release 12.2
> The following commands have been modified in Release 12.2
> clear bssgp statistics
> With new keywords, it is now possible to clear BSSGP statistics for specific BVCI or NSEI
> CLI (Exec Mode)
> clear bssgp statistics nse <nseid> [ bvc <bvci> ]
> show gmm-sm statistics
> New PLMN keyword set makes it possible to limit the display of GMM statistics for a specific PLMN:
> CLI (Exec Mode)
> show gmm-sm statistics [ gmm-only | plmn-id mcc <mcc> mnc <mnc> [ access-type { gprs | umts } ] | sm-only ] [ gprs-service <srvc_name> | iups-service <srvc_nam e> | sgsn-service <srvc_name> ] [ verbose ] [ | { grep grep_options | more } ]
> show ip traffic
> New sctp keyword obtains kernel SCTP traffic information for the specified card and CPU in a particular context.
> CLI (Exec Mode)
> show ip traffic sctp card <slot_number> cpu <cpu_number>
> show linecard dlci-utilizaton
> The following utilization counters have been added to this new display output:

> l | Port

> l | Path

> l | E1T1

> l | TS

> l | DLCI

> l | NSE

> l | NSVC

> l | Average DLCI Utilization

> l | Current Rx

> l | Current Tx

> l | 5 min Rx

> l | 5 min Tx

> l | 15 min Rx

> l | 15 min Tx

> show session disconnect-reasons
> The following session disconnect reasons is new in this release:

> l | sgsn-rnc-no-dual-pdp-init-pdp-deact(458)

> show subscribers
> The new wide-format keyword presents a wider screenful of information. This has been done to support more information in the IP field to support IPv4v6.
> CLI (Exec Mode)
> show subscribers sgsn-only wide-format
> TPO Commands - Modified in Release 12.0
> The following Traffic Performance Optimizer (TPO) have been modified in release 12.0.
> show active-charging tpo profile statistics
> This command displays TPO profile statistics. The output of this command includes the following new fields:

> l | Number of times TPO is disabled by P2P

> l | Number of times the TPO profile is selected

> CLI (Exec Mode)
> show active-charging tpo profile statistics [ name tpo_profile_name | all ] [ | { grep grep_options | more } ]
> XT2 Commands - Modified in Release 12.0
> The following commands have been modified in Release 12.0.
> None for this release.
> Obsolete Commands
> This section identifies performance management commands obsoleted in Release 12.x.

> l | Common Commands - Obsolete in Release 12.0

> l | Application Detection and Control Commands - Obsolete in Release 12.0

> l | Content Filtering Commands - Obsolete in Release 12.0

> l | ECS Commands - Obsolete in Release 12.0

> l | Firewall Commands - Obsolete in Release 12.0

> l | GGSN Commands - Obsolete in Release 12.0

> l | HA Commands - Obsolete in Release 12.0

> l | IPCF Commands - Obsolete in Release 12.1

> l | NAT Commands - Obsolete in Release 12.0

> l | PDSN Commands - Obsolete in Release 12.0

> l | SGSN Commands - Obsolete in Release 12.0

> Common Commands - Obsolete in Release 12.0
> The following common commands are now obsolete in Release 12.0.
> save logs facility
> CLI (Exec Mode)
> save logs facility facility
> Application Detection and Control Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Content Filtering Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> ECS Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Firewall Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> GGSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> IPCF Commands - Obsolete in Release 12.1
> This section provides information on obsolete IPCF commands in Release 12.1.
> IPCF is new product for this release.
> Mobility Management Entity - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> show mme-policy
> The show mme-policy command is no longer available in release 12.0 It has been replaced with the show lte-policy command.
> CLI (Exec Mode)
> show mme-policy { ho-restriction-list { name name | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary } } [ | { grep grep_options | more } ]
> HA Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> NAT Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> PDSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> SGSN Commands - Obsolete in Release 12.0
> The following commands are now obsolete in Release 12.0.
> None for this release.
> GTPP Storage Server Changes
> The following commands are now obsolete in Release 12.0.
> None for this release.
> Web Element Manager Changes
> There were no Web Element Manager changes in Release 12.0.
> There were no Web Element Manager changes in Release 12.1.
> There were no Web Element Manager changes in Release 12.2.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883