> FA Service Configuration Mode Commands
> The Foreign Agent Service Configuration Mode is used to create and manage the Foreign Agent (FA) services associated with the current context.
> advertise
> Configures agent advertisement parameters within the FA service.
> Product
> PDSN, GGSN, ASN GW
> Privilege
> Security Administrator, Administrator
> Syntax
> advertise {adv-delay seconds |adv-lifetime time | adv-interval { seconds | msec num } | num-adv-sent number | prefix-length-extn | reg-lifetime reg_time }
> no advertise{ prefix-length-extn | reg-lifetime }
> [default] advertise adv-delay
> no advertise prefix-length-extn
> Disables prefix-length-extn
> no advertise reg-lifetime
> Specifies that there is no limit to the registration lifetime that the FA service will allow in any Registration Request message from the mobile node.
> default advertise adv-delay
> Sets the initial delay for the unsolicited advertisement to the default value of 1000 ms.
> advertis e adv-delay seconds
> Default: 1000
> Sets the initial delay for the unsolicited advertisement.
> seconds is the advertisement delay in milliseconds and must be an integer from 10 through 5000.
> Important: This command is available for WiMAX CMIP calls only.
> adv-lifetime time
> Default: 9000
> Specifies the FA agent advertisement lifetime.
> The agent advertisement lifetime is the amount of time that an FA agent advertisement remains valid in the absence of further advertisements.
> time is measured in seconds and can be configured to an integer from 1 through 65535.
> adv-interval { seconds | msec num }
> Default: 5 seconds
> Specifies the amount of time between agent advertisements.
> seconds is the time in seconds and can be an integer from 1 through1800.
> msec num: Configures agent advertisement Interval in milliseconds. num can be an integer from 100 through 1800000.
> num-adv-sent number
> Default: 5
> Specifies the number of unanswered agent advertisements that the FA service sends upon PPP establishment before rejecting the session.
> number can be an integer from 1 through 65535.
> prefix-length-extn
> Default: Disabled
> When enabled, the FA includes the FA-service address in the Router Address field of the Agent Advertisement and appends a Prefix Length Extension in Agent Advertisements with a prefix length of 32.
> reg-lifetime reg_time
> Default: 600
> Specifies the longest registration lifetime that the FA service will allow in any Registration Request message from the mobile node.
> reg_time is measured in seconds and can be configured to an integer from 1 through 65534.
> Usage
> Use to tailor FA advertisements to meet your network needs and/or conditions.
> Example
> The following command configures the FA advertisement interval at 10 seconds, the advertise lifetime to 20000 seconds, and the maximum number of unanswered advertisements that will be set to 3.
> advertise adv-interval 10 adv-lifetime 20000 num-adv-sent 3
> authentication aaa
> This configuration enables or disables the authentication parameters for the FA service to override dynamic keys from AAA with static keys to support MIP registration with an HA that does not support dynamic keys.
> Product
> FA, ASN-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no | default ] authentication aaa-distributed-mip-keys override
> no
> Disable the override of dynamic keys from AAA.
> default
> By default the override behavior is disabled and the system uses dynamic keys from AAA after successful EAP authentication. If EAP authentication fails, the system uses static keys by default.
> Usage
> Specify how the system will perform authentication of registration request messages. By default dynamic MN-HA and FA-HA keys from AAA after successful EAP authentication used by a PMIP client in WiMAX calls for MIP registration with HA. This configuration in FA service overrides the dynamic keys from AAA with static keys to support MIP registration with an HA that does not support dynamic keys.
> Example
> The following command configures the FA service to override use of AAA MIP keys and force the use of statically configured FA-HA SPI/key for WiMAX calls.
> authentication aaa-distributed-mip-keys override
> authentication mn-aaa
> Specifies how the system handles authentication for mobile node re-registrations.
> Product
> PDSN, ASN GW, GGS
> Privilege
> Security Administrator, Administrator
> Syntax
> authentication mn-aaa { always | ignore-after-handoff | init-reg | init-reg-except-handoff | renew-and-dereg-noauth | renew-reg-noauth } [ optimize-retries ]
> always
> Specifies that the FA service performs authentication each time a mobile node registers. This is the default setting.
> ignore-after-handoff
> MN-AAA authentication is not done at the FA for a handoff Access Gateway (AGW).
> init-reg
> MN-AAA and MN-FAC extensions are required only in initialization RRQ.
> init-reg-except-handoff
> MN-AAA and MN-FAC extensions are not required in initialization RRQ after inter-Access Gateway (AGW) handoff.
> renew-and-dereg-noauth
> Specifies that the FA service does not perform authentication for mobile node re-registration or deregistration authorization requests. Initial registration is handled normally.
> renew-reg-noauth
> Specifies that the FA service does not perform authentication for mobile node re-registrations. Initial registration and de-registration are handled normally.
> optimize-retries
> Optimizes the number of Authentication retries sent to the AAA server.
> When an authentication request is pending for a MIP call at the AGW, if a retry RRQ is received from the mobile node, the AGW discards the old RRQ and keeps the most recent RRQ. Subsequently when the authentication succeeds, the AGW forwards the most recent RRQ to the HA. If the authentication fails, the AGW replies to the MN using the most recent RRQ.
> Usage
> Use this command to determine how the FA service handles mobile node re-registrations.
> The system is shipped from the factory with the mobile AAA authentication set to always.
> Example
> The following command configures the configures the FA service to perform mobile node authentication for every re-registration:
> authentication mn-aaa always
> The following command specifies that the FA service does not perform authentication for mobile node re-registrations:
> authentication mn-aaa renew-reg-noauth
> authentication mn-ha
> Configures whether the FA service looks for a Mobile Network-Home Agent (MN-HA) authentication extension in the RRP (registration reply).
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> authentication mn-ha { allow-noauth | always }
> allow-noauth
> Allows a reply that does not contain the auth extension.
> always
> A reply should always contain the auth extension to be accepted.
> This is the default setting.
> Usage
> Use this command to determine whether or not the FA service requires the MN-HA auth extension in the RRP.
> The system is shipped from the factory with this set to always.
> Example
> The following command configures the FA service to require a reply to contain the authentication extension to be accepted.:
> authentication mn-ha always
> bind
> Binds the FA service to a logical IP interface serving as the Pi interface and specifies the maximum number of subscribers that can access this service over the interface.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> bind address address [ max-subscribers count ]
> no bind address
> address
> Specifies the IP address (address) of the interface configured as the Pi interface. address is specified in IPv4 dotted-decimal notation.
> max-subscribers max#
> Default: 500000
> Specifies the maximum number of subscribers that can access this service on this interface.
> count can be configured to an integer from 0 through 500000.
> Important: The maximum number of subscribers supported is dependant on the license key installed and the number of active packet processing cards installed in the system. Refer to the license key command for additional information.
> Usage
> Associate or tie the FA service to a specific logical IP address. The logical IP address or interface takes on the characteristics of an Pi interface. Only one interface can be bound to a service. The interface should be configured prior to issuing this command.
> This command also sets a limit as to the number of simultaneous subscribers sessions that can be facilitated by the service/interface at any given time.
> When configuring the max-subscribers option, be sure to consider the following:

> • | The total number of interfaces you will configure for use as Pi interfaces

> • | The maximum number of subscriber sessions that all of these interfaces may handle during peak busy hours

> • | The average bandwidth for each of the sessions

> • | The type of physical port (10/100Base-T or 1000Base-Tx) that these interfaces will be bound to

> Taking these factors into account and distributing your subscriber session across all available interfaces will allow you to configure your interfaces to optimally handle sessions without degraded performance.
> Use the no bind address command to delete a previously configured binding.
> Example
> The following command would bind the logical IP interface with the address of 192.168.3.1 to the FA service and specifies that a maximum of 600 simultaneous subscriber sessions can be facilitated by the interface/service at any given time.
> bind address 192.168.3.1 max-subscribers 600
> The following command disables a binding that was previously configured:
> no bind address
> challenge-window
> Defines the number of recently sent challenge values that are considered valid by the FA.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> challenge-window number
> number
> Default: 2
> The number of recently sent challenge values that are considered valid. number must be an integer from 1 through 5.
> Usage
> Use this command to set the number of recently sent challenge values that are considered valid by the FA.
> Example
> Set the challenge window to 3:
> challenge-window 3
> default subscriber
> Specifies the name of a subscriber profile configured within the same context as the FA service from which to base the handling of all other subscriber sessions handled by the FA service.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> default subscriber profile_name
> no default subscriber profile_name
> profile_name
> Specifies the name of the configured subscriber profile. profile_name is an alphanumeric string of 1 through 63 characters that is case sensitive.
> Usage
> Each subscriber profile specifies “rules” such as permissions, PPP settings, and timeout values.
> By default, the FA service will use the information configured for the subscriber named default within the same context. This command allows for multiple FA services within the same context to apply different “rules” to sessions they process. Each set of rules can be configured under a different subscriber name which is pointed to by this command.
> Use the no default subscriber profile_name command to delete the configured default subscriber.
> Example
> To configure the FA service to apply the rules configured for a subscriber named user1 to every other subscriber session it processes, enter the following command:
> default subscriber user1
> dynamic-ha-assignment
> This command configures various dynamic HA assignment parameters.
> Product
> HA
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default | no ] dynamic-ha-assignment [ aaa-override mn-supplied-ha-addr | allow-failover ]
> default
> Feature is disabled by default.
> no
> Removes the feature and returns it to the default setting of disabled.
> aaa-override mn-supplied-ha-addr
> Enables the system to override the mobile node supplied HA IP address with the AAA provided HA address.
> allow-failover
> Enables/disables a failover retry for dynamic HA assignment from the AAA server.
> Usage
> Use this command to override the mobile node supplied HA IP address with the AAA supplied HA address.
> Use this command to enable or disable the failover feature that allows the system to receive and use a newer HA address from the AAA server in cases where the original HA address is not responding.
> A AAA server may assign different HA addresses each time a retransmitted MIP RRQ is authenticated during the MIP session setup. When this configuration is enabled, if the FA gets a new HA address from AAA during setup, it discards the previous HA address and start using the new address. This allows the FA session to connect to an available HA during setup.
> Example
> The following command enables the failover feature that allows the system to receive and use a newer HA address from the AAA server:
> dynamic-ha-assignment allow-failover
> dynamic-mip-key-update
> When enabled, the FA service processes MIP_Key_Update_Request from the AAA server and allows dynamic MIP key updates (DMUs).
> Default: Disabled
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> dynamic-mip-key-update
> no dynamic-mip-key-update
> no
> The FA service rejects MIP_Key_Update_Request from the AAA server, not allowing dynamic MIP key updating to occur and terminates the call.
> Usage
> Use this command to enable or disable the DMU feature in the FA service.
> Example
> To enable DMU and allow dynamic updates of MIP keys, enter the following command:
> dynamic-mip-key-update
> encapsulation allow gre
> Enables or disables the use of generic routing encapsulation (GRE) when establishing a Mobile IP (MIP) session. When enabled, if requested by a Mobile Node (MN), the FA requests the HA to use GRE encapsulation when establishing the MIP session. When disabled, the FA does not set the GRE bit in Agent Advertisements to the MN.
> Default: GRE is enabled.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> encapsulation allow gre
> no encapsulation allow gre
> Usage
> Use to disable or re-enable the use of GRE encapsulation for MIP sessions.
> Example
> To re-enable GRE encapsulation for MIP sessions, enter the following command:
> encapsulation allow gre
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> fa-ha-spi
> Configures the security parameter index (SPI) between the FA service and the HA.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> fa-ha-spi remote-address { ha_ip_address | ip_addr_mask_combo } spi-number number { encrypted secret enc_secret | secret } [ description string | hash-algorithm { hmac-md5 | md5 | rfc2002-md5 } | monitor-ha | replay-protection { timestamp | nonce } | timestamp-tolerance tolerance ]
> no fa-ha-spi remote-address { ha_ip_address | ip_addr_mask_combo } spi-number number
> remote-address { ha_ip_address | ip_addr_mask_combo }
> ha_ip_address: Specifies the IP address of the HA in IPv4 dotted-decimal notation.
> ip_addr_mask_combo: Specifies the IP address of the HA including network mask bits. ip_addr_mask_combo must be specified IPv4 dotted-decimal notation with CIDR subnet mask bits (x.x.x.x/xx).
> spi-number number
> Specifies the Security Parameter Index (SPI) which indicates a security context between the FA and the HA in accordance with RFC 2002.
> number can be configured to an integer from 256 through 4294967295.
> encrypted secret enc_secret | secret secret
> Configures the shared-secret between the FA service and the HA. The secret can be either encrypted or non-encrypted.

> • | encrypted secret enc_secret : Specifies the encrypted shared key (enc_secret) between the FA service and the HA. enc_secret must be an alphanumeric string of 1 through 254 characters that is case sensitive.

> Important: The encrypted keyword is intended only for use by the system while saving configuration scripts. The system displays the encrypted keyword in the configuration file as a flag that the variable following the secret keyword is the encrypted version of the plain text secret key. Only the encrypted secret key is saved as part of the configuration file.

> • | secret secret: Specifies the shared key (secret) between the FA service and the HA. secret must be an alphanumeric string of 1 through 127 characters that is case sensitive.

> description string
> This is a description for the SPI. string must be an alphanumeric string of 1 through 31 characters.
> hash-algorithm { hmac-md5 | md5 | rfc2002-md5 }
> Default: hmac-md5
> Specifies the hash-algorithm used between the FA service and the HA.

> • | hmac-md5: Configures the hash-algorithm to implement HMAC-MD5 per RFC 2002bis.

> • | md5: Configures the hash-algorithm to implement MD5 per RFC 1321.

> • | rfc2002-md5: Configures the hash-algorithm to implement keyed-MD5 per RFC 2002.

> monitor-ha
> Default: disabled
> Enables the HA monitor feature for this HA address.
> To set the behavior of the HA monitor feature, refer to the ha-monitor command in this chapter. To disable this command (if enabled) for this HA address, re-enter the entire fa-ha-spi command without the monitor-ha keyword.
> replay-protection { timestamp | nonce }
> Default: timestamp
> Specifies the replay-protection scheme that should be implemented by the FA service for this SPI.

> • | nonce: Configures replay protection to be implemented using NONCE per RFC 2002. Nonce is an arbitrary number used only once to sign a cryptographic communication.

> • | timestamp: Configures replay protection to be implemented using timestamps per RFC 2002.

> Important: This keyword should only be used in conjunction with Proxy Mobile IP support.
> timestamp-tolerance tolerance
> Default: 60
> Specifies the allowable difference (tolerance) in timestamps that is acceptable. If the difference is exceeded, then the session will be rejected. If this is set to 0, then timestamp tolerance checking is disabled at the receiving end.
> tolerance is measured in seconds and can be configured to an integer value from 0 through 65535.
> Important: This keyword should only be used in conjunction with Proxy Mobile IP support.
> +
> More than one of the above keywords can be entered within a single command.
> Usage
> An SPI is a security mechanism configured and shared by the FA service and the HA. Please refer to RFC 2002 for additional information.
> Though it is possible for FAs and HAs to communicate without SPIs being configured, the use of them is recommended for security purposes. It is also recommended that a “default” SPI with a remote address of 0.0.0.0/0 be configured on both the HA and FA to prevent hackers from spoofing addresses.
> Important: The SPI configuration on the HA must match the SPI configuration for the FA service on the system in order for the two devices to communicate properly.
> A maximum of 2,048 SPIs can be configured per FA service.
> Use the no version of this command to delete a previously configured SPI.
> Example
> The following command configures the FA service to use an SPI of 512 when communicating with an HA with the IP address 192.168.0.2. The key that would be shared between the HA and the FA service is q397F65. When communicating with this HA, the FA service will also be configured to use the rfc2002-md5 hash-algorithm.
> fa-ha-spi remote-address 192.168.0.2 spi-number 512 secret q397F65 hash-algorithm rfc2002-md5
> The following command deletes the configured SPI of 400 for an HA with an IP address of 172.100.3.200:
> no fa-ha-spi remote-address 172.100.3.200 spi-number 400
> gre
> Configures Generic Routing Encapsulation (GRE) parameters.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gre { checksum | checksum-verify | reorder-timeout timeout | sequence-mode { none | reorder } | sequence-numbers }
> no gre { checksum | checksum-verify | sequence-numbers }
> no
> Disables the specified functionality.
> checksum
> Default: disabled
> Enables the introduction of the checksum field in outgoing GRE packets.
> checksum-verify
> Default: disabled
> Enables verification of the GRE checksum (if present) in incoming GRE packets.
> reorder-timeout timeout
> Default: 100
> Configures maximum number of milliseconds to wait before processing reordered out-of-sequence GRE packets. timeout must be an integer from 0 through 5000.
> sequence-mode { none | reorder }
> Default: none
> Configures how incoming out-of-sequence GRE packets should be handled.
> none: Disables reordering of incoming out-of-sequence GRE packets.
> reorder: Enables reordering of incoming out-of-sequence GRE packets.
> sequence-numbers
> Default: Disabled.
> Enables insertion or removal of GRE sequence numbers in GRE packets.
> Usage
> Use this command to configure how the FA service handles GRE packets.
> Example
> To set maximum number of milliseconds to wait before processing reordered out-of-sequence GRE packets to 500 milliseconds, enter the following command:
> gre reorder-timeout 500
> To enable the reordering of incoming out of sequence GRE packets, enter the following command:
> gre sequence-mode reorder
> ha-monitor
> Configures the behavior of the HA monitor feature.
> Product
> PDSN, ASN GW, FA, HA
> Privilege
> Security Administrator, Administrator
> Syntax
> [ default ] ha-monitor [ interval sec| max-inactivity-time sec | num-retry num ]
> no ha-monitor
> default
> Restores the system default setting(s) for the command/keyword(s). This command is disabled by default.
> no
> Disables the HA monitoring feature for this FA service.
> interval sec
> Default: 30
> Configures the time interval before the next monitoring request message is sent to the HA.
> sec must be an integer from 1 through 36000.
> max-inactivity-time sec
> Default: 60
> Specifies the maximum amount of time the system will wait without receiving MIP control traffic from a HA before the HA monitoring mechanism is triggered.
> sec must be an integer from 30 through 600.
> num-retry num
> Default: 5
> Configures the number of time the system will attempt to send HA monitor requests before determining the HA is down and a trap is initiated.
> num must be an integer from 0 through 10.
> Usage
> Use this command to set parameters for the HA monitor feature. This feature allows the AGW/FA to monitor HAs with which it has MIP sessions. The monitoring feature is triggered when the AGW/FA does not receive any MIP traffic from a HA for a configured amount of time (max-inactivity-time). The AGW/FA starts sending special MIP RRQ monitor messages and waits for RRP monitor message responses from the HA. The RRQ monitor messages are addressed to the HA service address. The source address of the monitor-request messages is the FA service's IP address.
> The actions taken during monitoring are comprised of the following:

> • | If no monitor response is received during the interval time (interval), the AGW retransmits the monitor message a configured number of times (num-retry).

> • | If no response is received after retransmitting for the number configured in num-retry, the HA is considered down. The AGW/FA sends a trap (HAUnreachable) to the management station. Monitoring of this HA is stopped until a MIP control message is received from the particular HA and when the AGW/FA sends a trap (HAreachable) to the management station and starts monitoring the HA again.

> • | When an HA receives the RRQ from an FA, it verifies the message and identifies it as a monitor message based on a special reserved NAI (in the message) and a Monitor HA CVSE in the RRQ. The HA responds with an RRP with Reply code 0x00 (accepted) and includes the Monitor HA CVSE. When the FA receives the RRP from the HA, it updates the activity for the peer HA to maintain the “up” state.

> Important: This command only sets the behavior of the HA monitor feature. To enable the HA monitor feature for each HA address, refer to the fa-ha-spi command in this chapter. Up to 256 HAs can be monitored per system.
> Example
> The following commands set the HA monitor message interval to 45 seconds, the HA inactivity time to 60 seconds, and the number of HA monitor retries to 6:
> ha-monitor interval 45ha-monitor max-inactivity-time 60ha-monitor num-retry 6
> idle-timeout-mode
> Controls whether Mobile IP data and control packets or only Mobile IP data resets the session idle timer.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> idle-timeout-mode {aggressive | normal}
> aggressive
> Only Mobile IP data resets the session idle timer.
> normal
> Both Mobile IP data and control packets reset the session idle timer.
> Usage
> Use this command to control how the session idle timer is reset.
> Example
> The following command specifies that only Mobile IP data can reset the session idle timer:
> idle-timeout-mode aggressive
> ignore-mip-key-data
> When this command is enabled, if the Dynamic Mobile IP Key Update (DMU) is not enabled and the mobile node (MN) sends a MIP_Key_Data CVSE, the FA ignores the MIP_Key_Data extension and the call is continued like a regular Mobile IP (MIP) call.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ignore-mip-key-data
> no ignore-mip-key-data
> no
> Disable ignoring of MIP key data.
> Usage
> When DMU is not enabled, use this command to ignore MIP key data sent by the MN and allow the call to continue normally.
> Example
> To enable the FA to ignore MIP key data sent by the MN, enter the following command:
> ignore-mip-key-data
> ignore-stale-challenge
> Enables the system to accept RRQs with previously used challenges. This feature is disabled by default.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ignore-stale-challenge
> no ignore-stale-challenge
> no
> Disables this feature. If an RRQ is received with a previously used challenge and there are RRQs pending on the same session, accept the RRQ if it has a new Identification in the retransmitted RRQ. All other RRQs received with previously used challenge are rejected with the Stale Challenge (106) error code.
> Usage
> Use this command to allow the FA to accept stale challenges regardless of the ID field or if other RRQs are pending.
> Example
> To enable this functionality in the FA service, enter the following command;
> ignore-stale-challenge
> To disable this functionality, enter the following command;
> no ignore-stale-challenge
> ip local-port
> Configures the local User Datagram Protocol (UDP) port for the Pi interfaces’ IP socket on which to listen for Mobile IP Registration messages.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ip local-port port#
> port#
> Specifies the UDP port number.
> port# can be an integer from 1 through 65535.
> Usage
> Specify the UDP port that should be used for communications between the FA service and the HA.
> The system defaults to using local port 434.
> Example
> The following command specifies a UDP port of 3950 for FA-to-HA communication on the Pi interface:
> ip local-port 3950
> isakmp
> Configures support for IPSec within the FA-service.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> isakmp {peer-ha ha_address {crypto map map_name [ [ encrypted ] secret secret ]} | default { crypto map map_name [ [ encrypted ] secret secret]}}
> no isakmp { peer-ha peer_ip_address | default }
> no
> Deletes the reference to the crypto map for the specified HA, or deletes the reference for the default crypto map.
> peer-ha ha_address { crypto map map_name [ [ encrypted ] secret preshared_secret ] }
> Configures a crypto map for a peer HA.

> • | ha_address: The IP address of the HA with which the FA service will establish an IPSec SA. The address must be expressed in IPv4 dotted-decimal format.

> • | crypto map map_name: The name of a crypto map configured in the same context that defines the IPSec tunnel properties. map_name is the name of the crypto map expressed as an alphanumeric string of 1 through 127 characters.

> • | encrypted: This keyword is intended only for use by the system while saving configuration scripts. The system displays the encrypted keyword in the configuration file as a flag that the variable following the secret keyword is the encrypted version of the plain text secret key. Only the encrypted secret key is saved as part of the configuration file.

> • | secret secret: The pre-shared secret that will be used during the IKE negotiation. preshared_secret is the secret expressed as an alphanumeric string of 1 through 127 characters.

> default { crypto map map_name [ [ encrypted ] secret secret ] }
> Specifies the default crypto map to use when there is no matching crypto map configured for an HA address.

> • | crypto map map_name: The name of a crypto map configured in the same context that defines the IPSec tunnel properties. map_name is the name of the crypto map expressed as an alphanumeric string of 1 through 127 characters.

> • | encrypted: This keyword is intended only for use by the system while saving configuration scripts. The system displays the encrypted keyword in the configuration file as a flag that the variable following the secret keyword is the encrypted version of the plain text secret key. Only the encrypted secret key is saved as part of the configuration file.

> • | secret secret: The pre-shared secret that will be used during the IKE negotiation. preshared_secret is the secret expressed as an alphanumeric string of 1 through 127 characters.

> Usage
> Use this command to configure the FA-service’s per-HA IPSec parameters. These dictate how the FA service is to establish an IPSec SA with the specified HA.
> Important: For maximum security, the above command should be executed for every possible HA with which the FA service communicates.
> A default crypto map can also be configured using the default keyword. The default crypto map is used in the event that the AAA server returns an HA address that is not configured as an isakmp peer-ha.
> Important: For maximum security, the default crypto map should be configured in addition to peer-ha crypto maps instead of being used to provide IPSec SAs to all HAs.
> Note that once an IPSec tunnel is established between the FA and HA for a particular subscriber, all new Mobile IP sessions using the same FA and HA are passed over the tunnel regardless of whether or not IPSec is supported for the new subscriber sessions. Data for existing Mobile IP sessions is unaffected.
> Example
> The following command creates a reference for an HA with the IP address 10.2.3.4 to a crypto map named map1:
> isakmp peer-ha 10.2.3.4 crypto map map1
> The following command deletes the crypto map reference for the HA with the IP address 10.2.3.4.
> no isakmp peer-ha 10.2.3.4
> limit-reg-lifetime
> Enable the current default behavior of limiting the Mobile IP (MIP) lifetime to be smaller than the Idle, Absolute, or Long Duration timeouts. When disabled, this command allows a MIP lifetime that is longer than the Idle, Absolute or Long Duration timeouts.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no | default] limit-reg-lifetime
> no
> Allows a MIP lifetime that is longer than the Idle, Absolute or Long Duration timeouts.
> default
> Enables the default behavior of limiting the MIP lifetime to be smaller than the Idle, Absolute, or Long Duration timeouts.
> Usage
> Use the no keyword with this command to allow a MIP lifetime that is longer than the Idle, Absolute or Long Duration timeouts.
> Use the base command or the keyword to reset the FA service to the default behavior of limiting the MIP lifetime to be smaller than the Idle, Absolute, or Long Duration timeouts.
> Example
> Configure the FA service to allow a MIP lifetime that is longer than the Idle, Absolute or Long Duration timeouts by entering the following command:
> no limit-reg-lifetime
> Configure the FA service to the default behavior of limiting the MIP lifetime to be smaller than the Idle, Absolute, or Long Duration timeouts by entering either of the following commands:
> default limit-reg-lifetimelimit-reg-lifetime
> max-challenge-len
> For mobile subscribers, the FA generates a random number and sends it to the mobile node as part of the mobile authentication extension (Mobile-Foreign Authentication extension) as described in RFC 3012. This command sets the maximum length of the FA challenge in bytes.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> max-challenge-len length
> length
> Default: 16
> The maximum length, in bytes, of the FA challenge. This value must be an integer from 4 through 32.
> Usage
> Change the maximum allowed length of the randomly generated FA challenge its default of 16.
> Example
> Use the following command to change the maximum length of the FA challenge to 18 bytes:
> max-challenge-len 18
> mn-aaa-removal-indication
> Enables the FA to remove the Mobile Network-Final Assembly Code (MN-FAC) and MN-AAA extensions from RRQs. This is disabled by default.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> mn-aaa-removal-indication
> no mn-aaa-removal-indication
> no
> Disable the removal of the MN-FAC and MN-AAA extensions from RRQs.
> Usage
> Enable this feature if there is no need to authenticate the subscriber at HA using MN-AAA extension.
> Example
> The following command enables the FA service to remove MN-FAC and MN-AAA extensions from RRQs:
> mn-aaa-removal-indication
> multiple-reg
> Specifies the number of simultaneous Mobile IP sessions that will be supported for over a single PPP session.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> multiple-reg number
> number
> number can be configured to an integer from 1 through 3.
> Usage
> Use to support multiple registrations per subscriber.
> The system defaults to a setting of “1” for multiple simultaneous MIP sessions.
> Important: The system will only support multiple Mobile IP sessions per subscriber if the subscriber’s mobile node has a static IP address. The system will only allow a single Mobile IP session for mobile nodes that receive a dynamically assigned IP address. In addition, because only a single Mobile IP or proxy-Mobile IP session is supported for IP PDP contexts, this parameter must remain at its default configuration.
> Example
> The following command configures the number of supported simultaneous registrations for subscribers using this FA service to 3.
> multiple-reg 3
> optimize tunnel-reassembly
> Configures FA to HA optimization for tunnel reassembly.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> optimize tunnel-reassembly
> no optimize tunnel-reassembly
> Usage
> Enabling this functionality fragments large packets prior to encapsulation for easier processing. Tunnel reassembly optimization is disabled by default.
> Important: You should not use this command without first consulting Cisco Systems Technical Support. This command applies to very specific scenarios where packet reassembly is not supported at the far end of the tunnel. There are cases where the destination network may either discard the data, or be unable to reassemble the packets.
> Important: This functionality works best when the FA service is communicating with an HA service running in a system. However, an FA service running in the system communicating with an HA from a different manufacturer will operate correctly even if this parameter is enabled.
> Use the no version of this command to disable tunnel optimization if it was previously enabled.
> Example
> The following command enables tunnel reassembly optimization:
> optimize tunnel-reassembly
> private-address allow-no-reverse-tunnel
> This command enables the FA to allow calls with private addresses and no reverse tunneling.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> private-address allow-no-reverse-tunnel
> no private-address allow-no-reverse-tunnel
> no
> Disables the functionality. This is the default setting.
> Usage
> Use this command to let the FA allow sessions with private addresses that do not have the reverse tunnel bit set.
> Example
> To enable sessions with private addresses and no reverse tunneling, enter the following command:
> private-address allow-no-reverse-tunnel
> proxy-mip
> Configures parameters pertaining to Proxy Mobile IP support.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> proxy-mip { allow | ha-failover [ max-attempts max_attempts | num-attempts-before-switching num_attempts | timeout seconds ]| max-retransmissions number | renew-percent-time renew-time | retransmission-timeout time }
> no proxy-mip {allow | ha-failover }
> default proxy-mip {allow | ha-failover | max-retransmissions | renew-percent-time | retransmission-timeout}
> no
> Disables FA service support for Proxy Mobile IP or HA failover for Proxy Mobile IP.
> default
> Restores the specified option to the default setting as described below.
> allow
> Default: Disabled
> Enables FA service support for Proxy Mobile IP.
> ha-failover [max-attempts max_attempts | num-attempts-before-switching num_attempts | timeout seconds ]
> Default: Disabled
> Enables HA failover for the Proxy Mobile IP feature.

> • | max-attempts max_attempts - Configures the maximum number of retransmissions of Proxy MIP control messages. max_attempts must be an integer from 1 through 10. Default is 4

> • | num-attempts-before-switching num_attempts - Configures the total number of RRQ attempts (including retransmissions) before failing over to the alternate HA. num_attempts must be an integer from 1 through 5. Default is 2.

> • | timeout seconds - Configures the retransmission timeout (in seconds) of Proxy MIP control messages when failover happens. seconds must be an integer from 1 through 50. Default is 2

> max-retransmissions number
> Default: 5
> Configures the maximum number re-try attempts that the FA service is allowed to make when sending Proxy Mobile IP Registration Requests to the HA.
> number is the maximum number of retries and can be configured to an integer from 1 through 4294967295.
> renew-percent-time renew-time
> Default: 75
> Configures the amount of time that must pass prior to the FA sending a Proxy Mobile IP Registration Renewal Request.
> renew-time is entered as a percentage of the advertisement registration lifetime configured for the FA service. (Refer to the advertise command in this chapter). renew-time can be configured to an integer from 1 through 100.
> The following equation can be used to calculate renew-time:
> renew-time = (duration / lifetime) * 100
> duration = The desired amount of time that can pass prior to the FA sending a Proxy Mobile IP Registration Renewal Request
> lifetime = The advertisement registration lifetime configured for the FA service.
> duration / lifetime
> retransmission-timeout time
> Default: 3
> Configures the maximum amount of time allowed by the FA for a response from the HA before re-sending a Proxy Mobile IP Registration Request message.
> time is measured in seconds and can be configured to an integer from 1 through 100.
> Usage
> The proxy-mip command and its keywords configure the FA services support for Proxy Mobile IP.
> When enabled though the session license and feature use key, the system supports Proxy Mobile IP to provide a mobility solution for subscribers with mobile nodes (MNs) capable of supporting only Simple IP.
> In addition to the parameters configured via this command, the HA-FA SPI(s) must also be modified to support Proxy Mobile IP. Refer to the fa-ha-spi command for more information.
> Example
> The following command configures the FA service to wait up to 5 seconds for an HA to respond prior to re-sending an a Mobile IP Registration Request message:
> proxy-mip retransmission-timeout 5
> If the advertisement registration lifetime configured for the FA service is 900 seconds and you want the system to send a Proxy Mobile IP Registration Renewal Request message after 500 seconds, then the following command must be executed:
> proxy-mip renew-percent-time 50
> Note that 50 = (450 / 900) 100.
> reg-timeout
> Configures the FA registration reply timeout.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> reg-timeout time
> time
> Default: 45
> time is measured in seconds and can be configured to an integer from 1 through 65535.
> Usage
> Configure the amount of time that the FA service will wait for a Registration Reply from an HA before the call is rejected with a reply code of 78H (registration Timeout).
> Example
> The following command configures a registration timeout of 10.
> reg-timeout 10
> reverse-tunnel
> Enables the use of reverse tunneling for a Mobile IP (MIP) sessions when requested by the mobile node (MN).
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> reverse-tunnel
> no reverse-tunnel
> no
> Indicates the reverse tunnel option is to be disabled. When omitted, the reverse tunnel option is enabled.
> Usage
> Reverse tunneling involves tunneling datagrams originated by the MN to the HA via the FA service.
> When an MN arrives at a foreign network, it listens for agent advertisements and selects an FA that supports reverse tunnels. The MN requests this service when it registers through the selected FA. At this time, the MN may also specify a delivery technique such as Direct or the Encapsulating Delivery Style.
> The advantages of using reverse-tunneling:

> • | All datagrams from the mobile node seem to originate from its home network

> • | The FA can keep track of the HA that the mobile node is registered to and tunnel all datagrams from the mobile node to its HA

> Use the no option of this command to disable reverse tunneling. If reverse tunneling is disabled, and the mobile node does not request it, then triangular routing is used.
> The system defaults to reverse tunnel enabled.
> Important: If reverse tunneling is disabled on the system and an MN requests it, the call will be rejected with a reply code of 74H (reverse-tunneling unavailable).
> Example
> The following command disables reverse-tunneling support for the FA service:
> no reverse-tunnel
> revocation
> Enables the MIP revocation feature and configures revocation parameters.
> Product
> PDSN, ASN GW, GGSN PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> revocation { enable | max-retransmission number | negotiate-i-bit | retransmission-timeout secs | trigger internal-failure }
> no revocation enable | trigger internal-failure | negotiate-i-bit
> no revocation { enable | negotiate-i-bit | trigger internal-failure }
> Completely disables registration revocation on the FA.
> Disables sending revocation messages to the HA when a session is affected by an internal task failure.
> enable
> Enables the MIP registration revocation feature on the FA. When enabled, if revocation is negotiated with an HA, and a MIP binding is terminated, the FA can send a Revocation message to the HA. This feature is disabled by default.
> max-retransmission number
> Default: 3
> Specifies the maximum number of retransmissions of a Revocation message before the revocation fails. number must be an integer from 0 through 10.
> negotiate-i-bit
> Default: disabled
> Enables the FA to negotiate the i-bit via PRQ/RRP messages and processes the i-bit revocation messages.
> retransmission-timeout secs
> Default: 3
> Specifies the number of seconds to wait for a Revocation Acknowledgement from the HA before retransmitting the Revocation message. secs must be an integer from 1 through 10.
> trigger internal-failure
> Default: disabled
> Enable sending a revocation message to the HA for all sessions that are affected by an internal task failure.
> Usage
> Use this command to enable or disable the MIP revocation feature on the FA or to change settings for this feature. Both the HA and the FA must have Registration Revocation enabled and FA/HA authorization must be in use for Registration Revocation to be negotiated successfully.
> Example
> The following command enables Registration Revocation on the FA:
> revocation enable
> The following command sets the maximum number of retries for a Revocation message to 6:
> revocation max-retransmission 6
> The following command sets the timeout between retransmissions to 10:
> revocation retransmission-timeout 10
> threshold reg-reply-error
> Set an alarm or alert based on the number of registration reply errors per FA service.
> Product
> PDSN, ASN GW, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> threshold reg-reply-error high_thresh [ clear low_thresh ]
> no threshold reg-reply-error
> no
> Deletes the alert or alarm.
> high_thresh
> Default: 0
> The high threshold number of registration reply errors that must be met or exceeded within the polling interval to generate an alert or alarm. high_thresh can be an integer from 0 through 100000.
> Important: You must enter a value between 1 and 100000 to trigger an alert/alarm.
> clear low_thresh
> Default:0
> The low threshold number of registration reply errors that must be met or exceeded within the polling interval to clear an alert or alarm. low_thresh can be an integer from 0 through 100000.
> Important: This value is ignored for the Alert model. In addition, if this value is not configured for the Alarm model, the system assumes it is identical to the high threshold.
> Important: You must enter a value between 1 and 100000 to trigger an alert/alarm.
> Usage
> Use this command to set an alert or an alarm when the number of registration reply errors is equal to or greater than a specified number of calls per second.
> Alerts or alarms are triggered for the number of registration reply errors on the following rules:

> • | Enter condition: Actual number of registration reply errors > High Threshold

> • | Clear condition: Actual number of registration reply errors £ Low Threshold

> Example
> The following command configures a registration reply error threshold of 1000 and a low threshold of 500 for a system using the Alarm thresholding model:
> threshold reg-reply-error 1000 clear 500

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883