> FNG Service Configuration Mode Commands
> The FNG Service Configuration Mode is used to configure the properties required for the Femto Network Gateway (FNG) to interface with the Femto Access Points (FAPs) in the network.
> aaa aggregation
> Sets the system attributes for A12 aggregation for the FNG service.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> aaa aggregation { interface type a12| destination address ipv4_address | a12-group { context name [ aaa-group name ] | aaa-group name [ context name ] } }
> no aaa aggregation interface type a12
> no a12 destination address ipv4_address
> no aaa aggregation a12-group { context name [ aaa-group name ] | aaa-group name [ context name ] }
> aaa aggregation interface type a12
> Enables A12 aggregation functionality for the FNG service.
> aaa aggregation interface a12 destination address ipv4_address
> Adds a destination address for an AN-AAA server for A12 aggregation. A maximum of ten destination addresses can be configured.
> aaa aggregation a12-group { context name [ aaa-group name ] | aaa-group [ context name ] }
> Defines the AAA context and AAA group to be used for A12 aggregation.
> If the context name and AAA group are not specified, the FNG defaults to the FNG service context and the default AAA group in that context. If the AAA group is specified but the context is not specified, the FNG uses the FNG service context and the AAA group in that context. If the AAA group is not specified and the context is specified, the FNG uses the default AAA group in that context.
> no aaa aggregation interface type a12
> Disables A12 aggregation functionality for the FNG service.
> no aaa aggregation a12-destination address ipv4_address
> Deletes the specified destination address for an AN-AAA server.
> no aaa aggregation a12-group { context name [ aaa-group name ] | aaa-group [ context name ] }
> Deletes the specified AAA context and AAA group to be used for A12 aggregation.
> Usage
> Sets the system attributes for AAA aggregation in the FNG service.
> Example
> The following command enables the A12 functionality for the FNG service:
> aggregation interface type a12
> aaa authentication
> Specifies the AAA group to use for FAP authentication.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> aaa authentication { context-name name aaa-group name | context-name name aaa-group name }
> no aaa authentication
> no aaa authentication
> Removes any existing authentication configuration.
> context-name name aaa-group name
> Specifies the context name and the AAA group name configured in the context for FAP authentication.
> context-name name: Specifies the context where the AAA server group is defined as an alphanumeric string of 1 through 79 characters.
> aaa-group name: Specifies the name of the AAA group to be used for authentication as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to specify that during IPSec session establishment using IKEv2 setup, the FNG will use Radius AAA for FAP authentication.
> Example
> Use the following to configure device authentication for an AAA group named aaa-10 in the FNG context named fng1:
> aaa authentication context-name fng1 aaa-group aaa-10
> bind
> Binds the FNG service IP address to a crypto template and specifies the maximum number of sessions the FNG service supports.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> bind address ipv4_address { crypto-template string }[ max-sessions number ]
> no bind
> no bind
> Removes a previously configured binding.
> address ipv4_address
> Specifies the IPv4 address of the FNG service.
> crypto-template string
> Specifies the name of the crypto template to be bound to the FNG service.
> string is any value from 0 - 127 alpha and/or numeric characters.
> max-sessions number
> Specifies the maximum number of sessions to be supported by the FNG service as an integer from 0 through 1000000. Default: 1000000
> If the max-sessions value is changed on an existing system, the new value takes effect immediately if it is higher than the current value. If the new value is lower than the current value, existing sessions remain established, but no new sessions are permitted until usage falls below the newly-configured value.
> Usage
> Binds the IP address used as the connection point for establishing the IKEv2 sessions to a crypto template. It can also define the maximum number of sessions the FNG can support.
> Example
> The following command binds an FNG service with an IP address of 10.2.3.4 to the crypto template named T1 and sets the maximum number of sessions to 500000:
> bind address 10.2.3.4 crypto-template T1 max-sessions 500000
> default
> Sets or restores the default condition for the selected parameter.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> default { { aaa attribute 3gpp2-service-option } | duplicate-session-detection | ip source-violation { drop-limit | period } | setup-timeout | subscriber name }
> aaa attribute 3gpp2-service-option
> Sets or restores the default value of 4095.
> duplicate-session-detection
> Sets or restores the default option for duplicate session detection to be fapid-based.
> ip source-violation ( drop-limit | period }
> Sets or restores the IP source violation detection defaults, as follows:
> drop-limit: Sets or restores the maximum number of IP source violations within the detection period before dropping the call to the default value of 10.
> period: Sets or restores the detection period for IP source violations to the default value of 120 seconds.
> setup-timeout
> Sets or restores the maximum time allowed for session setup to the default value of 60 seconds.
> subscriber name
> Sets or restores the name of the default subscriber.
> name is a string of 1-127 characters.
> u sername mac-address-stripping
> The default behavior is to disable stripping the MAC address from the username.
> Usage
> Configures the default settings for a given parameter.
> Example
> Use the following command to set the maximum time allowed for session setup to the default value of 60 seconds:
> default setup-timeout
> duplicate-session-detection
> Configures the FNG to detect duplicate call sessions based on Femtocell Access Point (FAP) ID and to clear old call information.
> This feature is disabled by default.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> duplicate-session-detection { fapid-based }
> no duplicate-session-detection
> default duplicate-session-detection
> fapid-based
> Sets the FNG to detect duplicate call sessions based on the FAP ID.
> no duplicate-session-detection
> Disables duplicate session detection.
> default duplicate-session-detection
> Sets or restores the default option for duplicate session detection to be fapid-based.
> Usage
> By default, duplicate session detection is disabled.Use this command to enable this feature. It applies only to calls established after the feature has been enabled.
> The following command enables duplicate session detection based on FAP ID:
> duplicate-session-detection fapid-based
> ip source-violation
> Sets the parameters for IP source validation. Source validation is useful if packet spoofing is suspected or for verifying packet routing and labeling within the network.
> Source validation requires the source address of received packets to match the IP address assigned to the subscriber (either statically or dynamically) during the session.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> ip source-violation { clear-on-valid-packet | drop-limit num | period secs }
> no ip source-violation clear-on-valid-packet
> clear-on-valid-packet
> Configures the service to reset the drop-limit counters upon receipt of a properly addressed packet. Default: disabled
> drop-limit num
> Sets the maximum number of allowed IP source violations within the detection period before dropping a call as an integer from 1 through 1000000. Default: 10
> period secs
> Sets the detection period (in seconds) for IP source violations as an integer from 1 through 1000000. Default: 120
> Usage
> This function allows the operator to configure the network to prevent problems such as when a user gets handed back and forth between two gateways a number of times during a handoff scenario.
> When a subscriber packet is received with a source IP address violation, the system increments the IP source violation drop-limit counter and starts the timer for the IP source violation period. Every subsequent packet received with a bad source address during the IP source violation period causes the drop-limit counter to increment.
> For example, if the drop-limit is set to 10, after 10 source violations, the call is dropped. The detection period timer continues to count throughout this process.
> Example
> The following command sets the drop limit to 15 and leaves the other values at their default values:
> ip source-violation drop-limit 15
> setup-timeout
> Specifies the maximum time allowed to set up a session in seconds.
> Product
> FNG
> Privilege
> Security-Administrator, Administrator
> Syntax
> setup-timeout integer
> default setup-timeout
> setup-timeout integer
> Sets the session setup timer (in seconds) as an integer from 2 through 300. Default: 60
> default
> Sets or restores the default session setup timer value to 60 seconds.
> Usage
> The FNG clears both the user session and tunnels if a call does not initiate successfully before the session setup timer expires.
> Example
> The following command sets the session setup timeout value to the default value of 60 seconds:
> default setup-timeout

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883