> ACS Port Map Configuration Mode Commands
> The ACS Port Map Configuration Mode is used to define an application-port mapping in the ACS Configuration Mode. The application-port map associates a range of ports to a specific application/protocol within a rule definition (ruledef).
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> port
> This command allows you to add/remove an individual or a range of port numbers associated with an application or protocol from the current port map.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] port { port_number | range start_port_number to end_port_number }
> no
> If added previously, removes the specified port(s) from the current port map.
> port_number
> Specifies a port number to add to the current port map.
> port_number must be a port number, and must be an integer from 1 through 65535.
> range start_port_number to end_port_number
> Specifies a range of port numbers to add to the current port map.
> start_port_number specifies the starting port number of the range, it must be an integer from 1 through 65535, and must be less than end_port_number.
> end_port_number specifies the ending port number of the range, it must be an integer from 1 through 65535, and must be greater than start_port_number.
> Usage
> Use this command to add an individual or a range of port numbers to a port map. Up to 10 sets of ports can be configured in each port map.
> Example
> The following command adds all port numbers from 3112 through 5000 to the port map:
> port range 3112 to 5000

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883