> HNBGW-RANAP Schema Statistics
> The HNBGW-RANAP schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HNB-GW.
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the HNBGW-RANAP Schema

> Variables | Description | Data Type
> vpnname | The name of the context in which HNB-GW service is configured. This is a key variable. | String
> vpnid | The identity number of the context in which HNB-GW service is configured. This is a key variable. | String
> servname | The name of the HNB-GW service for which statistics are collected. This is a key variable. | String
> cs-initial-ue-rx | CS Domain: Indicates the total number of Initial UE message received. Trigger: When RANAP CS Domain Initial UE message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-dir-transfer-rx | CS Domain: Indicates the total number of Direct Transfer message received. Trigger: When RANAP CS Domain Direct Transfer message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-dir-transfer-tx | CS Domain: Indicates the total number of Direct Transfer message transmitted. Trigger: When RANAP CS Domain Direct Transfer message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-rx | CS Domain: Indicates the total number of Reset message received. Trigger: When RANAP CS Domain Reset message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-tx | CS Domain: Indicates the total number of Reset message transmitted. Trigger: When RANAP CS Domain Reset message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-ack-rx | CS Domain: Indicates the total number of Reset Ack message received. Trigger: When RANAP CS Domain Reset Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-ack-tx | CS Domain: Indicates the total number of Reset Ack message transmitted. Trigger: When RANAP CS Domain Reset Ack message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-res-rx | CS Domain: Indicates the total number of Reset Resource message received. Trigger: When RANAP CS Domain Reset Resource message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-res-tx | CS Domain: Indicates the total number of Reset Resource message transmitted. Trigger: When RANAP CS Domain Reset Resource message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-res-ack-rx | CS Domain: Indicates the total number of Reset Resource Ack message received. Trigger: When RANAP CS Domain Reset Resource Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reset-res-ack-tx | CS Domain: Indicates the total number of Reset Resource Ack message transmitted. Trigger: When RANAP CS Domain Reset Resource Ack message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-iu-rel-req-rx | CS Domain: Indicates the total number of Iu Release Request message received. Trigger: When RANAP CS Domain Iu Release Request message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-iu-rel-cmd-tx | CS Domain: Indicates the total number of Iu Release Command message transmitted. Trigger: When RANAP CS Domain Iu Release Command message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-iu-rel-comp-rx | CS Domain: Indicates the total number of Iu Release Complete message received. Trigger: When RANAP CS Domain Iu Release Complete message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-paging-req-tx | CS Domain: Indicates the total number of Paging Request message transmitted. Trigger: When RANAP CS Domain Paging Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-req-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-req-tx-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-req-tx-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx | CS Domain: Indicates the total number of RAB Assignment Response message received. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-rsp-rx-rab-setup-mod-rel-que-drop | CS Domain: Indicates the total number of RAB Assignment Response message received for RAB Set/Mod/Rel/Que Dropped. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for RAB Set/Mod/Rel/Que Dropped. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for UMTS AMR Codec for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for UMTS AMR Codec for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for UMTS AMR Codec for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for UMTS AMR Codec for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR Codec for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR Codec for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR Codec for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR Codec for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR Codec for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR Codec for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR Codec for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR Codec for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr-codec-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR Codec for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR Codec for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for UMTS AMR2 Codec for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for UMTS AMR2 Codec for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for UMTS AMR2 Codec for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for UMTS AMR2 Codec for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR2 Codec for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR2 Codec for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR2 Codec for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR2 Codec for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR2 Codec for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR2 Codec for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR2 Codec for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR2 Codec for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-amr2-codec-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for UMTS AMR2 Codec for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for UMTS AMR2 Codec for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for Other Codec for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for Other Codec for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for Other Codec for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for Other Codec for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Other Codec for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Other Codec for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Other Codec for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Other Codec for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Other Codec for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Other Codec for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Other Codec for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Other Codec for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-other-codec-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for Other Codec for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Other Codec for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for NO Codec for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for NO Codec for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for NO Codec for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for NO Codec for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for NO Codec for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for NO Codec for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for NO Codec for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for NO Codec for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for NO Codec for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for NO Codec for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for NO Codec for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for NO Codec for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-no-codec-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for NO Codec for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for NO Codec for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-setup-mod-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for Unknown Codec for RAB Setup/Mod. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for Unknown Codec for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-rel-tx | CS Domain: Indicates the total number of RAB Assignment Request message transmitted for Unknown Codec for RAB Release. Trigger: When RANAP CS Domain RAB Assignment Request message is transmitted by HNB-GW for Unknown Codec for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-setup-mod-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Unknown Codec for RAB Setup/Mod Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Unknown Codec for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-setup-mod-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Unknown Codec for RAB Setup/Mod Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Unknown Codec for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-rel-succ-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Unknown Codec for RAB Release Success. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Unknown Codec for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-rel-fail-rx | CS Domain: Indicates the total number of RAB Assignment Response message received for Unknown Codec for RAB Release Fail. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Unknown Codec for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-rab-ass-unknown-codec-rab-queued | CS Domain: Indicates the total number of RAB Assignment Response message received for Unknown Codec for RAB Queued. Trigger: When RANAP CS Domain RAB Assignment Response message is received by HNB-GW for Unknown Codec for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-tx | CS Domain: Indicates the total number of Relocation Request message transmitted. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-tx-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-ack-rx | CS Domain: Indicates the total number of Relocation Request Ack message received. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-ack-rx-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-ack-rx-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-ack-rx-rab-setup-dropped | CS Domain: Indicates the total number of Relocation Request Ack message received for RAB Setup Dropped. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for RAB Setup Dropped. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr-codec-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for UMTS AMR Codec for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for UMTS AMR Codec for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr-codec-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for UMTS AMR Codec for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for UMTS AMR Codec for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr-codec-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for UMTS AMR Codec for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for UMTS AMR Codec for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr2-codec-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for UMTS AMR2 Codec for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for UMTS AMR2 Codec for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr2-codec-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for UMTS AMR2 Codec for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for UMTS AMR2 Codec for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-amr2-codec-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for UMTS AMR2 Codec for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for UMTS AMR2 Codec for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-other-codec-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for Other Codec for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for Other Codec for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-other-codec-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for Other Codec for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for Other Codec for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-other-codec-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for Other Codec for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for Other Codec for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-no-codec-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for NO Codec for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for NO Codec for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-no-codec-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for NO Codec for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for NO Codec for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-no-codec-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for NO Codec for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for NO Codec for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-unknown-codec-rab-setup-tx | CS Domain: Indicates the total number of Relocation Request message transmitted for Unknown Codec for RAB Setup. Trigger: When RANAP CS Domain Relocation Request message is transmitted by HNB-GW for Unknown Codec for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-unknown-codec-rab-setup-succ-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for Unknown Codec for RAB Setup Success. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for Unknown Codec for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-req-unknown-codec-rab-setup-fail-rx | CS Domain: Indicates the total number of Relocation Request Ack message received for Unknown Codec for RAB Setup Fail. Trigger: When RANAP CS Domain Relocation Request Ack message is received by HNB-GW for Unknown Codec for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-detect-rx | CS Domain: Indicates the total number of Relocation Detect message received. Trigger: When RANAP CS Domain Relocation Detect message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-comp-rx | CS Domain: Indicates the total number of Relocation Complete message received. Trigger: When RANAP CS Domain Relocation Complete message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-fail-rx | CS Domain: Indicates the total number of Relocation Failure message received. Trigger: When RANAP CS Domain Relocation Failure message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-reloc-reqd-rx | CS Domain: Indicates the total number of Relocation Required message received. Trigger: When RANAP CS Domain Relocation Required message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-fwd-srns-ctx-req-rx | CS Domain: Indicates the total number of Fwd SRNS Context Request message received. Trigger: When RANAP CS Domain Fwd SRNS Context Request message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-srns-ctx-req-tx | CS Domain: Indicates the total number of SRNS Context Request message transmitted. Trigger: When RANAP CS Domain SRNS Context Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> cs-srns-ctx-rsp-rx | CS Domain: Indicates the total number of SRNS Context Response message received. Trigger: When RANAP CS Domain SRNS Context Response message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-initial-ue-rx | PS Domain: Indicates the total number of Initial UE message received. Trigger: When Initial UE message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-dir-transfer-rx | PS Domain: Indicates the total number of Direct Transfer message received. Trigger: When Direct Transfer message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-dir-transfer-tx | PS Domain: Indicates the total number of Direct Transfer message transmitted. Trigger: When Direct Transfer message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-rx | PS Domain: Indicates the total number of Reset message received. Trigger: When Reset message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-tx | PS Domain: Indicates the total number of Reset message transmitted. Trigger: When Reset message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-ack-rx | PS Domain: Indicates the total number of Reset Ack message received. Trigger: When Reset Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-ack-tx | PS Domain: Indicates the total number of Reset Ack message transmitted. Trigger: When Reset Ack message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-res-rx | PS Domain: Indicates the total number of Reset Resource message received. Trigger: When Reset Resource message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-res-tx | PS Domain: Indicates the total number of Reset Resource message transmitted. Trigger: When Reset Resource message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-res-ack-rx | PS Domain: Indicates the total number of Reset Resource Ack message received. Trigger: When Reset Resource Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reset-res-ack-tx | PS Domain: Indicates the total number of Reset Resource Ack message transmitted. Trigger: When Reset Resource Ack message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-iu-rel-req-rx | PS Domain: Indicates the total number of Iu Release Request message received. Trigger: When Iu Release Request message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-iu-rel-cmd-tx | PS Domain: Indicates the total number of Iu Release Command message transmitted. Trigger: When Iu Release Command message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-iu-rel-comp-rx | PS Domain: Indicates the total number of Iu Release Complete message received. Trigger: When Iu Release Complete message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-paging-req-tx | PS Domain: Indicates the total number of Paging Request message transmitted. Trigger: When Paging Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-req-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted. Trigger: When RAB Assignment Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-req-tx-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-req-tx-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx | PS Domain: Indicates the total number of RAB Assignment Response message received. Trigger: When RAB Assignment Response message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-rsp-rx-rab-setup-mod-rel-que-drop | PS Domain: Indicates the total number of RAB Assignment Response message received for RAB Set/Mod/Rel/Que Dropped. Trigger: When RAB Assignment Response message is received by HNB-GW for RAB Set/Mod/Rel/Que Dropped. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Conversational Class for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Conversational Class for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Conversational Class for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Conversational Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Conversational Class for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Conversational Class for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Conversational Class for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Conversational Class for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Conversational Class for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Conversational Class for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Conversational Class for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Conversational Class for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-conv-class-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for Conversational Class for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for Conversational Class for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Streaming Class for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Streaming Class for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Streaming Class for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Streaming Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Streaming Class for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Streaming Class for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Streaming Class for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Streaming Class for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Streaming Class for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Streaming Class for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Streaming Class for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Streaming Class for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-stream-class-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for Streaming Class for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for Streaming Class for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Interactive for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Interactive for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Interactive for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Interactive for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Interactive for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Interactive for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Interactive for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Interactive for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Interactive for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Interactive for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Interactive for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Interactive for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-inter-class-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for Interactive for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for Interactive for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Background for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Background for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Background for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Background for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Background for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Background for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Background for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Background for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Background for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Background for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Background for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Background for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-back-class-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for Background for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for Background for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-setup-mod-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Unknown for RAB Setup/Mod. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Unknown for RAB Setup/Mod. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-rel-tx | PS Domain: Indicates the total number of RAB Assignment Request message transmitted for Unknown for RAB Release. Trigger: When RAB Assignment Request message is transmitted by HNB-GW for Unknown for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-setup-mod-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Unknown for RAB Setup/Mod Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Unknown for RAB Setup/Mod Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-setup-mod-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Unknown for RAB Setup/Mod Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Unknown for RAB Setup/Mod Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-rel-succ-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Unknown for RAB Release Success. Trigger: When RAB Assignment Response message is received by HNB-GW for Unknown for RAB Release Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-rel-fail-rx | PS Domain: Indicates the total number of RAB Assignment Response message received for Unknown for RAB Release Fail. Trigger: When RAB Assignment Response message is received by HNB-GW for Unknown for RAB Release Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-rab-ass-unkwn-class-rab-queued | PS Domain: Indicates the total number of RAB Assignment Response message received for Unknown for RAB Queued. Trigger: When RAB Assignment Response message is received by HNB-GW for Unknown for RAB Queued. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-tx | PS Domain: Indicates the total number of Relocation Request message transmitted. Trigger: When Relocation Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-tx-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for RAB Setup message transmitted. Trigger: When Relocation Request message is transmitted by HNB-GW for RAB Setup message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-ack-rx | PS Domain: Indicates the total number of Relocation Request Ack message received. Trigger: When Relocation Request Ack message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-ack-rx-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request Ack message received for RAB Setup Success. Trigger: When Relocation Request Ack message is received by HNB-GW for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-ack-rx-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request Ack message received for RAB Setup Fail. Trigger: When Relocation Request Ack message is received by HNB-GW for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-conv-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for Conversational Class for RAB Setup. Trigger: When Relocation Request message is transmitted by HNB-GW for Conversational Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-conv-class-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request message received for Conversational Class for RAB Setup Success. Trigger: When Relocation Request message is received by HNB-GW for Conversational Class for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-conv-class-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request message received for Conversational Class for RAB Setup Fail. Trigger: When Relocation Request message is received by HNB-GW for Conversational Class for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-stream-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for Streaming Class for RAB Setup. Trigger: When Relocation Request message is transmitted by HNB-GW for Streaming Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-stream-class-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request message received for Streaming Class for RAB Setup Success. Trigger: When Relocation Request message is received by HNB-GW for Streaming Class for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-stream-class-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request message received for Streaming Class for RAB Setup Fail. Trigger: When Relocation Request message is received by HNB-GW for Streaming Class for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-inter-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for Interactive Class for RAB Setup. Trigger: When Relocation Request message is transmitted by HNB-GW for Interactive Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-inter-class-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request message received for Interactive Class for RAB Setup Success. Trigger: When Relocation Request message is received by HNB-GW for Interactive Class for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-inter-class-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request message received for Interactive Class for RAB Setup Fail. Trigger: When Relocation Request message is received by HNB-GW for Interactive Class for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-back-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for Background Class for RAB Setup. Trigger: When Relocation Request message is transmitted by HNB-GW for Background Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-back-class-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request message received for Background Class for RAB Setup Success. Trigger: When Relocation Request message is received by HNB-GW for Background Class for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-back-class-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request message received for Background Class for RAB Setup Fail. Trigger: When Relocation Request message is received by HNB-GW for Background Class for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-unkwn-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Request message transmitted for Unknown Class for RAB Setup. Trigger: When Relocation Request message is transmitted by HNB-GW for Unknown Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-unkwn-class-rab-setup-succ-rx | PS Domain: Indicates the total number of Relocation Request message received for Unknown Class for RAB Setup Success. Trigger: When Relocation Request message is received by HNB-GW for Unknown Class for RAB Setup Success. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-req-unkwn-class-rab-setup-fail-rx | PS Domain: Indicates the total number of Relocation Request message received for Unknown Class for RAB Setup Fail. Trigger: When Relocation Request message is received by HNB-GW for Unknown Class for RAB Setup Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-detect-rx | PS Domain: Indicates the total number of Relocation Detect message received. Trigger: When Relocation Detect message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-comp-rx | PS Domain: Indicates the total number of Relocation Complete message received. Trigger: When Relocation Complete message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-fail-rx | PS Domain: Indicates the total number of Relocation Failure message received. Trigger: When Relocation Failure message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-reqd-rx | PS Domain: Indicates the total number of Relocation Required message received. Trigger: When Relocation Required message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-prep-failure-tx | PS Domain: Indicates the total number of Relocation Prep Failure message transmitted. Trigger: When Relocation Prep Failure message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-fwd-srns-ctx-req-rx | PS Domain: Indicates the total number of Fwd SRNS Context Request message received. Trigger: When Fwd SRNS Context Request message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-cmd-tx | PS Domain: Indicates the total number of Relocation Command message transmitted. Trigger: When Relocation Command message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-cmd-tx-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-cmd-tx-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-cmd-tx-rab-setup-rel-local-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-invalid-rab-id | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Radio Network Layer Cause for Invalid Rab Id. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Radio Network Layer Cause for Invalid Rab Id. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-interact-othr-proc | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Radio Network Layer Cause for Interaction With Other Proc. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Radio Network Layer Cause for Interaction With Other Proc. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-sig-trans-res-fail | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Transport Layer Cause for Sig Transport Resource Fail. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Transport Layer Cause for Sig Transport Resource Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-iu-conn-fail-to-estab | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Transport Layer Cause for Iu Transport Conn failed to Establish. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Transport Layer Cause for Iu Transport Conn failed to Establish. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-trans-syn-err | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Causefor Transfer syntax error. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Causefor Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-abs-syn-err-ign | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error(Ignore). Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error(Ignore). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-semantic-err | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Cause for Semantic error. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-abs-syn-err-rej | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error (Reject). Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-msg-not-comp | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Cause for Msg not compatible with receiver state. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-falsely-construct-msg | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error (Falsely constructed msg). Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error (Falsely constructed msg). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-no-res-avalable | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Miscellaneous Cause for No Resource Available. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Miscellaneous Cause for No Resource Available. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-local-fail-unspecified | PS Domain: Indicates the total number of RAB Setup/Release Local Failure message transmitted for Miscellaneous Cause for Unspecified. Trigger: When RAB Setup/Release Local Failure message is transmitted by HNB-GW for Miscellaneous Cause for Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-conv-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Conversational Class for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for Conversational Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-conv-class-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Conversational Class for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for Conversational Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-conv-class-rab-setup-rel-local-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for Conversational Class for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for Conversational Class for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-stream-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Streaming Class for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for Streaming Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-stream-class-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Streaming Class for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for Streaming Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-stream-class-rab-setup-rel-local-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for Streaming Class for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for Streaming Class for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-inter-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Interactive Class for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for Interactive Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-inter-class-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Interactive Class for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for Interactive Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-inter-class-rab-setup-rel-local-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for Interactive Class for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for Interactive Class for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-back-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Background Class for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for Background Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-back-class-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Background Class for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for Background Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-back-class-rab-setup-rel-local-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for Background Class for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for Background Class for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-unkwn-class-rab-setup-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Unknown Class for RAB Setup. Trigger: When Relocation Command message is transmitted by HNB-GW for Unknown Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-unkwn-class-rab-rel-tx | PS Domain: Indicates the total number of Relocation Command message transmitted for Unknown Class for RAB Release. Trigger: When Relocation Command message is transmitted by HNB-GW for Unknown Class for RAB Release. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-reloc-unkwn-class-rab-setup-rel-lcl-fail | PS Domain: Indicates the total number of Relocation Command message transmitted for Unknown Class for RAB Setup/Release Local Failure. Trigger: When Relocation Command message is transmitted by HNB-GW for Unknown Class for RAB Setup/Release Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-ctx-req-tx | PS Domain: Indicates the total number of SRNS Context Request message transmitted. Trigger: When SRNS Context Request message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-ctx-rsp-rx | PS Domain: Indicates the total number of SRNS Context Response message received. Trigger: When SRNS Context Response message is received by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-data-fwd-cmd-tx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-rab-setup-tx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for RAB Setup Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for RAB Setup Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-invalid-rab-id | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Radio Network Layer Cause for Invalid Rab Id. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Radio Network Layer Cause for Invalid Rab Id. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-interact-with-othr-proc | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Radio Network Layer Cause for Interaction With Other Proc. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Radio Network Layer Cause for Interaction With Other Proc. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-sig-trans-res-fail | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Transport Layer Cause for Sig Transport Resource Fail. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Transport Layer Cause for Sig Transport Resource Fail. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-iu-trans-conn-fail-to-estab | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Transport Layer Cause for Iu Transport Conn failed to Establish. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Transport Layer Cause for Iu Transport Conn failed to Establish. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-trans-syn-err | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Causefor Transfer syntax error. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Causefor Transfer syntax error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-abs-syn-err-ign | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error(Ignore). Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error(Ignore). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-semantic-err | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Cause for Semantic error. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Semantic error. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-abs-syn-err-rej | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error (Reject). Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error (Reject). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-msg-not-comp | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Cause for Msg not compatible with receiver state. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Msg not compatible with receiver state. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-falsely-construct-msg | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Protocol Layer Cause for Abstract syntax error (Falsely constructed msg). Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Protocol Layer Cause for Abstract syntax error (Falsely constructed msg). Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-no-res-avalable | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Miscellaneous Cause for No Resource Available. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Miscellaneous Cause for No Resource Available. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-local-fail-unspecified | PS Domain: Indicates the total number of RAB Setup Local Failure message transmitted for Miscellaneous Cause for Unspecified. Trigger: When RAB Setup Local Failure message is transmitted by HNB-GW for Miscellaneous Cause for Unspecified. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-conv-class-rab-setup-rx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Conversational Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Conversational Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-conv-class-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Conversational Class for RAB Setup/Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Conversational Class for RAB Setup/Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-stream-class-rab-setup-rx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Streaming Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Streaming Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-stream-class-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Streaming Class for RAB Setup/Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Streaming Class for RAB Setup/Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-inter-class-rab-setup-rx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Interactive Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Interactive Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-inter-class-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Interactive Class for RAB Setup/Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Interactive Class for RAB Setup/Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-back-class-rab-setup-rx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Background Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Background Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-back-class-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Background Class for RAB Setup/Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Background Class for RAB Setup/Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-unkwn-class-rab-setup-rx | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Unknown Class for RAB Setup. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Unknown Class for RAB Setup. Availability: Across all HNB-GW Services | Unsigned Int32
> ps-srns-unkwn-class-rab-setup-local-fail | PS Domain: Indicates the total number of SRNS Data Fwd Command message transmitted for Unknown Class for RAB Setup/Local Failure. Trigger: When SRNS Data Fwd Command message is transmitted by HNB-GW for Unknown Class for RAB Setup/Local Failure. Availability: Across all HNB-GW Services | Unsigned Int32
> Important: See Bulk Statistics Overview chapter for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883