> MIP HA Assignment Table Configuration Mode Commands
> The Mobile IP HA Assignment Table Configuration Mode is used to assign specific Home Agent (HA) IP addresses to ranges of Mobile Node (MN) IP addresses.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> hoa-range
> This command assigns ranges of Mobile Node (MN) IP addresses to specific Home agent IP addresses.
> Product
> HA
> Privilege
> Security Administrator, Administrator
> Syntax
> hoa-range ip_addressip_address2 ha ip_address3
> no hoa-range ip_address ip_address2 ha ip_address3
> no
> Removes the specified Home Agent assignment from the assignment table.
> ip_address ip_address2
> Specifies a range of MN IP addresses. ip_address and ip_address2 must be specified in IPv4 dotted-decimal or IPv6 colon-separated notation.
> ha ip_address3
> Specifies the IP address of the Home Agent to assign to MNs that are within the specified range. ip_address3 must be specified in IPv4 dotted-decimal or IPv6 colon-separated notation.
> Usage
> Use this command to assign ranges of MN IP addresses to specific HAs.
> Important: A maximum of eight MIP HA assignment tables can be configured per context with a maximum of eight MIP HA assignment tables across all contexts.
> Important: A maximum of 256 non-overlapping hoa-ranges can be configured per MIP HA Assignment table with a maximum of 256 non-overlapping hoa-ranges across all MIP HA Assignment tables.
> Example
> The following command assigns any MN IP address that falls in the range of 192.168.100.0 through 192.168.101.0 to the HA with the IP address of 192.168.200.10:
> hoa-range 192.168.100.0 192.168.101.0 ha 192.168.200.10

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883