> ACS Packet Filter Configuration Mode Commands
> The ACS Packet Filter Configuration Mode is used to create and configure Active Charging Service (ACS) packet filters.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> direction
> This command allows you to specify the direction in which the current packet filter will be applied.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> direction { bi-directional | downlink | uplink }
> default direction
> default
> Configures this command with its default setting.
> Default: bi-directional
> bi-directional
> Specifies that the packet filter has to be applied in both uplink and downlink directions.
> downlink
> Specifies that the packet filter has to be applied only in the downlink direction.
> uplink
> Specifies that the packet filter has to be applied only in the uplink direction.
> Usage
> Use this command to specify the direction in which the packet filter has to be applied.
> Example
> The following command specifies that the packet filter must be applied in the downlink direction:
> direction downlink
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> ip local-port
> This command allows you to configure the IP 5-tuple local port(s) for the current packet filter.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip local-port { = port_number | range start_port_number to end_port_number }
> no ip local-port
> no
> If previously configured, deletes the ip local-port configuration from the current packet filter.
> port_number
> Specifies the port number of the transport protocol.
> port_number must be the port number, and must be an integer from 1 through 65535.
> range start_port_number to end_port_number
> Specifies a range of port numbers.
> start_port_number and end_port_number must be integers from 1 through 65535.
> end_port_number must be greater than start_port_number.
> Usage
> Use this command to configure the IP local port(s) for a packet filter.
> Example
> The following command configures the IP local port as 456:
> ip local-port 456
> ip protocol
> This command allows you to configure the IP protocol(s) for the current packet filter.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> In StarOS 8.x releases:
> ip protocol { = protocol_number | range start_protocol_number to end_protocol_number }
> no ip protocol
> In StarOS 9.0 and later releases:
> ip protocol = protocol_number
> no ip protocol
> no
> If previously configured, deletes the IP protocol configuration from the current packet filter.
> protocol_number
> Specifies the transport protocol field in the IP header.
> protocol_number must be the numerical value of the protocol, and must be an integer from 1 through 255.
> range start_protocol_number to end_protocol_number
> Important: In StarOS 9.0 and later releases this option is deprecated.
> Specifies a range of protocol assignment numbers.
> start_protocol_number and end_protocol_number must be integers from 1 through 255.
> end_protocol_number must be greater than start_protocol_number.
> Usage
> Use this command to configure the protocol(s) for a packet filter.
> Example
> The following command configures the protocol assignment number 300:
> ip protocol = 300
> ip remote-address
> This command allows you to configure the IP remote address(es) for the current packet filter.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> In StarOS 8.x releases:
> ip remote-address { = { ip_address | ip_address/mask } | range { ip_address | ip_address/mask } to { ip_address | ip_address/mask } }
> no ip remote-address
> In StarOS 9.0 and later releases:
> ip remote-address = { ip_address | ip_address/mask }
> no ip remote-address
> no
> If previously configured, deletes the IP remote-address configuration from the current packet filter.
> ip remote-address = { ip_address | ip_address/mask }
> ip_address specifies the IPv4/IPv6 address.
> ip_address/mask specifies the IPv4/IPv6 address and the number of subnet bits representing the subnet mask in shorthand.
> ip remote-address range { start_ip_address | start_ip_address/mask } to { end_ip_address | end_ip_address/mask }
> Important: In StarOS 9.0 and later releases this keyword has been deprecated.
> range specifies a range of IPv4/IPv6 addresses.
> start_ip_address and end_ip_address specify, for the range, the starting and ending IPv4/IPv6 addresses.end_ip_address must be greater than start_ip_address.
> start_ip_address/mask and end_ip_address/mask specify, for the range, the starting and ending IPv4/IPv6 address, and the number of subnet bits representing the subnet mask in shorthand. end_ip_address/mask must be greater than start_ip_address/mask.
> Usage
> Use this command to configure the remote address(es) for a packet filter.
> Example
> The following command configures the IP remote address as 10.2.3.4/24:
> ip remote-address 10.2.3.4/24
> ip remote-port
> This command allows you to configure the IP remote port(s) for the current packet filter.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> ip remote-port { = port_number | range start_port_number to end_port_number }
> no ip remote-port
> no
> If previously configured, deletes the ip remote-port configuration from the current packet filter.
> port_number
> Specifies the port number of the transport protocol.
> port_number must be the port number, and must be an integer from 1 through 65535.
> range start_port_number to end_port_number
> Specifies a range of port numbers.
> start_port_number and end_port_number must be integers from 1 through 65535.
> end_port_number must be greater than start_port_number.
> Usage
> Use this command to configure the IP remote port(s) for a packet filter.
> Example
> The following command configures the IP remote port as 789:
> ip remote-port = 789
> priority
> This command allows you to configure the current packet filter’s priority.
> Important: This command is deprecated in certain 9.0 releases and in 10.0 and later releases. The precedence values of packet filters (those from both dynamic and predefined rules) are assigned by the PCEF based on an internal process.
> Product
> ACS
> Privilege
> Security Administrator, Administrator
> Syntax
> priority priority
> no priority
> no
> If previously configured, deletes the priority configuration in the current packet filter.
> priority
> Specifies this packet filter’s priority
> priority must be an integer from 0 through 255.
> Usage
> Use this command to configure the packet filter’s priority. The priority must be configured for the packet filter to be used in a TFT. Packets are compared against packet filters in a prioritized fashion, with 0 being the highest priority. Without this setting, this filter will not be used.
> Example
> The following command configures the packet filter’s priority as 3:
> priority 3

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883