> ASN Service Profile Configuration Mode Commands
> Use the ASN Service Profile Configuration Mode to create and manage the service profiles table for the ASN-GW service subscribers within the current context.
> downlink-classifier
> Specifies which classifier to match for traffic flow in the downlink direction for subscribers in this service.
> Product
> ASN-GW
> Privilege
> Administrator
> Syntax
> [ no ] downlink-classifier class-map < class_map_name > [id < 0-65535 >] [priority < 0-255 >] [action { permit | deny } ]
> no
> Deletes the configured class map for this traffic flow in the ASN-GW service.
> class-map class_map_name
> Associates an existing Class-Map in the destination context to this traffic flow.
> For example:

> • | For downlink-classifier class-map c4, an id of 1 is generated or assigned.

> • | For downlink-classifier class-map c5, an id of 2 is generated or assigned.

> • | For downlink-classifier class-map c6, an id of 3 is generated or assigned.

> Refer to the Class-Map Configuration Mode Commands chapter for additional information on configuring the class maps.
> id < 0-65535 >
> Assure that id is unique in an asn-service-profile. If you do not configure the classier id, the sorted classifier name order is assigned as id.
> priority < 0-255 >
> Default: 0
> 0 = minimum, 255 = maximum
> Usage
> Use this command to configure classifier for downlink traffic with a configured Class-Map for the ASN-GW service subscribers.
> You can configure a maximum of four class-maps in one ASN-GW service profile.
> Access Class-Map Configuration Mode through the Context Configuration Mode.
> Example
> The following command applies the Class-Map class_1 to this traffic:
> downlink-classifier class-map class_1
> downlink-qos-id
> Specifies the QoS table identifier to traffic flowing in the downlink direction for subscribers in this service.
> Product
> ASN-GW
> Privilege
> Administrator
> Syntax
> downlink-qos-id < qos_table_id >
> [ no ] downlink-qos-id
> no
> Deletes the configured class map for this traffic flow in the ASN-GW service.
> qos_table_id
> Associates an existing ASN QoS descriptor identifier in the source context to this traffic flow.
> Refer to the ASN QoS Descriptor Configuration Mode Commands chapter of this reference for additional information on configuring QoS descriptor table identifiers.
> Usage
> Use this command to apply a QoS identifier for downlink traffic with a configured ASN QoS descriptor table identifier for the ASN-GW service subscribers.
> Configure only one QoS identifier per ASN-GW service profile.
> Access ASN QoS Descriptor Configuration Mode through Context Configuration Mode.
> Example
> The following command applies the QoS table identifier 123 to this traffic:
> downlink-qos-id 123
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> uplink-classifier
> Specifies which classifier to match for traffic flow in the uplink direction for subscribers in this service.
> Product
> ASN-GW
> Privilege
> Administrator
> Syntax
> [ no ] uplink-classifier class-map < class_map_name > [ id < 0-65535 > ] [ priority < 0-255 > ] [ action { permit | deny } ]
> no
> Deletes the configured class map for this traffic flow in the ASN-GW service.
> class-map class_map_name
> Specifiesan existing Class-Map in the destination context to this traffic flow. For example:

> • | For uplink-classifier class-map c1, an id of 1 is generated or assigned.

> • | For uplink-classifier class-map c2, an id of 2 is generated or assigned.

> • | For uplink-classifier class-map c3, an id of 3 is generated or assigned.

> Refer to the Class-Map Configuration Mode Commands chapter for additional information on configuring class maps.
> id < 0-65535 >
> Assure that id is unique in an asn-service-profile. If you do not configure the classier id, the sorted classifier name order is assigned as id.
> priority < 0-255 >
> Default: 0
> 0 = minimum, 255 = maximum
> Usage
> Use this command to configure classifier for uplink traffic with a configured Class-Map for the ASN-GW service subscribers.
> Configure a maximum of 4 class-maps per ASN-GW service profile.
> Access Class-Map Configuration Mode through Context Configuration Mode.
> Example
> The following command applies the Class-Map class_1 to this traffic:
> uplink-classifier class-map class_1
> uplink-qos-id
> Specifies the QoS table identifier to the traffic flow in the uplink direction for subscribers in this service.
> Product
> ASN-GW
> Privilege
> Administrator
> Syntax
> uplink-qos-id qos_table_id
> [ no ] uplink-qos-id
> no
> Deletes the configured class map for this traffic flow in the ASN-GW service.
> uplink_qos_id
> Associates an existing ASN QoS Descriptor Identifier in the source context to this traffic flow.
> Refer to the ASN QoS Descriptor Configuration Mode Commands chapter for additional information on configuring the QoS descriptor table identifier.
> Usage
> Use this command to apply a QoS identifier for uplink traffic with a configured ASN QoS Descriptor Table Identifier for the ASN-GW service subscribers.
> Configure only one QoS identifier per ASN-GW service profile.
> Access ASN QoS Descriptor Configuration Mode through Context Configuration Mode.
> Example
> The following command applies the QoS table identifier 123 to this traffic:
> uplink-qos-id 123

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883