> PCC-Data-Service Configuration Mode Commands
> The PCC-Data-Service Configuration Mode is used to configure the data flow parameters for the media data, as well as corresponding attributes that are necessary for charging and policy enforcement decisions for the media parameters represented by its service flows in the PCC-service. A maximum of ten service data flows can be configured in a PCC-Data-Service instance.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> flow direction in
> This command configures the flow service parameters for incoming data flow in PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] flow direction in protocol {ip | tcp | udp} from {src_ip_addr | any} port {src_port_num | any} to {dest_ip_addr | any} port {dest_port_num | any}
> no
> Removes the configured data service flow parameters from PCC-Data-Service instance for IPCF configuration.
> protocol {ip | tcp | udp}
> This keyword configures the data flow parameters for specific protocol.
> Following protocols are supported through this keyword:

> • | ip: Sets the parameters for IP traffic.

> • | tcp: Sets the parameters for TCP traffic.

> • | UDP: Sets the parameters for UDP traffic.

> from {src_ip_addr | any} port {src_port_num | any}
> This keyword configures the data flow condition parameters for specific protocol through IP address and port as source of flow.
> Following parameters are defined with this keyword:

> • | src_ip_addr: specifies the specific IP address in IPv4/IPv6 notation as source of flow.

> • | any: specifies that flow from any source IP address/port can be analyzed or considered.

> • | port src_port_num: specifies the specific source port parameter for flow.

> src_port_num is the source port number of flow and must be an integer from 1 through 65535.
> to {dest_ip_addr | any} port {dest_port_num | any}
> This keyword configures the data flow condition parameters for specific protocol through IP address and port as source of flow.
> Following parameters are defined with this keyword:

> • | dest_ip_addr: specifies the specific IP address in IPv4/IPv6 notation as destination of flow.

> • | any: specifies that flow to any destination IP address/port can be analyzed or considered.

> • | port dest_port_num: specifies the specific destination port parameter for flow.

> dest_port_num is the destination port number of flow and must be an integer from 1 through 65535.
> Usage
> Use this command to configure the flow service parameters for incoming data flow in PCC-Data-Service instance for IPCF Configuration.
> Example
> Following command sets the data service parameters for tcp type protocol from any IP/port source to any IP/port in incoming direction with in a PCC-Data-Service.
> flow direction in protocol tcp from any port any to any port any
> flow direction out
> This command configures the flow service parameters for outgoing data flow in PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] flow direction in protocol {ip | tcp | udp} from {src_ip_addr | any} port {src_port_num | any} to {dest_ip_addr | any} port {dest_port_num | any}
> no
> Removes the configured data service flow parameters from PCC-Data-Service instance on IPCF node.
> protocol {ip | tcp | udp}
> This keyword configures the data flow parameters for specific protocol.
> Following protocols are supported through this keyword:

> • | ip: Sets the parameters for IP traffic.

> • | tcp: Sets the parameters for TCP traffic.

> • | UDP: Sets the parameters for UDP traffic.

> from {src_ip_addr | any} port {src_port_num | any}
> This keyword configures the data flow condition parameters for specific protocol through IP address and port as source of flow.
> Following parameters are defined with this keyword:

> • | src_ip_addr: specifies the specific IP address in IPv4/IPv6 notation as source of flow.

> • | any: specifies that flow from any source IP address/port can be analyzed or considered.

> • | port src_port_num: specifies the specific source port parameter for flow.

> src_port_num is the source port number of flow and must be an integer from 1 through 65535.
> to {dest_ip_addr | any} port {dest_port_num | any}
> This keyword configures the data flow condition parameters for specific protocol through IP address and port as source of flow.
> Following parameters are defined with this keyword:

> • | dest_ip_addr: specifies the specific IP address in IPv4/IPv6 notation as destination of flow.

> • | any: specifies that flow to any destination IP address/port can be analyzed or considered.

> • | port dest_port_num: specifies the specific destination port parameter for flow.

> dest_port_num is the destination port number of flow and must be an integer from 1 through 65535.
> Usage
> Use this command to configure the flow service parameters for outgoing data flow in PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the data service parameters for tcp type protocol from any IP/port source to any IP/port in outgoing direction with in a PCC-Data-Service.
> flow direction out protocol tcp from any port any to any port any
> metering-method
> This command specifies the metering method to be used by PCEF for offline charging in a PCC-Data-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] metering-method {both-duration-volume | duration | volume}
> no
> Removes the configured metering method from PCC-Data-Service instance on IPCF node.
> In such scenario, the metering method pre-configured at PCEF is considered.
> both-duration-volume
> Specifies the metering method as based on volume of data usage and duration of session, both for offline charging in a PCC-Data-Service instance on IPCF node.
> duration
> Specifies the metering method as based on the duration of session usage for offline charging in a PCC-Data-Service instance on IPCF node.
> volume
> Specifies the metering method as based on the volume of data usage for offline charging in a PCC-Data-Service instance on IPCF node.
> Usage
> Use this command to define the metering method to be used for offline charging in a PCC-Data-Service instance on IPCF node.
> If no metering method is defined, the metering method preconfigured at PCEF is considered.
> Example
> Following command sets the metering method as based on volume of data usage and duration of session, both for offline charging in a PCC-Data-Service instance on IPCF node.
> metering-method both-duration-volume
> monitoring-key
> This command defines the monitoring key under which data is monitored for the PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> monitoring-key mon_key_value
> [no] monitoring-key
> no
> Removes the configured monitoring-key from PCC-Data-Service instance on IPCF node.
> mon_key_value
> Specifies the monitoring key value under which data usage is monitored for the PCC-Data-Service instance and must be an integer from 1 through 65535.
> Usage
> Use this command to define the monitoring key under which data is monitored for the PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the monitoring key 123 for data monitoring in PCC-Data-Service instance on IPCF node.
> monitoring-key 123
> precedence
> This command defines the precedence that is assigned to the Dynamic PCC rule created for a PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> precedence preced_value
> [no] precedence
> no
> Removes the configured precedence value from PCC-Data-Service instance on IPCF node.
> preced_value
> Specifies the precedence that is assigned to the dynamic PCC rule created for a PCC-Data-Service instance and must be an integer from 1 through 65535.
> Usage
> Use this command to define the precedence value that is assigned to the Dynamic PCC rule created for a PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the precedence value 2 to assign to the dynamic PCC rule created for a PCC-Data-Service instance on IPCF node.
> precedence 2
> qos-profile
> This command defines the PCC-QoS-Profile which is to use for the PCC-Data-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> qos-profile qos_prof_name
> [no] qos-profile
> no
> Removes the configured PCC-QoS-Profile from PCC-Data-Service instance on IPCF node.
> qos_prof_name
> Specifies the pre-configured PCC-QoS-Profile name which is to use for the PCC-Data-Service instance.
> Usage
> Use this command to define the PCC-QoS-Profile for a PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the PCC-QoS-Profile ipcf_qos_prof1 for PCC-Data-Service instance on IPCF node.
> qos-profile ipcf_qos_prof1
> rating-group
> This command defines the PCC-Rating-Group that is assigned for a PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> rating-group rating_grp_id
> [no] rating-group
> no
> Removes the configured PCC-Rating-Group Id from PCC-Data-Service instance on IPCF node.
> rating_grp_id
> Specifies the PCC-Rating-Group Id that is assigned to the PCC-Data-Service instance and must be an integer from 1 through 99.
> Usage
> Use this command to define the PCC-Rating Id value for a PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the Rating Group id 11 for a PCC-Data-Service instance on IPCF node.
> rating-group 11
> reporting-level
> This command specifies the reporting level to be used by PCEF to report the data usage for the related PCC rule in a PCC-Data-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] reporting-level {service-identifier-level | rating-group-level}
> no
> Removes the configured usage reporting level from PCC-Data-Service instance on IPCF node.
> In such scenario, the reporting level configured at PCEF is considered.
> service-identifier-level
> Sets the data usage reporting level to be used by PCEF to report the data usage for the related PCC rule at the service identifier level in a PCC-Data-Service instance on IPCF node.
> rating-group-level
> Sets the data usage reporting level to be used by PCEF to report the data usage for the related PCC rule at the Rating-group level in a PCC-Data-Service instance on IPCF node.
> Usage
> Use this command to define the reporting level to be used by PCEF to report the data usage for the related PCC rule in a PCC-Data-Service instance on IPCF node.
> If no reporting level is defined, the reporting level preconfigured at PCEF is considered.
> Example
> Following command sets the reporting level at ‘Rating-group’ level which is to be used by PCEF to report the data usage for the related PCC rule in a PCC-Data-Service instance on IPCF node.
> reporting-level rating-group-level
> service-identifier
> This command defines the service identifier for a PCC-Data-Service instance.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> service-identifier svc_id
> [no] service-identifier
> no
> Removes the configured Service Identifier from PCC-Data-Service instance on IPCF node.
> svc_id
> Specifies the Service Identifier that is assigned to the PCC-Data-Service instance and must be an integer from 1 through 65535.
> Usage
> Use this command to define the Service Identifier for a PCC-Data-Service instance on IPCF node.
> Example
> Following command sets the Service Identifier 1011 for a PCC-Data-Service instance on IPCF node.
> service-identifier 1011

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883