> HSGW Schema Statistics
> The HSGW schema provides operational statistics that can be used for monitoring and troubleshooting the following products: HSGW
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the HSGW Schema

> Variables | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the HSGW service. This is a key variable. | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the HSGW service. This is an internal reference number. This is a key variable. Type: Gauge | Int32
> servname | Displays the name of the HSGW service for which the statistics are displayed. This is a key variable. | String
> servid | The identification number of the service configured on the system that is currently facilitating the HSGW service. This is an internal reference number. This is a key variable. Type: Gauge | Int32
> sessstat-totcur-ue | Session Statistics - Total Current - UE Active Type: Gauge | Int32
> sessstat-totcur-pdn | Session Statistics - Total Current - PDN Type: Gauge | Int32
> sessstat-totcur-bearers | Session Statistics - Total Current - Bearers Type: Gauge | Int32
> sessstat-totcur-pdn-ipv4 | Session Statistics - Total Current - PDN IPv4 Type: Gauge | Int32
> sessstat-totcur-pdn-ipv6 | Session Statistics - Total Current - PDN IPv6 Type: Gauge | Int32
> sessstat-totcur-pdn-ipv4v6 | Session Statistics - Total Current - PDN IPv4v6 Type: Gauge | Int32
> sessstat-totsetup-ue | Session Statistics - Total Setup - UE | Int32
> sessstat-totsetup-pdn | Session Statistics - Total Setup - PDN | Int32
> sessstat-totsetup-bearers | Session Statistics - Total Setup - Bearers | Int32
> sessstat-pdnsetuptype-ipv4 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4 | Int32
> sessstat-pdnsetuptype-ipv6 | Session Statistics - Total PDNs Setup Per PDN-type - IPv6 | Int32
> sessstat-pdnsetuptype-ipv4v6 | Session Statistics - Total PDNs Setup Per PDN-type - IPv4v6 | Int32
> sessstat-pdnrel-ipv4 | Session Statistics - Total PDNs Released - IPv4Ctr32Servicesessstat | Int32
> sessstat-pdnrel-ipv6 | Session Statistics - Total PDNs Released - IPv6 | Int32
> sessstat-pdnrel-ipv4v6 | Session Statistics - Total PDNs Released - IPv4v6 | Int32
> sessstat-pdnrelrsn-pcf | Session Statistics - Total PDNs Released Reason - PCFMME Ini | Int32
> sessstat-pdnrelrsn-pgw | Session Statistics - Total PDNs Released Reason -PGW Ini | Int32
> sessstat-pdnrelrsn-pcrf | Session Statistics - Total PDNs Released Reason -PCRF Ini | Int32
> sessstat-pdnrelrsn-local | Session Statistics - Total PDNs Released Reason -Local | Int32
> sessstat-pdnrelrsn-other | Session Statistics - Total PDNs Released Reason -Other | Int32
> sessstat-pdnrej-ipv4 | Session Statistics - Total PDNs Rejected - IPv4 | Int32
> sessstat-pdnrej-ipv6 | Session Statistics - Total PDNs Rejected - IPv6 | Int32
> sessstat-pdnrej-ipv4v6 | Session Statistics - Total PDNs Rejected - IPv4v6 | Int32
> sessstat-pdnrejrsn-pgw | Session Statistics - Total PDNs Rejected Reason - PGW Reject | Int32
> sessstat-pdnrejrsn-apnauth | Session Statistics - Total PDNs Rejected Reason - APN Auth FailureLicense | Int32
> sessstat-pdnrejrsn-other | Session Statistics - Total PDNs Rejected Reason - OtherNewcall Policy | Int32
> sessstat-pdnrejrsn-pgwrej | Session Statistics - Total PDNs Rejected Reason - No PGW AvailableOverload | Int32
> sessstat-pdnrejrsn-pdnexists | Session Statistics - Total PDNs Rejected Reason - PDN Already ExisCongestion | Int32
> sessstat-pdnrejrsn-adminrej | Session Statistics - Total PDNs Rejected Reason - Admin Prohibited | Int32
> sessstat-pdnrejrsn-limitexceed | Session Statistics - Total PDNs Rejected Reason - PDN Limit ExceededOther | Int32
> sessstat-pdnrejrsn-unreach | Session Statistics - Total PDNs Rejected Reason - PDN GW Unreachable | Int32
> sessstat-pdnrejrsn-rscunavail | Session Statistics - Total PDNs Rejected Reason - Resource Unavailable | Int32
> sessstat-pdnrejrsn-sublimit | Session Statistics - Total PDNs Rejected Reason - Subscription Limitation | Int32
> sessstat-totinter-ho | Session Statistics - HandOff Statistics - Total Inter HSGW HO | Int32
> sessstat-totintra-ho | Session Statistics - HandOff Statistics - Total Intra HSGW HO | Int32
> sessstat-active | Session Statistics - HandOff Statistics - Active | Int32
> sessstat-dormant | Session Statistics - HandOff Statistics - Dormant | Int32
> sessstat-a10s-totcur | Session Statistics - A10 Statistics - Total A10s Current | Int32
> sessstat-a10s-maincur | Session Statistics - A10 Statistics - Main A10s Current | Int32
> sessstat-a10s-auxcur | Session Statistics - A10 Statistics - Aux A10s Current | Int32
> sessstat-a10s-totsetup | Session Statistics - A10 Statistics - Total A10s Setup | Int32
> sessstat-a10s-mainsetup | Session Statistics - A10 Statistics - Main A10s Setup | Int32
> sessstat-a10s-auxsetup | Session Statistics - A10 Statistics - Aux A10s Setup | Int32
> sessstat-a10s-totrel | Session Statistics - A10 Statistics - Total A10s Released | Int32
> sessstat-a10s-mainrel | Session Statistics - A10 Statistics - Main A10s Released | Int32
> sessstat-a10s-auxrel | Session Statistics - A10 Statistics - Aux A10s Released | Int32
> totepsbearsetup-qci1 | Total EPS Bearers Setup - QCI 1 | Int32
> totepsbearsetup-qci2 | Total EPS Bearers Setup - QCI 2 | Int32
> totepsbearsetup-qci3 | Total EPS Bearers Setup - QCI 3 | Int32
> totepsbearsetup-qci4 | Total EPS Bearers Setup - QCI 4 | Int32
> totepsbearsetup-qci5 | Total EPS Bearers Setup - QCI 5 | Int32
> totepsbearsetup-qci6 | Total EPS Bearers Setup - QCI 6 | Int32
> totepsbearsetup-qci7 | Total EPS Bearers Setup - QCI 7 | Int32
> totepsbearsetup-qci8 | Total EPS Bearers Setup - QCI 8 | Int32
> totepsbearsetup-qci9 | Total EPS Bearers Setup - QCI 9 | Int32
> totepsbearsetup-other | Total EPS Bearers Setup - Other | Int32
> totepsbearrel-qci1 | Total EPS Bearers Released - QCI 1 | Int32
> totepsbearrel-qci2 | Total EPS Bearers Released - QCI 2 | Int32
> totepsbearrel-qci3 | Total EPS Bearers Released - QCI 3 | Int32
> totepsbearrel-qci4 | Total EPS Bearers Released - QCI 4 | Int32
> totepsbearrel-qci5 | Total EPS Bearers Released - QCI 5 | Int32
> totepsbearrel-qci6 | Total EPS Bearers Released - QCI 6 | Int32
> totepsbearrel-qci7 | Total EPS Bearers Released - QCI 7 | Int32
> totepsbearrel-qci8 | Total EPS Bearers Released - QCI 8 | Int32
> totepsbearrel-qci9 | Total EPS Bearers Released - QCI 9 | Int32
> totepsbearrel-other | Total EPS Bearers Released - Other | Int32
> totepsbearmod-qci1 | Total EPS Bearers Modified - QCI 1 | Int32
> totepsbearmod-qci2 | Total EPS Bearers Modified - QCI 2 | Int32
> totepsbearmod-qci3 | Total EPS Bearers Modified - QCI 3 | Int32
> totepsbearmod-qci4 | Total EPS Bearers Modified - QCI 4 | Int32
> totepsbearmod-qci5 | Total EPS Bearers Modified - QCI 5 | Int32
> totepsbearmod-qci6 | Total EPS Bearers Modified - QCI 6 | Int32
> totepsbearmod-qci7 | Total EPS Bearers Modified - QCI 7 | Int32
> totepsbearmod-qci8 | Total EPS Bearers Modified - QCI 8 | Int32
> totepsbearmod-qci9 | Total EPS Bearers Modified - QCI 9 | Int32
> totepsbearmod-other | Total EPS Bearers Modified - Other | Int32
> totepsbearrelrsn-pgw | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PGW Ini | Int32
> totepsbearrelrsn-pcrf | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PCRF Ini | Int32
> totepsbearrelrsn-hsgw | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - HSGW IniS1 Error Ind | Int32
> totepsbearrelrsn-pdn | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - PDN DownS5 Error Ind | Int32
> totepsbearrelrsn-other | Total EPS Bearers Released - Total Dedicated Bearers Released Reason - Other | Int32
> datastat-uplink-qci1totbyte | Data Statistics - Uplink Statistics - QCI 1 Total-Bytes | Int64
> datastat-uplink-qci1totpkt | Data Statistics - Uplink Statistics - QCI 1 Total-Packets | Int64
> datastat-uplink-qci2totbyte | Data Statistics - Uplink Statistics - QCI 2 Total-Bytes | Int64
> datastat-uplink-qci2totpkt | Data Statistics - Uplink Statistics - QCI 2 Total-Packets | Int64
> datastat-uplink-qci3totbyte | Data Statistics - Uplink Statistics - QCI 3 Total-Bytes | Int64
> datastat-uplink-qci3totpkt | Data Statistics - Uplink Statistics - QCI 3 Total-Packets | Int64
> datastat-uplink-qci4totbyte | Data Statistics - Uplink Statistics - QCI 4 Total-Bytes | Int64
> datastat-uplink-qci4totpkt | Data Statistics - Uplink Statistics - QCI 4 Total-Packets | Int64
> datastat-uplink-qci5totbyte | Data Statistics - Uplink Statistics - QCI 5 Total-Bytes | Int64
> datastat-uplink-qci5totpkt | Data Statistics - Uplink Statistics - QCI 5 Total-Packets | Int64
> datastat-uplink-qci6totbyte | Data Statistics - Uplink Statistics - QCI 6 Total-Bytes | Int64
> datastat-uplink-qci6totpkt | Data Statistics - Uplink Statistics - QCI 6 Total-Packets | Int64
> datastat-uplink-qci7totbyte | Data Statistics - Uplink Statistics - QCI 7 Total-Bytes | Int64
> datastat-uplink-qci7totpkt | Data Statistics - Uplink Statistics - QCI 7 Total-Packets | Int64
> datastat-uplink-qci8totbyte | Data Statistics - Uplink Statistics - QCI 8 Total-Bytes | Int64
> datastat-uplink-qci8totpkt | Data Statistics - Uplink Statistics - QCI 8 Total-Packets | Int64
> datastat-uplink-qci9totbyte | Data Statistics - Uplink Statistics - QCI 9 Total-Bytes | Int64
> datastat-uplink-qci9totpkt | Data Statistics - Uplink Statistics - QCI 9 Total-Packets | Int64
> datastat-uplink-othertotbyte | Data Statistics - Uplink Statistics - Other Total-Bytes | Int64
> datastat-uplink-othertotpkt | Data Statistics - Uplink Statistics - Other Total-Packets | Int64
> datastat-downlink-qci1totbyte | Data Statistics - Downlink Statistics - QCI 1 Total-Bytes | Int64
> datastat-downlink-qci1totpkt | Data Statistics - Downlink Statistics - QCI 1 Total-Packets | Int64
> datastat-downlink-qci2totbyte | Data Statistics - Downlink Statistics - QCI 2 Total-Bytes | Int64
> datastat-downlink-qci2totpkt | Data Statistics - Downlink Statistics - QCI 2 Total-Packets | Int64
> datastat-downlink-qci3totbyte | Data Statistics - Downlink Statistics - QCI 3 Total-Bytes | Int64
> datastat-downlink-qci3totpkt | Data Statistics - Downlink Statistics - QCI 3 Total-Packets | Int64
> datastat-downlink-qci4totbyte | Data Statistics - Downlink Statistics - QCI 4 Total-Bytes | Int64
> datastat-downlink-qci4totpkt | Data Statistics - Downlink Statistics - QCI 4 Total-Packets | Int64
> datastat-downlink-qci5totbyte | Data Statistics - Downlink Statistics - QCI 5 Total-Bytes | Int64
> datastat-downlink-qci5totpkt | Data Statistics - Downlink Statistics - QCI 5 Total-Packets | Int64
> datastat-downlink-qci6totbyte | Data Statistics - Downlink Statistics - QCI 6 Total-Bytes | Int64
> datastat-downlink-qci6totpkt | Data Statistics - Downlink Statistics - QCI 6 Total-Packets | Int64
> datastat-downlink-qci7totbyte | Data Statistics - Downlink Statistics - QCI 7 Total-Bytes | Int64
> datastat-downlink-qci7totpkt | Data Statistics - Downlink Statistics - QCI 7 Total-Packets | Int64
> datastat-downlink-qci8totbyte | Data Statistics - Downlink Statistics - QCI 8 Total-Bytes | Int64
> datastat-downlink-qci8totpkt | Data Statistics - Downlink Statistics - QCI 8 Total-Packets | Int64
> datastat-downlink-qci9totbyte | Data Statistics - Downlink Statistics - QCI 9 Total-Bytes | Int64
> datastat-downlink-qci9totpkt | Data Statistics - Downlink Statistics - QCI 9 Total-Packets | Int64
> datastat-downlink-othertotbyte | Data Statistics - Downlink Statistics - Other Total-Bytes | Int64
> datastat-downlink-othertotpkt | Data Statistics - Downlink Statistics - Other Total-Packets | Int64
> ipv4-pdn-to-user-pkt | Data Statistics - IPv4 PDN to user packets | Int64
> ipv4-pdn-to-user-byte | Data Statistics - IPv4 PDN to user bytes | Int64
> ipv4-pdn-from-user-pkt | Data Statistics - IPv4 PDN from user packets | Int64
> ipv4-pdn-from-user-byte | Data Statistics - IPv4 PDN from user bytes | Int64
> ipv6-pdn-to-user-pkt | Data Statistics - IPv6 PDN to user packets | Int64
> ipv6-pdn-to-user-byte | Data Statistics - IPv6 PDN to user bytes | Int64
> ipv6-pdn-from-user-pkt | Data Statistics - IPv6 PDN from user packets | Int64
> ipv6-pdn-from-user-byte | Data Statistics - IPv6 PDN from user bytes | Int64
> ipv4v6-pdn-ipv4-to-user-pkt | Data Statistics - IPv4v6 PDN IPv4 to user packets | Int64
> ipv4v6-pdn-ipv4-to-user-byte | Data Statistics - IPv4v6 PDN IPv4 to user bytes | Int64
> ipv4v6-pdn-ipv4-from-user-pkt | Data Statistics - IPv4v6 PDN IPv4 from user packets | Int64
> ipv4v6-pdn-ipv4-from-user-byte | Data Statistics - IPv4v6 PDN IPv4 from user bytes | Int64
> ipv4v6-pdn-ipv6-to-user-pkt | Data Statistics - IPv4v6 PDN IPv6 to user packets | Int64
> ipv4v6-pdn-ipv6-to-user-byte | Data Statistics - IPv4v6 PDN IPv6 to user bytes | Int64
> ipv4v6-pdn-ipv6-from-user-pkt | Data Statistics - IPv4v6 PDN IPv6 from user packets | Int64
> ipv4v6-pdn-ipv6-from-user-byte | Data Statistics - IPv4v6 PDN IPv6 from user bytes | Int64
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883