> Fault Management
> This chapter identifies additions and changes made to fault management features in Release 12.x.
> Topics covered in this chapter are:

> l | SNMP MIB Objects and Alarms

> l | Cisco ANA Management Application Integration MIBs

> l | Web Element Manager Fault Management

> SNMP MIB Objects and Alarms
> This section lists additions and changes to MIB objects and alarms in Release 12.x.

> l | SNMP MIB Objects and Alarms in Release 12.0

> l | SNMP MIB Objects and Alarms in Release 12.1

> l | SNMP MIB Objects and Alarms in Release 12.2

> SNMP MIB Objects and Alarms in Release 12.0
> This section lists additions and changes to MIB objects and alarms in Release 12.0.

> l | New Objects

> l | Modified Objects

> l | Obsoleted Objects

> l | Deleted Objects

> l | New Alarms

> l | Modified Alarms

> l | Obsoleted Alarms

> l | Deleted Alarms

> New Objects

> l | starMVGEndpointName

> l | starMVGCauseCode

> l | starThreshEPDGCurrSess

> l | starThreshClearEPDGCurrSess

> l | starThreshSystemCapacity

> l | starThreshClearSystemCapacity

> l | starThreshCPUUtilization

> l | starThreshClearCPUUtilization

> l | starApsCommandSuccess

> l | starApsCommandFailure

> l | starApsSwitchSuccess

> l | starApsSwitchFailure

> l | starApsModeMismatch

> l | starApsChannelMismatch

> l | starApsByteMismatch

> l | starApsFeProtLineFailure

> l | starApsLossOfRedundancy

> l | starApsLossOfRedundancyClear

> l | starEmsBulkStatFilterDetails

> l | starEmsBulkStatCurrentDouble

> l | starEmsBulkStatThresholdDouble

> l | starEmsConfigBackupFileName

> l | starEmsConfigBackupFtpFailed

> l | starEmsConfigBackupFtpSuccess

> l | starEmsBulkStatIncrementalCounterThresholdAboveLimit

> l | starEmsBulkStatIncrementalCounterThresholdNormal

> l | starEmsBulkStatGaugeCounterUsageOverLimit

> l | starEmsBulkStatGaugeCounterUsageNormal

> l | starEmsConfigBackupFileDiff

> l | starMURThreshComaparator

> l | starMURKPITable

> l | starMURKPIEntry

> l | starMURGatewayName

> l | starMURKPIName

> l | starMUREntityName

> l | starMURThreshConfiguredString

> l | starMURThreshMeasuredString

> l | starMURKPIThreshCritical

> l | starMURKPIThreshCriticalClear

> l | starMURKPIThreshMajor

> l | starMURKPIThreshMajorClear

> l | starMURKPIThreshMinor

> l | starMURKPIThreshMinorClear

> l | starMURKPIThreshWarning

> l | starMURKPIThreshWarningClear

> l | starSGSServiceStart

> l | starSGSServiceStop

> l | starSgsnGnMsgDelay

> l | starSgsnGnMsgDelayClear

> l | starENBID

> l | starThreshPCCPolicySessions,

> l | starThreshClearPCCPolicySessions,

> l | starThreshPerServicePCCPolicySessions,

> l | starThreshClearPerServicePCCPolicySessions,

> l | starThreshPCCQuotaSessions,

> l | starThreshClearPCCQuotaSessions,

> l | starThreshPerServicePCCQuotaSessions,

> l | starThreshClearPerServicePCCQuotaSessions,

> l | starThreshPCCAFSessions,

> l | starThreshClearPCCAFSessions

> l | starThreshPerServicePCCAFSessions

> l | starThreshClearPerServicePCCAFSessions

> Modified Objects

> l | starPCFRrqRcvd

> l | starPCFRrqAccepted

> l | starPCFRrqDenied

> l | starPCFRrqDiscarded

> l | starPCFInitialRrqRcvd

> l | starPCFInitialRrqAccepted

> l | starPCFIntraPDSNActiveHORrqAccepted

> l | starPCFIntraPDSNDormantHORrqAccepted

> l | starPCFInterPDSNHORrqAccepted

> l | starPCFInitialRrqDenied

> l | starPCFInitialRrqDiscarded

> l | starPCFRenewRrqRcvd

> l | starPCFRenewRrqAccepted

> l | starPCFRenewActiveRrqAccepted

> l | starPCFRenewDormantRrqAccepted

> l | starPCFRenewRrqDenied

> l | starPCFRenewRrqDiscarded

> l | starPCFDeregRrqRcvd

> l | starPCFDeregRrqAccepted

> l | starPCFDeregDormantRrqAccepted

> l | starPCFDeregRrqDenied

> l | starPCFDeregRrqDiscarded

> l | starPCFIntraPDSNActiveAnidHORrqAccepted

> l | starPCFIntraPDSNDormantAnidHORrqAccepted

> l | starPCFDeniedUnSpeReason

> l | starPCFDeniedUnSpeReason

> l | starPCFDeniedInsufResource

> l | starPCFDeniedMobNodeAuthFail

> l | starPCFDeniedIdentMismatch

> l | starPCFDeniedPoorFormedReq

> l | starPCFDeniedUnknownPDSNAddr

> l | starPCFDeniedRevTunnelUnavail

> l | starPCFDeniedRevTunnelRequire

> l | starPCFDeniedUnrecogVendorId

> l | starPCFDeniedSessionClosed

> l | starPCFDeniedBsnSessionInfoUnavail

> l | starPCFRegUpdTransmitted

> l | starPCFRegUpdAccepted

> l | starPCFRegUpdateRpLifetimeExpiry

> l | starPCFRegUpdateUpperLayerIntiated

> l | starPCFRegUpdateOtherReason

> l | starPCFRegUpdateHORelease

> l | starPCFRegUpdateSessmgrDied

> l | starPCFAuxA10ConnectionsSetup

> l | starPCFSessionsDenied

> l | starPCFSessionsInit

> l | starPCFSessionsReneg

> l | starPCFDiscLcpRemote

> l | starPCFDiscRpRemote

> l | starPCFDiscRpLocal

> l | starPCFDiscMaxIpcpRetr

> l | starPCFDiscMaxIpv6cpRetr

> l | starPCFDiscMaxLcpRetr

> l | starPCFDiscAuthFail

> l | starPCFDiscSessSetupTimeout

> l | starPCFDiscFlowAddFail

> l | starPCFDiscInvDestContext

> l | starPCFDiscLcpOptFail

> l | starPCFDiscIpcpOptFail

> l | starPCFDiscIpv6cpOptFail

> l | starPCFDiscNoRemIpAddr

> l | starPCFDiscDetectionFail

> l | starPCFDiscMisc

> l | starPCFCurrentSessions

> l | starPCFSessionsSetup

> l | starPCFSessionsRelsese

> l | starPCFCurrentRevaSessions

> l | starEmsBulkStatThreshold

> l | starEmsBulkStatCurrent

> l | starEmsBulkStatCounterThresholdAboveLimit

> l | starEmsBulkStatCounterThresholdNormal

> l | starEmsBulkStatCounterUsageOverLimit

> l | starEmsBulkStatCounterUsageNormal

> l | starEmsNotifMgmtGroup

> l | starEmsNotifGroup

> l | starMURNotifMgmtGroup

> l | starPCFRrqRcvd

> l | StarentCardType

> - has added support for the following hardware Enumerations:

> l | pscA(24) -- Packet Services Card A

> l | ppc(25) -- Packet Processing Card

> l | lcchan3p2(26) -- Channelized Line card 2 Port

> l | lcchan3p4(27) -- Channelized Line card 4 Port

> l | fanctrl6(28) -- Fan control revision 6

> l | vioc(29) -- Virtual I/O Card

> l | gpdsp(30) -- GP-DSP Daughter Card

> l | xme(31), --XME Daughter Card

> l | vop(32) -- VOP Daughter Card

> l | edc(33)

> Obsoleted Objects
> None for this release.
> Deleted Objects
> None for this release.
> New Alarms

> l | starSGSNRNCNoResetAck

> Modified Alarms
> None for this release.
> Obsoleted Alarms
> None for this release.
> Deleted Alarms
> None for this release.
> Web Element Manager Path
> Select Configuration | SNMP Configuration.
> SNMP MIB Objects and Alarms in Release 12.1
> This section lists additions and changes to MIB objects and alarms in Release 12.1.

> l | New Objects

> l | Modified Objects

> l | Obsoleted Objects

> l | Deleted Objects

> l | New Alarms

> l | Modified Alarms

> l | Obsoleted Alarms

> l | Deleted Alarms

> New Objects
> None for this release
> Modified Objects

> l | starSSCProcessStartFail

> l | starSSCFTPServerUnreachable

> l | starSSCFTPServerReachable

> l | starSSCObjectGroup

> l | starSSCNotifGroup

> l | starPPTDBBackupDestinationNotAccessible

> l | starPPTDBBackupNotEnoughDiskSpace

> l | starPPTNotifMgmtGroup

> Obsoleted Objects
> None for this release.
> Deleted Objects
> None for this release
> New Alarms
> None for this release.
> Modified Alarms
> None for this release.
> Obsoleted Alarms
> None for this release.
> Deleted Alarms
> None for this release.
> Web Element Manager Path
> Select Configuration | SNMP Configuration.
> SNMP MIB Objects and Alarms in Release 12.2
> This section lists additions and changes to MIB objects and alarms in Release 12.2.
> New Objects

> l | StarCLIDatabaseUsername

> l | starPCCNtfyIntfPeerName

> l | starSessGTPPGroupName

> l | starMMES1PathTable

> l | starMMES1PathEntry

> l | starMMES1PathSvcID

> l | starMMES1PathENBID

> l | starMMES1PathVpnName

> l | starMMES1PathServName

> l | starMMES1PathSelfAddr

> l | starMMES1PathSelfPort

> l | starMMES1PathPeerAddr

> l | starMMES1PathPeerPort

> l | starLAGPartner

> l | starECSTotalDNSLearntIPThresholdInstance

> l | starECSTotalDNSLearntIPThresholdconfigured

> l | starECSTotalDNSLearntIPThresholdmeasured

> l | starPeerAddressIpv6

> Modified Objects

> l | StarGGSNSerEntry.

> l | starPCFSvcID

> The description has been modified to read:
> The service identification is made up from first 8 chars of the context name and the first 8 chars of the service name separated by (:), with the length of this structure at the beginning.

> l | starentCardType

> The following hardware Enumerations apply as of April 30, 2012:

> l | fanctrl6(28) -- Fan control revision 6

> l | vioc(29) -- Virtual I/O Card

> l | gpdsp(30) -- GP-DSP Daughter Card

> l | xme(31), --XME Daughter Card

> l | vop(32) -- VOP Daughter Card

> l | edc(33) -- EDC Card

> l | mio(34) -- Management & I/O Card

> l | mio10g10p(35) -- Management & 10x10Gb I/O Card

> l | mio10g20p(36) -- Management & 20x10Gb I/O Card

> l | mio40g2p(37) -- Management & 2x40Gb I/O Card

> l | mio40g4p(38) -- Management & 4x40Gb I/O Card

> l | mio40g12p(39) -- Management & 12x40Gb I/O Card

> l | miodc(40) -- MIO Daughter Card

> l | fsc(41) -- Fabric Card

> l | dpc(42) -- Data Processing Card

> l | mdpc(43) -- M Data Processing Card

> l | dpcdc(44) -- DPC Daughter Card

> l | ssc(45) -- System Status Card

> l | StarentCardType

> The following hardware Enumerations apply as of March 30, 2012:

> l | lcchan3p2(26) -- Channelized Line Card 2 Port

> l | lcchan3p4(27) -- Channelized Line Card 4 Port

> l | vioc(28) -- Virtual I/O Card

> l | gpdsp(39) -- GP-DSP Daughter Card

> l | xme(30), --XME Daughter Card

> l | vop(31) -- VOP Daughter Card

> l | edc(32)

> The following objects have been modified with the addition of new optional OID strings and a new CLI. These are described in the “SNMP Issues” section of the Cisco ANA Management Application Integration MIBs chapter in the Cisco ASR 5000 Series SNMP MIB Reference.

> l | sysDesc

> l | sysObjectId

> Obsoleted Objects

> l | None for this release

> Deleted Objects
> None for this release.
> New Alarms

> l | starThreshCardTemperatureNearPowerOffLimit

> l | starThreshClearCardTemperaturePowerOffLimit

> l | starAAAArchiveStarted

> l | starThreshAAAAcctArchiveQueue-1

> l | starThreshClearAAAAcctArchiveQueue-1

> l | starThreshAAAAcctArchiveQueue-2

> l | starThreshClearAAAAcctArchiveQueue-2

> l | starThreshAAAAcctArchiveQueue-3

> l | starThreshClearAAAAcctArchiveQueue-3

> l | starIPSecNodePeerDown

> l | starIPSecNodePeerUp

> l | starCdrPurged

> l | starLocalUserAdded

> l | starLocalUserRemoved

> l | starLocalUserPrivilegeChanged

> l | starOsShellAccessed

> l | starTestModeEntered

> l | starLicenseFeaturesModified

> l | starHiddenAccessEnabled

> l | starHiddenAccessDisabled

> l | starLawfulInterceptChanged

> l | starMMES1PathFail

> l | starMMES1PathSetup

> l | starAAAArchiveStarted

> l | starIPsecNodeIpv6PeerDown

> l | starIPsecNodeIpv6PeerUPstarAAAArchiveStarted

> l | starLAGGroupDown

> l | starLAGGroupUp

> l | starECSTotalDNSLearntIPv4Threshold

> l | starECSTotalDNSLearntIPv4ThresholdClear

> l | starECSTotalDNSLearntIPv6Threshold

> l | starECSTotalDNSLearntIPv6ThresholdClear

> l | starECSTotalDNSLearntIPv6Threshold

> l | starECSTotalDNSLearntIPv6ThresholdClear

> Modified Alarms
> The following alarms have changed trap numbers as follows:

> l | starECSTotalDNSLearntIPv4Threshold is now trap 1192

> l | starECSTotalDNSLearntIPv4ThresholdClear is now trap 1193

> The following alarms have changed traqp numbers as follows:

> l | starAAAArchiveStarted from 1191 to 1197

> l | starECSTotalDNSLearntIPv4Threshold 1192 to 1198

> l | starECSTotalDNSLearntIPv4ThresholdClear 1193 to 1199

> l | starECSTotalDNSLearntIPv6Threshold1194 to 1200

> l | starECSTotalDNSLearntIPv6ThresholdClear 1195 to 1201

> Obsoleted Alarms

> l | starPowerFilterUnitFailed

> l | starThreshPortSpecRxUtil

> l | starThreshClearPortSpecRxUtil

> l | starThreshPortSpecTxUtil

> l | starThreshClearPortSpecTxUtil

> Deleted Alarms
> None for this release.
> Web Element Manager Path
> Select Configuration | SNMP Configuration.
> Cisco ANA Management Application Integration MIBs
> The following MIBs are used to make a Cisco chassis available to customers using the Cisco ANA management application. These are supported in releases 12.0 and 12.2.

> l | IF MIB

> l | ENTITY MIB

> Please refer to the Cisco ASR 5000 Series SNMP MIB Reference.
> Web Element Manager Fault Management
> This section describes the Fault Management changes made in WEB Element Manager Releases 12.0 and 12.2.
> Web Element Manager Release 12.0
> The following enhancements were made to WEM Release 12.0.
> Addition to fm.cfg File for Setting Alarm Info Location Field
> A new section has been introduced to the fm.cfg file for setting the location field in the alarm information, as follows:

> l | Display card and port numbers only for card (hardware) related alarms. Setting this configuration will show only the card and port number instead of the complete varbind object list. WEM will show this information based on the value of the starSlotNum and ifindex objects. A WEM server restart is required.

> The format is <card-number/port-number>.
> Possible values are:

> l | ENABLE: Shows only card/port value in location information for card alarms. This is the default value.

> l | DISABLE: Show the values in default format with complete object information.

> l | UseCardPortNumber = ENABLE.

> l | All the WEM specific alarms have a varbind object starEmsNotifRaisedTime which carries the time when WEM generated the trap. This varbind object can be skipped in the location field. A WEM server restart is required.

> Possible values are:

> l | ENABLE: Skips the starEmsNotifRaisedTime varbind object. This is the default value.

> l | DISABLE: Shows the starEmsNotifRaisedTime varbind object.

> l | SkipWEMEventTimeObject = ENABLE.

> l | For alarms generated for SNMPv2 traps there are two standard SNMPv2 varbind objects (snmpTrapOid and sysUpTime). These varbind objects can be skipped in the location field.

> Also, note that for card/port related alarms, the value of the UseCardPortNumber parameter will override the configuration.
> A WEM server restart is required.

> l | ENABLE: Skips the SNMPv2 trap objects snmpTrapOid and sysUpTime. This is the default value.

> l | DISABLE: Shows the SNMPv2 standard objects.

> l | SkipSNMPv2StdObjects = ENABLE

> Web Element Manager Path

> l | On the WEM server: <ems_dir>/server/etc/fm.cfg

> Web Element Manager Release 12.2
> The following Fault Management changes were made in Web Element Manager Release 12.2.
> New Northbound Interface IRP Table Traps
> WEM supports the Northbound Interface as defined in the 3GPP standards for Telecom Management. 3GPP defines a standard interface (Interface-N) between the EMS and the NMS. It also defines Integration Reference Points (IRPs) through which various aspects of system management (FCAPS) are performed by the NMS.
> For WEM Release 12.2, support for unacknowledge_Alarms and acknowledge_Alarms has been added. These appear in the Alarm Operations category in the IRP table in the Overview chapter in the Cisco Web Element Manager Installation and Administration Guide.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883