> show orbem
> This chapter describes the output of the show orbem command.
> show orbem client id
> show orbem client id Command Output Descriptions

> Field | Description
> Application Server ID | The name of the ORBEM client as configured by the client command in the ORBEM configuration mode.
> State | The status of the ORBEM client as “Enabled” or “Disabled”. This indicates whether or not the system is manageable by the external Web Element Manager server: enabled indicates that it can be managed, disabled indicates that it is unmanageable. If the status is “Disabled”, it can be enabled by executing the activate client id command in the ORBEM Configuration Mode.
> Privileges | Indicates the management capabilities of the client as “FCAPS” (Fault, Configuration, Accounting, Performance, and Security).

> ‌
> show orbem status
> show orbem status Command Output Descriptions

> Field | Description
> Service State | Indicates whether the service state of the ORBEM client on the system is enabled (on) or disabled (off).
> Management Functions | Indicates which management functions ORBEM is currently allowing. Possible values for this field are:
> • | Fault
> • | Configuration
> • | Accounting
> • | Performance
> • | Security
> IOP URL | Indicates the universal resource locator (URL) of the system interface over which the Inter-ORB Protocol (IOP) will communicate.
> SSL Port | Indicates the Secure Socket Layer Inter-ORB Protocol (SIOP) TCP port that will be used by the ORB server (that runs on the system) to communicate with the client.
> TCP port | Indicates the Internet Inter-ORB Protocol (IIOP) Transport Control Protocol (TCP) port that will be used by the ORB server (that runs on the system) to communicate with the client. This is only used if IIOP transport is needed in addition to SIOP.
> Notification SSL Port | Indicates the TCP port number to be used by the CORBA event notification service SIOP transport.
> Notification TCP Port | Indicates the TCP port number to be used by the CORBA event notification service IIOP transport.
> Session Timeout | Indicates the amount of time an ORBEM client-session can be open and remain idle before ORBEM terminates the session. This value is a global value that is applied to all configured ORBEM clients.
> Max Login Attempts | Indicates the maximum number of times a client can attempt to login before ORBEM de-activates the client id.
> IIOP Transport | Indicates whether the Internet Inter-ORB Protocol (IIOP) transport is enabled (on) or disabled (off).
> Notification | Indicates whether the CORBA event notification service on the system is enabled (on) or disabled (off).
> Number of Current Sessions | Indicates the number of ORBEM sessions that currently exist.
> Number of Event Channels Open | Indicates the number of ORBEM event channels that are currently open.
> Number of Operations Completed | Indicates the number of ORBEM operations that have been completed.
> Number of Events Processed | Indicates the number of ORBEM events that have been processed.
> Avg Operation Processing time | Indicates the average processing time in seconds of recent ORBEM events.
> (last 1000) | Indicates the average processing time in seconds of the last 1000 ORBEM events.

> ‌
> show orbem session table
> show orbem session table Command Output Descriptions

> Field | Description
> Session ID | The identification number for the ORBEM session. This is a number used within the system to reference the session.
> Application Server | Indicates server that the ORBEM session is established with by the client id that was configured for the server.
> Context Name | The name of the context on the system that is facilitating the ORBEM configuration.
> Last transaction | Indicates the date and time of the last transaction between the system and the application server.

> ‌
> show orbem session table
> show orbem session table Command Output Descriptions

> Field | Description
> Session ID | The identification number for the ORBEM session. This is a number used within the system to reference the session.
> Application Server | Indicates server that the ORBEM session is established with by the client id that was configured for the server.
> Context Name | The name of the context on the system that is facilitating the ORBEM configuration.
> Last transaction | Indicates the date and time of the last transaction between the system and the application server.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883