> P-GW Node Level Schema Statistics
> The P-GW schema provides operational statistics that can be used for monitoring and troubleshooting the following products: P-GW
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the P-GW Service Schema

> Variables | Description | Data Type
> vpnname | The name of the context configured on the system that is currently facilitating the P-GW service. This is a key variable. Type: Information | String
> vpnid | The identification number of the context configured on the system that is currently facilitating the P-GW service. This is an internal reference number. This is a key variable. Type: Information | Int32
> servname | Displays the name of the P-GW service for which the statistics are displayed. This is a key variable. Type: Information | String
> servid | The identification number of the service configured on the system that is currently facilitating the P-GW service. This is an internal reference number. This is a key variable. Type: Information | Int32
> sess-cur | The total number of sessions currently established on this system. Type: Gauge | Int32
> sessstat-bearact-def | Session Statistics - Total default bearers active Type: Gauge | Int32
> sessstat-bearact-emergency-def | Session Statistics - Total emergency default bearers active Type: Gauge | Int32
> sessstat-bearact-emergency-auth-imsi-def | Session Statistics - Total emergency default bearers (Auth-IMSI) active Type: Gauge | Int32
> sessstat-bearact-emergency-unauth-imsi-def | Session Statistics - Total emergency default bearers (Unauth-IMSI) active Type: Gauge | Int32
> sessstat-bearact-emergency-only-imei-def | Session Statistics - Total emergency default bearers (Only IMEI) active Type: Gauge | Int32
> sessstat-bearact-ded | Session Statistics - Total dedicated bearers active Type: Gauge | Int32
> sessstat-bearact-ue-init-ded | Session Statistics - Total bearers active - UE-initiated Type: Gauge | Int32
> sessstat-bearact-nw-init-ded | Session Statistics - Total bearers active - Network-initiated Type: Gauge | Int32
> sessstat-bearact-emergency-ded | Session Statistics - Total emergency dedicated bearers active Type: Gauge | Int32
> sessstat-bearact-emergency-auth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Auth-IMSI) active Type: Gauge | Int32
> sessstat-bearact-emergency-unauth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Unauth-IMSI) active Type: Gauge | Int32
> sessstat-bearact-emergency-only-imei-ded | Session Statistics - Total emergency dedicated bearers (Only IMEI) active Type: Gauge | Int32
> sessstat-bearact-nw-init-ded-att | Session Statistics - Total bearers active - Network-initiated dedicated bearers Type: Gauge | Int32
> sessstat-bearsetup-def | Session Statistics - Total default bearers setup Type: Counter | Int32
> sessstat-bearsetup-emergency-def | Session Statistics - Total emergency default bearers setup Type: Counter | Int32
> sessstat-bearsetup-emergency-auth-imsi-def | Session Statistics - Total emergency default bearers (Auth-IMSI) setup Type: Counter | Int32
> sessstat-bearsetup-emergency-unauth-imsi-def | Session Statistics - Total emergency default bearers (Unauth-IMSI) setup Type: Counter | Int32
> sessstat-bearsetup-emergency-only-imei-def | Session Statistics - Total emergency default bearers (Only IMEI) setup Type: Counter | Int32
> sessstat-bearsetup-ded | Session Statistics - Total dedicated bearers setup Type: Counter | Int32
> sessstat-bearsetup-ue-init-ded | Session Statistics - Total bearers rejected - Network-req reject - No Resource Type: Counter | Int32
> sessstat-bearsetup-nw-init-ded | Session Statistics - Total bearers setup - Dedicated bearers - Network-initiated Type: Counter | Int32
> sessstat-bearsetup-emergency-ded | Session Statistics - Total emergency dedicated bearers setup Type: Counter | Int32
> sessstat-bearsetup-emergency-auth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Auth-IMSI) setup Type: Counter | Int32
> sessstat-bearsetup-emergency-unauth-imsi-ded | Session Statistics - Total emergency dedicated bearers (Unauth-IMSI) setup Type: Counter | Int32
> sessstat-bearsetup-emergency-only-imei-ded | Session Statistics - Total emergency dedicated bearers (Only IMEI) setup Type: Counter | Int32
> sessstat-bearrel-def | Session Statistics - Total default bearers released Type: Counter | Int32
> sessstat-bearrel-ded | Session Statistics - Total dedicated bearers released Type: Counter | Int32
> sessstat-bearrel-nwdefadmin | Session Statistics - Total bearers released - Network Default Admin disconnect Type: Counter | Int32
> sessstat-bearrel-nwdefgtp | Session Statistics - Total bearers released - Network Default GTP-U error ind Type: Counter | Int32
> sessstat-bearrel-nwdefsgw | Session Statistics - Total bearers released - Network Default S-GW Path failure Type: Counter | Int32
> sessstat-bearrel-nwdefmme | Session Statistics - Total bearers released - Network Default MME initiated release Type: Counter | Int32
> sessstat-bearrel-nwdedadmin | Session Statistics - Total bearers released - Network Dedicated Admin disconnect Type: Counter | Int32
> sessstat-bearrel-nwdedgtp | Session Statistics - Total bearers released - Network Dedicated GTP-U error ind Type: Counter | Int32
> sessstat-bearrel-nwdedmme | Session Statistics - Total bearers released - Network Dedicated MME initiated release Type: Counter | Int32
> sessstat-bearrel-nwdeddefbear | Session Statistics - Total bearers released - Network Dedicated Default bearer release Type: Counter | Int32
> sessstat-bearrel-nwdedgxdisc | Session Statistics - Total bearers released - Network Dedicated GX Disconnect Type: Counter | Int32
> sessstat-bearrelfail-def | Session Statistics - Total bearers release failure - Default bearers Type: Counter | Int32
> sessstat-bearrelfail-ded | Session Statistics - Total bearers release failure - Dedicated bearers Type: Counter | Int32
> sessstat-bearrej-def | Session Statistics - Total bearers rejected - Default bearers Type: Counter | Int32
> sessstat-bearrej-ded | Session Statistics - Total bearers rejected - Dedicated bearers Type: Counter | Int32
> sessstat-bearrej-emergency-def | Session Statistics - Total bearers rejected - Emergency default bearers Type: Counter | Int32
> sessstat-bearrej-emergency-ded | Session Statistics - Total bearers rejected - Emergency dedicated bearers Type: Counter | Int32
> sessstat-bearrej-nores | Session Statistics - Total bearers rejected - No Resource Type: Counter | Int32
> sessstat-bearrej-uereq | Session Statistics - Total bearers rejected - UE-req reject Type: Counter | Int32
> sessstat-bearrej-uereq-nores | Session Statistics - Total bearers rejected - UE-req reject - No Resource Type: Counter | Int32
> sessstat-bearrej-misapn | Session Statistics - Total bearers rejected - Missing or unknown APN Type: Counter | Int32
> sessstat-bearrej-nwreq | Session Statistics - Total bearers rejected - Network-req reject Type: Counter | Int32
> sessstat-bearrej-nwreq-nores | Session Statistics - Total bearers rejected - Network-req reject - No Resource Type: Counter | Int32
> sessstat-bearrej-nwreq-nomem | Session Statistics - Total bearers rejected - Network-req reject - No memory available Type: Counter | Int32
> sessstat-bearrej-nwreq-sysfail | Session Statistics - Total bearers rejected - Network-req reject - System failure Type: Counter | Int32
> sessstat-bearrej-apnmode | Session Statistics - Total bearers rejected - APN selection -Mode mismatch Type: Counter | Int32
> sessstat-bearrej-pdn | Session Statistics - Total bearers rejected - Pref PDN -Type not supported Type: Counter | Int32
> sessstat-bearrej-apnrestr | Session Statistics - Total bearers rejected - APN restr violation Type: Counter | Int32
> sessstat-bearrej-subsauth | Session Statistics - Total bearers rejected - Subs auth failed Type: Counter | Int32
> sessstat-bearrej-subsaddrnotallow | Session Statistics - Total bearers rejected - Subscriber’s static address not allowed Type: Counter | Int32
> sessstat-bearrej-subsaddrnotalloc | Session Statistics - Total bearers rejected - Subscriber’s static address not allocated Type: Counter | Int32
> sessstat-bearrej-dynaddrnotalloc | Session Statistics - Total bearers rejected - Dynamic address not allocated Type: Counter | Int32
> sessstat-bearrej-subsaddrnotpres | Session Statistics - Total bearers rejected - Subscriber’s static address not present Type: Counter | Int32
> sessstat-bearmod-ueinit | Session Statistics - Total bearers modified - UE-initiated modification Type: Counter | Int32
> sessstat-bearmod-nwinit | Session Statistics - Total bearers modified - Network-initiated modification Type: Counter | Int32
> sessstat-bearmod-ueqos | Session Statistics - Total bearers modified - UE-initiated quality of service (QoS) modification Type: Counter | Int32
> sessstat-bearmod-uetft | Session Statistics - Total bearers modified - UE-initiated TFT modification Type: Counter | Int32
> sessstat-bearmod-nwqos | Session Statistics - Total bearers modified - Network-initiated QoS modification Type: Counter | Int32
> sessstat-bearmod-nwtft | Session Statistics - Total bearers modified - Network-initiated TFT modification Type: Counter | Int32
> sessstat-bearmodfail-ueinit | Session Statistics - Total bearers modification failure - UE-initiated modification failed Type: Counter | Int32
> sessstat-bearmodfail-nwinit | Session Statistics - Total bearers modification failure - Network-initiated modification failed Type: Counter | Int32
> sessstat-bearmodfail-uenores | Session Statistics - Total bearers modification failure - UE-initiated No res available Type: Counter | Int32
> sessstat-bearmodfail-uesemtft | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in TFT oper Type: Counter | Int32
> sessstat-bearmodfail-uesyntft | Session Statistics - Total bearers modification failure - UE-initiated Syntax error in TFT oper Type: Counter | Int32
> sessstat-bearmodfail-uesempkt | Session Statistics - Total bearers modification failure - UE-initiated Semantic error in packet filter Type: Counter | Int32
> sessstat-bearmodfail-uesynpkt | Session Statistics - Total bearers modification failure - UE-initiated syntax error in packet filter Type: Counter | Int32
> sessstat-bearmodfail-nwnores | Session Statistics - Total bearers modification failure - Network-initiated - No res available Type: Counter | Int32
> sessstat-bearmodfail-nwnomem | Session Statistics - Total bearers modification failure - Network-initiated - No memory available Type: Counter | Int32
> sessstat-bearmodfail-nwsysfail | Session Statistics - Total bearers modification failure - Network-initiated - System failure Type: Counter | Int32
> sessstat-bearmodfail-nwsemtft | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in TFT oper Type: Counter | Int32
> sessstat-bearmodfail-nwsyntft | Session Statistics - Total bearers modification failure - Network-initiated syntax error in TFT oper Type: Counter | Int32
> sessstat-bearmodfail-nwsempkt | Session Statistics - Total bearers modification failure - Network-initiated Semantic error in packet filter Type: Counter | Int32
> sessstat-bearmodfail-nwsynpkt | Session Statistics - Total bearers modification failure - Network-initiated syntax error in packet filter Type: Counter | Int32
> sessstat-bearmodfail-qos-uenores | Session Statistics - Total bearer modification failures - User equipment quality of service no response errors Type: Counter | Int32
> sessstat-bearmodfail-qos-uesemtft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT semantics errors Type: Counter | Int32
> sessstat-bearmodfail-qos-uesyntft | Session Statistics - Total bearer modification failures - User equipment quality of service TFT syntax errors Type: Counter | Int32
> sessstat-bearmodfail-qos-uesempkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet semantics errors Type: Counter | Int32
> sessstat-bearmodfail-qos-uesynpkt | Session Statistics - Total bearer modification failures - User equipment quality of service packet syntax errors Type: Counter | Int32
> sessstat-bearmodfail-qos-nwnores | Session Statistics - Total bearer modification failures - Network-initiated quality of service no response Type: Counter | Int32
> sessstat-bearmodfail-qos-nwnomem | Session Statistics - Total bearer modification failures - Network-initiated quality of service no memory Type: Counter | Int32
> sessstat-bearmodfail-qos-nwsysfail | Session Statistics - Total bearer modification failures - Network-initiated quality of service system failures Type: Counter | Int32
> sessstat-bearmodfail-qos-nwsemtft | Session Statistics - Total bearer modification failures - Network-initiated quality of service semantics of TFT Type: Counter | Int32
> sessstat-bearmodfail-qos-nwsyntft | Session Statistics - Total modified bearer failures - Network-initiated TFT syntax Type: Counter | Int32
> sessstat-bearmodfail-qos-nwsempkt | Session Statistics - Total modified bearer failures - Network quality of service semantics packets Type: Counter | Int32
> sessstat-bearmodfail-qos-nwsynpkt | Session Statistics - Total modified bearer failures - Network quality of service syntax of packets Type: Counter | Int32
> sessstat-beardel-ded | Session Statistics - Total deleted dedicated bearers Type: Counter | Int32
> sessstat-nw-init-qos-update-att | Session Statistics - Total bearers modified - Network initiated - quality of service (QoS) modifications attempted Type: Counter | Int32
> sessstat-nw-init-no-qos-update-att | Session Statistics - Total bearers modified - Network initiated - no quality of service (QoS) modifications attempted Type: Counter | Int32
> sessstat-nw-init-bearer-fail-cause | Session Statistics - Total bearers modification failure - Network-initiated Syntax error in packet filter Type: Counter | Int32
> sessstat-pdn-ipv4active | Session Statistics - Total PDN-Type Statistics - IPv4 Active Type: Gauge | Int32
> sessstat-pdn-ipv4setup | Session Statistics - Total PDN-Type Statistics - IPv4 Setup Type: Counter | Int32
> sessstat-pdn-ipv4rel | Session Statistics - Total PDN-Type Statistics - IPv4 Released Type: Counter | Int32
> sessstat-pdn-ipv6active | Session Statistics - Total PDN-Type Statistics - IPv6 Active Type: Gauge | Int32
> sessstat-pdn-ipv6setup | Session Statistics - Total PDN-Type Statistics - IPv6 Setup Type: Counter | Int32
> sessstat-pdn-ipv6rel | Session Statistics - Total PDN-Type Statistics - IPv6 Released Type: Counter | Int32
> sessstat-pdn-ipv4v6active | Session Statistics - Total PDN-Type Statistics - IPv4v6 Active Type: Gauge | Int32
> sessstat-pdn-ipv4v6setup | Session Statistics - Total PDN-Type Statistics - IPv4v6 Setup Type: Counter | Int32
> sessstat-pdn-ipv4v6rel | Session Statistics - Total PDN-Type Statistics - IPv4v6 Released Type: Counter | Int32
> sessstat-ipv4addaloc | Session Statistics - IPv4 address allocation Type: Counter | Int32
> sessstat-ipaddaloc-ipv4loacalpool | Session Statistics - IP address allocation Statistics - IPv4 Local pool address assign Type: Counter | Int32
> sessstat-ipaddaloc-ipv4staticaddr | Session Statistics - IP address allocation Statistics - IPv4 Static address assign Type: Counter | Int32
> sessstat-ipaddaloc-ipv4radaddr | Session Statistics - IP address allocation Statistics - IPv4 Radius provided address assign Type: Counter | Int32
> sessstat-ipv6addaloc | Session Statistics - IPv6 address allocation Type: Counter | Int32
> sessstat-ipaddaloc-ipv6auto | Session Statistics - IP address allocation Statistics - IPv6 Stateless auto config Type: Counter | Int32
> subplmnstat-homesubact | Subscriber PLMN Statistics - Home subscribers sessions active Type: Gauge | Int32
> subplmnstat-homesubsetup | Subscriber PLMN Statistics - Home subscribers sessions setup Type: Counter | Int32
> subplmnstat-homesubrel | Subscriber PLMN Statistics - Home subscribers sessions released Type: Counter | Int32
> subplmnstat-roamsubact | Subscriber PLMN Statistics - Roaming subscribers sessions active Type: Gauge | Int32
> subplmnstat-roamsubsetup | Subscriber PLMN Statistics - Roaming subscribers sessions setup Type: Counter | Int32
> subplmnstat-roamsubrel | Subscriber PLMN Statistics - Roaming subscribers sessions released Type: Counter | Int32
> subplmnstat-visitsubact | Subscriber PLMN Statistics - Visiting subscribers sessions active Type: Gauge | Int32
> subplmnstat-visitsubsetup | Subscriber PLMN Statistics - Visiting subscribers sessions setup Type: Counter | Int32
> subplmnstat-visitsubrel | Subscriber PLMN Statistics - Visiting subscribers sessions released Type: Counter | Int32
> sgitunstat-ipv4sessact | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions active Type: Gauge | Int32
> sgitunstat-ipv4sesssetup | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions setup Type: Counter | Int32
> sgitunstat-ipv4sessrel | SGi tunneling Statistics - IPv4 IP-in-IP tunnel sessions released Type: Counter | Int32
> sgitunstat-ipv4gresessact | SGi tunneling Statistics - IPv4 GRE tunnel sessions active Type: Gauge | Int32
> sgitunstat-ipv4gresesssetup | SGi tunneling Statistics - IPv4 GRE tunnel sessions setup Type: Counter | Int32
> sgitunstat-ipv4gresessrel | SGi tunneling Statistics - IPv4 GRE tunnel sessions released Type: Counter | Int32
> sgitunstat-ipv6sessact | SGi tunneling Statistics - IPv6 6to4 tunnel sessions active Type: Gauge | Int32
> sgitunstat-ipv6sesssetup | SGi tunneling Statistics - IPv6 6to4 tunnel sessions setup Type: Counter | Int32
> sgitunstat-ipv6sessrel | SGi tunneling Statistics - IPv6 6to4 tunnel sessions released Type: Counter | Int32
> handoverstat-intersgsnatt | Handover Statistics - Total number of inter-SGSN handover attempts Type: Counter | Int32
> handoverstat-intersgsnsucc | Handover Statistics - Total number of successful inter-SGSN handovers Type: Counter | Int32
> handoverstat-intersgsnfail | Handover Statistics - Total number of failed inter-SGSN handovers Type: Counter | Int32
> handoverstat-intersgwatt | Handover Statistics - Total number of inter-SGW handover attempts Type: Counter | Int32
> handoverstat-intersgwsucc | Handover Statistics - Total number of successful inter-SGW handovers Type: Counter | Int32
> handoverstat-intersgwfail | Handover Statistics - Total number of failed inter-SGW handovers Type: Counter | Int32
> handoverstat-interhsgwatt | Handover Statistics - Total number of inter-HSGW handover attempts Type: Counter | Int32
> handoverstat-interhsgwsucc | Handover Statistics - Total number of successful inter-HSGW handovers Type: Counter | Int32
> handoverstat-interhsgwfail | Handover Statistics - Total number of failed inter-HSGW handovers Type: Counter | Int32
> handoverstat-gngptolteatt | Handover Statistics - Number of Gn/Gp to LTE attempted handovers Type: Counter | Int32
> handoverstat-gngptoltesucc | Handover Statistics - Number of Gn/Gp to LTE successful handovers Type: Counter | Int32
> handoverstat-gngptoltefail | Handover Statistics - Number of Gn/Gp to LTE failed handovers Type: Counter | Int32
> handoverstat-ltetogngpatt | Handover Statistics - Number of LTE to Gn/Gp attempted handovers Type: Counter | Int32
> handoverstat-ltetogngpsucc | Handover Statistics - Number of LTE to Gn/Gp successful handovers Type: Counter | Int32
> handoverstat-ltetogngpfail | Handover Statistics - Number of LTE to Gn/Gp failed handovers Type: Counter | Int32
> handoverstat-ltetoehrpdatt | Handover Statistics -Number of LTE to eHPRD attempted handovers Type: Counter | Int32
> handoverstat-ltetoehrpdsucc | Handover Statistics - Number of LTE to eHPRD successful handovers Type: Counter | Int32
> handoverstat-ltetoehrpdfail | Handover Statistics - Number of LTE to eHRPD failed handovers Type: Counter | Int32
> handoverstat-ehrpdtolteatt | Handover Statistics - Number of eHPRD to LTE attempted handovers Type: Counter | Int32
> handoverstat-ehrpdtoltesucc | Handover Statistics - Number of eHPRD to LTE successful handovers Type: Counter | Int32
> handoverstat-ehrpdtoltefail | Handover Statistics - Number of eHPRD to LTE failed handovers Type: Counter | Int32
> subqosstat-bearact-qci1 | Subscriber QoS Statistics - Total bearers active - QCI 1 Type: Gauge | Int32
> subqosstat-bearact-qci2 | Subscriber QoS Statistics - Total bearers active - QCI 2 Type: Gauge | Int32
> subqosstat-bearact-qci3 | Subscriber QoS Statistics - Total bearers active - QCI 3 Type: Gauge | Int32
> subqosstat-bearact-qci4 | Subscriber QoS Statistics - Total bearers active - QCI 4 Type: Gauge | Int32
> subqosstat-bearact-qci5 | Subscriber QoS Statistics - Total bearers active - QCI 5 Type: Gauge | Int32
> subqosstat-bearact-qci6 | Subscriber QoS Statistics - Total bearers active - QCI 6 Type: Gauge | Int32
> subqosstat-bearact-qci7 | Subscriber QoS Statistics - Total bearers active - QCI 7 Type: Gauge | Int32
> subqosstat-bearact-qci8 | Subscriber QoS Statistics - Total bearers active - QCI 8 Type: Gauge | Int32
> subqosstat-bearact-qci9 | Subscriber QoS Statistics - Total bearers active - QCI 9 Type: Gauge | Int32
> subqosstat-bearact-qcinongbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (Non-GBR) Type: Gauge | Int32
> subqosstat-bearact-qcigbr | Subscriber QoS Statistics - Total bearers active - Non-Standard QCI (GBR) Type: Gauge | Int32
> subqosstat-bearsetup-qci1 | Subscriber QoS Statistics - Total bearers setup - QCI 1 Type: Counter | Int32
> subqosstat-bearsetup-qci2 | Subscriber QoS Statistics - Total bearers setup - QCI 2 Type: Counter | Int32
> subqosstat-bearsetup-qci3 | Subscriber QoS Statistics - Total bearers setup - QCI 3 Type: Counter | Int32
> subqosstat-bearsetup-qci4 | Subscriber QoS Statistics - Total bearers setup - QCI 4 Type: Counter | Int32
> subqosstat-bearsetup-qci5 | Subscriber QoS Statistics - Total bearers setup - QCI 5 Type: Counter | Int32
> subqosstat-bearsetup-qci6 | Subscriber QoS Statistics - Total bearers setup - QCI 6 Type: Counter | Int32
> subqosstat-bearsetup-qci7 | Subscriber QoS Statistics - Total bearers setup - QCI 7 Type: Counter | Int32
> subqosstat-bearsetup-qci8 | Subscriber QoS Statistics - Total bearers setup - QCI 8 Type: Counter | Int32
> subqosstat-bearsetup-qci9 | Subscriber QoS Statistics - Total bearers setup - QCI 9 Type: Counter | Int32
> subqosstat-bearsetup-qcinongbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subqosstat-bearsetup-qcigbr | Subscriber QoS Statistics - Total bearers setup - Non-Standard QCI (GBR) Type: Counter | Int32
> subqosstat-bearrel-qci1 | Subscriber QoS Statistics - Total bearers released - QCI 1 Type: Counter | Int32
> subqosstat-bearrel-qci2 | Subscriber QoS Statistics - Total bearers released - QCI 2 Type: Counter | Int32
> subqosstat-bearrel-qci3 | Subscriber QoS Statistics - Total bearers released - QCI 3 Type: Counter | Int32
> subqosstat-bearrel-qci4 | Subscriber QoS Statistics - Total bearers released - QCI 4 Type: Counter | Int32
> subqosstat-bearrel-qci5 | Subscriber QoS Statistics - Total bearers released - QCI 5 Type: Counter | Int32
> subqosstat-bearrel-qci6 | Subscriber QoS Statistics - Total bearers released - QCI 6 Type: Counter | Int32
> subqosstat-bearrel-qci7 | Subscriber QoS Statistics - Total bearers released - QCI 7 Type: Counter | Int32
> subqosstat-bearrel-qci8 | Subscriber QoS Statistics - Total bearers released - QCI 8 Type: Counter | Int32
> subqosstat-bearrel-qci9 | Subscriber QoS Statistics - Total bearers released - QCI 9 Type: Counter | Int32
> subqosstat-bearrel-qcinongbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subqosstat-bearrel-qcigbr | Subscriber QoS Statistics - Total bearers released - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-totuppktfwd | Subscriber Data Statistics - Total Uplink packets forwarded Type: Counter | Int32
> subdatastat-uppktfwd-qci1 | Subscriber Data Statistics -Uplink packets forwarded - QCI 1 Type: Counter | Int32
> subdatastat-uppktfwd-qci2 | Subscriber Data Statistics -Uplink packets forwarded - QCI 2 Type: Counter | Int32
> subdatastat-uppktfwd-qci3 | Subscriber Data Statistics -Uplink packets forwarded - QCI 3 Type: Counter | Int32
> subdatastat-uppktfwd-qci4 | Subscriber Data Statistics -Uplink packets forwarded - QCI 4 Type: Counter | Int32
> subdatastat-uppktfwd-qci5 | Subscriber Data Statistics -Uplink packets forwarded - QCI 5 Type: Counter | Int32
> subdatastat-uppktfwd-qci6 | Subscriber Data Statistics -Uplink packets forwarded - QCI 6 Type: Counter | Int32
> subdatastat-uppktfwd-qci7 | Subscriber Data Statistics -Uplink packets forwarded - QCI 7 Type: Counter | Int32
> subdatastat-uppktfwd-qci8 | Subscriber Data Statistics -Uplink packets forwarded - QCI 8 Type: Counter | Int32
> subdatastat-uppktfwd-qci9 | Subscriber Data Statistics -Uplink packets forwarded - QCI 9 Type: Counter | Int32
> subdatastat-uppktfwd-stdqcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-uppktfwd-stdqcigbr | Subscriber Data Statistics - Uplink packets forwarded - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktfwd-qcinongbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-uppktfwd-qcigbr | Subscriber Data Statistics - Uplink packets forwarded - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktfwd-totgbr | Subscriber Data Statistics - Uplink packets forwarded - Total GBR Type: Counter | Int32
> subdatastat-uppktfwd-totnongbr | Subscriber Data Statistics - Uplink packets forwarded - Total Non-GBR Type: Counter | Int32
> subdatastat-totupbytefwd | Subscriber Data Statistics - Total Uplink bytes forwarded Type: Counter | Int64
> subdatastat-upbytefwd-qci1 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 1 Type: Counter | Int64
> subdatastat-upbytefwd-qci2 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 2 Type: Counter | Int64
> subdatastat-upbytefwd-qci3 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 3 Type: Counter | Int64
> subdatastat-upbytefwd-qci4 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 4 Type: Counter | Int64
> subdatastat-upbytefwd-qci5 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 5 Type: Counter | Int64
> subdatastat-upbytefwd-qci6 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 6 Type: Counter | Int64
> subdatastat-upbytefwd-qci7 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 7 Type: Counter | Int64
> subdatastat-upbytefwd-qci8 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 8 Type: Counter | Int64
> subdatastat-upbytefwd-qci9 | Subscriber Data Statistics - Uplink bytes forwarded - QCI 9 Type: Counter | Int64
> subdatastat-upbytefwd-stdqcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-upbytefwd-stdqcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytefwd-qcinongbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-upbytefwd-qcigbr | Subscriber Data Statistics - Uplink bytes forwarded - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytefwd-totgbr | Subscriber Data Statistics - Uplink bytes forwarded - Total GBR Type: Counter | Int64
> subdatastat-upbytefwd-totnongbr | Subscriber Data Statistics - Uplink bytes forwarded - Total NON-GBR Type: Counter | Int64
> subdatastat-totdownpktfwd | Subscriber Data Statistics - Total Downlink packets forwarded Type: Counter | Int32
> subdatastat-downpktfwd-qci1 | Subscriber Data Statistics - Downlink packets forwarded - QCI 1 Type: Counter | Int32
> subdatastat-downpktfwd-qci2 | Subscriber Data Statistics - Downlink packets forwarded - QCI 2 Type: Counter | Int32
> subdatastat-downpktfwd-qci3 | Subscriber Data Statistics - Downlink packets forwarded - QCI 3 Type: Counter | Int32
> subdatastat-downpktfwd-qci4 | Subscriber Data Statistics - Downlink packets forwarded - QCI 4 Type: Counter | Int32
> subdatastat-downpktfwd-qci5 | Subscriber Data Statistics - Downlink packets forwarded - QCI 5 Type: Counter | Int32
> subdatastat-downpktfwd-qci6 | Subscriber Data Statistics - Downlink packets forwarded - QCI 6 Type: Counter | Int32
> subdatastat-downpktfwd-qci7 | Subscriber Data Statistics - Downlink packets forwarded - QCI 7 Type: Counter | Int32
> subdatastat-downpktfwd-qci8 | Subscriber Data Statistics - Downlink packets forwarded - QCI 8 Type: Counter | Int32
> subdatastat-downpktfwd-qci9 | Subscriber Data Statistics - Downlink packets forwarded - QCI 9 Type: Counter | Int32
> subdatastat-downpktfwd-stdqcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-downpktfwd-stdqcigbr | Subscriber Data Statistics - Downlink packets forwarded - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktfwd-qcinongbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-downpktfwd-qcigbr | Subscriber Data Statistics - Downlink packets forwarded - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktfwd-totgbr | Subscriber Data Statistics - Downlink packets forwarded - Total GBR Type: Counter | Int32
> subdatastat-downpktfwd-totnongbr | Subscriber Data Statistics - Downlink packets forwarded - Total Non-GBR Type: Counter | Int32
> subdatastat-totdownbytefwd | Subscriber Data Statistics - Total Downlink bytes forwarded Type: Counter | Int64
> subdatastat-downbytefwd-qci1 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 1 Type: Counter | Int64
> subdatastat-downbytefwd-qci2 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 2 Type: Counter | Int64
> subdatastat-downbytefwd-qci3 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 3 Type: Counter | Int64
> subdatastat-downbytefwd-qci4 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 4 Type: Counter | Int64
> subdatastat-downbytefwd-qci5 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 5 Type: Counter | Int64
> subdatastat-downbytefwd-qci6 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 6 Type: Counter | Int64
> subdatastat-downbytefwd-qci7 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 7 Type: Counter | Int64
> subdatastat-downbytefwd-qci8 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 8 Type: Counter | Int64
> subdatastat-downbytefwd-qci9 | Subscriber Data Statistics - Downlink bytes forwarded - QCI 9 Type: Counter | Int64
> subdatastat-downbytefwd-stdqcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytefwd-stdqcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytefwd-qcinongbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytefwd-qcigbr | Subscriber Data Statistics - Downlink bytes forwarded - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytefwd-totgbr | Subscriber Data Statistics - Downlink bytes forwarded - Total GBR Type: Counter | Int64
> subdatastat-downbytefwd-totnongbr | Subscriber Data Statistics - Downlink bytes forwarded - Total Non-GBR Type: Counter | Int64
> subdatastat-totuppktdrop | Subscriber Data Statistics - Total Uplink packets dropped Type: Counter | Int32
> subdatastat-uppktdrop-qci1 | Subscriber Data Statistics -Uplink packets dropped - QCI 1 Type: Counter | Int32
> subdatastat-uppktdrop-qci2 | Subscriber Data Statistics -Uplink packets dropped - QCI 2 Type: Counter | Int32
> subdatastat-uppktdrop-qci3 | Subscriber Data Statistics -Uplink packets dropped - QCI 3 Type: Counter | Int32
> subdatastat-uppktdrop-qci4 | Subscriber Data Statistics -Uplink packets dropped - QCI 4 Type: Counter | Int32
> subdatastat-uppktdrop-qci5 | Subscriber Data Statistics -Uplink packets dropped - QCI 5 Type: Counter | Int32
> subdatastat-uppktdrop-qci6 | Subscriber Data Statistics -Uplink packets dropped - QCI 6 Type: Counter | Int32
> subdatastat-uppktdrop-qci7 | Subscriber Data Statistics -Uplink packets dropped - QCI 7 Type: Counter | Int32
> subdatastat-uppktdrop-qci8 | Subscriber Data Statistics -Uplink packets dropped - QCI 8 Type: Counter | Int32
> subdatastat-uppktdrop-qci9 | Subscriber Data Statistics -Uplink packets dropped - QCI 9 Type: Counter | Int32
> subdatastat-uppktdrop-stdqcinongbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-uppktdrop-stdqcigbr | Subscriber Data Statistics - Uplink packets dropped - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktdrop-qcinongbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-uppktdrop-qcigbr | Subscriber Data Statistics - Uplink packets dropped - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktdrop-totgbr | Subscriber Data Statistics - Uplink packets dropped - Total GBR Type: Counter | Int32
> subdatastat-uppktdrop-totnongbr | Subscriber Data Statistics - Uplink packets dropped - Total Non-GBR Type: Counter | Int32
> subdatastat-totupbytedrop | Subscriber Data Statistics - Total Uplink bytes dropped Type: Counter | Int64
> subdatastat-upbytedrop-qci1 | Subscriber Data Statistics - Uplink bytes dropped - QCI 1 Type: Counter | Int64
> subdatastat-upbytedrop-qci2 | Subscriber Data Statistics - Uplink bytes dropped - QCI 2 Type: Counter | Int64
> subdatastat-upbytedrop-qci3 | Subscriber Data Statistics - Uplink bytes dropped - QCI 3 Type: Counter | Int64
> subdatastat-upbytedrop-qci4 | Subscriber Data Statistics - Uplink bytes dropped - QCI 4 Type: Counter | Int64
> subdatastat-upbytedrop-qci5 | Subscriber Data Statistics - Uplink bytes dropped - QCI 5 Type: Counter | Int64
> subdatastat-upbytedrop-qci6 | Subscriber Data Statistics - Uplink bytes dropped - QCI 6 Type: Counter | Int64
> subdatastat-upbytedrop-qci7 | Subscriber Data Statistics - Uplink bytes dropped - QCI 7 Type: Counter | Int64
> subdatastat-upbytedrop-qci8 | Subscriber Data Statistics - Uplink bytes dropped - QCI 8 Type: Counter | Int64
> subdatastat-upbytedrop-qci9 | Subscriber Data Statistics - Uplink bytes dropped - QCI 9 Type: Counter | Int64
> subdatastat-upbytedrop-stdqcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-upbytedrop- stdqcigbr | Subscriber Data Statistics - Uplink bytes dropped - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytedrop-qcinongbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-upbytedrop-qcigbr | Subscriber Data Statistics - Uplink bytes dropped - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytedrop-totgbr | Subscriber Data Statistics - Uplink bytes dropped - Total GBR Type: Counter | Int64
> subdatastat-upbytedrop-totnongbr | Subscriber Data Statistics - Uplink bytes dropped - Total Non-GBR Type: Counter | Int64
> subdatastat-totdownpktdrop | Subscriber Data Statistics - Total Downlink packets dropped Type: Counter | Int32
> subdatastat-downpktdrop-qci1 | Subscriber Data Statistics - Downlink packets dropped - QCI 1 Type: Counter | Int32
> subdatastat-downpktdrop-qci2 | Subscriber Data Statistics - Downlink packets dropped - QCI 2 Type: Counter | Int32
> subdatastat-downpktdrop-qci3 | Subscriber Data Statistics - Downlink packets dropped - QCI 3 Type: Counter | Int32
> subdatastat-downpktdrop-qci4 | Subscriber Data Statistics - Downlink packets dropped - QCI 4 Type: Counter | Int32
> subdatastat-downpktdrop-qci5 | Subscriber Data Statistics - Downlink packets dropped - QCI 5 Type: Counter | Int32
> subdatastat-downpktdrop-qci6 | Subscriber Data Statistics - Downlink packets dropped - QCI 6 Type: Counter | Int32
> subdatastat-downpktdrop-qci7 | Subscriber Data Statistics - Downlink packets dropped - QCI 7 Type: Counter | Int32
> subdatastat-downpktdrop-qci8 | Subscriber Data Statistics - Downlink packets dropped - QCI 8 Type: Counter | Int32
> subdatastat-downpktdrop-qci9 | Subscriber Data Statistics - Downlink packets dropped - QCI 9 Type: Counter | Int32
> subdatastat-downpktdrop-stdqcinongbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-downpktdrop-stdqcigbr | Subscriber Data Statistics - Downlink packets dropped - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktdrop-qcinongbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-downpktdrop-qcigbr | Subscriber Data Statistics - Downlink packets dropped - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktdrop-totgbr | Subscriber Data Statistics - Downlink packets dropped - Total GBR Type: Counter | Int32
> subdatastat-downpktdrop-totnongbr | Subscriber Data Statistics - Downlink packets dropped - Total Non-GBR Type: Counter | Int32
> subdatastat-totdownbytedrop | Subscriber Data Statistics - Total Downlink bytes dropped Type: Counter | Int64
> subdatastat-downbytedrop-qci1 | Subscriber Data Statistics - Downlink bytes dropped - QCI 1 Type: Counter | Int64
> subdatastat-downbytedrop-qci2 | Subscriber Data Statistics - Downlink bytes dropped - QCI 2 Type: Counter | Int64
> subdatastat-downbytedrop-qci3 | Subscriber Data Statistics - Downlink bytes dropped - QCI 3 Type: Counter | Int64
> subdatastat-downbytedrop-qci4 | Subscriber Data Statistics - Downlink bytes dropped - QCI 4 Type: Counter | Int64
> subdatastat-downbytedrop-qci5 | Subscriber Data Statistics - Downlink bytes dropped - QCI 5 Type: Counter | Int64
> subdatastat-downbytedrop-qci6 | Subscriber Data Statistics - Downlink bytes dropped - QCI 6 Type: Counter | Int64
> subdatastat-downbytedrop-qci7 | Subscriber Data Statistics - Downlink bytes dropped - QCI 7 Type: Counter | Int64
> subdatastat-downbytedrop-qci8 | Subscriber Data Statistics - Downlink bytes dropped - QCI 8 Type: Counter | Int64
> subdatastat-downbytedrop-qci9 | Subscriber Data Statistics - Downlink bytes dropped - QCI 9 Type: Counter | Int64
> subdatastat-downbytedrop-stdqcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytedrop-stdqcigbr | Subscriber Data Statistics - Downlink bytes dropped - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytedrop-qcinongbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytedrop-qcigbr | Subscriber Data Statistics - Downlink bytes dropped - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytedrop-totgbr | Subscriber Data Statistics - Downlink bytes dropped - Total GBR Type: Counter | Int64
> subdatastat-downbytedrop-totnongbr | Subscriber Data Statistics - Downlink bytes dropped - Total Non-GBR Type: Counter | Int64
> subdatastat-totuppktdropmbrexc | Subscriber Data Statistics - Total Uplink packets Drop mbr exceed Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci1 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 1 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci2 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 2 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci3 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 3 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci4 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 4 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci5 | Subscriber Data Statistics - Uplink packets Drop mbr exceed- QCI 5 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci6 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 6 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci7 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 7 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci8 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 8 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qci9 | Subscriber Data Statistics - Uplink packets Drop mbr exceed - QCI 9 Type: Counter | Int32
> subdatastat-uppktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int32
> subdatastat-uppktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-uppktdropmbrexc-qcigbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-uppktdropmbrexc-totgbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total GBR Type: Counter | Int32
> subdatastat-uppktdropmbrexc-totnongbr | Subscriber Data Statistics - Uplink packets Drop mbr exceed - Total Non-GBR Type: Counter | Int32
> subdatastat-totupbytedropmbrexc | Subscriber Data Statistics - Total Uplink bytes Drop mbr exceed Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci1 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 1 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci2 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 2 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci3 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 3 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci4 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 4 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci5 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed- QCI 5 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci6 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 6 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci7 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 7 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci8 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 8 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qci9 | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - QCI 9 Type: Counter | Int64
> subdatastat-upbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int64
> subdatastat-upbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-upbytedropmbrexc-qcigbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-upbytedropmbrexc-totgbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total GBR Type: Counter | Int64
> subdatastat-upbytedropmbrexc-totnongbr | Subscriber Data Statistics - Uplink bytes Drop mbr exceed - Total NON-GBR Type: Counter | Int64
> subdatastat-totdownpktdropmbrexc | Subscriber Data Statistics - Total Downlink packets Drop mbr exceed Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci1 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 1 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci2 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 2 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci3 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 3 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci4 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 4 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci5 | Subscriber Data Statistics - Downlink packets Drop mbr exceed- QCI 5 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci6 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 6 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci7 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 7 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci8 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 8 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qci9 | Subscriber Data Statistics - Downlink packets Drop mbr exceed - QCI 9 Type: Counter | Int32
> subdatastat-downpktdropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (Non-GBR Type: Counter | Int32
> subdatastat-downpktdropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int32
> subdatastat-downpktdropmbrexc-qcigbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int32
> subdatastat-downpktdropmbrexc-totgbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total GBR Type: Counter | Int32
> subdatastat-downpktdropmbrexc-totnongbr | Subscriber Data Statistics - Downlink packets Drop mbr exceed - Total NON-GBR Type: Counter | Int32
> subdatastat-totdownbytedropmbrexc | Subscriber Data Statistics - Total Downlink bytes Drop mbr exceed Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci1 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 1 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci2 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 2 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci3 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 3 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci4 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 4 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci5 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed- QCI 5 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci6 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 6 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci7 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 7 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci8 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 8 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qci9 | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - QCI 9 Type: Counter | Int64
> subdatastat-downbytedropmbrexc-stdqcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytedropmbrexc-stdqcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qcinongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (Non-GBR) Type: Counter | Int64
> subdatastat-downbytedropmbrexc-qcigbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Non-Standard QCI (GBR) Type: Counter | Int64
> subdatastat-downbytedropmbrexc-totgbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total GBR Type: Counter | Int64
> subdatastat-downbytedropmbrexc-totnongbr | Subscriber Data Statistics - Downlink bytes Drop mbr exceed - Total NON-GBR Type: Counter | Int64
> apnambrratelimit-uppktdrop | APN AMBR Rate Limiting Statistics - Uplink packets dropped Type: Counter | Int32
> apnambrratelimit-downpktdrop | APN AMBR Rate Limiting Statistics - Downlink packets dropped Type: Counter | Int32
> apnambrratelimit-upbytedrop | APN AMBR Rate Limiting Statistics - Uplink bytes dropped Type: Counter | Int64
> apnambrratelimit-downbytedrop | APN AMBR Rate Limiting Statistics - Downlink bytes dropped Type: Counter | Int64
> ipv4-pdn-to-user-pkt | Subscriber Data Statistics - IPv4 PDN to user packets Type: Counter | Int64
> ipv4-pdn-to-user-byte | Subscriber Data Statistics - IPv4 PDN to user bytes Type: Counter | Int64
> ipv4-pdn-from-user-pkt | Subscriber Data Statistics - IPv4 PDN from user packets Type: Counter | Int64
> ipv4-pdn-from-user-byte | Subscriber Data Statistics - IPv4 PDN from user bytes Type: Counter | Int64
> ipv6-pdn-to-user-pkt | Subscriber Data Statistics - IPv6 PDN to user packets Type: Counter | Int64
> ipv6-pdn-to-user-byte | Subscriber Data Statistics - IPv6 PDN to user bytes Type: Counter | Int64
> ipv6-pdn-from-user-pkt | Subscriber Data Statistics - IPv6 PDN from user packets Type: Counter | Int64
> ipv6-pdn-from-user-byte | Subscriber Data Statistics - IPv6 PDN from user bytes Type: Counter | Int64
> ipv4v6-pdn-ipv4-to-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv4 to user packets Type: Counter | Int64
> ipv4v6-pdn-ipv4-to-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv4 to user bytes Type: Counter | Int64
> ipv4v6-pdn-ipv4-from-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv4 from user packets Type: Counter | Int64
> ipv4v6-pdn-ipv4-from-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv4 from user bytes Type: Counter | Int64
> ipv4v6-pdn-ipv6-to-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv6 to user packets Type: Counter | Int64
> ipv4v6-pdn-ipv6-to-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv6 to user bytes Type: Counter | Int64
> ipv4v6-pdn-ipv6-from-user-pkt | Subscriber Data Statistics - IPv4v6 PDN IPv6 from user packets Type: Counter | Int64
> ipv4v6-pdn-ipv6-from-user-byte | Subscriber Data Statistics - IPv4v6 PDN IPv6 from user bytes Type: Counter | Int64
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883