> Technical Specifications
> This chapter lists physical dimensions, power specifications, mounting requirements and interface specifications for ASR 5000 system components.
> It includes the following sections:

> • | Physical Dimensions

> • | Weights

> • | Power Specifications

> • | Mounting Requirements

> • | Interface Specifications

> Physical Dimensions
> The ASR 5000 can be mounted in any standard (EIA-310-D, IEC 60297) 19-inch (482.6 mm) equipment cabinet or telecommunications rack. The table below lists the dimensions for the chassis and each component that can be placed within the chassis.
> Physical Dimensions - ASR 5000 Chassis and Components

> Component | Height | Width | Depth
> Chassis | 24.50 in. (62.23 cm) | 17.5 in. (44.45 cm) | 24.0 in. (60.96 cm)
> Application Card | 17.05 in. (46.31 cm) | 1.01in. (2.56 cm) | 14.10 in. (35.81cm)
> Line Card (half-height) | 8.59 in. (21.82 cm) | 1.01in. (2.56 cm) | 5.24 in. (13.31cm)
> XGLC (full-height) | 17.48 in. (44.40 cm) | 1.01in. (2.56 cm) | 5.24 in. (13.31cm)
> Fan Tray (Lower) | 2.50 in. (6.35 cm) | 16.25 in. (41.27 cm) | 17.25 in. (43.82 cm)
> Fan Tray (Upper) | 2.875 in. (7.30 cm) | 16.25 in. (41.27 cm) | 19.375 in. (49.21 cm)
> Power Filtering Unit (PFU) | 3.6 in. (9.14 cm) | 8.25 in. (20.96 cm) | 5.12 in. (13.00 cm)

> ‌
> Weights
> The following table identifies the maximum weights for fully-loaded systems—cards installed in all slots and all other components installed.
> ASR 5000 ComponentWeights

> Component | Weight
> Chassis
> Empty | 65 lbs. (29.48 kg)
> As Shipped (empyty chassis with PFUs, fan trays, bezels and blanking panels) | 160 lbs. (72.57 kg)
> Shipping ( as shipped chassis, shipping container and packing materials) | 251 lbs. (113.85 kg)
> Fully loaded (as shipped chassis with all slots filled with cards) | 307 lbs. (139.25 kg)
> Packet Processing Cards
> Packet Services Card (PSC) | 11.50 lbs. (5.22 kg)
> Packet Services Card 2 (PSC2) | 11.50 lbs. (5.22 kg)
> Packet Service Card 3 (PSC3) | 11.0 lbs. (4.95 kg)
> Packet Processing Card (PPC) | 11.50 lbs. (5.22 kg)
> Switch Process I/O Card (SPIO) | 1.25 lbs. (0.57 kg)
> System Management Card (SMC) | 10.00 lbs. (4.54 kg)
> Line Cards
> Channelized Line Card (CLC) | 1.25 lbs. (0.57 kg)
> Channelized Line Card 2 (CLC2) | 1.25 lbs. (0.57 kg)
> Fast Ethernet (10/100) Line Card (FELC) | 1.00 lbs. (0.45 kg)
> Fast Ethernet (10/100) Line Card 2 (FLC2) | 1.00 lbs. (0.45 kg)
> Gigabit Ethernet Line Card (GELC/GLC2) | 1.00 lbs. (0.45 kg)
> Optical Line Card (OLC) | 1.25 lbs. (0.57 kg)
> Optical Line Card 2 (OLC2) | 1.25 lbs. (0.57 kg)
> Quad Gigabit Ethernet Line Card (QGLC) | 1.25 lbs. (0.57 kg)
> Redundancy Crossbar Card (RCC) | 1.00 lbs. (0.45 kg)
> 10 Gigabit Ethernet Line Card (XGLC) | 2.25 lbs. (1.02 kg)

> ‌
> Power Specifications
> The following table provides essential power specifications for the chassis and all associated cards within the system.
> Chassis Power Requirements

> Characteristic | Value
> Input Voltage | Maximum range: -40VDC to -60VDC Nominal range: -48VDC to -60 VDC
> TUV Rated Peak Current Load | 165A @ -48 VDC
> Maximum Peak Power Load | 5760W
> Chassis Maximum Power Load | 800W
> Line Card (rear-installed) Maximum Power Load | SPIO: 15W FELC/FLC2: 13.5W GELC/GLC2: 10.5W QGLC: 15W XGLC: 25W OLC2:23W CLC2: 23W RCC: 20W
> Application Card (front-installed) Maximum Power Load | SMC: 130W PPC: 325W PSC: 250W PSC2: 325W PSC3: 330W

> ‌
> Estimating Power Requirements
> Use the following formula to estimate total power consumption for each deployed chassis.
> (Total Application Card Maximum Power Load) + (Total Line Card Maximum Power Load) + (Chassis Maximum Power Load)
> Example
> The calculation for estimating the power required for an ASR 5000 installation with 3 PSCs, 2 SMCs, 2 SPIOs, 2 RCCs, and 4 GELC/GLC2s would be:
> (250W x 3) + (130W x 2) + (20W x 2) + (13.5W x 4) + 800W = 1934W
> Mounting Requirements
> Each 24.5 in. (62.23 cm.) height chassis requires 14 Rack Units (RUs) of space. You can mount the system into any 19-inch (482.6 mm) equipment rack or telco cabinet with the mounting brackets supplied with the chassis. Additional hardware (not supplied), such as extension brackets, may be used to install the chassis in a standard 23-inch (584.2 mm) cabinet or rack. Both front and mid-mount installations are possible, depending on the position of the mounting brackets on the chassis.
> You can mount a maximum of three ASR 5000 chassis in a 2- or 4-post equipment rack or telco cabinet, provided that all system cooling and ventilation requirements are met. Three stacked chassis will occupy a minimum of 42 RUs.
> Caution: When planning chassis installation, ensure that equipment rack or cabinet hardware does not hinder air flow at any of the intake or exhaust vents. Also, make sure that the rack/cabinet hardware, as well as the ambient environment, allow the system to function within the required limits. For more information, refer to Environmental Specifications in this guide.
> Rack mounting requires the use of industry-standard (EIA-310-D, IEC 60297) equipment racks and cabinets, as well as supplier-recommended fasteners. The following figure depicts how three chassis can be mounted in a 42 RU equipment rack.
> Three ASR 5000 Chassis in a 42 RU Rack
> Interface Specifications
> Following is a list of interfaces for use within the chassis. Each interface is shown with its specific pin-out.
> Important: Some interfaces, such as an RJ-45 interface used for Ethernet connectivity, may have more than one pin-out configuration, depending on the type of cable used.
> SPIO Card Interfaces
> Each interface on the SPIO card is described below. In each accompanying figure, the interface is shown in the same orientation as the way it appears on the card.
> Console Port Interface
> The Console port is an RJ-45 RS-232 interface used to access the command line interface. The interface communicates at a baud rate of 9600 to 115,200 bps (115.2 Kbps). The default is 115,200 bps.
> The interface’s pin out detail is provided in the following figure and table.
> SPIO Console Port Pin-out
> SPIO Console Port Pin-out

> Pin | Signal Description | Signal Type
> 1 | Clear to Send (CTS) | Input
> 2 | Data set Ready (DSR) | Input
> 3 | Receive Data (RX) | Input
> 4 | Signal Ground (SGND) | N/A
> 5 | Ready to Send (RTS) | Output
> 6 | Transmit Data (TX) | Output
> 7 | Data Carrier Detect (DCD) | Input
> 8 | Data Terminal Ready (DTR) | Output

> ‌
> Console Cable Specifications
> SPIO cards are shipped with a console cable assembly that includes a 7-foot (2 meter) serial cable with RJ-45 connectors on each end, and an RJ-45-to-DB-9 adapter. Use the RJ-45-to-DB-9 adapter to connect the console cable to a terminal server or terminal emulation device such as a laptop computer. The cable’s pin-out is provided in the following figure and table.
> SPIO Console Cable Assembly
> RJ-45 to DB-9 Cable

> Signal Description | Signal Type | RJ-45 Pin | DB-9 Pin
> Clear to Send (CTS) | Input | 1 | 7
> Data set Ready (DSR) | Input | 2 | 4
> Receive Data (RX) | Input | 3 | 3
> Signal Ground (SGND) | N/A | 4 | 5
> Ready to Send (RTS) | Output | 5 | 8
> Transmit Data (TX) | Output | 6 | 2
> Data Carrier Detect (DCD) | Input | 7 | 1
> Data Terminal Ready (DTR) | Output | 8 | 6

> ‌
> To construct a RJ-45 to DB-25 cable for modem connectivity, refer to the table that follows.
> RJ-45 to DB-25 Cable

> Signal Description | Signal Type | RJ-45 Pin | DB-25 Pin
> Clear to Send (CTS) | Input | 1 | 5
> Data set Ready (DSR) | Input | 2 | 6
> Receive Data (RX) | Input | 3 | 3
> Signal Ground (SGND) | - | 4 | 7
> Ready to Send (RTS) | Output | 5 | 4
> Transmit Data (TX) | Input | 6 | 2
> Data Carrier Detect (DCD) | Output | 7 | 8
> Data Terminal Ready (DTR) | Output | 8 | 20

> ‌
> Fiber SFP Interface
> The fiber SFP interface has two host connectors that receive SFP transceivers.
> SPIO Gb Ethernet Fiber SFP Pin-out
> Fiber SFP Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | 0 dBm
> Min TX: | -9.5 dBm
> Max RX: | 0 dBm (saturation average power)
> Min RX: | -20 (typ) / -17 (max) dBm (sensitivity average power)

> ‌
> 10/100/1000 Mbps RJ-45 Interface
> The two RJ-45 interfaces are auto-sensing 10/100/1000 Ethernet (10Base-T/100Base-TX/1000Base-T) that require unshielded twisted pair (UTP) copper cable. Refer to the following figure and table for pin-outs for the RJ-45 Ethernet ports.
> SPIO RJ-45 Ethernet Interface Pin-outs
> SPIO RJ-45 Ethernet Interface Pin-outs

> Pin | 10Base-T 10Mbps Cat3 | 100Base-TXx 100Mbps Cat5 | 1000Base-Tx 1Gbps Cat5+
> 1 | TX+ | TX+ | BI DA+
> 2 | TX- | TX- | BI DA-
> 3 | RX+ | RX+ | BI DB+
> 4 | na | na | BI DC+
> 5 | na | na | BI DC-
> 6 | RX- | RX- | BI DB-
> 7 | na | na | BI DD+
> 8 | na | na | BI DD-

> ‌
> Central Office Alarm Interface
> The Central Office (CO) alarm interface is a 10-pin Molex connector supporting three dry-contact relay switches. The three normally closed (NC) relays can support normally open (NO) or NC devices. The following two figures show the pin-out details for this interface and the next figure shows an example CO alarm configuration.
> SPIO CO Alarms Interface Pin-out
> SPIO CO Alarms Interface Pin-out

> Pin | Signal
> 1 | Major Alarm - Normally closed
> 2 | Major Alarm - Common
> 3 | Major Alarm - Normally open
> 4 | Minor Alarm - Normally closed
> 5 | Minor Alarm - Common
> 6 | Minor Alarm - Normally open
> 7 | Critical Alarm - Normally closed
> 8 | Critical Alarm - Common
> 9 | Critical Alarm - Normally open
> 10 | Not Used

> ‌
> The 8-foot ((2.4 meter) CO alarm cable shipped with the chassis supports redundant SPIO card installations. The CO alarm cable is a “Y” cable, with two connectors on one end. Each connects to one of the SPIO cards. On the opposite end is a 9-pin terminal block that you can mount to the telco cabinet or equipment rack frame. The figure shows the CO Alarm cable. The following table provides the CO Alarm cable pin-outs.
> CO Alarms Cable Assembly
> CO Alarms Cable Pinout

> CO Alarms IF Pin No. | Cable Connector Pin No. | Cable Wire Color | Cable Terminal Block Position No. | Signal
> 1 | 6 | Black | 1 | Major Alarm - Normally closed
> 2 | 7 | Orange | 2 | Major Alarm - Common
> 3 | 8 | Red | 3 | Major Alarm - Normally open
> 4 | 9 | Brown | 4 | Minor Alarm - Normally closed
> 5 | 10 | Yellow | 5 | Minor Alarm - Common
> 6 | 1 | Green | 6 | Minor Alarm - Normally open
> 7 | 2 | Blue | 7 | Critical Alarm - Normally closed
> 8 | 3 | Violet | 8 | Critical Alarm - Common
> 9 | 4 | Gray | 9 | Critical Alarm - Normally open
> 10 | 5 | Not Applicable | Not Applicable | Not Applicable

> ‌
> Electrical Characteristics
> Each of the three dry-contact relay switches is rated to support a maximum switching current of 1A@30VDC. The relay contacts should not be directly connected to high current devices, such as sirens or flashing lights.
> Central Office Alarm Wiring Example
> The example in the following figure shows how each of the three dry-contact relay switches can control up to two alarming devices. In this example, the CO alarm interface is connected to a CO alarms monitoring panel. A green LED is wired to indicate a normal condition (normally closed relay). A red LED is wired to indicate an alarm condition (normally open relay).
> CO Alarm Wiring Example
> In this wiring example, with each relay switch in its NC position, the green LED is illuminated. If a relay switch were in the NO position, the red LED would be illuminated.
> BITS Timing Interface
> Important: This interface is not used on SPIOs when the system is configured to perform data services.
> BITS BNC Timing Interface
> The BNC version of the SPIO interface card uses a BNC connector. The following figure shows the BITS BNC timing interface.
> SPIO BITS BNC Timing Interface Pin-out
> BITS 3-Pin Timing Interface
> This 3-pin version of the SPIO interface card uses a 3-pin wire-wrap connector instead of a BNC interface. The following figure shows the BITS 3-wire timing interface wire-wrap pin-out.
> SPIO T1 BITS Timing Wire-Wrap Pin-out
> Fast Ethernet Line Card (FELC/FLC2) Interfaces
> Each of the eight RJ-45 interfaces available on the FELC/FLC2 supports auto-sensing 10 Base-Tx or 100 Base-Tx Ethernet interfaces.
> 10/100 Mbps RJ-45 Interface
> The RJ-45 interfaces on the Fast Ethernet line card support the following cable types and transfer rates. The following figure shows the pin-outs for the RJ-45 Ethernet ports.
> Ethernet 10/100 Line Card RJ-45 Ethernet Interface Pin-outs
> Ethernet 10/100 Line Card RJ-45 Ethernet Interface Pin-outs

> Pin | 10Base-T 10MbpsCat3 | 100Base-TX 100MbpsCat5
> 1 | TX+ | TX+
> 2 | TX- | TX-
> 3 | RX+ | RX+
> 4 | na | na
> 5 | na | na
> 6 | RX- | RX-
> 7 | na | na
> 8 | na | na

> ‌
> Gigabit Ethernet Line Card (GELC/GLC2)/Quad Gigabit Ethernet Line Card (QGLC) SFPs
> QGLC/1000Base-SX
> The 1000Base-SX fiber SFP interface on the GELC/GLC2 has one pair of fiber connectors, as shown below. The QGLC has four pairs.
> GELC/GLC2/QGLC Fiber Connector
> SX Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | 0 dBm
> Min TX: | -9.5 dBm
> Max RX: | 0 dBm (saturation average power)
> Min RX: | -20 (typ) / -17 (max) dBm (sensitivity average power)

> ‌
> QGLC/1000Base-LX Interface
> The 1000Base-LX fiber SFP interface on the Ethernet 1000 LX line card has one pair of host connectors. The QGLC has four pairs.
> QGLC/1000 Base-LX Fiber Connector
> LX Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | 0 dBm
> Min TX: | -9.5 dBm
> Max RX: | 0 dBm (saturation average power)
> Min RX: | -20 (typ) / -19 (max) dBm (sensitivity average power)

> ‌
> RJ-45 SFP Interface
> The 1000Base-T SFP interface on the Ethernet 1000/Quad Gig-E copper line cards require unshielded twisted pair (UTP) copper CAT-5 cable with BER less than 10e-10. Pin-outs for the RJ-45 Ethernet ports are:
> GELC/GLC2/QGLC RJ-45 Ethernet Interface Pin-outs
> GELC/GLC2/QGLC RJ-45 Ethernet Interface Pin-outs

> Pin | 1000Base-Tx 1Gbps Cat5+
> 1 | BI DA+
> 2 | BI DA-
> 3 | BI DB+
> 4 | BI DC+
> 5 | BI DC-
> 6 | BI DB-
> 7 | BI DD+
> 8 | BI DD-
> RX = Receive Data TX = Transmit Data BI = BI directional data DA, DB, DC, DD = Data Pair A, B, C, and D

> ‌
> 10 Gigabit Ethernet Line Card (XGLC) SFP+
> XGLC 10GBase-SR
> The 10GBase-SR fiber SFP+ interface on the XGLC has one pair of fiber connectors, as shown below.
> XGLC 10GBase-SR Fiber Connector
> XGLC 10GBase SR Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | -1.0 dBm
> Min TX: | -7.3 dBm
> Max RX: | -1.0 dBm (saturation average power)
> Min RX: | -11.1 (max) dBm (sensitivity average power)

> ‌
> XGLC 10 Base-LR Interface
> The 10GBase-LR fiber SFP+ interface on the XGLC has one pair of host connectors.
> XGLC 10GBase LR Fiber Connector
> XGLC 10GBase LR Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | 0.5 dBm
> Min TX: | -8.2 dBm
> Max RX: | 0.5 dBm (saturation average power)
> Min RX: | -12.6 (max) dBm (sensitivity average power)

> ‌
> Fiber ATM/POS OC-3 (OLC2) Multi-Mode Interface
> Fiber ATM/POS OC-3 SM IR-1 Interface
> The fiber-optic SFP interface on OLC2 Optical ATM Line Cards with the SM IR-1 interface has one pair of host connectors as shown in The following figure.
> OLC2 (ATM) SM IR-1 SFP Pin-out
> SM IR-1 Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | -8 dBm
> Min TX: | -15 dBm
> Max RX: | -8 dBm (saturation average power)
> Min RX: | -28 (max) dBm (sensitivity average power)

> ‌
> The fiber-optic SFP interface on OLC2 Optical ATM Line Cards with the multi-mode interface has one pair of host connectors as shown in figure that follows.
> OLC2 (ATM) Multi-Mode SFP Pin-out
> Multi-Mode Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | -14 dBm
> Min TX: | -19 dBm
> Max RX: | -12 dBm (saturation average power)
> Min RX: | -30 (max) dBm (sensitivity average power)

> ‌
> Channelized Line Cards
> Channelized Line Card (CLC2) with Single-mode Interface
> The optical SFP interface on the 4-port CLC2 with the single-mode interface has four pairs of connectors that receive SFP transceivers, as shown in the following figure.
> Channelized Line Cards with Single-Mode SFP Pin-out
> Single-Mode Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | -8 dBm
> Min TX: | -15 dBm
> Max RX: | -8 dBm (saturation average power)
> Min RX: | -28 (max) dBm (sensitivity average power)

> ‌
> Channelized Line Cards (CLC2) with Multi-Mode Interface
> The fiber SFP interface on the 4-port CLC2 with the multi-mode interface has four pairs of connectors that receive SFP transceivers, as shown in the following figure.
> Channelized Line Cards with Multi-Mode SFP Pin-out
> Multi-Mode Fiber Interface Transmit and Receive Levels

> Signal | Level
> Max TX: | -14 dBm
> Min TX: | -19 dBm
> Max RX: | -12 dBm (saturation average power)
> Min RX: | -30 (max) dBm (sensitivity average power)

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883