> ASN Paging Group Configuration Mode Commands
> Use the Paging Group Configuration Mode to create and manage Paging Agents for the paging and location register controller within the Access Service Network Paging Controller and Location Registry (ASN PC-LR) service.
> Important: This functionality is still in development stage.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> paging
> Configures the paging parameters within the paging group for PC-LR functionality.
> Product
> ASN PC-LR
> Privilege
> Administrator
> Syntax
> paging { cycle cycle_value | interval interval_value | node id mac_address address ip_address | offset algorithm uniform start start_value increment inc_value count count_value }
> no paging { cycle | node id mac_address | offset }
> no
> Disables the configured paging parameters within this paging group.
> cycle cycle_value
> Specifies the cycle in which the paging message is transmitted within the paging group as an integer from 0 through 65535.
> interval interval_value
> Specifies the maximum duration in frames of Paging Listening Interval; used in calculation of Paging Listening Interval.
> interval_value must be an integer from 1 through 5.
> node id mac_address address ip_address
> id mac_address: Configures the MAC address of the node in the paging group.
> mac_address must be in one of the following formats:
> nn:nn:nn:nn:nn:nn or nn-nn-nn-nn-nn-nn
> address ip_address: Specifies the IP address of the node in IPv4 dottted-decimal or IPv6 colon-separated notation.
> Important: Configure up to 128 paging nodes per paging group.
> offset algorithm uniform start start_value increment inc_value count count_value
> start start_value: Specifies the starting value of the available offset as an integer from 0 through 65535.
> increment inc_value: Specifies the distance between two offsets as n integer from 0 through 65535.
> count count_value: Specifies the number of offsets available as an integer from 0 through 65535.
> Offsets are uniformly load balanced across the available range. For this configuration:
> paging offset algorithm uniform start 10 increment 10 count 4
> the following occurs:
> if MS1, MS2,...MS100, perform IM-Entry, then offset assigned: MS1=10, MS2=20, MS3=30, MS4=40, MS5=10, MS6=20, etc.
> Usage
> Use this command to define the paging behavior of a paging group. There must be only one instance of paging parameters per paging group.
> Example
> The following example configures the paging cycle for a paging group to 10.
> paging cycle 10
> The following example configures a paging node in the group:
> paging node id 00:05:47:00:37:44 address 12.345.76.789

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883