> LTE TAI Management Database Configuration Mode Commands
> The LTE TAI Management Database Configuration Mode is used to create and manage the LTE Tracking Area Identifier (TAI) management database configuration for LTE polices configured on this system.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> tai-mgmt-obj
> Creates new, or removes/enters existing, LTE Tracking Area Identifier (TAI) object configurations.
> Product
> MME
> Privilege
> Administrator
> Syntax
> [ no ] tai-mgmt-obj object_name [ -noconfirm ]
> no
> Removes a configured TAI management object from the TAI management database.
> -noconfirm
> Executes the command without any additional prompt and confirmation from the user.
> object_name
> Specifies the name of the TAI management object and enters the LTE TAI Management Object Configuration Mode as an alphanumeric string of 1 through 64 characters.
> Usage
> Use this command to enter the LTE TAI Management Object Configuration Mode for an existing object or for a newly defined object. This command is also used to remove an existing object.
> Entering this command results in the following prompt:
> [context_name]hostname(tai-mgmt-obj)#
> LTE TAI Management Object Configuration Mode commands are defined in the LTE TAI Management Object Configuration Mode Commands chapter.
> Example
> The following command creates a TAI management object called tai-obj3 and enters the LTE TAI Management Object Configuration Mode:
> tai-mgmt-obj tai-obj3
> timezone
> Configures the timezone to be used for the UE timezone in S11 and Non Access Stratum (NAS) messages.
> Product
> MME
> Privilege
> Administrator
> Syntax
> timezone { + | - } hours value [ minutes { 0 | 15 | 30 | 45 } ]
> no timezone
> Removes the timezone configuration from the management database.
> + | -
> Specifies the offset direction from the Coordinated Universal Time (UTC).
> hours value
> Specifies the offset from UTC in hours. value must be an integer from 0 through 14.
> minutes { 0 | 15 | 30 | 45 }
> Optionally specifies the offset minutes added to the hours value.
> Usage
> Use this command to configure the timezone to be used for the UE timezone in S11 and NAS messages.
> Important: Time zone configurations at the TAI Management Object level take precedence over time zone configurations at the TAI Management Database level. If neither is configured, the system defaults to the MME time zone.
> Example
> The following command sets the timezone mapping for this management database to plus-3 hours and 15 minutes from UTC:
> timezone + hours 3 minutes 15

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883